{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["DOORS v.1.0 export July 2025","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"DOORS v.1.0 export July 2025","index":0,"n_rows":50195,"n_cols":12,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[{"$nulls":9},"EARM"]
["ECSS Source Reference","DOORS Project","ECSS Req. Identifier","Type","IE PUID","RCM Version","ECSS Change Status","Original requirement","Text of Note of Original requirement","4. Applicability\n(A/M/D/N)","5. Modified or New requirement\n(full text)","6. Justification\n(only in case of M, D or N in colum 4)"]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","4a","Requirement","ECSS-Q-ST-30-11_0140001",1,"Created","The user of this Standard shall verify that the ordered assurance level of procured components is compatible with the intended application."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2a","Requirement","ECSS-Q-ST-30-11_0140002",1,"Created","Derating shall be applied in consideration of temperature limits recommended."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2b","Requirement","ECSS-Q-ST-30-11_0140003",1,"Created","The derating requirements of this Standard shall not be used as a justification to upgrade the quality level of components."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2c","Requirement","ECSS-Q-ST-30-11_0140004",1,"Created","The derating requirements shall be taken into account at the beginning of the design cycle of an equipment for any consequential design trade-off to be made. Specific attention shall be paid to, for example, breadboards and engineering models where parameter derating was not considered."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2d","Requirement","ECSS-Q-ST-30-11_0140005",1,"Created","Component families and groups excluded in this Standard are due to the lack of experimental data and failure history. For these components, the user shall consult a component design and reliability specialist to apply the requirements of this Standard."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2e","Requirement","ECSS-Q-ST-30-11_0140006",1,"Created","Components may be excluded from this Standard if they are used for short durations of less than one month provided the device ratings are not exceeded; for example, components used in solar generator deployment systems, redundancy commutation and launchers (except in some specific cases, noted family by family). In these cases, the designer shall ensure that the applied stress level does not exceed the component maximum rating. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2f","Requirement","ECSS-Q-ST-30-11_0140007",1,"Created","In the same way, during a test (e.g. qualification and EMC), derating requirements are applied on operating conditions and not on test conditions, even if during some periods, the temperature range reached is higher than the derated value. However, the specified maximum ratings shall not be exceeded. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2g","Requirement","ECSS-Q-ST-30-11_0140008",1,"Created","Derating shall be applied on normal operating conditions and not on the fault condition. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.3.2h","Requirement","ECSS-Q-ST-30-11_0140009",1,"Created","Where components are required to operate in protection mode or in fail-safe mode in order to prevent failure propagation (e.g. short-circuit protection), the components concerned shall meet the derating requirements and application rules when performing the protection or fail-safe function under the worst failure case (i.e. highest stress applied to the components that can last throughout the mission)."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-30-11_0140010",1,"Created","If ratings are provided for transients or surge conditions, the same derating figures as for steady-state equivalent parameters shall be used."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.4.2b","Requirement","ECSS-Q-ST-30-11_0140011",1,"Created","If ratings are not provided for transient or surge conditions, then it shall be assured that the transient or surge values are below the steady-state specified maximum ratings."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.4.2c","Requirement","ECSS-Q-ST-30-11_0140012",1,"Created","Repetitive transients, e.g. in a switching DC/DC converter operation, and clock transmission lines, shall not exceed the derated steady-state values, superseded by no more than 90 % of the rated manufacturer values if not compatible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.4.2d","Requirement","ECSS-Q-ST-30-11_0140013",1,"Created","Where radiation sensitive components are identified, it is the user’s responsibility that the chosen component technologies are suitable and that the mitigation factors, such as shielding, meet the customer’s requirement. The electrical derating shall be in accordance with this Standard."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-30-11_0140014",1,"Created","For hybrids, individual components shall be in conformance with their respective derating rules."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.2.1a","Requirement","ECSS-Q-ST-30-11_0140015",1,"Created","The capacitor stress sum value of steady-state voltage, AC voltage shall not exceed the load ratios specified hereunder. For transients refer to clause 5.4."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.2.1b","Permission","ECSS-Q-ST-30-11_0140079",1,"Created","Multilayer capacitors with a DC voltage rating less than 100 V may be used in low voltage (less than 10 V) continuous applications provided they have been submitted to a low voltage (1,5 V) 85 % humidity at 85 °C test or other approved method. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.2.1c","Recommendation","ECSS-Q-ST-30-11_0140080",1,"Created","Physical limitation for type II: maximum surge dV/dt approximate to 100 V/ms. This should be verified with the manufacturer."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.2.1d","Recommendation","ECSS-Q-ST-30-11_0140081",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1a","Requirement","ECSS-Q-ST-30-11_0140019",1,"Created","The capacitor stress sum value of steady-state voltage and AC voltage shall not exceed the load ratio specified hereunder. For transients refer to clause 5.4."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1b","Requirement","ECSS-Q-ST-30-11_0140020",1,"Created","100 % surge current screening shall be applied for all surface mounted capacitors types."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1c","Requirement","ECSS-Q-ST-30-11_0140021",1,"Created","Surge current shall be derated to 75 % of the Isurge max. Isurge max is defined as Vrated/(ESR+Rs). Vrated is the maximum rated voltage, ESR is the maximum specified value and Rs is the value of series resistance specified in the circuit for surge current testing as defined in the applicable procurement specification."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1d","Requirement","ECSS-Q-ST-30-11_0140022",1,"Created","Reverse voltage shall not exceed 75 % of the manufacturer’s specified maximum value for the reverse voltage."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1e","Requirement","ECSS-Q-ST-30-11_0140023",1,"Created","Ripple power shall never exceed 50 % of the manufacturer’s specified maximum value."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.3.1f","Recommendation","ECSS-Q-ST-30-11_0140082",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.4.1a","Requirement","ECSS-Q-ST-30-11_0140025",1,"Created","Reverse voltage shall not exceed 75 % of the manufacturer’s specified maximum value for the reverse voltage."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.4.1b","Requirement","ECSS-Q-ST-30-11_0140026",1,"Created","Manufacturer’s ratings for ripple power or current shall never be exceeded. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.4.1c","Recommendation","ECSS-Q-ST-30-11_0140083",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.5.1a","Requirement","ECSS-Q-ST-30-11_0140028",1,"Created","Self healing requirements for polyethylene terepthalate (PET, polyester) film:\n    1. To have a clearing process in any case, the minimum energy available shall be greater than the manufacturer’s specified value (typical self healing energy is 5 mJ minimum).\n    2. To prevent any risk of destruction during self healing, capacitor banks shall not provide energy greater than 15 J."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.5.1b","Requirement","ECSS-Q-ST-30-11_0140029",1,"Created","For other films, clearing recommendations from manufacturers shall be followed."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.5.1c","Recommendation","ECSS-Q-ST-30-11_0140084",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.6.1a","Recommendation","ECSS-Q-ST-30-11_0140085",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.7.1a","Recommendation","ECSS-Q-ST-30-11_0140086",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.8.1a","Recommendation","ECSS-Q-ST-30-11_0140087",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.9.1a","Recommendation","ECSS-Q-ST-30-11_0140088",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.10.1a","Recommendation","ECSS-Q-ST-30-11_0140089",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.11.1a","Requirement","ECSS-Q-ST-30-11_0140036",1,"Created","For power connectors, power and return lines shall be separated by at least one unassigned contact to reduce the short-circuit risk."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.11.1b","Requirement","ECSS-Q-ST-30-11_0140037",1,"Created","Connector savers shall be used during testing of equipment to minimize number of mating and demating cycles."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.11.1c","Requirement","ECSS-Q-ST-30-11_0140038",1,"Created","When multi-pin connectors are close to one another, they shall be configured such that mating with a wrong connector is not possible or the contact assignments shall be chosen such that mating with a wrong connector does not cause damage to the unit itself nor to any other element of the system."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.11.1d","Requirement","ECSS-Q-ST-30-11_0140039",1,"Created","The connector and its constituent parts shall be from the same manufacturer."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.12.1a","Requirement","ECSS-Q-ST-30-11_0140040",1,"Created","Connector savers shall be used during testing of equipment to minimize number of mating and demating cycles."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.14.1a","Requirement","ECSS-Q-ST-30-11_0140041",1,"Created","Some diodes can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60. Where power cycling is critical this should be considered."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.15.1a","Requirement","ECSS-Q-ST-30-11_0140042",1,"Created","Some diodes can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.17.1a","Requirement","ECSS-Q-ST-30-11_0140043",1,"Created","Fuses shall be avoided whenever possible. The derating requirements in 6.17.2 (below) are only applicable to Cermet types. The application and the deratings of other fuse technologies shall be justified."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.17.1b","Requirement","ECSS-Q-ST-30-11_0140044",1,"Created","The largest fuse rating compatible with the source capability shall be used."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.17.1c","Requirement","ECSS-Q-ST-30-11_0140045",1,"Created","The power supply shall be capable of delivering three times the specified fuse rated current in order to obtain short fusing times."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.18.1a","Requirement","ECSS-Q-ST-30-11_0140046",1,"Created","For custom-made inductors and transformers, the maximum rated temperature shall be evaluated taking into consideration the temperature characteristics of the materials used."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.19.1a","Requirement","ECSS-Q-ST-30-11_0140047",1,"Created","Some devices can be radiation sensitive: this shall be recorded and approved in accordance with ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.20.1a","Requirement","ECSS-Q-ST-30-11_0140048",1,"Created","Some devices can be radiation sensitive: this shall be recorded and approved in accordance with ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.21.1a","Requirement","ECSS-Q-ST-30-11_0140049",1,"Created","Some linear circuits can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.21.1b","Requirement","ECSS-Q-ST-30-11_0140050",1,"Created","Additional margins can be applied for radiation effects."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.22.1a","Requirement","ECSS-Q-ST-30-11_0140051",1,"Created","Some linear circuits can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.23.1a","Requirement","ECSS-Q-ST-30-11_0140052",1,"Created","Some MMICs can be radiation sensitive: the choice of MMICs shall be based on suitability and application. Justification shall be in accordance with ECSS-Q-ST-60 and provided in accordance with this Standard, and at the design reviews."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.23.2a","Requirement","ECSS-Q-ST-30-11_0140053",1,"Created","Each discrete cell (capacitors, resistors, diodes and transistors) constituting analogue custom MMICs shall be derated in accordance with this document’s requirements for the applicable family. For digital cells, apply the derating rules applicable to integrated circuits."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.23.2b","Requirement","ECSS-Q-ST-30-11_0140054",1,"Created","When operational reliability data is available, the compression level shall be derated to 2 dB under the highest compression level showing no drift. MMICs having no compression data shall not be submitted to more than 1 dB of compression."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.24.1a","Requirement","ECSS-Q-ST-30-11_0140055",1,"Created","For all ICs not considered in the previous subgroups, the following derating rules shall be followed:\n    1. Manufacturer’s derating values.\n    2. Maximum junction temperature: 110 °C or Tj max - 40 °C, whichever is lower.\n    3. For the part of the IC similar to logic ICs, apply the derating rules for logic subgroups, for the part similar to linear ICs, apply the derating rules for linear subgroups and so forth."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.24.1b","Requirement","ECSS-Q-ST-30-11_0140056",1,"Created","Some integrated circuits can be radiation sensitive: this shall be recorded and approved in accordance with ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1a","Requirement","ECSS-Q-ST-30-11_0140057",1,"Created","The coil supply voltage shall be within the specified voltage range or between the specified rated and the maximum coil voltage."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1b","Requirement","ECSS-Q-ST-30-11_0140058",1,"Created","The minimum coil pulse duration for latching relays shall be 10 times the sum of latch time (tL) and bounce time (tB) or 30 ms, whichever is greater."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1c","Requirement","ECSS-Q-ST-30-11_0140059",1,"Created","Current derating does not apply to contacts that only carry current and do not switch it or to contacts that switch at zero current. In the latter case, the number of operations is limited to the qualified number of operations."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1d","Requirement","ECSS-Q-ST-30-11_0140060",1,"Created","Rated contact load voltage should not be exceeded since it has a strong impact on the contact current: this shall be recorded and approved in accordance with ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1e","Requirement","ECSS-Q-ST-30-11_0140061",1,"Created","A double throw contact shall not be used to switch a load (movable contact) between a power supply and ground (stationary contacts). This type of configuration may be accepted in the following conditions:\n    1. when switching off the power supply the other stationary contact is not connected to ground, or\n    2. the potential difference between stationary contacts is less than 10 V and the switched current less than 0,1 A."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1f","Requirement","ECSS-Q-ST-30-11_0140062",1,"Created","Paralleled relays shall not be used to increase current switching capabilities of contacts. When relays are paralleled for redundancy, in order to increase the system’s reliability, the sum of the paralleled currents shall not exceed the contact current rating. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.25.1g","Requirement","ECSS-Q-ST-30-11_0140063",1,"Created","Suppression diodes shall not be used inside relays. "]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.26.1.1a","Requirement","ECSS-Q-ST-30-11_0140064",1,"Created","The mentioned temperatures cited below refer to case temperatures."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.26.1.9a","Requirement","ECSS-Q-ST-30-11_0140065",1,"Created","Average power < 50 % of nominal rating\n \nwhere\nVp\tis the pulse amplitude\nR\tis the resistance\ntp\tis the pulse width\nT\tis the cycle duration"]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.26.1.10a","Requirement","ECSS-Q-ST-30-11_0140066",1,"Created","If ratings are provided for transient or surge condition, the same derating figures as for steady-state equivalent parameters shall be used."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.26.1.10b","Requirement","ECSS-Q-ST-30-11_0140067",1,"Created","If ratings are not provided for transient or surge condition, then it shall be assured that the transient or surge values are below the steady-state specified ratings."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.26.2a","Requirement","ECSS-Q-ST-30-11_0140068",1,"Created","Actual rated power shall be specified in the applicable heater design drawing. It shall be determined from the specified heating area (s) in cm2 taking into account the thermal properties of the mounted heater in the application."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.28.1a","Requirement","ECSS-Q-ST-30-11_0140069",1,"Created","Some transistors can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.29.1a","Requirement","ECSS-Q-ST-30-11_0140070",1,"Created","Only SEE radiation characterized MOSFETs shall be used in space applications."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.29.1b","Requirement","ECSS-Q-ST-30-11_0140071",1,"Created","The user shall consider power cycling when this is critical to his application."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.30.1a","Requirement","ECSS-Q-ST-30-11_0140072",1,"Created","Some transistors can be radiation sensitive: the issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.31.1a","Requirement","ECSS-Q-ST-30-11_0140073",1,"Created","Some transistors can be radiation sensitive: this issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.33.1a","Requirement","ECSS-Q-ST-30-11_0140074",1,"Created","Light emitting diodes can be radiation sensitive, in particular, there is a high sensitivity to proton displacement damage: this issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.33.1b","Requirement","ECSS-Q-ST-30-11_0140075",1,"Created","Opto-couplers can be radiation sensitive, in particular, operation at low diode currents increases radiation sensitivity: this issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.33.1c","Requirement","ECSS-Q-ST-30-11_0140076",1,"Created","Photo-transistors can be radiation sensitive: this issue shall be recorded in the design file and the components selection shall be reviewed and approved as described in ECSS-Q-ST-60."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.34.1a","Requirement","ECSS-Q-ST-30-11_0140077",1,"Created","For connectorized components, connector savers shall be used during testing of equipment to minimize number of mating and demating cycles."]
["ECSS-Q-ST-30-11C","ECSS - Superseded v1.0","6.36a","Requirement","ECSS-Q-ST-30-11_0140078",1,"Created","For hybrids, individual components shall be in conformance with their respective derating rules."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.1a","Requirement","ECSS-Q-ST-70-13_0610001",1,"Created","The supplier shall identify, manage and process materials and parts with hazardous characteristics according to ECSS-Q-ST-40."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.1b","Requirement","ECSS-Q-ST-70-13_0610002",1,"Created","The supplier shall keep the health and safety precautions according to the supplier’s national safety regulations."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-70-13_0610003",1,"Created","The supplier shall prepare the material samples according to the process specifications or manufacturer’s data."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1b","Requirement","ECSS-Q-ST-70-13_0610004",1,"Created","The material samples shall be representative of batch variance."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1c","Requirement","ECSS-Q-ST-70-13_0610005",1,"Created","If it is not practicable to test completed assemblies, the supplier shall submit samples made from the same materials and by the same processes as those used in the manufacture of the assemblies."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1d","Requirement","ECSS-Q-ST-70-13_0610006",1,"Created","The sample for testing shall have clean flat surfaces which do not overlap the sample holder described in clause 5.1.4."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1e","Requirement","ECSS-Q-ST-70-13_0610007",1,"Created","The width of the test sample surface face shall be at least equal to the width of the tape used in the test procedure."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1f","Requirement","ECSS-Q-ST-70-13_0610008",1,"Created","The nominal tape width shall be 20 mm."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1g","Requirement","ECSS-Q-ST-70-13_0610009",1,"Created","The supplier shall specify the number of samples to be taken from a qualification batch, test programme, or production batch at the start of the test in conformance with the DRD in Annex A.."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1h","Requirement","ECSS-Q-ST-70-13_0610010",1,"Created","The supplier shall test at least ten test samples."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1i","Requirement","ECSS-Q-ST-70-13_0610011",1,"Created","If it is not practicable to obtain test samples from the finished article, the supplier shall furnish bonded test samples for the test.\n    ","NOTE These samples are not used for any other purpose than the designated test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1j","Requirement","ECSS-Q-ST-70-13_0610012",1,"Created","The supplier shall furnish a certificate of conformity for the purpose of traceability.\n    ","NOTE This certificate of conformity is delivered by the manufacturer in order to provide evidence that the product is compliant with the manufacturer’s process."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.1k","Requirement","ECSS-Q-ST-70-13_0610013",1,"Created","The supplier shall mark all test samples with identification to maintain traceability but in such a way as not to degrade the quality of the sample during testing."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.2a","Requirement","ECSS-Q-ST-70-13_0610014",1,"Created","The suppler shall perform the same cleaning and other treatments of the sample as that applied to the finished article, which the sample is intended to represent, prior to integration into the spacecraft."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.2b","Requirement","ECSS-Q-ST-70-13_0610015",1,"Created","The supplier shall not carry out further cleaning or other treatments."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.3a","Requirement","ECSS-Q-ST-70-13_0610016",1,"Created","The supplier shall handle the samples only with clean nylon or lint-free gloves."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.3b","Requirement","ECSS-Q-ST-70-13_0610017",1,"Created","The supplier shall store the samples in a controlled area, with an ambient temperature of (22 ± 3) °C and relative humidity of (55 ± 10) %."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.3c","Requirement","ECSS-Q-ST-70-13_0610018",1,"Created","The supplier shall shield coated surfaces from contact by using polyethylene or polypropylene bags or sheets."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.3d","Requirement","ECSS-Q-ST-70-13_0610019",1,"Created","The supplier shall avoid physical damage by packing the polyethylene or polypropylene-wrapped workpieces in clean, dust- and lint-free material."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.3e","Requirement","ECSS-Q-ST-70-13_0610020",1,"Created","The supplier shall label limited-life materials with their shelf lives and dates of manufacture, or date of delivery if date of manufacture is not known."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.4.1a","Requirement","ECSS-Q-ST-70-13_0610021",1,"Created","The supplier shall identify materials submitted for testing in conformance to annex A of ECSS-Q-ST-70-02."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.2.4.2a","Requirement","ECSS-Q-ST-70-13_0610022",1,"Created","The supplier shall identify assemblies submitted for testing, as a minimum, by:\n    1. trade name and batch number;\n    2. name of manufacturer or supplier through whom the purchase was made;\n    3. configuration control status of the assembly."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.3.1a","Requirement","ECSS-Q-ST-70-13_0610023",1,"Created","The work area shall be clean and free of dust."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.3.1b","Requirement","ECSS-Q-ST-70-13_0610024",1,"Created","The supplier shall filter the air used for ventilation to prevent contamination of the sample."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.3.2a","Requirement","ECSS-Q-ST-70-13_0610025",1,"Created","The supplier shall environmentally condition the sample for a nominal 24 hour period at (22 ± 3) °C with a relative humidity of (55 ± 10) %.\n    ","NOTE 1 The humidity requirement can be achieved either in a conditioning room, or by dessicators filled with silica gel or a saturated salt solution.\nNOTE 2 A saturated salt solution of calcium nitrate gives approximately 51 % relative humidity at the testing temperature.\n"]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.1a","Requirement","ECSS-Q-ST-70-13_0610026",1,"Created","The supplier shall use the equipment as detailed in clauses 5.1.4.2 and 5.1.4.3."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.2a","Requirement","ECSS-Q-ST-70-13_0610027",1,"Created","The supplier shall employ a power-driven machine capable of maintaining a specified constant rate of loading and able to be used for both tensile and compressive testing."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.2b","Requirement","ECSS-Q-ST-70-13_0610028",1,"Created","The machine shall have a fixed or essentially stationary member supporting a load cell and the tape holder."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.2c","Requirement","ECSS-Q-ST-70-13_0610029",1,"Created","A movable member shall carry the sample holder."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.2d","Requirement","ECSS-Q-ST-70-13_0610030",1,"Created","The applied compressive and tensile loads, as measured and recorded, shall be accurate within 1 percent of the load."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.2e","Requirement","ECSS-Q-ST-70-13_0610031",1,"Created","The rate of travel of the sample holder shall be at a nominal rate of 0,2 cm/min."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.3a","Recommendation","ECSS-Q-ST-70-13_0610074",1,"Created","The tape holder should be of a design similar to that depicted in Figure 5-1."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.3b","Requirement","ECSS-Q-ST-70-13_0610033",1,"Created","The part shall be screwed into the fixed member of the testing machine or be located firmly on it."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.3c","Requirement","ECSS-Q-ST-70-13_0610034",1,"Created","The supplier shall clamp a length of pressure-sensitive tape from one tape holder over the rubber block to the other tape holder."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.3d","Requirement","ECSS-Q-ST-70-13_0610035",1,"Created","The surface of the pressure-sensitive tape in contact with the flat surface of the rubber block shall be 4 cm2 ± 5 %."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.4a","Requirement","ECSS-Q-ST-70-13_0610036",1,"Created","The sample holder shall be firmly located beneath the tape holder on the movable member of the testing machine.\n    ","NOTE 1 A suitable design is seen in Figure 5-1.\nNOTE 2 This preferred system utilizes “top hat” supports onto which individual samples can be mechanically clamped or bonded in such a way that there is no relative movement between the support and the test sample at any time during the test cycle."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.4b","Requirement","ECSS-Q-ST-70-13_0610037",1,"Created","In case a “top hat” sample support is used, it shall slide into a horizontal fixture slot in such a way that its top surface is parallel to and directly beneath the rubber face of the tape holder."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.1.4.5a","Requirement","ECSS-Q-ST-70-13_0610038",1,"Created","The supplier shall employ a range of pressure-sensitive tapes for the tests with peel adhesion strengths of 220, 330, 440 and 670 g/cm, all with a tolerance of ± 10 %."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.1.1a","Requirement","ECSS-Q-ST-70-13_0610039",1,"Created","The supplier shall locate the test sample on the sample holder in conformance with the requirements stated in clause 5.1.4.3."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.1.1b","Requirement","ECSS-Q-ST-70-13_0610040",1,"Created","If an adhesive bond is used between the sample and the sample support, this shall in no way interfere with the area under test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.1.1c","Requirement","ECSS-Q-ST-70-13_0610041",1,"Created","The supplier shall ensure that there is no physical or chemical interaction between any adhesive employed during sample preparation and the sample materials."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.1.2a","Requirement","ECSS-Q-ST-70-13_0610042",1,"Created","The supplier shall condition the loaded sample support for a nominal 24 hours in conformance with the requirements stated in clause 5.1.3.2 before the test starts."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.2a","Recommendation","ECSS-Q-ST-70-13_0610076",1,"Created","The supplier should run the peel and pull-off test as described in Annex B."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.2b","Requirement","ECSS-Q-ST-70-13_0610044",1,"Created","If the supplier uses a different procedure, the supplier shall submit it for customer approval."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.2.3a","Requirement","ECSS-Q-ST-70-13_0610045",1,"Created","The supplier shall apply the conditions specified in clause 5.1.2.3 unless other post test disposal instructions are given."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3a","Requirement","ECSS-Q-ST-70-13_0610046",1,"Created","The supplier shall classify samples which have been tested and are not seen to be disturbed in any way by the processing described in clause 5.2.2 as having passed this test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3b","Requirement","ECSS-Q-ST-70-13_0610047",1,"Created","The supplier shall examine samples in detail, which have been disturbed during the test sequence."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3c","Requirement","ECSS-Q-ST-70-13_0610048",1,"Created","The supplier shall carry out a visual examination for sample defects at ×7 magnification."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3d","Recommendation","ECSS-Q-ST-70-13_0610077",1,"Created","In case defects are detected at ×7 magnification, the supplier should use higher magnifications during further analysis for locating microscopic defects on any fracture surfaces."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3e","Requirement","ECSS-Q-ST-70-13_0610050",1,"Created","The supplier shall report defects and the appearance of the fracture.\n    ","NOTE 1 Defects for instance can be air bubbles or material inclusions.\nNOTE 2 Appearance of the fracture for instance can be rough, ductile, smooth or brittle."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3f","Requirement","ECSS-Q-ST-70-13_0610051",1,"Created","The supplier shall state the particular material or interface along which the fracture path has propagated through the test sample.\n    ","NOTE This can be wholly or partly an adhesion fracture, a cohesive separation or an adherent fracture as schematically drawn in Figure C-1."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3g","Requirement","ECSS-Q-ST-70-13_0610052",1,"Created","The supplier shall take a photographic record of the tested samples at appropriate level of magnification.\n    ","NOTE Typical topographical features are recorded at ×2, ×20, ×50, ×100, ×250, ×500 or ×1000 magnifications."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3h","Requirement","ECSS-Q-ST-70-13_0610053",1,"Created","The supplier shall agree with the customer on the granularity level of failure analysis to be performed on failed samples, prior to the test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.3i","Requirement","ECSS-Q-ST-70-13_0610054",1,"Created","The supplier shall perform the failure analysis as agreed with the customer.\n    ","NOTE This failure analysis can include metallographic studies, chemical analysis or scanning electronic microscopy."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.1a","Requirement","ECSS-Q-ST-70-13_0610055",1,"Created","The supplier shall retain the quality records for at least ten years or in conformance with project business agreement requirements, and in conformance with the Test result sheet - DRD in Annex A.\n    ","NOTE Example of such quality records are logbooks."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-70-13_0610056",1,"Created","The supplier shall disposition any nonconformance which is observed in respect of the test process in conformance with the quality assurance requirements specified in ECSS-Q-ST-10-09."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.3a","Requirement","ECSS-Q-ST-70-13_0610057",1,"Created","The supplier shall use only measuring equipment calibrated to traceable reference standard."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.3b","Requirement","ECSS-Q-ST-70-13_0610058",1,"Created","The supplier shall record any suspected or actual equipment failure as a project nonconformance report according to ECSS-Q-ST-20.\n    ","NOTE This is to ensure that previous results can be examined to ascertain whether or not re-inspection and retesting is required."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.3c","Requirement","ECSS-Q-ST-70-13_0610059",1,"Created","The supplier shall notify the customer of the nonconformance details."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","5.4.4a","Requirement","ECSS-Q-ST-70-13_0610060",1,"Created","The supplier shall maintain traceability throughout the process from incoming inspection to final test, including details of test equipment and personnel employed in performing the task."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1a","Requirement","ECSS-Q-ST-70-13_0610061",1,"Created","The test result sheet shall contain the trade names of the materials under test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1b","Requirement","ECSS-Q-ST-70-13_0610062",1,"Created","The test result sheet shall contain the batch numbers of the materials under test."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1c","Requirement","ECSS-Q-ST-70-13_0610063",1,"Created","The test result sheet shall contain name of manufacturer or supplier through whom the purchase was made."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1d","Requirement","ECSS-Q-ST-70-13_0610064",1,"Created","The test result sheet shall contain summary of the preparation and conditioning schedule.\n    ","NOTE This can be for instance the mixing proportions, coating thickness, cure time and temperature, post-cure or cleaning procedure."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1e","Requirement","ECSS-Q-ST-70-13_0610065",1,"Created","The test result sheet shall contain details of the testing room environment conditions and test equipment."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1f","Requirement","ECSS-Q-ST-70-13_0610066",1,"Created","The test result sheet shall contain details of the test parameters outlined in Annex B.\n    ","NOTE This also includes any variation in testing environment conditions."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1g","Requirement","ECSS-Q-ST-70-13_0610067",1,"Created","The test result sheet shall contain details of equipment used for visual, mechanical, chemical and physical property measurement or inspection, as outlined in Annex B and test specifications where they exist."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1h","Requirement","ECSS-Q-ST-70-13_0610068",1,"Created","The test result sheet shall contain the number of sample tests."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1i","Requirement","ECSS-Q-ST-70-13_0610069",1,"Created","The test result sheet shall contain the results of the values obtained for peel or pull-off strength."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1j","Requirement","ECSS-Q-ST-70-13_0610070",1,"Created","The test result sheet shall contain the peel strength indicated by the manufacturer of the pressure-sensitive tape used."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1k","Requirement","ECSS-Q-ST-70-13_0610071",1,"Created","The test result sheet shall contain the results of any failure analysis carried out according to clause 5.3."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1l","Requirement","ECSS-Q-ST-70-13_0610072",1,"Created","The test result sheet shall contain the mode of fracture and any photographic records.\n    ","NOTE An indication of the various fracture line is given in Figure C-1."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0","A.2.1m","Requirement","ECSS-Q-ST-70-13_0610073",1,"Created","In case of failures, the test result sheet shall contain the following details of failure mode:\n    1. deficient design;\n    2. poor workmanship;\n    3. wrong fabrication or application procedure;\n    4. wrong choice of materials;\n    5. others."]
["ECSS-Q-ST-70-13C","ECSS - Superseded v1.0",null,"Permission","ECSS-Q-ST-70-13_0610078",1,"Created","The supplier may use the template given in Figure A-1."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.1a","Requirement","ECSS-Q-ST-60_0480001",1,"Created","The supplier shall establish and implement throughout the duration of the business agreement a component programme which ensures that the requirements of the project as defined by the customer and the supplier in the related business agreement are in compliance with this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.2.1a","Requirement","ECSS-Q-ST-60_0480002",1,"Created","The supplier shall identify the organization responsible for the management of the component programme, and describe the organization’s approaches (including the procurement system and its rationale) and capability to efficiently implement, manage, and control the component requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.2.1b","Requirement","ECSS-Q-ST-60_0480003",1,"Created","The supplier’s organization shall comply with all the requirements of ECSS-M-ST-10."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.2.2a","Requirement","ECSS-Q-ST-60_0480004",1,"Created","The supplier shall prepare a Component Control Plan (CCP) in conformance with its DRD in Annex A."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.2.2b","Permission","ECSS-Q-ST-60_0480446",1,"Created","The CCP may be part of the overall project PA plan."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.2.2c","Requirement","ECSS-Q-ST-60_0480006",1,"Created","The supplier shall submit the CCP to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.3a","Requirement","ECSS-Q-ST-60_0480007",1,"Created","At supplier's level, the Parts Control Board (PCB) shall be chaired by a member of the supplier’s PA team with designated responsibility for components management. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.3b","Requirement","ECSS-Q-ST-60_0480008",1,"Created","The composition of the PCB shall as a minimum include additionally the suppliers’ parts engineer, the customer’s representative and the lower tier subcontractor parts engineers.\n    ","NOTE The approval of the selection and usage of EEE parts are implemented through Parts Control Boards (PCBs) held between the customer and the supplier (or lower tier subcontractor)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.3c","Permission","ECSS-Q-ST-60_0480447",1,"Created","Other pertinent experts from the customer or suppliers may also participate, on request."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.3d","Requirement","ECSS-Q-ST-60_0480010",1,"Created","Depending on the progress of the program, the main PCB activities shall be:\n    1. Review and approval of the supplier's EEE component control plan and any associated documents,\n    2. Parts type reduction and standardization,\n    3. Parts approval including evaluation activities,\n    4. Problem assessment (e.g. alerts, nonconformances, RFD, RFW and delivery delays)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4a","Requirement","ECSS-Q-ST-60_0480011",1,"Created","For each equipment, its supplier shall issue a DCL in an editable electronic format, identifying all component types needed. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4b","Requirement","ECSS-Q-ST-60_0480012",1,"Created","This list shall be kept under configuration control (issue and identification of changes). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4c","Requirement","ECSS-Q-ST-60_0480013",1,"Created","The DCL shall be issued as a minimum at PDR and CDR (as designed) and at flight hardware delivery (as built)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4d","Requirement","ECSS-Q-ST-60_0480014",1,"Created","After equipment CDR, all modifications affecting the PAD information shall be implemented, in the \"as design\" DCL, through the CN / CR process and submitted to the customer for approval.\n    ","NOTE For PAD generation, see 4.2.4d."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4e","Requirement","ECSS-Q-ST-60_0480015",1,"Created","The “as design” DCL shall be sent to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4f","Requirement","ECSS-Q-ST-60_0480016",1,"Created","Any change of parts during equipment manufacturing (e.g. type and manufacturer) shall be handled through RFWs submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4g","Requirement","ECSS-Q-ST-60_0480017",1,"Created","The “as built” DCL reflecting the actual EEE parts assembled into the flight hardware and their date code, shall be provided to the customer for review at the delivery of the flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.4h","Requirement","ECSS-Q-ST-60_0480018",1,"Created","The content of the DCL shall be in conformance with its DRD in Annex B."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.5a","Requirement","ECSS-Q-ST-60_0480019",1,"Created","EEE components used in GSE, which are physically and directly interfacing to flight hardware, shall meet the requirements of this document."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.1.5b","Requirement","ECSS-Q-ST-60_0480020",1,"Created","Flight hardware connectors interfaces to GSE shall be protected by connector savers."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.1a","Requirement","ECSS-Q-ST-60_0480021",1,"Created","The supplier shall ensure that the following requirements are met during his selection process:\n    1. Project requirements (e.g. quality levels, component policy, manufacturing and delivery schedules and budgets, quantities),\n    2. Design requirements (e.g. component type, case, dimensions, materials),\n    3. Production requirements (e.g. packaging, thermal and storage constraints, component mounting process),\n    4. Operational requirements (e.g. electrical, mechanical, radiation, reliability, assembly, and lifetime).\n        ","NOTE The supplier of each product is responsible for the selection of components, which enable the performance, lifetime, environmental, material, safety, quality and reliability requirements of the product of which they form a part, to be satisfied in all respects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1a","Requirement","ECSS-Q-ST-60_0480022",1,"Created","The supplier shall establish and maintain in his own facility, and ensure that his suppliers also establish and maintain, procedures for selecting and controlling all components intended for use in deliverable products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1b","Requirement","ECSS-Q-ST-60_0480023",1,"Created","Components shall be selected on the basis of proven qualification, characterization, and previous space experience and data, relevant with regard to the requirements for the programme, from manufacturers or sources (preferably European) employing effective Product Assurance Programmes in manufacturing and test."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1c","Requirement","ECSS-Q-ST-60_0480024",1,"Created","Preference shall be given to components which necessitate the least evaluation or qualification effort. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1d","Requirement","ECSS-Q-ST-60_0480025",1,"Created","Starting with the design phase of the project the supplier shall ensure maximum use of preferred (see 4.2.2.3) and qualified components to achieve an effective component reduction and standardization. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1e","Requirement","ECSS-Q-ST-60_0480026",1,"Created","When selecting items, the supplier shall check the current data, applicability of the basis of qualification, problem notifications and alerts, and adequacy of specifications. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.1f","Requirement","ECSS-Q-ST-60_0480027",1,"Created","The supplier shall implement a type reduction activity."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2a","Requirement","ECSS-Q-ST-60_0480028",1,"Created","The supplier shall ensure that non-hermetically sealed materials of components meet the requirements of ECSS-Q-ST-70 regarding off-gassing, out-gassing, flammability, toxicity and any other criteria specified for the intended use. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2b","Requirement","ECSS-Q-ST-60_0480029",1,"Created","The supplier shall evaluate the robustness of selected EEE components against the stresses induced by the assembly techniques to be employed."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2c","Requirement","ECSS-Q-ST-60_0480030",1,"Created","With respect to health and safety, beryllium oxide (except if identified in the procurement specification), cadmium, lithium, magnesium, mercury, zinc, radioactive material and all material which may cause safety hazards shall not be used."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2d","Requirement","ECSS-Q-ST-60_0480031",1,"Created","For limited life duration, known instability, safety hazards or reliability risk reasons, EEE components listed below shall not be used:\n    1. EEE components with pure tin (less than 3% Pb in case of SnPb alloy) used as a finish on the leads, terminations and external surfaces of components and packages.\n    2. Hollow core resistors,\n    3. Potentiometers (except for mechanism position monitoring),\n    4. Non-metallurgically bonded diodes,\n    5. Semiconductor dice with unglassivated active area,\n    6. Wet slug tantalum capacitors other than capacitor construction using double seals and a tantalum case,\n    7. Any component whose internal construction uses metallurgic bonding with a melting temperature not compatible with the end-application mounting conditions,\n    8. Wire link fuses < 5A,\n    9. TO5 relays without double welding of the mechanism to the header or with any type of integrated diodes inside,"]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2e","Requirement","ECSS-Q-ST-60_0480032",1,"Created","For limited life duration, known instability, safety hazards or reliability risk reasons, EEE components listed below shall not be used for new designs:\n    1. RNC90 > 100 kW,\n    2. TO3 and DO4/DO5 packages."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2f","Permission","ECSS-Q-ST-60_0480448",1,"Created","The use of pure tin in internal cavities may be authorized, on a case-by-case basis, based on the demonstration that there is no alternative product and there is no risk (supported by a technical justification)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2g","Requirement","ECSS-Q-ST-60_0480034",1,"Created","As per clause 4.2.2.2e, the justification of the use of pure tin shall be presented during a PCB for customer’s approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.2h","Requirement","ECSS-Q-ST-60_0480035",1,"Created","The use of pure tin (inside or outside the part) shall be declared in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.3a","Requirement","ECSS-Q-ST-60_0480036",1,"Created","Parts shall be chosen from the EPPL part I."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.3b","Requirement","ECSS-Q-ST-60_0480037",1,"Created","For parts not selected from the EPPL part I, the following sources shall be considered in the following order of precedence:\n    1. EPPL part II (when compatible with the project requirements)\n    2. ESCC QPL and QML, \n    3. NPSL level 1 (with disposition of the associated application notes) and level 2 or 3 (when compatible with the project requirements),\n    4. MIL QPL's and QML's."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.3c","Requirement","ECSS-Q-ST-60_0480038",1,"Created","Parts subject to export restrictions or regulations shall not be preferred. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4a","Requirement","ECSS-Q-ST-60_0480039",1,"Created","The radiation requirements for EEE components are project specific."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4b","Requirement","ECSS-Q-ST-60_0480040",1,"Created","The supplier who is responsible for the design of the piece of hardware shall demonstrate the compliance of its components selection with the radiation constraints of the project."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4c","Requirement","ECSS-Q-ST-60_0480041",1,"Created","For this demonstration, the supplier shall consider all types of radiation including cosmic (Heavy Ions), electromagnetic, trapped (charged particles - electrons, protons - in radiation belts) and solar (flares). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4d","Requirement","ECSS-Q-ST-60_0480042",1,"Created","Due consideration shall be given to the mission orbit and trajectory, the duration, the associated spatial and temporal variations of the radiation environment as well as all protective factors such as shielding. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4e","Requirement","ECSS-Q-ST-60_0480043",1,"Created","The supplier shall assess the actual radiation tolerance of the selected components for compliance with the radiation requirements in term of total dose, displacement damage and Single Events Effects (SEE). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4f","Requirement","ECSS-Q-ST-60_0480044",1,"Created","The supplier shall identify components which are not compliant with the radiation requirements as critical radiation sensitive components. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4g","Requirement","ECSS-Q-ST-60_0480045",1,"Created","The supplier shall implement a Radiation Hardness Assurance Programme, documented by a plan to be approved by the customer, for radiation sensitive components, covering the collection of all relevant information and specifying the necessary actions in terms of evaluation and procurement testing, planning and control. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4h","Requirement","ECSS-Q-ST-60_0480046",1,"Created","The supplier shall issue an Equipment Radiation Analysis document identifying all sensitive components w.r.t. the relevant radiation effects, possibly their impact and giving an adequate engineering solution (e.g. local shielding, design solution, specific test, and RVT) for the relevant equipment."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.4i","Requirement","ECSS-Q-ST-60_0480047",1,"Created","The Equipment Radiation Analysis document shall be submitted to the customer for approval.\n    ","NOTE More detailed information about the above requirements is given in ECSS-E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.5a","Requirement","ECSS-Q-ST-60_0480048",1,"Created","The supplier shall implement derating rules for components used in his designs in accordance with the requirements of ECSS-Q-ST-30-11."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.2.5b","Requirement","ECSS-Q-ST-60_0480049",1,"Created","For wire link fuses, the current derating factor shall be 50 % with an additional derating of 0,2 %/°C for an increase in the temperature of fuse body above 25 °C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1a","Requirement","ECSS-Q-ST-60_0480050",1,"Created","The supplier shall perform a component evaluation in absence of an approved demonstration that a component has the ability to conform to the requirements for functional performance, quality, dependability, and environmental resistance as required for the project."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1b","Requirement","ECSS-Q-ST-60_0480051",1,"Created","The supplier shall plan and carry out the evaluation."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1c","Requirement","ECSS-Q-ST-60_0480052",1,"Created","The scope and planning of the component evaluation shall be derived from the results of an assessment of the design and intended application of the component. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1d","Requirement","ECSS-Q-ST-60_0480053",1,"Created","An evaluation plan shall be sent to the customer for approval, and include the following elements:\n    1. Component Manufacturer Assessment,\n    2. Constructional Analysis,\n    3. Evaluation Testing,\n    4. Radiation Hardness. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1e","Requirement","ECSS-Q-ST-60_0480054",1,"Created","In the definition of the evaluation programme any information including pertinent reliability, analysis and test data from the manufacturer of the component and previous use in comparable applications shall be considered."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1f","Requirement","ECSS-Q-ST-60_0480055",1,"Created","Omission of any of these elements, or the introduction of alternative activities, shall be justified."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1g","Requirement","ECSS-Q-ST-60_0480056",1,"Created","All tests and inspections shall be carried out on representative samples of the component type from the current production of the manufacturer selected for the component procurement for the flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1h","Requirement","ECSS-Q-ST-60_0480057",1,"Created","For programmable devices, the representativeness shall include the programming hardware tools and the compatibility of the software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1i","Requirement","ECSS-Q-ST-60_0480058",1,"Created","The supplier shall review the evaluation results to determine their impact on the content of the procurement specification which shall be amended as necessary."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.1j","Requirement","ECSS-Q-ST-60_0480059",1,"Created","The supplier shall summarize the evaluation results in the evaluation report and send it to the customer for approval.\n    ","NOTE For guidance for the assessment of the space environmental aspects refer to ECSS-E-ST-10-04 and ECSS-E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.2.2a","Requirement","ECSS-Q-ST-60_0480060",1,"Created","The supplier shall perform an evaluation against the ESCC basic specification no. 20200 and the ancillary specifications for dedicated component families and shall include, but not necessarily be limited to, a survey of:\n    1. The overall manufacturing facility and its organization and management,\n    2. The manufacturer’s system for inspection and manufacturing control including all relevant specifications, procedures, and internal documents,\n    3. The production line used for the component."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.2.2b","Requirement","ECSS-Q-ST-60_0480061",1,"Created","The complete manufacturer assessment, including the survey report and the associated corrective actions, shall be part of the evaluation report."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.3a","Requirement","ECSS-Q-ST-60_0480062",1,"Created","Constructional analysis shall be carried out on representative components. \n    ","NOTE The primary aim is to provide an early indication of a component’s constructional suitability for meeting the specified performances of the space project application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.3b","Requirement","ECSS-Q-ST-60_0480063",1,"Created","The Constructional Analysis shall comprise destructive and non-destructive inspections, analyses, and testing, to identify:\n    1. Design and construction technology,\n    2. Materials used,\n    3. Inherent reliability aspects,\n    4. Quality of workmanship,\n    5. Potential hazards."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.3c","Requirement","ECSS-Q-ST-60_0480064",1,"Created","The findings of the analysis shall be contained within a Constructional Analysis Report and shall be included in the Evaluation Report."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.4a","Requirement","ECSS-Q-ST-60_0480065",1,"Created","The evaluation shall determine which inspections or tests are required to provide the confidence that the component type under evaluation, when assembled and tested in accordance with the procurement specification, successfully meets the project requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.3.4b","Requirement","ECSS-Q-ST-60_0480066",1,"Created","The supplier shall review the already existing data in order to adapt and minimize the content of the evaluation testing while ensuring that there are inputs and pertinent results covering the following topics:\n    1. Endurance test (operating at elevated temperature and electrical stress),\n    2. Mechanical stress (shock, vibration, constant acceleration),\n    3. Environmental stress (thermal shock, temperature cycling, high and low temperature storage, humidity),\n    4. Assembly capability testing,\n    5. Radiation testing, for total dose and single event effects sensitivity.\n        ","NOTE For guidance refer to ESCC basic specification no. 22600 and the ancillary specifications for dedicated component families. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.4a","Requirement","ECSS-Q-ST-60_0480067",1,"Created","The supplier shall document the procedure for approval of each component type intended for use in flight products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.4b","Requirement","ECSS-Q-ST-60_0480068",1,"Created","The approval of components shall be based on consideration of all pertinent data including both the electrical and environmental performance as well as the established quality and the dependability assurance requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.4c","Requirement","ECSS-Q-ST-60_0480069",1,"Created","The supplier shall maintain a system of traceability of the acceptance and approval of each component used in flight products."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.4d","Requirement","ECSS-Q-ST-60_0480070",1,"Created","The approval process by the customer shall be organized as follows:\n    1. All space qualified parts by listing them in the DCL,\n    2. A PAD in conformance with Annex D is required for any other part,\n    3. A PAD in conformance with Annex D is required for space qualified parts when:\n        (a) additional controls are required (e.g. precap, buy-off, LAT or LVT, RVT, DPA),\n        (b) used outside the specified limits,\n        (c) specific tests are required during procurement as per Table 7-1,\n        (d) pure tin is used inside or outside the part."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.2.4e","Requirement","ECSS-Q-ST-60_0480071",1,"Created","When a PAD is required, the customer’s approval process shall include 2 steps:\n    1. step 1: approval of the part type and attached action plan, through the PAD process for the PDR.\n    2. step 2: approval of the results of the action plan defined during step 1 through the final approval of the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1a","Requirement","ECSS-Q-ST-60_0480072",1,"Created","The supplier shall ensure that all procured components meet the programme requirements with respect to inspection, screening and tests."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1b","Requirement","ECSS-Q-ST-60_0480073",1,"Created","Class 1 components shall meet the quality levels ands supplementary conditions specified in Table 7-1."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1c","Requirement","ECSS-Q-ST-60_0480074",1,"Created","The supplier shall be responsible for manufacturer surveillance and control throughout the procurement programme."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1d","Requirement","ECSS-Q-ST-60_0480075",1,"Created","For non qualified parts, the supplier shall put in place a configuration control system to ensure that any change of the product (e.g. mask, manufacturing and assembly process) affecting evaluation, performance, quality, reliability and interchangeability is communicated to him by the manufacturer (e.g. PCN)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1e","Requirement","ECSS-Q-ST-60_0480076",1,"Created","The supplier shall ensure the compatibility of the change with its application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1f","Requirement","ECSS-Q-ST-60_0480077",1,"Created","The change shall be submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.1g","Requirement","ECSS-Q-ST-60_0480078",1,"Created","To reduce the risk of procuring counterfeit components, when parts are not directly procured from the manufacturer, the supplier shall procure parts only from distributors duly franchised by the parts manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2a","Requirement","ECSS-Q-ST-60_0480079",1,"Created","The supplier shall procure EEE components according to controlled specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2b","Requirement","ECSS-Q-ST-60_0480080",1,"Created","International specifications systems, recognized as suitable for space applications (e.g. ESCC, MIL), shall be used by the supplier. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2c","Requirement","ECSS-Q-ST-60_0480081",1,"Created","Any new specification shall be prepared and designed by the supplier as per existing international specification systems (ESCC, MIL). Preference shall be given to ESCC format when agreed to by the manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2d","Requirement","ECSS-Q-ST-60_0480082",1,"Created","The content of any new specification shall be in conformance with Annex C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2e","Requirement","ECSS-Q-ST-60_0480083",1,"Created","The use of any new specification shall be submitted to the customer for approval through the approval process (see clause 4.2.4) "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2f","Requirement","ECSS-Q-ST-60_0480084",1,"Created","Upon request, any new procurement specification prepared in the frame of the project, shall be delivered to the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.2g","Requirement","ECSS-Q-ST-60_0480085",1,"Created","The supplier shall keep each procurement specification under configuration control."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.3a","Requirement","ECSS-Q-ST-60_0480086",1,"Created","All components to be incorporated into flight standard hardware shall be subjected to screening. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.3b","Requirement","ECSS-Q-ST-60_0480087",1,"Created","The screening test requirements shall be so designed that accumulated stress does not jeopardize component reliability. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.3c","Requirement","ECSS-Q-ST-60_0480088",1,"Created","All screening tests shall be performed at the component manufacturer’s premises or at a facility approved either by the qualification approval authority, where applicable (e.g. ESCC), or otherwise by the supplier."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.3d","Requirement","ECSS-Q-ST-60_0480089",1,"Created","The applicable quality levels defined in Table 7-1 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.3e","Requirement","ECSS-Q-ST-60_0480090",1,"Created","For active parts (transistors, diodes) packaged in TO3, DO4 or DO5, the PIND test method shall be submitted to the customer’s approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.4a","Requirement","ECSS-Q-ST-60_0480091",1,"Created","The procurement entity shall carry out, at the manufacturer’s premises, a customer precap inspection for non-space qualified parts listed below:\n    1. Capacitors (ceramic, mica and plastic film)\n    2. Crystals\n    3. Oscillators\n    4. Discrete semiconductors (including diodes and transistors)\n    5. Filters\n    6. Fuses (cermet)\n    7. Inductors, coils (not applicable to in-house products)\n    8. Monolithic microcircuits (including MMICs)\n    9. Hybrid circuits\n    10. Relays\n    11. Resistors (high precision, fixed, metal foil - RNC90)\n    12. Switches (including mechanical and thermal)\n    13. Optoelectronic devices (e.g. opto-couplers, LEDs, CCDs and sensors)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.4b","Requirement","ECSS-Q-ST-60_0480092",1,"Created","The procurement entity shall carry out, at the manufacturer’s premises, a customer precap inspection on critical space qualified parts , including as a minimum relays, crystals, oscillators and hybrids."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.4c","Requirement","ECSS-Q-ST-60_0480093",1,"Created","When not covered by MIL or ESCC specifications, methods and accept/reject criteria for customer’s precap inspection shall be documented by a procedure to be presented to the customer, on request, for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.5a","Requirement","ECSS-Q-ST-60_0480094",1,"Created","The supplier shall ensure that any lot or datecode of EEE parts is submitted to a lot acceptance procedure (in line with applied normative systems) according to the following rules:\n    1. Space qualified parts: \n        (a) ESCC: user’s lot acceptance on the procured lot is not required due to periodic lot validation testing performed by the manufacturer.\n        (b) MIL: QCI or TCI performed by the manufacturer is in accordance with the quality level of the MIL specification.\n    2. Non-space qualified parts: \n        (a) The content of the lot acceptance is ESCC level LAT1 or level LAT2 or LVT (subgroups 1, 2 and 3) or comparable QCI. \n        (b) The lot acceptance may be replaced by the review of available data less than 2 years old and provided there have been no changes to the manufacturing process and no changes to the part design and construction.\n        (c) In case of partial available data, any complementary lot acceptance content is defined by the supplier within the PCB.\n        (d) The PCB documents and justifies any reduced lot acceptance based on available data for customer approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.5b","Requirement","ECSS-Q-ST-60_0480095",1,"Created","The sample size for lot acceptance which may be reduced in some cases, shall be submitted to the customer for approval through the approval process (see clause 4.2.4). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.6a","Requirement","ECSS-Q-ST-60_0480096",1,"Created","The procurement entity shall carry out, at the manufacturer’s premises, a final customer source inspection for non-space qualified parts, based on inspections, tests and review activities to verify that the requirements of the purchase order are met prior to shipment of the flight parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.6b","Requirement","ECSS-Q-ST-60_0480097",1,"Created","The buy-off shall include:\n    1. External visual inspection,\n    2. Witnessing electrical measurements,\n    3. Verifying mechanical dimensions,\n    4. Review and verification of the data-package."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.6c","Permission","ECSS-Q-ST-60_0480449",1,"Created","The buy-off may be replaced by an incoming inspection at the procurement entity's facilities."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.6d","Requirement","ECSS-Q-ST-60_0480099",1,"Created","If the buy-off is replaced by an incoming inspection at the procurement entity's facilities, it shall be reported in the PAD submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.7a","Requirement","ECSS-Q-ST-60_0480100",1,"Created","The procurement entity shall perform incoming inspection at his premises on all components to verify conformance with the purchase order requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.7b","Requirement","ECSS-Q-ST-60_0480101",1,"Created","The incoming inspection shall include the following items:\n    1. Marking control,\n    2. Quantity verification,\n    3. Packing checking,\n    4. Review of the manufacturer delivered documentation,\n    5. Additional tests based on the type of component, criticality and heritage with the manufacturer (e.g. solderability tests, electrical tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.7c","Requirement","ECSS-Q-ST-60_0480102",1,"Created","The incoming inspection shall be documented by a procedure to be sent, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.7d","Requirement","ECSS-Q-ST-60_0480103",1,"Created","If the parts have passed successfully a final CSI (or buy-off), the incoming inspection may be reduced. The minimum shall be:\n    1. Verification of the manufacturer’s CoC\n    2. Packing checking,\n    3. Quantity verification."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.7e","Requirement","ECSS-Q-ST-60_0480104",1,"Created","In case the incoming inspection has been performed by a procurement agent, the incoming inspection performed by the end-user, may be reduced. The minimum shall be:\n    1. Packing checking,\n    2. Quantity verification."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.8a","Requirement","ECSS-Q-ST-60_0480105",1,"Created","Radiation sensitive components, as defined in clause 4.2.2.4, and for which applicable existing test data is insufficient shall be subjected to RVT."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.8b","Requirement","ECSS-Q-ST-60_0480106",1,"Created","RVT shall be performed in accordance with internationally recognized standards, such as ESCC Basic Specifications No. 22900 and No 25100.\n    ","NOTE Additional information on test methods is given in MIL-STD-750 Test Method 1080, MIL-STD-883 Test Method 1019 and JEDEC JESD57."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.8c","Requirement","ECSS-Q-ST-60_0480107",1,"Created","In such a case, a PAD in conformance with Annex D shall be issued and processed as per clause 4.2.4."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.8d","Requirement","ECSS-Q-ST-60_0480108",1,"Created","The results of RVT shall be documented by a report. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.8e","Requirement","ECSS-Q-ST-60_0480109",1,"Created","When RVT is performed in the frame of the project, the supplier shall send the related report to the customer for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9a","Requirement","ECSS-Q-ST-60_0480110",1,"Created","The DPA shall be performed on 3 samples per lot for non-space qualified parts belonging to the following categories:\n    1. Capacitors (ceramic, tantalum and variable)\n    2. Crystals\n    3. Oscillators\n    4. Discrete semiconductors (including diodes and transistors)\n    5. Filters\n    6. Monolithic microcircuits (including MMICs)\n    7. Hybrid circuits\n    8. Relays\n    9. Switches (including mechanical and thermal)\n    10. Optoelectronic devices (e.g. opto-couplers, LED’s, CCD’s and sensors)\n    11. Passive microwave devices (e.g. mixers, couplers, isolators and switches)"]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9b","Requirement","ECSS-Q-ST-60_0480111",1,"Created","The DPA shall be performed on 3 samples per lot on critical space qualified parts, including as a minimum relays and oscillators. For other space qualified parts families, DPA is not required."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9c","Requirement","ECSS-Q-ST-60_0480112",1,"Created","DPA may be carried out on representative samples of the components families when procured from the same manufacturer and same package without major change in the process, with a limited datecode range of 13 weeks. Such reductions shall be submitted to the customer for approval through the PAD process.\n    ","NOTE In complement of above conditions, for series of integrated circuits, series of thermal switches, series of active discrete and series of passive components (e.g. 54xxxx, 1N63xx, …), representative samples can be from the same family considering technology limit and their complexity."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9d","Requirement","ECSS-Q-ST-60_0480113",1,"Created","The DPA sample size may be reduced in some cases which shall be submitted to the customer for approval through the PAD process."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9e","Requirement","ECSS-Q-ST-60_0480114",1,"Created","The DPA process shall be documented by a procedure to be sent, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9f","Requirement","ECSS-Q-ST-60_0480115",1,"Created","The supplier shall verify that the outcome of the DPA is satisfactory prior to the installation of the components into flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9g","Permission","ECSS-Q-ST-60_0480450",1,"Created","Independent laboratories may perform DPA when approved by the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9h","Permission","ECSS-Q-ST-60_0480451",1,"Created","DPA may be performed by the manufacturer if witnessed by the supplier (or approved representative)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9i","Requirement","ECSS-Q-ST-60_0480118",1,"Created","For health and safety reasons, any test producing beryllium oxide dust shall be omitted."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.9j","Requirement","ECSS-Q-ST-60_0480119",1,"Created","The results of DPA shall be documented by a report sent to the customer, on request, for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.10a","Permission","ECSS-Q-ST-60_0480452",1,"Created","Components from a supplier’s or parts procurement agent’s stock may be used provided the following criteria are met:\n    1. The parts are stored according to the minimum conditions given in clause 4.4 ,\n    2. The minimum overall requirements (including screening) are in accordance with the project requirements, \n    3. The lot homogeneity and traceability can be demonstrated, \n    4. The EEE parts documentation is available and the content is acceptable in accordance with the project requirements (including radiation data, if necessary), \n    5. There are no open NCR’s and no unresolved alerts with respect to their date code."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.10b","Requirement","ECSS-Q-ST-60_0480121",1,"Created","For components meeting the above criteria, and which have a lot / date code exceeding the period defined in ECSS-Q-ST-60-14 clause 5, the relifing procedure ECSS-Q-ST-60-14 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.11a","Requirement","ECSS-Q-ST-60_0480122",1,"Created","The manufacturer’s CoC shall be delivered to the parts procurer. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.11b","Requirement","ECSS-Q-ST-60_0480123",1,"Created","Any other data (i.e. LAT or LVT, QCI orTCI), defined in the applicable procurement documents, shall be available at the manufacturer’s facilities or delivered to the parts’ procurer in line with the purchase order. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.3.11c","Requirement","ECSS-Q-ST-60_0480124",1,"Created","For non qualified parts, the documentation minimum storage period shall be 10 years after delivery of components by the manufacturer. \n    ","NOTE For qualified parts, the documentation storage period is under the responsibility of the manufacturer and the qualifying authority."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.4a","Requirement","ECSS-Q-ST-60_0480125",1,"Created","The supplier shall establish and implement procedures for handling and storage of components in order to prevent possible degradation. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.4b","Requirement","ECSS-Q-ST-60_0480126",1,"Created","The procedures shall be applicable at any facility dealing with components for flight application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.4c","Requirement","ECSS-Q-ST-60_0480127",1,"Created","On request, handling and storage procedures shall be sent to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.4d","Requirement","ECSS-Q-ST-60_0480128",1,"Created","As a minimum, the following areas shall be covered:\n    1. Control of the environment in accordance with ESCC Basic Specification No. 24900.\n    2. Measures and facilities to segregate and protect components during receiving inspection, storage, and delivery to manufacturing. \n    3. Control measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.1a","Requirement","ECSS-Q-ST-60_0480129",1,"Created","The supplier shall establish and implement the requirements of this document including methods, organizations and documents used to control the selection and procurement of components in accordance with the requirements of ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.2a","Requirement","ECSS-Q-ST-60_0480130",1,"Created","The supplier shall establish and maintain a nonconformance control system in accordance with the general requirements in ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.2b","Requirement","ECSS-Q-ST-60_0480131",1,"Created","Any observed deviation of EEE components from requirements as laid down in applicable specifications, procedures and drawings shall be controlled by the nonconformance control system.\n    ","NOTE This includes failures, malfunctions, deficiencies and defects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.2c","Requirement","ECSS-Q-ST-60_0480132",1,"Created","The nonconformance control system shall handle all nonconformances occurring on EEE components during:\n    1. Manufacture (if available), screening and acceptance tests, \n    2. Incoming inspection,\n    3. Integration and test of equipment,\n    4. Storage and handling."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.2d","Requirement","ECSS-Q-ST-60_0480133",1,"Created","For ESCC qualified components the supplier shall apply the ESCC basic specification no 22800."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.3a","Requirement","ECSS-Q-ST-60_0480134",1,"Created","The supplier shall take into account all received alerts from international alert systems, from manufacturers or sent by the customer and shall validate that there are no alerts on the proposed parts with respect to the batch information (including date-code). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.3b","Requirement","ECSS-Q-ST-60_0480135",1,"Created","If alerts become available at a later stage, the supplier shall analyse the alerts, analyse the project risk and propose an action plan for customer approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.3c","Requirement","ECSS-Q-ST-60_0480136",1,"Created","The supplier shall initiate and distribute within the project notifications for all major problems arising on EEE parts during procurement, incoming inspection or during all levels of equipment manufacturing or testing, which are of general concern."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.4a","Requirement","ECSS-Q-ST-60_0480137",1,"Created","The traceability of individual components during manufacturing and testing shall be maintained as required by the procurement specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.4b","Requirement","ECSS-Q-ST-60_0480138",1,"Created","The traceability shall be maintained through incoming, storage, and installation at the procurer and user of the component in accordance with programme PA requirements. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.4c","Requirement","ECSS-Q-ST-60_0480139",1,"Created","In any case, the traceability requirements imposed by the supplier on the EEE parts manufacturer or distributor shall allow managing the adequacy of the tests performed by the supplier (i.e. evaluation, lot validation, any additional test or inspection). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.4d","Requirement","ECSS-Q-ST-60_0480140",1,"Created","The traceability of EEE parts during installation in equipment, shall be ensured by the supplier through maintaining the traceability to the manufacturer’s lot/datecode number of the EEE parts actually mounted. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.4e","Requirement","ECSS-Q-ST-60_0480141",1,"Created","If the as built DCL has not yet been delivered, the supplier shall be able to provide this information (part type actually installed with its relevant lot/datecode number) within one week."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.5a","Requirement","ECSS-Q-ST-60_0480142",1,"Created","If tests are performed by sampling, the sampled parts shall be selected so that they are representative of the lot distribution. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.5.5b","Requirement","ECSS-Q-ST-60_0480143",1,"Created","For radiation tests, the set of test samples used shall be a representative distribution for the wafer lot. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.1a","Requirement","ECSS-Q-ST-60_0480144",1,"Created","For the specific component types identified in clauses 4.6.2, 4.6.3, 4.6.4 and 4.6.5 reference shall be made to applicable standards, in addition to the requirements of this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.2a","Requirement","ECSS-Q-ST-60_0480145",1,"Created","ECSS-Q-ST-60-02 shall apply for the design development."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.3a","Requirement","ECSS-Q-ST-60_0480146",1,"Created","ECSS-Q-ST-60-05 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4a","Requirement","ECSS-Q-ST-60_0480147",1,"Created","For FPGA, ECSS-Q-ST-60-02, shall apply for the design development. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4b","Requirement","ECSS-Q-ST-60_0480148",1,"Created","The PAD shall allow traceability to the information related to the procurement of blank parts, the programming process and the acceptance of the programmed parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4c","Permission","ECSS-Q-ST-60_0480453",1,"Created","The programming process and the acceptance of the programmed parts may be part of PCB, for customer approval, if not indicated in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4d","Requirement","ECSS-Q-ST-60_0480150",1,"Created","One time programmable components shall be submitted to a post-programming sequence. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4e","Requirement","ECSS-Q-ST-60_0480151",1,"Created","A dynamic post-programming burn-in shall be applied to FPGA’s, in conformance with ESCC9000 subclause 8.21, except for the duration, that is 160 h minimum."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4f","Requirement","ECSS-Q-ST-60_0480152",1,"Created","The supplier shall prepare a post-programming procedure for customer’s approval, depending on part types (including when necessary electrical tests, programming conditions and equipment, burn-in conditions, additional screening tests and specific marking after programming). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4g","Requirement","ECSS-Q-ST-60_0480153",1,"Created","The lot acceptance procedure, as defined in clause 4.3.5, shall be performed on devices coming from the flight lot and programmed using on the same kind of the hardware tools and compatible software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.4h","Permission","ECSS-Q-ST-60_0480454",1,"Created","In case of several designs based on the same lot of blank parts, the lot acceptance procedure, as defined in clause,4.3.5, may be limited to one representative flight programmed design."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.6.5a","Requirement","ECSS-Q-ST-60_0480155",1,"Created","ECSS-Q-ST-60-12 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","4.7a","Requirement","ECSS-Q-ST-60_0480156",1,"Created","Any result from inspection or control shall be documented (including, precap, lot acceptance, buy-off, incoming, relifing and complementary tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.1a","Requirement","ECSS-Q-ST-60_0480157",1,"Created","The supplier shall establish and implement throughout the duration of the business agreement a component programme which ensures that the requirements of the project as defined by the customer and the supplier in the related business agreement are in compliance with this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-60_0480158",1,"Created","The supplier shall identify the organization responsible for the management of the component programme, and describe the organization’s approaches (including the procurement system and its rationale) and capability to efficiently implement, manage, and control the component requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.2.2a","Requirement","ECSS-Q-ST-60_0480159",1,"Created","The supplier shall prepare a compliance matrix to the clauses of this standard. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.2.2b","Requirement","ECSS-Q-ST-60_0480160",1,"Created","The supplier shall submit his compliance matrix to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.3a","Requirement","ECSS-Q-ST-60_0480161",1,"Created","At supplier's level, the Parts Control Board (PCB) shall be chaired by a member of the supplier’s PA team with designated responsibility for components management. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.3b","Requirement","ECSS-Q-ST-60_0480162",1,"Created","The composition of the PCB shall as a minimum include additionally the suppliers’ parts engineer, the customer’s representative and the lower tier subcontractor parts engineers.\n    ","NOTE The approval of the selection and usage of EEE parts are implemented through Parts Control Boards (PCBs) held between the customer and the supplier (or lower tier subcontractor). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.3c","Permission","ECSS-Q-ST-60_0480455",1,"Created","Other pertinent experts from the customer or suppliers may also participate, on request."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.3d","Requirement","ECSS-Q-ST-60_0480164",1,"Created","Depending on the progress of the program, the main PCB activities shall be:\n    1. Review and approval of the supplier's EEE component control plan and any associated documents\n    2. Parts approval including evaluation activities,\n    3. Problem assessment (e.g. alerts, nonconformances, RFD, RFW and delivery delays)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4a","Requirement","ECSS-Q-ST-60_0480165",1,"Created","For each equipment, its supplier shall issue a DCL in an editable electronic format, identifying all component types needed. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4b","Requirement","ECSS-Q-ST-60_0480166",1,"Created","This list shall be kept under configuration control (issue and identification of changes). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4c","Requirement","ECSS-Q-ST-60_0480167",1,"Created","The DCL shall be issued as a minimum at PDR and CDR (as designed) and at flight hardware delivery (as built)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4d","Requirement","ECSS-Q-ST-60_0480168",1,"Created","After equipment CDR, all modifications affecting the PAD information shall be implemented, in the \"as design\" DCL, through the CN / CR process and submitted to the customer for approval.\n    ","NOTE For PAD generation, see 5.2.4."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4e","Requirement","ECSS-Q-ST-60_0480169",1,"Created","The “as design” DCL shall be sent to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4f","Requirement","ECSS-Q-ST-60_0480170",1,"Created","Any change of parts during equipment manufacturing (e.g. type and manufacturer) shall be handled through RFWs submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4g","Requirement","ECSS-Q-ST-60_0480171",1,"Created","The “as built” DCL reflecting the actual EEE parts assembled into the flight hardware and their date code, shall be provided to the customer for review at the delivery of the flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.4h","Requirement","ECSS-Q-ST-60_0480172",1,"Created","The content of the DCL shall be in conformance with its DRD in Annex B."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.5a","Requirement","ECSS-Q-ST-60_0480173",1,"Created","EEE components used in GSE, which are physically and directly interfacing to flight hardware, shall meet the requirements of this document."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.1.5b","Requirement","ECSS-Q-ST-60_0480174",1,"Created","Flight hardware connectors interfaces to GSE shall be protected by connector savers."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-60_0480175",1,"Created","The supplier shall ensure that the following requirements are met during his selection process:\n    1. Project requirements (e.g. quality levels, component policy, manufacturing and delivery schedules and budgets, and quantities), \n    2. Design requirements (e.g. component type, case, dimensions, and materials), \n    3. Production requirements (e.g. packaging, thermal and storage constraints, component mounting and process), \n    4. Operational requirements (e.g. electrical, mechanical, radiation, reliability, assembly, and lifetime).\n        ","NOTE The supplier of each product is responsible for the selection of components, which enable the performance, lifetime, environmental, material, safety, quality and reliability requirements of the product of which they forms a part, to be satisfied in all respects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.1a","Requirement","ECSS-Q-ST-60_0480176",1,"Created","The supplier shall establish and maintain in his own facility, and ensure that his suppliers also establish and maintain, procedures for selecting and controlling all components intended for use in deliverable products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.1b","Requirement","ECSS-Q-ST-60_0480177",1,"Created","Components shall be selected on the basis of proven qualification, characterization, and previous space experience and data, relevant with regard to the requirements for the programme, from manufacturers or sources (preferably European) employing effective Product Assurance Programmes in manufacturing and test. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.1c","Requirement","ECSS-Q-ST-60_0480178",1,"Created","Preference shall be given to components which necessitate the least evaluation or qualification effort. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.1d","Requirement","ECSS-Q-ST-60_0480179",1,"Created","When selecting items, the supplier shall check the current data, applicability of the basis of qualification, problem notifications and alerts, and adequacy of specifications. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2a","Requirement","ECSS-Q-ST-60_0480180",1,"Created","The supplier shall ensure that non-hermetically sealed materials of components meet the requirements of ECSS-Q-ST-70 regarding off-gassing, out-gassing, flammability, toxicity and any other criteria specified for the intended use. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2b","Requirement","ECSS-Q-ST-60_0480181",1,"Created","The supplier shall evaluate the robustness of selected EEE components against the stresses induced by the assembly techniques to be employed."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2c","Requirement","ECSS-Q-ST-60_0480182",1,"Created","With respect to health and safety, beryllium oxide (except if identified in the procurement specification), cadmium, lithium, magnesium, mercury, zinc, radioactive material and all material which may cause safety hazard shall not be used."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2d","Requirement","ECSS-Q-ST-60_0480183",1,"Created","For limited life duration, known instability, safety hazard or reliability risk reasons, the use of EEE components listed below shall not be used:\n    1. EEE components with pure tin (less than 3% Pb in case of SnPb alloy) used as a finish on the leads, terminations and external surfaces of components and packages. \n    2. Hollow core resistors,\n    3. Potentiometers (except for mechanism position monitoring),\n    4. Non-metallurgically bonded diodes,\n    5. Semiconductor dice with unglassivated on active area,\n    6. Wet slug tantalum capacitors other than capacitor construction using double seals and a tantalum case,\n    7. Any component whose internal construction uses metallurgic bonding with a melting temperature not compatible with the end-application mounting conditions,\n    8. Wire link fuses < 5A,\n    9. TO5 relays without double welding of the mechanism to the header or with any type of integrated diodes inside."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2e","Requirement","ECSS-Q-ST-60_0480184",1,"Created","For limited life duration, known instability, safety hazards or reliability risk reasons, EEE components listed below shall not be used for new designs:\n    1. RNC90 > 100 kW,\n    2. TO3 and DO4/DO5 packages."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2f","Permission","ECSS-Q-ST-60_0480456",1,"Created","The use of pure tin in internal cavities may be authorized, on a case-by-case basis, based on the demonstration that there is no alternative product and there is no risk (supported by a technical justification)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2g","Requirement","ECSS-Q-ST-60_0480186",1,"Created","As per 5.2.2.2e., the justification of the use of pure tin shall be presented during a PCB for customer’s approval,"]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.2h","Requirement","ECSS-Q-ST-60_0480187",1,"Created","The use of pure tin (inside or outside the part) shall be declared in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-60_0480188",1,"Created","The radiation requirements for EEE components are project specific."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3b","Requirement","ECSS-Q-ST-60_0480189",1,"Created","The supplier who is responsible for the design of the piece of hardware shall demonstrate the compliance of its components selection with the radiation constraints of the project. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3c","Requirement","ECSS-Q-ST-60_0480190",1,"Created","For this demonstration, the supplier shall consider all types of radiation including cosmic (Heavy Ions), electromagnetic, trapped (charged particles - electrons, protons - in radiation belts) and solar (flares). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3d","Requirement","ECSS-Q-ST-60_0480191",1,"Created","Due consideration shall be given to the mission orbit and trajectory, the duration, the associated spatial and temporal variations of the radiation environment as well as all protective factors such as shielding. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3e","Requirement","ECSS-Q-ST-60_0480192",1,"Created","The supplier shall assess the actual radiation tolerance of the selected components for compliance with the radiation requirements in term of total dose, displacement damage and Single Events Effects (SEE). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3f","Requirement","ECSS-Q-ST-60_0480193",1,"Created","The supplier shall identify components which are not compliant with the radiation requirements as critical radiation sensitive components. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3g","Requirement","ECSS-Q-ST-60_0480194",1,"Created","The supplier shall implement a Radiation Hardness Assurance Programme, documented by a plan to be approved by the customer, for radiation sensitive components, covering the collection of all relevant information and specifying the necessary actions in terms of evaluation and procurement testing, planning and control. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3h","Requirement","ECSS-Q-ST-60_0480195",1,"Created","The supplier shall issue an Equipment Radiation Analysis document identifying all sensitive components w.r.t. the relevant radiation effects, possibly their impact and giving an adequate engineering solution (e.g. local shielding, design solution, specific test, RVT) for the relevant equipment."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.3i","Requirement","ECSS-Q-ST-60_0480196",1,"Created","The Equipment Radiation Analysis document shall be submitted to the customer for approval.\n    ","NOTE More detailed information about the above requirements is given in ECSS-E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.4a","Requirement","ECSS-Q-ST-60_0480197",1,"Created","The supplier shall implement derating rules for components used in his designs in accordance with the requirements of ECSS-Q-ST-30-11. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.2.4b","Requirement","ECSS-Q-ST-60_0480198",1,"Created","For wire link fuses, the current derating factor shall be 50% with an additional derating of 0,2%/°C for an increase in the temperature of fuse body above 25°C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1a","Requirement","ECSS-Q-ST-60_0480199",1,"Created","The supplier shall perform a component evaluation in absence of an approved demonstration that a component has the ability to conform to the requirements for functional performance, quality, dependability, and environmental resistance as required for the project."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1b","Requirement","ECSS-Q-ST-60_0480200",1,"Created","The supplier shall plan and carry out the evaluation."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1c","Requirement","ECSS-Q-ST-60_0480201",1,"Created","The scope and planning of the component evaluation actions shall be derived from the results of an assessment of the design and intended application of the component. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1d","Requirement","ECSS-Q-ST-60_0480202",1,"Created","An evaluation plan shall be sent to the customer for approval, and include the following elements:\n    1. Constructional Analysis,\n    2. Evaluation Testing,\n    3. Radiation Hardness. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1e","Requirement","ECSS-Q-ST-60_0480203",1,"Created","In the definition of the evaluation programme any information including pertinent reliability, analysis and test data from the manufacturer of the component and previous use in comparable application shall be considered."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1f","Requirement","ECSS-Q-ST-60_0480204",1,"Created","Omission of any of these elements, or the introduction of alternative activities, shall be justified."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1g","Requirement","ECSS-Q-ST-60_0480205",1,"Created","All tests and inspections shall be carried out on representative samples of the component type from the current production of the manufacturer selected for the component procurement for the flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1h","Requirement","ECSS-Q-ST-60_0480206",1,"Created","For programmable devices, the representativeness shall include the programming hardware tools and the compatibility of the software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1i","Requirement","ECSS-Q-ST-60_0480207",1,"Created","The supplier shall review the evaluation results to determine their impact on the content of the procurement specification which shall be amended as necessary."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.1j","Requirement","ECSS-Q-ST-60_0480208",1,"Created","The supplier shall summarize the evaluation results in the evaluation report and sent it to the customer for approval.\n    ","NOTE For guidance for the assessment of the environmental aspects refer to ECSS-E-ST-10-04 and ECSS-E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.2a","Requirement","ECSS-Q-ST-60_0480209",1,"Created","A component manufacturer assessment is not required. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.3a","Requirement","ECSS-Q-ST-60_0480210",1,"Created","Constructional analysis shall be carried out on representative components. \n    ","NOTE The primary aim of constructional analysis is to provide an early indication of a component’s constructional suitability for meeting the specified performances of the space project application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.3b","Requirement","ECSS-Q-ST-60_0480211",1,"Created","The Constructional Analysis shall comprise destructive and non-destructive inspections, analyses, and testing, to identify:\n    1. Design and construction technology,\n    2. Materials used,\n    3. Inherent reliability aspects,\n    4. Quality of workmanship,\n    5. Potential hazards."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.3c","Requirement","ECSS-Q-ST-60_0480212",1,"Created","The findings of the analysis shall be contained within a Constructional Analysis Report and shall be included in the Evaluation Report."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.4a","Requirement","ECSS-Q-ST-60_0480213",1,"Created","The evaluation shall determine which inspections or tests are required to provide the confidence that the component type under evaluation, when assembled and tested in accordance with the procurement specification, successfully meets the project requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.3.4b","Requirement","ECSS-Q-ST-60_0480214",1,"Created","The supplier shall review the already existing data in order to adapt and minimize the content of the evaluation testing while ensuring that there are inputs and pertinent results covering the following topics:\n    1. Endurance test (operating at elevated temperature and electrical stress),\n    2. Mechanical stress (shock, vibration, constant acceleration),\n    3. Environmental stress (thermal shock, temperature cycling, high and low temperature storage, humidity),\n    4. Assembly capability testing,\n    5. Radiation testing, for total dose and single event effects sensitivity.\n        ","NOTE For guidance refer to ESCC basic specification no. 22600 and the ancillary specifications for dedicated component families. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-Q-ST-60_0480215",1,"Created","The supplier shall document the procedure for approval of each component type intended for use in flight products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.4b","Requirement","ECSS-Q-ST-60_0480216",1,"Created","The approval of components shall be based on consideration of all pertinent data including both the electrical and environmental performances as well as the established quality and the dependability assurance requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.4c","Requirement","ECSS-Q-ST-60_0480217",1,"Created","The supplier shall maintain a system of traceability of the acceptance and approval of each component used in flight products."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.4d","Requirement","ECSS-Q-ST-60_0480218",1,"Created","The approval process by the customer shall be organized as follows:\n    1. All parts belonging to EPPL, NPSL or qualified according to quality levels defined in Table 7-2 are approved by listing them in the DCL,\n    2. A PAD in conformance with Annex D is required for any other part (including CECC parts),\n    3. A PAD in conformance with Annex D is also required for EPPL, NPSL or qualified parts when:\n        (a) additional controls are required (e.g. precap, buy-off, LAT or LVT, RVT, DPA),\n        (b) used outside the specified limits,\n        (c) specific tests are required during procurement as per Table 7-2,\n        (d) pure tin is used inside or outside the part.\n    4. A Justification Document is required for any commercial part, instead of PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.2.4e","Requirement","ECSS-Q-ST-60_0480219",1,"Created","When a PAD or a Justification Document is required, the customer’s approval process shall include 2 steps:\n    1. step 1: approval of the part type and attached action plan, through the PAD or Justification Document process for the PDR.\n    2. step 2: approval of the results of the action plan defined during step 1 through the final approval of the PAD or the Justification Document."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1a","Requirement","ECSS-Q-ST-60_0480220",1,"Created","The supplier shall ensure that all procured components meet the programme requirements with respect to inspection, screening and tests."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1b","Requirement","ECSS-Q-ST-60_0480221",1,"Created","Class 2 components shall meet the quality levels and supplementary conditions specified in Table 7-2."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1c","Requirement","ECSS-Q-ST-60_0480222",1,"Created","The supplier shall be responsible for manufacturer surveillance and control throughout the procurement programme."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1d","Requirement","ECSS-Q-ST-60_0480223",1,"Created","For non qualified parts, the supplier shall put in place a configuration control system to ensure that any change of the product (e.g. mask, manufacturing and assembly process) affecting evaluation, performance, quality, reliability and interchangeability is communicated to him by the manufacturer (e.g. PCN)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1e","Requirement","ECSS-Q-ST-60_0480224",1,"Created","The supplier shall ensure the compatibility of the change with its application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1f","Requirement","ECSS-Q-ST-60_0480225",1,"Created","The change shall be submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.1g","Requirement","ECSS-Q-ST-60_0480226",1,"Created","To reduce the risk of procuring counterfeit components, when parts are not directly procured from the manufacturer, the supplier shall procure parts only from distributors duly franchised by the parts manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2a","Requirement","ECSS-Q-ST-60_0480227",1,"Created","The supplier shall procure EEE components according to controlled specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2b","Requirement","ECSS-Q-ST-60_0480228",1,"Created","International specifications systems, new specifications or manufacturer’s datasheets under configuration shall be used by the supplier. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2c","Requirement","ECSS-Q-ST-60_0480229",1,"Created","Any new specification shall be prepared and designed by the supplier as per existing international specification systems (ESCC, MIL). Preference shall be given to ESCC format when agreed to by the manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2d","Requirement","ECSS-Q-ST-60_0480230",1,"Created","The content of any new specification shall be in conformance with Annex C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2e","Requirement","ECSS-Q-ST-60_0480231",1,"Created","The use of any new specification or datasheet shall be submitted to the customer for approval through the approval process (see clause 5.2.4)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2f","Requirement","ECSS-Q-ST-60_0480232",1,"Created","Upon request, any new procurement specification prepared in the frame of the project, shall be delivered to the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.2g","Requirement","ECSS-Q-ST-60_0480233",1,"Created","The supplier shall keep each procurement specification or manufacturer’s datasheet under configuration control. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.3a","Requirement","ECSS-Q-ST-60_0480234",1,"Created","All components to be incorporated into flight standard hardware shall be subjected to screening. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.3b","Requirement","ECSS-Q-ST-60_0480235",1,"Created","The screening test requirements shall be so designed that accumulated stress does not jeopardize component reliability. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.3c","Requirement","ECSS-Q-ST-60_0480236",1,"Created","All screening tests shall be performed at the component manufacturer’s premises or at facility approved either by the qualification approval authority, where applicable (e.g. ESCC), or otherwise by the supplier.."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.3d","Requirement","ECSS-Q-ST-60_0480237",1,"Created","The applicable quality levels defined in Table 7-2 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.3e","Requirement","ECSS-Q-ST-60_0480238",1,"Created","For active parts (transistors, diodes) packaged in TO3, DO4 or DO5, the PIND test method shall be submitted to the customer’s review. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.4a","Requirement","ECSS-Q-ST-60_0480239",1,"Created","The procurement entity shall carry out, at the manufacturer’s premises, a customer precap inspection for the following non-space qualified parts types: relays, crystals, oscillators and hybrids."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.4b","Requirement","ECSS-Q-ST-60_0480240",1,"Created","When not covered by MIL or ESCC specifications, methods and accept/reject criteria for customer’s precap inspection shall be documented by a procedure to be presented to the customer, on request, for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.5a","Requirement","ECSS-Q-ST-60_0480241",1,"Created","The supplier shall ensure that any lot or datecode of EEE parts is submitted to a lot acceptance procedure (in line with applied normative systems) according to the following rules:\n    1. Space qualified parts: \n        (a) ESCC: user’s lot acceptance on the procured lot is not required due to periodic lot validation testing performed by the manufacturer.\n        (b) MIL: QCI or TCI performed by the manufacturer is in accordance with the quality level of the MIL specification.\n    2. Non-space qualified parts: \n        (a) The content of the lot acceptance is defined according to the available data. \n        (b) The proposed lot acceptance is approved through the approval process (see clause 5.2.4). \n    3. Commercial parts:\n        (a) The content of the lot acceptance is defined according to information provided by the justification document. \n        (b) The proposed lot acceptance is approved through the approval process (see clause 5.2.4). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.5b","Permission","ECSS-Q-ST-60_0480457",1,"Created","The sample size for lot acceptance which may be reduced in some cases is submitted to the customer for approval through the approval process (see clause 5.2.4)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.6a","Requirement","ECSS-Q-ST-60_0480243",1,"Created","The procurement entity shall carry out, at the manufacturer’s premises, a final customer source inspection for non-space qualified parts based on inspections, tests and review activities to verify that the requirements of the purchase order are met prior to shipment of the flight parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.6b","Requirement","ECSS-Q-ST-60_0480244",1,"Created","The buy-off shall include:\n    1. External visual inspection,\n    2. Witnessing electrical measurements,\n    3. Verifying mechanical dimensions,\n    4. Review and verification of the data-package."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.6c","Permission","ECSS-Q-ST-60_0480458",1,"Created","The buy-off may be replaced by an incoming inspection at the procurement entity's facilities; "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.6d","Requirement","ECSS-Q-ST-60_0480246",1,"Created","If the buy-off is replaced by an incoming inspection at the procurement entity's facilities; it shall be reported in the PAD which is submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.7a","Requirement","ECSS-Q-ST-60_0480247",1,"Created","The procurement entity shall perform incoming inspection at his premises on all components to verify conformance with the purchase order requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.7b","Requirement","ECSS-Q-ST-60_0480248",1,"Created","The incoming inspection shall include the following items:\n    1. Marking control,\n    2. Quantity verification,\n    3. Packing checking,\n    4. Review of the manufacturer delivered documentation,\n    5. Additional tests based on the type of component, criticality and heritage with the manufacturer (e.g. solderability tests, electrical tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.7c","Requirement","ECSS-Q-ST-60_0480249",1,"Created","The incoming inspection shall be documented by a procedure to be presented, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.7d","Requirement","ECSS-Q-ST-60_0480250",1,"Created","If the parts have passed successfully a final CSI (or buy-off), the incoming inspection may be reduced. The minimum shall be:\n    1. Verification of the manufacturer’s CoC,\n    2. Packing checking,\n    3. Quantity verification."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.7e","Requirement","ECSS-Q-ST-60_0480251",1,"Created","In case the incoming inspection has been performed by a procurement agent, the incoming inspection performed by the end-user, may be reduced. The minimum shall be:\n    1. Packing checking,\n    2. Quantity verification"]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.8a","Requirement","ECSS-Q-ST-60_0480252",1,"Created","Radiation sensitive components, as defined in clause, 5.2.2.3 and for which applicable existing test data is insufficient shall be subjected to RVT."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.8b","Requirement","ECSS-Q-ST-60_0480253",1,"Created","RVT shall be performed in accordance with internationally recognized standards, such as ESCC Basic Specifications No. 22900 and No.25100.\n    ","NOTE Additional information on test methods is given in MIL-STD-750 Test Method 1080, MIL-STD-883 Test Method 1019 and JEDEC JESD57."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.8c","Requirement","ECSS-Q-ST-60_0480254",1,"Created","In such a case, a PAD in conformance with Annex D shall be issued and processed as per clause 5.2.4. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.8d","Requirement","ECSS-Q-ST-60_0480255",1,"Created","The results of RVT shall be documented by a report. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.8e","Requirement","ECSS-Q-ST-60_0480256",1,"Created","When RVT is performed in the frame of the project, the supplier shall send the related report to the customer for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9a","Requirement","ECSS-Q-ST-60_0480257",1,"Created","The DPA shall be performed on 3 samples per lot for the following non-space qualified parts types: as a minimum relays, oscillators and commercial parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9b","Requirement","ECSS-Q-ST-60_0480258",1,"Created","DPA may be carried out on representative samples of the components families when procured from the same manufacturer and same package without major change in the process, with a limited datecode range of 13 weeks. Such reductions shall be submitted to the customer for approval through the PAD (or Justification document) process.\n    ","NOTE In complement of above conditions, for series of integrated circuits, series of thermal switches, series of active discrete and series of passive components (e.g. 54xxxx, 1N63xx, …), representative samples can be from the same family considering technology limit and their complexity."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9c","Requirement","ECSS-Q-ST-60_0480259",1,"Created","The DPA sample size may be reduced in some cases which shall be submitted to the customer for approval through the PAD (or Justification document) process."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9d","Requirement","ECSS-Q-ST-60_0480260",1,"Created","The DPA process shall be documented by a procedure to be sent, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9e","Requirement","ECSS-Q-ST-60_0480261",1,"Created","The supplier shall verify that the outcome of the DPA is satisfactory prior to the installation of the components into flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9f","Permission","ECSS-Q-ST-60_0480459",1,"Created","Independent laboratories may perform DPA when approved by the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9g","Permission","ECSS-Q-ST-60_0480460",1,"Created","DPA may be performed by the manufacturer if witnessed by the supplier (or approved representative)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9h","Requirement","ECSS-Q-ST-60_0480264",1,"Created","For health and safety reasons, any test producing beryllium oxide dust shall be omitted."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.9i","Requirement","ECSS-Q-ST-60_0480265",1,"Created","The results of DPA shall be documented by a report sent to the customer, on request, for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.10a","Permission","ECSS-Q-ST-60_0480461",1,"Created","Components from a supplier’s or parts procurement agent’s stock may be used provided the following criteria are met:\n    1. The parts are stored according to the minimum conditions given in clause 5.4,\n    2. The minimum overall requirements (including screening) are in accordance with the project requirements, \n    3. The lot homogeneity and traceability can be demonstrated, \n    4. The EEE parts documentation is available and the content is acceptable in accordance with the project requirements (including radiation data, if necessary), \n    5. There are no open NCR’s and no unresolved alerts with respect to their date code."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.10b","Requirement","ECSS-Q-ST-60_0480267",1,"Created","For components meeting the above criteria, and which have a lot / date code exceeding the period defined in ECSS-Q-ST-60-14 clause 5, the relifing procedure ECSS-Q-ST-60-14 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.11a","Requirement","ECSS-Q-ST-60_0480268",1,"Created","The manufacturer’s CoC shall be delivered to the parts procurer. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.11b","Requirement","ECSS-Q-ST-60_0480269",1,"Created","Any other data (i.e. LAT or LVT, QCI or TCI), defined in the applicable procurement documents, shall be available at the manufacturer’s facilities or delivered to the parts’ procurer in line with the purchase order. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.3.11c","Requirement","ECSS-Q-ST-60_0480270",1,"Created","For non qualified parts, the documentation minimum storage period shall be 10 years after delivery of components by the manufacturer. \n    ","NOTE For qualified parts, the documentation storage period is under the responsibility of the manufacturer and the qualifying authority."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.4a","Requirement","ECSS-Q-ST-60_0480271",1,"Created","The supplier shall establish and implement procedures for handling and storage of components in order to prevent possible degradation. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.4b","Requirement","ECSS-Q-ST-60_0480272",1,"Created","The procedures shall be applicable at any facility dealing with components for flight application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.4c","Requirement","ECSS-Q-ST-60_0480273",1,"Created","On request, handling and storage procedures shall be sent to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.4d","Requirement","ECSS-Q-ST-60_0480274",1,"Created","As a minimum, the following areas shall be covered:\n    1. Control of the environment in accordance with ESCC Basic Specification No. 24900.\n    2. Measures and facilities to segregate and protect components during receiving inspection, storage, and delivery to manufacturing. \n    3. Control measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-60_0480275",1,"Created","The supplier shall establish and implement the requirements of this document including methods, organizations and documents used to control the selection and procurement of components in accordance with the requirements of ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-60_0480276",1,"Created","The supplier shall establish and maintain a nonconformance control system in accordance with the general requirements in ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.2b","Requirement","ECSS-Q-ST-60_0480277",1,"Created","Any observed deviation of EEE components from requirements as laid down in applicable specifications, procedures and drawings shall be controlled by the nonconformance control system.\n    ","NOTE This includes failures, malfunctions, deficiencies and defects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.2c","Requirement","ECSS-Q-ST-60_0480278",1,"Created","The nonconformance control system shall handle all nonconformances occurring on EEE components during: \n    1. Manufacture (if available), screening and acceptance tests, \n    2. Incoming inspection,\n    3. Integration and test of equipment,\n    4. Storage and handling."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.2d","Requirement","ECSS-Q-ST-60_0480279",1,"Created","For ESCC qualified components the supplier shall apply the ESCC basic specification no 22800."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.3a","Requirement","ECSS-Q-ST-60_0480280",1,"Created","The supplier shall take into account all received alerts from international alert systems, from manufacturers or sent by the customer and shall validate that there are no alert on the proposed parts with respect to the batch information (including date-code). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.3b","Requirement","ECSS-Q-ST-60_0480281",1,"Created","If alerts become available at a later stage, the supplier shall analyse the alerts, analyse the project risk and propose an action plan for customer approval. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.4a","Requirement","ECSS-Q-ST-60_0480282",1,"Created","The traceability of individual components during manufacturing and testing shall be maintained as required by the procurement specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.4b","Requirement","ECSS-Q-ST-60_0480283",1,"Created","The traceability shall be maintained through incoming, storage, and installation at the procurer and user of the component in accordance with programme PA requirements. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.4c","Requirement","ECSS-Q-ST-60_0480284",1,"Created","In any case, the traceability requirements imposed by the supplier on the EEE parts manufacturer or distributor shall allow managing the adequacy of the tests performed by the supplier (i.e. evaluation, lot validation, any additional test or inspection). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.4d","Requirement","ECSS-Q-ST-60_0480285",1,"Created","The traceability of EEE parts during installation in equipment, shall be ensured by the supplier through maintaining traceability to the manufacturer lot/datecode number of the EEE parts actually mounted. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.4e","Requirement","ECSS-Q-ST-60_0480286",1,"Created","If the as built DCL has not yet been delivered, the supplier shall be able to provide this information (part type actually installed with its relevant lot/datecode number) within one week. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.5.5a","Requirement","ECSS-Q-ST-60_0480287",1,"Created","For radiation tests, the set of test samples used shall be a representative distribution for the wafer lot."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.1a","Requirement","ECSS-Q-ST-60_0480288",1,"Created","For the specific component types identified in clauses, 5.6.2, 5.6.3, 5.6.4 and 5.6.5 reference shall be made to applicable standards, in addition to the requirements of this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.2a","Requirement","ECSS-Q-ST-60_0480289",1,"Created","ECSS-Q-ST-60-02 shall apply for the design development. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.3a","Requirement","ECSS-Q-ST-60_0480290",1,"Created","ECSS-Q-ST-60-05 shall apply. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4a","Requirement","ECSS-Q-ST-60_0480291",1,"Created","For FPGA, ECSS-Q-ST-60-02, shall apply for the design development. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4b","Requirement","ECSS-Q-ST-60_0480292",1,"Created","The PAD shall allow traceability to the information related to the procurement of blank parts, the programming and the acceptance of the programmed parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4c","Permission","ECSS-Q-ST-60_0480462",1,"Created","The programming and the acceptance of the programmed parts may be part of PCB, for customer approval, if not indicated in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4d","Requirement","ECSS-Q-ST-60_0480294",1,"Created","One time programmable components shall be submitted to a post-programming sequence. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4e","Requirement","ECSS-Q-ST-60_0480295",1,"Created","A dynamic post-programming burn-in shall be applied to FPGA’s, in conformance with ESCC9000 subclause 8.21, except for the duration, that is 160 h minimum."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4f","Requirement","ECSS-Q-ST-60_0480296",1,"Created","The supplier shall prepare a post-programming procedure for customer’s approval, depending on part types (including when necessary electrical tests, programming conditions and equipment, burn-in conditions, additional screening tests and specific marking after programming)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4g","Requirement","ECSS-Q-ST-60_0480297",1,"Created","The lot acceptance procedure, as defined in clause 5.3.5, shall be performed on devices coming from the flight lot and programmed using on the same kind of hardware tools and compatible software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.4h","Permission","ECSS-Q-ST-60_0480463",1,"Created","In case of several designs based on the same lot of blank parts, the lot acceptance procedure, as defined in clause 5.3.5, may be limited to one representative flight programmed design."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.6.5a","Requirement","ECSS-Q-ST-60_0480299",1,"Created","ECSS-Q-ST-60-12 shall apply. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","5.7a","Requirement","ECSS-Q-ST-60_0480300",1,"Created","Any result from inspection or control shall be documented (including, precap, lot acceptance, buy-off, incoming, relifing and complementary tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.1a","Requirement","ECSS-Q-ST-60_0480301",1,"Created","The supplier shall establish and implement throughout the duration of the business agreement a component programme which ensures that the requirements of the project as defined by the customer and the supplier in the related business agreement are in compliance with this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.2.1a","Requirement","ECSS-Q-ST-60_0480302",1,"Created","The supplier shall identify the organization responsible for the management of the component programme, and describe the organization’s approaches (including the procurement system and its rationale) and capability to efficiently implement, manage, and control the component requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.2.2a","Requirement","ECSS-Q-ST-60_0480303",1,"Created","The supplier shall prepare a compliance matrix to the clauses of this standard. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.2.2b","Requirement","ECSS-Q-ST-60_0480304",1,"Created","The supplier shall submit his compliance matrix to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.3a","Requirement","ECSS-Q-ST-60_0480305",1,"Created","A PCB is not required."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4a","Requirement","ECSS-Q-ST-60_0480306",1,"Created","For each equipment, its supplier shall issue a DCL in an editable electronic format, identifying all component types needed. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4b","Requirement","ECSS-Q-ST-60_0480307",1,"Created","The DCL shall be kept under configuration control (issue and identification of changes). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4c","Requirement","ECSS-Q-ST-60_0480308",1,"Created","The DCL shall be issued as a minimum at PDR and CDR (as designed) ."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4d","Requirement","ECSS-Q-ST-60_0480309",1,"Created","After equipment CDR, all modifications affecting the PAD information shall be implemented, in the \"as design\" DCL, through the CN / CR process and submitted to the customer for approval.\n    ","NOTE For PAD generation, see 6.2.4d."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4e","Requirement","ECSS-Q-ST-60_0480310",1,"Created","The “as design” DCL shall be sent to the customer for approval. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4f","Requirement","ECSS-Q-ST-60_0480311",1,"Created","Any change of parts during equipment manufacturing (e.g. type and manufacturer) shall be handled through RFWs submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.4g","Requirement","ECSS-Q-ST-60_0480312",1,"Created","The content of the DCL shall be in conformance with the DRD in Annex B."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.5a","Requirement","ECSS-Q-ST-60_0480313",1,"Created","EEE components used in GSE, which are physically and directly interfacing to flight hardware, shall meet the requirements of this document."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.1.5b","Requirement","ECSS-Q-ST-60_0480314",1,"Created","Flight hardware connectors interfaces to GSE shall be protected by connector savers."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.1a","Requirement","ECSS-Q-ST-60_0480315",1,"Created","The supplier shall ensure that the following requirements are met during his selection process:\n    1. Project requirements (e.g. quality levels, component policy, manufacturing and delivery schedules and budgets, quantities),\n    2. Design requirements (e.g. component type, case, dimensions, materials),\n    3. Production requirements (e.g. packaging, thermal and storage constraints, component mounting process),\n    4. Operational requirements (e.g. electrical, mechanical, radiation, reliability, assembly, lifetime).\n        ","NOTE The supplier of each product is responsible for the selection of components, which enable the performance, lifetime, environmental, material, safety, quality and reliability requirements of the product of which they form a part, to be satisfied in all respects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.1a","Requirement","ECSS-Q-ST-60_0480316",1,"Created","The supplier shall establish and maintain in his own facility, and ensure that his suppliers also establish and maintain, procedures for selecting and controlling all components intended for use in deliverable products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.1b","Requirement","ECSS-Q-ST-60_0480317",1,"Created","Components shall be selected on the basis of proven qualification, characterization, and previous space experience and data, relevant with regard to the requirements for the programme, from manufacturers or sources (preferably European) employing effective Product Assurance Programmes in manufacturing and test. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.1c","Requirement","ECSS-Q-ST-60_0480318",1,"Created","Preference shall be given to components which necessitate the least evaluation or qualification effort. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.1d","Requirement","ECSS-Q-ST-60_0480319",1,"Created","When selecting items, the supplier shall check the current data, applicability of the basis of qualification, problem notifications and alerts, and adequacy of specifications. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2a","Requirement","ECSS-Q-ST-60_0480320",1,"Created","The supplier shall ensure that non-hermetically sealed materials of components meet the requirements of ECSS-Q-ST-70 regarding off-gassing, out-gassing, flammability, toxicity and any other criteria specified for the intended use. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2b","Requirement","ECSS-Q-ST-60_0480321",1,"Created","The supplier shall evaluate the robustness of selected EEE components against the stresses induced by the assembly techniques to be employed."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2c","Requirement","ECSS-Q-ST-60_0480322",1,"Created","With respect to health and safety, beryllium oxide (except if identified in the procurement specification), cadmium, lithium, magnesium, mercury, zinc, radioactive material and all material which may cause safety hazard shall not be used."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2d","Requirement","ECSS-Q-ST-60_0480323",1,"Created","For limited life duration , known instability, safety hazard or reliability risk reasons, the use of EEE components listed below shall not be used:\n    1. EEE components with pure tin (less than 3% Pb in case of SnPb alloy) used as a finish on the leads, terminations and external surfaces of components and packages,\n    2. Hollow core resistors,\n    3. Potentiometers (except for mechanism position monitoring),\n    4. Non-metallurgically bonded diodes,\n    5. Semiconductor dice with unglassivated active area,\n    6. Wet slug tantalum capacitors other than capacitor construction using double seals and a tantalum case,\n    7. Any component whose internal construction uses metallurgic bonding with a melting temperature not compatible with the end-application mounting conditions,\n    8. Wire link fuses < 5 A,\n    9. TO5 relays without double welding of the mechanism to the header or with any type of integrated diodes inside."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2e","Requirement","ECSS-Q-ST-60_0480324",1,"Created","For limited life duration, known instability, safety hazard or reliability risk reasons, the use of EEE components listed below shall not be used for new designs:\n    1. RNC90 > 100 kW,\n    2. TO3 and DO4/DO5 packages."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2f","Permission","ECSS-Q-ST-60_0480464",1,"Created","The use of pure tin in internal cavities may be authorized, on a case-by-case basis, based on the demonstration that there is no alternative product and there is no risk (supported by a technical justification)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2g","Requirement","ECSS-Q-ST-60_0480326",1,"Created","As per 6.2.2.2e, the justification of the use of pure tin shall be presented during a PCB for customer’s approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.2h","Requirement","ECSS-Q-ST-60_0480327",1,"Created","The use of pure tin (inside or outside the part) shall be declared in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.3a","Requirement","ECSS-Q-ST-60_0480328",1,"Created","Reference documents for the selection of components are not prescribed."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4a","Requirement","ECSS-Q-ST-60_0480329",1,"Created","The radiation requirements for EEE components are project specific."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4b","Requirement","ECSS-Q-ST-60_0480330",1,"Created","The supplier who is responsible for the design of the piece of hardware shall demonstrate the compliance of its components selection with the radiation constraints of the project. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4c","Requirement","ECSS-Q-ST-60_0480331",1,"Created","For this demonstration, the supplier shall consider all types of radiation including cosmic (Heavy Ions), electromagnetic, trapped (charged particles - electrons, protons - in radiation belts) and solar (flares). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4d","Requirement","ECSS-Q-ST-60_0480332",1,"Created","Due consideration shall be given to the mission orbit and trajectory, the duration, the associated spatial and temporal variations of the radiation environment as well as all protective factors such as shielding. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4e","Requirement","ECSS-Q-ST-60_0480333",1,"Created","The supplier shall assess the actual radiation tolerance of the selected components for compliance with the radiation requirements in term of total dose, displacement damage and Single Events Effects (SEE). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4f","Requirement","ECSS-Q-ST-60_0480334",1,"Created","The supplier shall identify components which are not compliant with the radiation requirements as critical radiation sensitive components. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4g","Requirement","ECSS-Q-ST-60_0480335",1,"Created","The supplier shall implement a Radiation Hardness Assurance Programme, documented by a plan to be approved by the customer, for radiation sensitive components, covering the collection of all relevant information and specifying the necessary actions in terms of evaluation and procurement testing, planning and control. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4h","Requirement","ECSS-Q-ST-60_0480336",1,"Created","The supplier shall issue an Equipment Radiation Analysis document identifying all sensitive components w.r.t. the relevant radiation effects, possibly their impact and giving an adequate engineering solution (e.g. shielding, design solution, specific test, and RVT) or the relevant equipment."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.4i","Requirement","ECSS-Q-ST-60_0480337",1,"Created","The Equipment Radiation Analysis document shall be submitted to the customer for approval.\n    ","NOTE More detailed information about the above requirements is given in ECSS-E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.5a","Requirement","ECSS-Q-ST-60_0480338",1,"Created","The supplier shall implement derating rules for components used in his designs in accordance with the requirements of ECSS-Q-ST-30-11."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.2.5b","Requirement","ECSS-Q-ST-60_0480339",1,"Created","For wire link fuses, the current derating factor shall be 50% with an additional derating of 0,2%/°C for an increase in the temperature of fuse body above 25°C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1a","Requirement","ECSS-Q-ST-60_0480340",1,"Created","The supplier shall perform a component evaluation in absence of an approved demonstration that a component has the ability to conform to the requirements for functional performance, quality, dependability, and environmental resistance as required for the project."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1b","Requirement","ECSS-Q-ST-60_0480341",1,"Created","The supplier shall plan and carry out the evaluation."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1c","Requirement","ECSS-Q-ST-60_0480342",1,"Created","The scope and planning of the component evaluation actions shall be derived from the results of an assessment of the design and intended application of the needed component. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1d","Requirement","ECSS-Q-ST-60_0480343",1,"Created","An evaluation plan shall be sent to the customer for approval, and include the following elements:\n    1. Constructional Analysis,\n    2. Evaluation Testing,\n    3. Radiation Hardness. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1e","Requirement","ECSS-Q-ST-60_0480344",1,"Created","In the definition of the evaluation programme any information including pertinent reliability, analysis and test data from the manufacturer of the component and previous use in comparable application shall be considered."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1f","Requirement","ECSS-Q-ST-60_0480345",1,"Created","Omission of any of these elements, or the introduction of alternative activities, shall be justified."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1g","Requirement","ECSS-Q-ST-60_0480346",1,"Created","All tests and inspections shall be carried out on representative samples of the component type from the current production of the manufacturer selected for the component procurement for the flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1h","Requirement","ECSS-Q-ST-60_0480347",1,"Created","For programmable devices, the representativeness shall include the programming hardware tools and the compatibility of the software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1i","Requirement","ECSS-Q-ST-60_0480348",1,"Created","The supplier shall review the evaluation results to determine their impact on the content of the procurement specification which shall be amended as necessary."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1j","Requirement","ECSS-Q-ST-60_0480349",1,"Created","The supplier shall summarize the evaluation results in the evaluation report and sent it to the customer for approval."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.1k","Requirement","ECSS-Q-ST-60_0480350",1,"Created","It shall be reviewed to determine if they will have an impact on the content of the procurement specification.\n    ","NOTE For guidance for the assessment of the environmental aspects refer to ECSS-E-ST-10-04 and ECSS E-ST-10-12."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.2a","Requirement","ECSS-Q-ST-60_0480351",1,"Created","A component manufacturer assessment is not required. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.3a","Requirement","ECSS-Q-ST-60_0480352",1,"Created","Constructional analysis shall be carried out on representative components.\n    ","NOTE The primary aim is to provide an early indication of a component’s constructional suitability for meeting the specified performances of the space project application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.3b","Requirement","ECSS-Q-ST-60_0480353",1,"Created","The Constructional Analysis shall comprise destructive and non-destructive inspections, analyses, and testing, to identify:\n    1. Design and construction technology,\n    2. Materials used,\n    3. Inherent reliability aspects,\n    4. Quality of workmanship,\n    5. Potential hazards."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.3c","Requirement","ECSS-Q-ST-60_0480354",1,"Created","The findings of the analysis shall be contained within a Constructional Analysis Report and shall be included in the Evaluation Report."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.4a","Requirement","ECSS-Q-ST-60_0480355",1,"Created","The evaluation shall determine which inspections or tests are required to provide the confidence that the component type under evaluation, when assembled and tested in accordance with the procurement specification, successfully meets the project requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.3.4b","Requirement","ECSS-Q-ST-60_0480356",1,"Created","The supplier shall review the already existing data in order to adapt and minimize the content of the evaluation testing while ensuring that there are inputs and pertinent results covering the following topics:\n    1. Endurance test (operating at elevated temperature and electrical stress),\n    2. Mechanical stress (shock, vibration, constant acceleration),\n    3. Environmental stress (thermal shock, temperature cycling, high and low temperature storage, humidity),\n    4. Assembly capability testing,\n    5. Radiation testing, for total dose and single event effects sensitivity.\n        ","NOTE For guidance refer to ESCC basic specification no. 22600 and the ancillary specifications for dedicated component families. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.4a","Requirement","ECSS-Q-ST-60_0480357",1,"Created","The supplier shall document the procedure for approval of each component type intended for use in flight products. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.4b","Requirement","ECSS-Q-ST-60_0480358",1,"Created","The approval of components shall be based on consideration of all pertinent data including both the electrical and environmental performances as well as the established quality and the dependability assurance requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.4c","Requirement","ECSS-Q-ST-60_0480359",1,"Created","The supplier shall maintain a system of traceability of the acceptance and approval of each component used in flight products."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.4d","Requirement","ECSS-Q-ST-60_0480360",1,"Created","The approval process by the customer shall be organized as follows:\n    1. All parts are approved by listing then in the DCL,\n    2. A PAD in conformance with Annex D is required for parts when:\n        (a) additional controls are required (e.g. precap, buy-off, LAT or LVT, RVT, DPA),\n        (b) used outside the specified limits,\n        (c) specific tests are required during procurement as per Table 7-3.\n        (d) pure tin is used inside or outside the part\n    3. Justification Document is required for any commercial part, instead of PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.2.4e","Requirement","ECSS-Q-ST-60_0480361",1,"Created","When a PAD or a Justification Document is required, the customer’s approval process shall include 2 steps:\n    1. step 1: approval of the part type and attached action plan, through the PAD or Justification Document process for the PDR.\n    2. step 2: approval of the results of the action plan defined during step 1 through the final approval of the PAD or the Justification Document."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.1a","Requirement","ECSS-Q-ST-60_0480362",1,"Created","The supplier shall ensure that all procured components meet the programme requirements with respect to inspection, screening and tests."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.1b","Requirement","ECSS-Q-ST-60_0480363",1,"Created","Class 3 components shall meet the quality levels and supplementary conditions specified in Table 7-3."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.1c","Requirement","ECSS-Q-ST-60_0480364",1,"Created","The supplier shall be responsible for manufacturer surveillance and control throughout the procurement programme."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.1d","Requirement","ECSS-Q-ST-60_0480365",1,"Created","To reduce the risk of procuring counterfeit components, when parts are not directly procured from the manufacturer, the supplier shall procure parts only from distributors duly franchised by the parts manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2a","Requirement","ECSS-Q-ST-60_0480366",1,"Created","The supplier shall procure EEE components according to controlled specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2b","Requirement","ECSS-Q-ST-60_0480367",1,"Created","International specifications systems, new specifications or manufacturer’s datasheets under configuration shall be used by the supplier. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2c","Requirement","ECSS-Q-ST-60_0480368",1,"Created","Any new specification shall be prepared and designed by the supplier as per existing international specification systems (ESCC, MIL). Preference shall be given to ESCC format when agreed to by the manufacturer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2d","Requirement","ECSS-Q-ST-60_0480369",1,"Created","The content of any new specification shall be in conformance with the procurement specification DRD in Annex C."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2e","Requirement","ECSS-Q-ST-60_0480370",1,"Created","The use of any new specification or datasheet shall be submitted to the customer for review through the approval process (see clause 6.2.4)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2f","Requirement","ECSS-Q-ST-60_0480371",1,"Created","Upon request, any new procurement specification prepared in the frame of the project, shall be delivered to the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.2g","Requirement","ECSS-Q-ST-60_0480372",1,"Created","The supplier shall keep each procurement specification or manufacturer’s datasheet under configuration control."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.3a","Requirement","ECSS-Q-ST-60_0480373",1,"Created","All components to be incorporated into flight standard hardware shall be subjected to screening."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.3b","Requirement","ECSS-Q-ST-60_0480374",1,"Created","The screening test requirements shall be so designed that accumulated stress does not jeopardize component reliability. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.3c","Requirement","ECSS-Q-ST-60_0480375",1,"Created","All screening tests shall be performed at the component manufacturer’s premises or at a facility approved either by the qualification approval authority, where applicable (e.g. ESCC), or otherwise by the supplier ."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.3d","Requirement","ECSS-Q-ST-60_0480376",1,"Created","The applicable quality levels defined in Table 7-3 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.3e","Requirement","ECSS-Q-ST-60_0480377",1,"Created","For active parts (transistors, diodes) packaged in TO3, DO4 or DO5, the PIND test method shall be submitted to the customer’s review. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.4a","Requirement","ECSS-Q-ST-60_0480378",1,"Created","A customer precap is not required."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.5a","Requirement","ECSS-Q-ST-60_0480379",1,"Created","The supplier shall ensure that any lot or datecode of EEE parts is submitted to a lot acceptance procedure (in line with applied normative systems) according to the following rules:\n    1. Space qualified parts: \n        (a) ESCC: user’s lot acceptance on the procured lot is not required due to periodic lot validation testing performed by the manufacturer.\n        (b) MIL: QCI or TCI performed by the manufacturer is in accordance with the quality level of the MIL specification.\n    2. Non-space qualified parts: \n        (a) The content of the lot acceptance is defined according to the available data. \n        (b) The proposed lot acceptance is approved through the approval process (see clause 6.2.4).\n    3. Commercial parts:\n        (a) The content of the lot acceptance is defined according to information provided by the justification document.\n        (b) The proposed lot acceptance is approved through the approval process (see clause 6.2.4)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.5b","Requirement","ECSS-Q-ST-60_0480380",1,"Created","The sample size for lot acceptance which may be reduced in some cases, shall be submitted to the customer approval through the approval process (see clause 6.2.4)"]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.6a","Requirement","ECSS-Q-ST-60_0480381",1,"Created","A buy-off is not required."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.7a","Requirement","ECSS-Q-ST-60_0480382",1,"Created","The procurement entity shall perform incoming inspection at his premises on all components to verify conformance with the purchase order requirements."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.7b","Requirement","ECSS-Q-ST-60_0480383",1,"Created","The incoming inspection shall include the following items:\n    1. Marking control,\n    2. Quantity verification,\n    3. Packing checking,\n    4. Review of the manufacturer delivered documentation,\n    5. Additional tests based on the type of component, criticality and heritage with the manufacturer (e.g. solderability tests, electrical tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.7c","Requirement","ECSS-Q-ST-60_0480384",1,"Created","The incoming inspection shall be documented by a procedure to be presented, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.7d","Requirement","ECSS-Q-ST-60_0480385",1,"Created","If the parts have passed successfully a final CSI (or buy-off), the incoming inspection may be reduced. The minimum shall be :\n    1. Verification of the manufacturer’s CoC,\n    2. Packing checking,\n    3. Quantity verification."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.7e","Requirement","ECSS-Q-ST-60_0480386",1,"Created","In case the incoming inspection has been performed by a procurement agent, the incoming inspection performed by the end-user, may be reduced. The minimum shall be : :\n    1. Packing checking,\n    2. Quantity verification."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.8a","Requirement","ECSS-Q-ST-60_0480387",1,"Created","Radiation sensitive components, as defined in clause 6.2.2.4 and for which applicable existing test data is insufficient shall be subjected to RVT."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.8b","Requirement","ECSS-Q-ST-60_0480388",1,"Created","RVT shall be performed in accordance with internationally recognized standards, such as ESCC Basic Specifications No. 22900 and No.25100. \n    ","NOTE Additional information on test methods is given in MIL-STD-750 Test Method 1080, MIL-STD-883 Test Method 1019 and JEDEC JESD57."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.8c","Requirement","ECSS-Q-ST-60_0480389",1,"Created","In such a case, a PAD in conformance with Annex D shall be issued and processed as per clause 6.2.4."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.8d","Requirement","ECSS-Q-ST-60_0480390",1,"Created","The results of RVT shall be documented by a report. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.8e","Requirement","ECSS-Q-ST-60_0480391",1,"Created","When RVT is performed in the frame of the project, the supplier shall send the related report to the customer for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9a","Requirement","ECSS-Q-ST-60_0480392",1,"Created","The DPA shall be performed on 3 samples per lot for the following non-space qualified part types, as a minimum relays and commercial parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9b","Requirement","ECSS-Q-ST-60_0480393",1,"Created","DPA may be carried out on representative samples of the components families when procured from the same manufacturer and same package without major change in the process, with a limited datecode range of 13 weeks. Such reductions shall be submitted to the customer for approval through the PAD (or Justification document) process.\n    ","NOTE In complement of above conditions, for series of integrated circuits, series of thermal switches, series of active discrete and series of passive components (e.g. 54xxxx, 1N63xx, …), representative samples can be from the same family considering technology limit and their complexity."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9c","Requirement","ECSS-Q-ST-60_0480394",1,"Created","The DPA sample size may be reduced in some cases which shall be submitted to the customer for approval through the PAD process."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9d","Requirement","ECSS-Q-ST-60_0480395",1,"Created","The DPA process shall be documented by a procedure to be sent, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9e","Requirement","ECSS-Q-ST-60_0480396",1,"Created","The supplier shall verify that the outcome of the DPA is satisfactory prior to the installation of the components into flight hardware."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9f","Permission","ECSS-Q-ST-60_0480465",1,"Created","Independent laboratories may perform DPA when approved by the customer."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9g","Permission","ECSS-Q-ST-60_0480466",1,"Created","DPA may be performed by the manufacturer if witnessed by the supplier (or approved representative)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9h","Requirement","ECSS-Q-ST-60_0480399",1,"Created","Methods and accept/reject criteria for inspection component (material, design, construction, workmanship) shall be documented by a procedure to be presented to the customer, on request, for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9i","Requirement","ECSS-Q-ST-60_0480400",1,"Created","For health and safety reasons, any test producing beryllium oxide dust shall be omitted."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.9j","Requirement","ECSS-Q-ST-60_0480401",1,"Created","The results of DPA shall be documented by a report sent to the customer, on request, for information."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.10a","Permission","ECSS-Q-ST-60_0480467",1,"Created","Components from a supplier’s or parts procurement agent’s stock may be used provided the following criteria are met:\n    1. The parts are stored according to the minimum conditions given in clause 6.4, \n    2. The minimum overall requirements (including screening) are in accordance with the project requirements, \n    3. The lot homogeneity and traceability can be demonstrated, \n    4. The EEE parts documentation is available and the content is acceptable in accordance with the project requirements (including radiation data, if necessary), \n    5. There are no open NCR’s and no unresolved alerts with respect to their date code."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.10b","Requirement","ECSS-Q-ST-60_0480403",1,"Created","For components meeting the above criteria, and which have a lot / date code exceeding the period defined in ECSS-Q-ST-60-14 clause 5, the relifing procedure ECSS-Q-ST-60-14 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.11a","Requirement","ECSS-Q-ST-60_0480404",1,"Created","The manufacturer’s CoC shall be delivered to the parts procurer. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.11b","Requirement","ECSS-Q-ST-60_0480405",1,"Created","Any other data (i.e. LAT or LVT, QCI or TCI), defined in the applicable procurement documents, shall be available at the manufacturer’s facilities or delivered to the parts’ procurer in line with the purchase order. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.3.11c","Requirement","ECSS-Q-ST-60_0480406",1,"Created","For non qualified parts, the documentation minimum storage period shall be 10 years after delivery of components by the manufacturer. \n    ","NOTE For qualified parts, the documentation storage period is under the responsibility of the manufacturer and the qualifying authority."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.4a","Requirement","ECSS-Q-ST-60_0480407",1,"Created","The supplier shall establish and implement procedures for handling and storage of components in order to prevent possible degradation."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.4b","Requirement","ECSS-Q-ST-60_0480408",1,"Created","The procedures shall be applicable at any facility dealing with components for flight application."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.4c","Requirement","ECSS-Q-ST-60_0480409",1,"Created","On request, these procedures shall be sent to the customer for review."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.4d","Requirement","ECSS-Q-ST-60_0480410",1,"Created","As a minimum, the following areas shall be covered:\n    1. Control of the environment in accordance with ESCC Basic Specification No. 24900.\n    2. Measures and facilities to segregate and protect components during receiving inspection, storage, and delivery to manufacturing. \n    3. Control measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.1a","Requirement","ECSS-Q-ST-60_0480411",1,"Created","The supplier shall establish and implement the requirements of this document including methods, organizations and documents used to control the selection and procurement of components in accordance with the requirements of ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.2a","Requirement","ECSS-Q-ST-60_0480412",1,"Created","The supplier shall establish and maintain a nonconformance control system in accordance with the general requirements in ECSS-Q-ST-20."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.2b","Requirement","ECSS-Q-ST-60_0480413",1,"Created","Any observed deviation of EEE components from requirements as laid down in applicable specifications, procedures and drawings shall be controlled by the nonconformance control system.\n    ","NOTE This includes failures, malfunctions, deficiencies and defects."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.2c","Requirement","ECSS-Q-ST-60_0480414",1,"Created","The nonconformance control system shall handle all nonconformances occurring on EEE components during: \n    1. Manufacture (if available), screening and acceptance tests, \n    2. Incoming inspection,\n    3. Integration and test of equipment,\n    4. Storage and handling."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.2d","Requirement","ECSS-Q-ST-60_0480415",1,"Created","For ESCC qualified components the supplier shall apply the ESCC basic specification no 22800."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.3a","Requirement","ECSS-Q-ST-60_0480416",1,"Created","The supplier shall take into account all received alerts from international alert systems, from manufacturers or sent by the customer and shall validate that there are no alerts on the proposed parts with respect to the batch information (including date-code). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.3b","Requirement","ECSS-Q-ST-60_0480417",1,"Created","If alerts become available at a later stage, the supplier shall analyse the alerts, analyse the project risk and propose an action plan for customer approval. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.4a","Requirement","ECSS-Q-ST-60_0480418",1,"Created","The traceability of individual components during manufacturing and testing shall be maintained as required by the procurement specifications."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.4b","Requirement","ECSS-Q-ST-60_0480419",1,"Created","The traceability shall be maintained through incoming, storage, and installation at the procurer and user of the component in accordance with programme PA requirements. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.4c","Requirement","ECSS-Q-ST-60_0480420",1,"Created","In any case, the traceability requirements imposed by the supplier on the EEE parts manufacturer or distributor shall allow managing the adequacy of the tests performed by the supplier (i.e. evaluation, lot validation, any additional test or inspection). "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.4d","Requirement","ECSS-Q-ST-60_0480421",1,"Created","The traceability of EEE parts during installation in equipment, shall be ensured by the supplier through maintaining the traceability to the manufacturer’s lot/datecode number of the EEE parts actually mounted. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.4e","Requirement","ECSS-Q-ST-60_0480422",1,"Created","The supplier shall be able to provide these information (part type actually installed with its relevant lot/datecode number) within one working day (when the flight system is on launch pad) or within one week (in the other cases)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.5.5a","Requirement","ECSS-Q-ST-60_0480423",1,"Created","For radiation tests, the set of test samples used shall be a representative distribution for the wafer lot. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.1a","Requirement","ECSS-Q-ST-60_0480424",1,"Created","For the specific component types identified in clauses 6.6.2, 6.6.3, 6.6.4, and 6.6.5 reference shall be made to applicable standards, in addition to the requirements of this standard."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.2a","Requirement","ECSS-Q-ST-60_0480425",1,"Created","ECSS-Q-60-02 shall apply for the design development."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.3a","Requirement","ECSS-Q-ST-60_0480426",1,"Created","ECSS-Q-ST-60-05 shall apply."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4a","Requirement","ECSS-Q-ST-60_0480427",1,"Created","For FPGA, ECSS-Q-ST-60-02, shall apply for the design development. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4b","Requirement","ECSS-Q-ST-60_0480428",1,"Created","The PAD shall allow traceability to the information related to the procurement of blank parts, the programming and the acceptance of the programmed parts."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4c","Permission","ECSS-Q-ST-60_0480468",1,"Created","The programming and the acceptance of the programmed parts may be part of a separate document, for customer approval, if not indicated in the PAD."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4d","Requirement","ECSS-Q-ST-60_0480430",1,"Created","One time programmable components shall be submitted to a post-programming sequence. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4e","Requirement","ECSS-Q-ST-60_0480431",1,"Created","A dynamic post-programming burn-in shall be applied to FPGA’s, in conformance with ESCC9000 subclause 8.21, except for the duration, that is 160 h minimum."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4f","Requirement","ECSS-Q-ST-60_0480432",1,"Created","The supplier shall prepare a post-programming procedure for customer’s approval, depending on part types (including when necessary electrical tests, programming conditions and equipment, burn-in conditions, additional screening tests and specific marking after programming)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4g","Requirement","ECSS-Q-ST-60_0480433",1,"Created","The lot acceptance procedure, as defined in clause 6.3.5, shall be performed on devices coming from the flight lot and programmed using on the same kind of hardware tools and compatible software."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.4h","Permission","ECSS-Q-ST-60_0480469",1,"Created","In case of several designs based on the same lot of blank parts, the lot acceptance procedure, as defined in clause 6.3.5, may be limited to one representative flight programmed design."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.6.5a","Requirement","ECSS-Q-ST-60_0480435",1,"Created","ECSS-Q-ST-60-12 shall apply. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","6.7a","Requirement","ECSS-Q-ST-60_0480436",1,"Created","Any result from inspection or control shall be documented (including, precap, lot acceptance, buy-off, incoming, relifing and complementary tests)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","A.2.1a","Requirement","ECSS-Q-ST-60_0480437",1,"Created","The CCP shall include or refer to the following information:\n    1. A description of the purpose, content and the reason prompting its preparation,\n    2. A list of the applicable and reference documents,\n    3. Any additional terms, definitions and abbreviations,\n    4. The organizational breakdown structure, responsibility descriptions, management approach and concurrent engineering,\n    5. Control of lower level suppliers, procurement agents (if any) and manufacturers,\n    6. Procurement system,\n    7. Radiation control programme,\n    8. Component selection and standardization,\n    9. Component data acquisition and assessment,\n    10. Component evaluation and related testing approach,\n    11. Component approval,\n    12. Component testing, inspection and storage,\n    13. Component quality assurance activities,\n    14. Assessment of problem notifications and alerts,\n    15. Programme planning with schedule of tasks linked to programme milestones,\n    16. Specific components control and back-up plans whenever there is evidence of possible schedule, quality or technical problems,\n    17. Reporting and deliverables, \n    18. Compliance matrix to the clauses of this standard. "]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","A.2.2a","Permission","ECSS-Q-ST-60_0480470",1,"Created","In conformance with 4.2.2.1b the CCP may be part of the overall project PA plan."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","B.2.1a","Requirement","ECSS-Q-ST-60_0480439",1,"Created","The DCL shall include or refer to the following information:\n    1. A description of the purpose, content and the reason prompting its preparation, \n    2. A list of the applicable and reference documents,\n    3. Any additional terms, definitions or abbreviations,\n    4. Component number (commercial equivalent designation),\n    5. Family (ESCC group code),\n    6. Package,\n    7. Value or range of values with tolerance for non qualified parts,\n    8. Component manufacturer (name, country),\n    9. Generic procurement specification, \n    10. Detail procurement specification (with issue and revision for non qualified parts),\n    11. Specification amendment (including issue and revision),\n    12. Name of the procurement agent (CPPA, supplier, distributor),\n    13. Quality level and lot test (ESCC LAT or LVT, MIL TCI or QCI or CI),\n    14. Space qualified status (yes or no),\n    15. RVT (yes or no),\n    16. Reference of the PAD or Justification Document, where required,\n    17. Approval status of the part,\n    18. Change identification between each DCL issue,\n    19. Date-code (only for “as built” DCL)."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","C.2.1a","Requirement","ECSS-Q-ST-60_0480440",1,"Created","The procurement specification shall include or refer to the following information:\n    1. A description of the purpose, content and the reason prompting its preparation, \n    2. A list of the applicable and reference documents,\n    3. Any additional terms, definitions or abbreviations,\n    4. Absolute maximum ratings,\n    5. Electrical and mechanical parameters and limits,\n    6. Screening, burn-in, and acceptance requirements,\n    7. Package material and lead finish,\n    8. Documentation/data requirements,\n    9. Delta limits when applicable,\n    10. Criteria for percent defective allowable,\n    11. LAT or LVT, QCI or TCI,\n    12. Marking,\n    13. Storage requirements,\n    14. Requirements for lot homogeneity,\n    15. Serialization (when applicable),\n    16. Protective packaging and handling requirements,\n    17. Radiation Verification Testing requirements, when applicable."]
["ECSS-Q-ST-60C Rev. 1","ECSS - Superseded v1.0","D.2a","Requirement","ECSS-Q-ST-60_0480441",1,"Created","The information given in Table D-1 shall be provided."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.1a","Requirement","ECSS-Q-ST-20_0380001",1,"Created","The supplier shall prepare, maintain and implement a QA plan in conformance with the DRD in Annex A."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.1b","Requirement","ECSS-Q-ST-20_0380002",1,"Created","The QA plan shall be submitted to the customer for approval.\n    NOTE Information on the schedule for delivery of the QA plan is given in Annex I."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.2a","Requirement","ECSS-Q-ST-20_0380003",1,"Created","The supplier shall establish a documented training programme for the personnel whose performance determines or affects product quality."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.2b","Requirement","ECSS-Q-ST-20_0380004",1,"Created","Personnel performing special processes shall be trained and certified by internal or external training programmes.\n    NOTE The term “special process” is defined in ECSS-S-ST-00-01, Note 3 of the definition of “process”."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.2c","Requirement","ECSS-Q-ST-20_0380005",1,"Created","Personnel inspecting or controlling special processes, or performing non-destructive testing and evaluation, shall be trained and certified according to training programmes and standards accepted by the customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.1.2d","Requirement","ECSS-Q-ST-20_0380006",1,"Created","The supplier shall maintain records of the training."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-20_0380007",1,"Created","The supplier shall implement Critical-items control in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-Q-ST-20_0380008",1,"Created","The supplier shall implement a nonconformance control system in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.3a","Requirement","ECSS-Q-ST-20_0380009",1,"Created","The supplier shall manage alerts in conformance with ECSS-Q-ST-10, clause 5.2.9."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-Q-ST-20_0380010",1,"Created","The supplier shall establish and maintain a documented stamp control system to ensure the correct and legitimate use of all fabrication and inspection stamps."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4b","Requirement","ECSS-Q-ST-20_0380011",1,"Created","Stamps shall be used to:\n    1. signify the completion of operations and processes, and\n    2. indicate inspection performance at source and incoming inspection, in process inspection and tests, final inspection, end point testing, storage and shipment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4c","Requirement","ECSS-Q-ST-20_0380012",1,"Created","The use of stamps shall be restricted to authorized personnel as identified in the stamp control system."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4d","Requirement","ECSS-Q-ST-20_0380013",1,"Created","Stamps shall be traceable to individuals responsible for their use."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4e","Requirement","ECSS-Q-ST-20_0380014",1,"Created","Stamps shall be applied directly to parts and materials, when specified by engineering drawings and specifications, and associated documents, records, labels."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4f","Requirement","ECSS-Q-ST-20_0380015",1,"Created","Stamping materials and methods shall be compatible with the articles and their use."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.4g","Permission","ECSS-Q-ST-20_0380225",1,"Created","Signatures instead of stamps may be used provided that similar traceability and responsibility records are maintained and available."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.5a","Requirement","ECSS-Q-ST-20_0380017",1,"Created","The supplier shall ensure that a bidirectional and unequivocal relationship between parts, materials or products and associated documentation or records is established and maintained."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.5b","Requirement","ECSS-Q-ST-20_0380018",1,"Created","The supplier shall be capable to trace data, personnel and equipment related to procurement, manufacturing, inspection, test, assembly, integration and operations activities."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.5c","Requirement","ECSS-Q-ST-20_0380019",1,"Created","The supplier shall be capable to trace backward the locations of materials, parts, sub-assemblies."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.5d","Requirement","ECSS-Q-ST-20_0380020",1,"Created","The supplier shall be capable to trace forward the locations of materials from raw stock."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.5e","Requirement","ECSS-Q-ST-20_0380021",1,"Created","The supplier shall establish controls to ensure that:\n    1. identification numbers are assigned in a systematic and consecutive manner,\n    2. identification numbers of scrapped or destroyed items are not used again,\n    3. identification numbers, once allocated, are not changed, unless the change is authorized by the customer.\n        NOTE Requirements for identification are addressed in ECSS-M-ST-40."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6a","Requirement","ECSS-Q-ST-20_0380022",1,"Created","The supplier shall control, calibrate and maintain inspection, measuring and test equipment, whether owned by the supplier, on loan, or provided by the customer to demonstrate the conformance of product to the specified requirements."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6b","Requirement","ECSS-Q-ST-20_0380023",1,"Created","The supplier shall use equipment in a manner which ensures that measurement uncertainty is known and is consistent with the specified measurement capability."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6c","Requirement","ECSS-Q-ST-20_0380024",1,"Created","The supplier shall include in the calculations of all measurements the total error in the measurement process attributable to the cumulative error from the calibration chain, measuring equipment and those contributed by personnel, procedures and the environment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6d","Requirement","ECSS-Q-ST-20_0380025",1,"Created","The supplier shall record the basis for the calculation of the cumulative errors as specified in requirement 5.2.6c."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6e","Requirement","ECSS-Q-ST-20_0380026",1,"Created","The supplier shall select inspection, measuring and test equipment in conformance with the required measurement accuracy and precision."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6f","Requirement","ECSS-Q-ST-20_0380027",1,"Created","The supplier shall identify, calibrate and adjust all inspection, measuring and test equipment and devices that can affect product quality at prescribed intervals, or prior to use, against certified equipment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6g","Requirement","ECSS-Q-ST-20_0380028",1,"Created","The supplier shall establish, document and maintain calibration procedures, including details of equipment type, identification number, location, frequency of checks, check method, acceptance criteria and the action to be taken when results exceed the specified accuracy."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6h","Requirement","ECSS-Q-ST-20_0380029",1,"Created","The supplier shall ensure that the inspection, measuring and test equipment is capable of the specified accuracy and precision."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6i","Requirement","ECSS-Q-ST-20_0380030",1,"Created","The supplier shall identify inspection, measuring and test equipment with a suitable indicator or approved identification record to show the calibration status."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6j","Requirement","ECSS-Q-ST-20_0380031",1,"Created","The supplier shall maintain calibration records for inspection, measuring and test equipment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6k","Requirement","ECSS-Q-ST-20_0380032",1,"Created","The supplier shall assess and document the validity of previous inspection and test results when inspection, measuring or test equipment is found to be out of calibration."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6l","Requirement","ECSS-Q-ST-20_0380033",1,"Created","The supplier shall ensure that the environmental conditions are suitable for the calibrations, inspections, measurements and tests being carried out."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6m","Requirement","ECSS-Q-ST-20_0380034",1,"Created","The supplier shall ensure that inspection, measuring and test facilities, including both test hardware and test software are protected against adjustments, which can invalidate the calibration setting."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6n","Requirement","ECSS-Q-ST-20_0380035",1,"Created","The supplier shall ensure that the inspection, measuring and test equipment is handled, preserved and stored such that the accuracy and fitness for use is maintained."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6o","Requirement","ECSS-Q-ST-20_0380036",1,"Created","The supplier shall check the test hardware or test software used for inspection to prove that it is capable of verifying the acceptability of the product prior to release for use during production and installation, and recheck it at specified intervals. \n    NOTE 1 Examples of test hardware are: jigs, fixtures, templates and patterns. \n    NOTE 2 Test aids such as test leads, break-out boxes, mains leads and similar items are not subject to the entire set of requirements defined in this clause, but are validated in a way appropriate to their usage."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6p","Requirement","ECSS-Q-ST-20_0380037",1,"Created","The supplier shall establish the extent and frequency of such checks and shall maintain records as evidence of control."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.6q","Requirement","ECSS-Q-ST-20_0380038",1,"Created","The supplier shall make the measurement design data available to the customer upon request."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.1a","Requirement","ECSS-Q-ST-20_0380039",1,"Created","The supplier shall prevent handling damage during all phases of manufacturing, assembly, integration, testing, storage, transportation and operation.\n    NOTE Possible prevention measures are:\n\ta. protection of items during handling,\n\tb. handling devices, or\n\tc. procedures and instructions."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.2a","Requirement","ECSS-Q-ST-20_0380040",1,"Created","The supplier shall place the following items in secure storage areas:\n    1. incoming materials,\n    2. intermediate items needing temporary storage, and\n    3. end items before shipping."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.2b","Requirement","ECSS-Q-ST-20_0380041",1,"Created","The supplier shall place the following items in designated segregated areas:\n    1. limited life materials,\n    2. suspended limited life materials,\n    3. nonconforming items awaiting NRB disposition,\n    4. scraped items,\n    5. items designated to be stored separately for health or safety reasons."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.2c","Requirement","ECSS-Q-ST-20_0380042",1,"Created","Each segregated area shall be identified and labelled for its intended use."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.2d","Requirement","ECSS-Q-ST-20_0380043",1,"Created","The supplier shall maintain control over acceptance into and withdrawal from storage areas."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.2e","Requirement","ECSS-Q-ST-20_0380044",1,"Created","The supplier shall maintain records to ensure that all stored items are within the usable life limits, controlled and retested, and to provide traceability within the storage or segregated area."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.7.3a","Requirement","ECSS-Q-ST-20_0380045",1,"Created","The supplier shall ensure that items subject to deterioration, corrosion or contamination through exposure to any environmental elements are preserved by methods that ensure maximum protection consistent with life and usage.\n    NOTE Examples of such environmental elements are: air and moisture."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.8.1a","Requirement","ECSS-Q-ST-20_0380046",1,"Created","Statistical quality control and analysis methods shall be used to maintain or improve the specified control of quality, when statistically significant with respect to the product characteristics and to quantities produced.\n    NOTE Examples of statistical quality control and analysis methods are sample inspection plans, determination of quality levels, statistical process control and process capabilities studies."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.8.1b","Requirement","ECSS-Q-ST-20_0380047",1,"Created","When employing statistical quality control and analysis methods, the supplier shall ensure that all the conditions for use are enforced.\n    NOTE Example of such conditions are sample significance, recording and elaboration of data, and formulation of clear decision rules."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.8.1c","Requirement","ECSS-Q-ST-20_0380048",1,"Created","Statistical quality control applications, when used by the supplier for acceptance of materials, parts, processes and products, shall be submitted to the customer for approval. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.8.2a","Requirement","ECSS-Q-ST-20_0380049",1,"Created","When sampling plans are used the supplier shall define and justify the following:\n    1. sample size, sample selection methods and criteria for inspection severity, \n    2. acceptance / rejection criteria, and \n    3. screening of rejected lots."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.2.8.2b","Requirement","ECSS-Q-ST-20_0380050",1,"Created","The supplier shall maintain records of the sampling tests, together with the identification of the characteristics to which sampling is applied."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.1.1a","Requirement","ECSS-Q-ST-20_0380051",1,"Created","The supplier shall ensure that the product is designed such that it can be produced with the specified level of quality.\n    NOTE Produceability includes provisions for the following aspects:\n\t· Design simplification and standardization, reduction in part types and part number.\n\t· Guidelines for selection of preferred parts, materials and processes.\n\t· Unambiguous definitions of the requirements and limits to be used.\n\t· Definition of tolerance build-up methods, in order to simplify manufacturing, assembly, inspection.\n\t· Standardization of interfaces.\n\t· Part accessibility for assembly and inspection.\n\t· Definition of design criteria consistent with the capability of manufacturing processes.\n\t· Definition of design methods to ensure that the cleanliness requirements are compatible with the capability of related cleanliness procedures and facilities."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.1.2a","Requirement","ECSS-Q-ST-20_0380052",1,"Created","The supplier shall ensure that the product is designed such that its performances and characteristics can be reproduced over different models and serial production.\n    NOTE Repeatability includes provisions for the following aspects:\n\t• Definition of standard tolerances generally applicable.\n\t• Recommended design concepts and solutions to ensure repeatability.\n\t• Recommended manufacturing processes having proven repeatability.\n\t• Design criteria that optimize implementation of automated manufacturing methods, or computer-aided manufacturing."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.1.3a","Requirement","ECSS-Q-ST-20_0380053",1,"Created","The supplier shall ensure that the product is designed such that it can be inspected and tested under representative conditions, for production, AIV and operational environment.\n    NOTE Inspectability and testability include provisions for the following aspects:\n\t• Definition of inspection and test requirements, including acceptance or rejection criteria, expressed in an unambiguous and quantified manner.\n\t• Part and component accessibility for inspection and test.\n\t• Definition of tolerance methods for dimensional inspection performance (e.g. functional tolerances).\n\t• Definition of recommended design techniques to facilitate fault detection, identification and location (e.g. test points, modularity, built-in test software, and feedback loops)."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.1.4a","Requirement","ECSS-Q-ST-20_0380054",1,"Created","The supplier shall ensure that the product is designed such that it can be operated in accordance with programme constraints and requirements, throughout its whole life cycle including handling, storage, transportation, integration and operations."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.1a","Requirement","ECSS-Q-ST-20_0380055",1,"Created","The supplier shall ensure that requirement verification is performed progressively, as each stage of the project is completed, and provides the organized base of data upon which qualification and acceptance is incrementally declared."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.1b","Requirement","ECSS-Q-ST-20_0380056",1,"Created","The supplier shall ensure that top-down requirement allocations and bottom-up requirement verifications are complete and consistent."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.1c","Requirement","ECSS-Q-ST-20_0380057",1,"Created","The supplier shall ensure that a system for tracking requirements and verification of results is established and maintained during the whole project life cycle."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.1d","Requirement","ECSS-Q-ST-20_0380058",1,"Created","The supplier shall ensure that verification methods are adequate and consistent with the type and criticality of the requirements."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.1e","Requirement","ECSS-Q-ST-20_0380059",1,"Created","The supplier shall ensure that appropriate reference to the verification documentation is recorded and status updated at project reviews up to final acceptance."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.2a","Requirement","ECSS-Q-ST-20_0380060",1,"Created","The supplier shall ensure that the objectives of the analysis are defined in relation with the development logic defined in the verification plan."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.2b","Requirement","ECSS-Q-ST-20_0380061",1,"Created","The following items shall be identified:\n    1. reference of the configuration item definition under analysis;\n    2. environmental constraints considered in the analysis;\n    3. basic assumptions, analysis methods, mathematical models."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.3a","Requirement","ECSS-Q-ST-20_0380062",1,"Created","The supplier shall ensure that design reviews are conducted in accordance with project requirements and written procedures.\n    NOTE Design reviews address the following items:\n\t• Quality requirements and criteria for design, produceability, repeatability, testability and operability are adequately considered in design documentation.\n\t• Methods and data required for procurement, manufacturing, inspection and test are available and validated.\n\t• Risks of not achieving requirements are highlighted and adequately controlled."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.1a","Requirement","ECSS-Q-ST-20_0380063",1,"Created","The supplier shall ensure that all configuration items and their constituent items, either off-the-shelf or specifically designed, are properly qualified with margins commensurate with the application and use environment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.1b","Requirement","ECSS-Q-ST-20_0380064",1,"Created","The supplier QA shall review and approve the qualification plan."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.1c","Requirement","ECSS-Q-ST-20_0380065",1,"Created","The supplier QA shall review and approve the qualification results."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.2a","Requirement","ECSS-Q-ST-20_0380066",1,"Created","Qualification by similarity with an identical or similar product shall be justified by providing evidence that the new application is within the limits of the previously qualified design."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.2b","Requirement","ECSS-Q-ST-20_0380067",1,"Created","Any difference in definition with respect to the reference product and any difference in the required qualification tests shall be identified."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.2c","Requirement","ECSS-Q-ST-20_0380068",1,"Created","The need for complementary qualification tests shall be analysed and the decision justified and submitted to the customer for approval."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.2d","Requirement","ECSS-Q-ST-20_0380069",1,"Created","For this purpose the supplier shall:\n    1. evaluate the as-designed or as-built configuration and related nonconformances,\n    2. ensure that qualification requirements and qualification ranges are compatible with project requirements,\n    3. ensure that qualification test results meet the requirements and any nonconformances are available for evaluation, and\n    4. ensure that a logbook of the selected model is available for review."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.3a","Requirement","ECSS-Q-ST-20_0380070",1,"Created","The product used for qualification testing shall be produced in accordance with a full and clearly identified manufacturing and inspection file. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.3b","Requirement","ECSS-Q-ST-20_0380071",1,"Created","To obtain authorization to initiate qualification tests the supplier shall demonstrate that:\n    1. the qualification model is fully representative of the flight model and any differences have been analysed to evaluate their effect on the qualification status;\n    2. inspection and test requirements are expressed in an unambiguous and quantified manner including:\n        (a) test sequence;\n        (b) test conditions;\n        (c) test standards, if any;\n        (d) applicable test levels, durations and tolerances;\n        (e) accuracy in measurement.\n    3. the qualification test procedures and facilities are defined, available and conforming to requirements of clause 5.6."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.4a","Requirement","ECSS-Q-ST-20_0380072",1,"Created","The supplier shall report the qualification status in conformance with the “Qualification status list” DRD as defined in ECSS-Q-ST-10."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.4.5a","Requirement","ECSS-Q-ST-20_0380073",1,"Created","Once the design is qualified, the supplier shall assess all subsequent changes, deviations and anomalies for their impact on the qualification status and shall perform requalification as necessary."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.3.2.5a","Requirement","ECSS-Q-ST-20_0380074",1,"Created","The supplier shall ensure that all design changes and modifications are identified, documented, reviewed and approved before their implementation."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.1.1a","Requirement","ECSS-Q-ST-20_0380075",1,"Created","The supplier QA shall participate in the approval and the selection of procurement sources.\n    NOTE The selection of procurement sources for EEE components is defined in ECSS-Q-ST-60."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.1.2a","Requirement","ECSS-Q-ST-20_0380076",1,"Created","The supplier shall select its suppliers on the basis of one of the following criteria:\n    1. The supplier has been certified by the final customer, and has a current approval to furnish items or services of the type and quality level being procured.\n        NOTE Third party certification (for instance against ISO 9001) can be also considered.\n    2. The supplier is furnishing, or has furnished within the past two years, items or services of the type and quality level being procured under other contracts with the final customer.\n    3. The supplier has demonstrated continuous capability to furnish items or services of the type and quality level being procured, supported by objective documentation.\n        NOTE This criterion does not apply if the supplier has not furnished items or services of the type being procured for more than two years.\n    4. Supplier’s capability of satisfying business agreement requirements is demonstrated by a pre-award audit by the relevant customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.1.2b","Requirement","ECSS-Q-ST-20_0380077",1,"Created","The supplier shall document and maintain on file results of supplier selection process."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.1.3a","Requirement","ECSS-Q-ST-20_0380078",1,"Created","The supplier shall establish and maintain records of all procurement sources involved in business agreement performance."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.1.3b","Requirement","ECSS-Q-ST-20_0380079",1,"Created","The supplier shall submit to the customer, upon request, the list of procurement sources, including all the information in the records 5.4.1.3a, for information."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-20_0380080",1,"Created","The supplier shall ensure that supplies are identified and that all applicable requirements are defined in the procurement documents."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.2b","Requirement","ECSS-Q-ST-20_0380081",1,"Created","The supplier shall ensure that requirements to those contained in lower tier procurement documents are traceable."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.2c","Requirement","ECSS-Q-ST-20_0380082",1,"Created","The procurement documents shall contain, by statement or reference:\n    1. comprehensive technical descriptions of the items and services to be procured,\n    2. details of the applicable requirements, such as requirements for preservation, packaging, marking, shipping, accompanying documentation and provisions for limited-life items,\n    3. details of QA activities to be performed, such as inspection and test characteristics, records and reports,\n    4. details of supplier’s QA activities at source, and\n    5. special acceptance conditions."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.2d","Requirement","ECSS-Q-ST-20_0380083",1,"Created","The supplier’s quality assurance organization shall review procurement documents prior to release, to verify the correct selection of procurement sources and appropriateness of their content."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.3a","Requirement","ECSS-Q-ST-20_0380084",1,"Created","The supplier shall exercise surveillance over all the activities carried out by lower level suppliers during business agreement performance."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.3b","Requirement","ECSS-Q-ST-20_0380085",1,"Created","The surveillance programme shall include audits, reviews, mandatory inspection points, as well as direct supervision by supplier’s resident personnel at his suppliers’ facilities and source inspection.\n    NOTE Example of review is the manufacturing readiness review."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.3c","Requirement","ECSS-Q-ST-20_0380086",1,"Created","The supplier shall select among the following criteria to define the type and extent of surveillance:\n    1. Testing or inspections cannot be accomplished by the supplier.\n        NOTE For example, environments or test equipment not available at supplier’s facility.\n    2. Verification tests are destructive in nature and the quality cannot be verified solely by inspection or test at supplier’s facility.\n    3. Supplies are designated for direct shipment from source to a customer site or the using site.\n    4. Manufacturing and AIV of complex equipment or subsystems.\n        NOTE For example, payloads.\n    5. Past performance or quality history of the lower level supplier is marginal.\n    6. Functional criticality and technical complexity of the supplies.\n    7. The degree of responsibility placed on the procurement source."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.3d","Requirement","ECSS-Q-ST-20_0380087",1,"Created","The supplier shall ensure that each of his suppliers implements surveillance on their lower level suppliers, in accordance with the same criteria."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.3e","Permission","ECSS-Q-ST-20_0380226",1,"Created","Surveillance may be delegated by the customer to third parties."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.1a","Requirement","ECSS-Q-ST-20_0380089",1,"Created","The supplier shall ensure that all incoming supplies, including documentation and packaging, whether delivered on his own premises or elsewhere, conform to the requirements of the procurement documents."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.1b","Requirement","ECSS-Q-ST-20_0380090",1,"Created","The supplier shall perform inspections in accordance with established procedures and instructions, to ensure that quality level is properly determined. \n    NOTE 1 Sampling plans in receiving inspection are defined in 5.2.8.2\n    NOTE 2 Receiving inspection of components is defined in ECSS-Q-ST-60.\n    NOTE 3 Lot or batch acceptance of materials and mechanical parts is defined in ECSS-Q-ST-70."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.1c","Requirement","ECSS-Q-ST-20_0380091",1,"Created","Receiving inspectors shall have available the procurement documents, specifications, drawings and any other document relevant to incoming supplies as required in the procurement documents."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.2a","Requirement","ECSS-Q-ST-20_0380092",1,"Created","Receiving inspection activities shall include:\n    1. verification of the packaging conditions and of the status of environmental sensors,\n    2. visual inspection of the delivered items,\n    3. verification of correct identification and, where appropriate, configuration identification for conformance to the ordering data,\n    4. verification of the evidence of inspection and tests performed by the supplier and associated documentation,\n    5. verification of the performance of supplier’s source inspection, when required,\n    6. performance of inspections and tests on selected characteristics of incoming supplies or test specimens submitted with the supplies,\n    7. identification of the shelf life of limited-life items,\n    8. identification of the inspection status and physical separation of the supplies in the receiving inspection area according to the following categories:\n        (a) items for which the receiving inspection has not been completed;\n        (b) conforming items;\n        (c) nonconforming items.\n    9. prevention of unauthorized use of uninspected items,\n    10. identification of the items to be released for production with conformance status and traceability data to be recorded in manufacturing documents,\n    11. maintenance of receiving inspection records in conformance with 5.4.4.4."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.3a","Requirement","ECSS-Q-ST-20_0380093",1,"Created","Receiving inspection of items supplied by the customer shall consist of the verification of identity and integrity after transportation.\n    NOTE Additional inspections and tests, if any, are specified in the business agreement."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.4.4.4a","Requirement","ECSS-Q-ST-20_0380094",1,"Created","The supplier shall maintain receiving inspection records to ensure traceability and the availability of historical data to monitor supplier performance and quality trends."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-20_0380095",1,"Created","The supplier shall document the planning of manufacturing, assembly and integration operations and inspections in the manufacturing plan or flow chart for the product, including the sequence of operations and associated inspections and tests."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1b","Requirement","ECSS-Q-ST-20_0380096",1,"Created","The planning shall include the identification of MIPs in conformance with 5.5.8, together with the reference to the procedures by which the various activities are performed and the required cleanliness levels and temperature and humidity requirements of the facilities."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1c","Requirement","ECSS-Q-ST-20_0380097",1,"Created","Instructions shall direct the actual performance of manufacturing, assembly and integration operations and inspections, to ensure that the activities proceed in an orderly manner and according to the planned sequence.\n    NOTE For example: shop travellers."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1d","Requirement","ECSS-Q-ST-20_0380098",1,"Created","The supplier shall issue and maintain manufacturing, assembly and integration documents in accordance with established and formal procedures."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1e","Requirement","ECSS-Q-ST-20_0380099",1,"Created","The QA organization shall review and approve such documents, and any modifications thereof, to ensure that they include or refer to:\n    1. Identification of the item to be manufactured or equipment to be used.\n    2. Configuration data, including parts lists, drawings, changes and specifications.\n    3. Identification of the production and inspection equipment to be used for the manufacturing, assembly and integration of the item.\n        NOTE Examples of production and inspection equipment are tools, jigs and fixtures.\n    4. Identification of critical characteristics.\n        NOTE Critical characteristics are defined in ECSS-Q-ST-30.\n    5. Detailed definition, by description or reference, of manufacturing, assembly, integration, inspections and test operations to be performed, and special conditions to be maintained.\n    6. Provisions for inspections and tests to be witnessed by customer representative.\n    7. Accept or reject criteria (with tolerances) and workmanship standards.\n    8. Details of sampling inspection procedures to be used, if any.\n    9. Detailed procedures for the activities to be performed."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1f","Requirement","ECSS-Q-ST-20_0380100",1,"Created","Only “first off” shop travellers shall be reviewed unless subsequent travellers incorporate a significant change of inspection requirements or order of events."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.1g","Requirement","ECSS-Q-ST-20_0380101",1,"Created","The supplier shall also provide for detail support documents and instructions, such as drawings, procedure and instruction sheets, to enable operations to be correctly performed."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-20_0380102",1,"Created","The supplier shall perform an internal review of the readiness for manufacturing, prior to starting the manufacture of the first flight-standard product."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.2b","Requirement","ECSS-Q-ST-20_0380103",1,"Created","The manufacturing readiness review shall evaluate the following aspects:\n    1. status of product definition and requirements, differences with the status of the qualification model, and impacts of these differences;\n    2. status of manufacturing, assembly, inspection and test documentation, differences with the status of the qualification model, and impacts of these differences;\n    3. validation status of manufacturing processes, with particular emphasis on critical processes;\n    4. implementation of dispositions for risk reduction, as defined by risk assessment, into the manufacturing, assembly, integration, inspection and test procedures;\n    5. availability of specified production, measuring and inspection equipment, and calibration status, when relevant;\n    6. cleanliness of facilities, with respect to the specified cleanliness levels;\n    7. facility temperature and humidity with respect to requirements.\n"]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.1a","Requirement","ECSS-Q-ST-20_0380104",1,"Created","The supplier shall monitor all processes used for manufacturing, assembly and integration, and enforce all applicable process requirements."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.1b","Requirement","ECSS-Q-ST-20_0380105",1,"Created","The supplier shall ensure that all manufacturing processes are covered by documented process specifications or standards.\n    NOTE Manufacturing process specifications are defined in ECSS-Q-ST-70."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.1c","Requirement","ECSS-Q-ST-20_0380106",1,"Created","Process specifications shall include QA provisions, methods for inspection and test, number of samples, accept or reject criteria."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.1d","Requirement","ECSS-Q-ST-20_0380107",1,"Created","Process witness samples shall be stored in controlled conditions."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.2a","Requirement","ECSS-Q-ST-20_0380108",1,"Created","The supplier shall establish and implement procedures and controls for special processes, to ensure that:\n    1. Special processes are validated for the intended application.\n        NOTE Validation of special processes is defined in ECSS-Q-ST-70.\n    2. Personnel who perform special processes or evaluate the process performance are trained and certified or can demonstrate their proficiency through their regular activity.\n    3. Materials, equipment, computer systems and software, and procedures involved in the performance of the special process are validated and monitored.\n    4. Coordination is maintained with the cognizant engineering function to ensure proper selection of the non-destructive or destructive methods for the evaluation of process performance."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.3.3a","Recommendation","ECSS-Q-ST-20_0380227",1,"Created","Statistical methods for process control should be used for early detection of significant variations in manufacturing processes, in order to determine, analyse and eliminate the causes of undesirable variations."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.4a","Requirement","ECSS-Q-ST-20_0380110",1,"Created","The supplier shall employ workmanship standards throughout all phases of manufacturing, assembly and integration, to ensure acceptable and consistent workmanship quality levels."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.4b","Requirement","ECSS-Q-ST-20_0380111",1,"Created","Workmanship standards shall identify acceptance or rejection criteria."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.4c","Requirement","ECSS-Q-ST-20_0380112",1,"Created","Physical samples or visual aids shall be reviewed and agreed by the customer when they are used for the purpose of acceptance or rejection of items."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.5a","Requirement","ECSS-Q-ST-20_0380113",1,"Created","The supplier shall ensure that only conforming items are released and used, and that those not required for the operation involved are removed from work operation areas."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.5b","Requirement","ECSS-Q-ST-20_0380114",1,"Created","Items having limited-life or definite characteristics of quality degradation or drift with age or use shall be marked to indicate the dates, test times or cycles at which life was initiated and at which the useful life expires."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.5c","Requirement","ECSS-Q-ST-20_0380115",1,"Created","Sensitive items shall be processed or manufactured, inspected and tested in a controlled environment to prevent any degradation.\n    NOTE Requirements for the selection and control of materials and parts are defined in ECSS-Q-ST-70."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1a","Requirement","ECSS-Q-ST-20_0380116",1,"Created","The supplier shall make provisions for accountability, identification and maintenance of manufacture, assembly and integration tooling."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1b","Requirement","ECSS-Q-ST-20_0380117",1,"Created","Manufacture, assembly and integration tooling shall be checked for its dimensional accuracy, regarding the product drawings, and correct function."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1c","Requirement","ECSS-Q-ST-20_0380118",1,"Created","The QA organization shall approve tooling prior to use."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1d","Requirement","ECSS-Q-ST-20_0380119",1,"Created","The approval shall be stamped in conformance with 5.2.4, and recorded."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1e","Requirement","ECSS-Q-ST-20_0380120",1,"Created","Tools shall be checked for accuracy during the production life at adequate intervals."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1f","Requirement","ECSS-Q-ST-20_0380121",1,"Created","Tools shall be submitted to re-approval following modification."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1g","Requirement","ECSS-Q-ST-20_0380122",1,"Created","Tools shall be properly stored to prevent misuse, damage and deterioration."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1h","Requirement","ECSS-Q-ST-20_0380123",1,"Created","Unnecessary tools shall be removed from working areas."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.1i","Requirement","ECSS-Q-ST-20_0380124",1,"Created","Records shall be kept of all manufacturing equipment. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.2a","Requirement","ECSS-Q-ST-20_0380125",1,"Created","The supplier shall ensure that computer-aided techniques and data for processing and machining are validated prior to use and controlled during their use in manufacturing."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.6.2b","Requirement","ECSS-Q-ST-20_0380126",1,"Created","The supplier shall ensure that provisions are made for the testing, approval and configuration control of the software involved and prevention of its being tampered with."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.1a","Requirement","ECSS-Q-ST-20_0380127",1,"Created","The supplier shall establish controls for cleanliness of spacecraft hardware and facilities, and the limitation of sources of contamination.\n    NOTE Cleanliness and contamination control methods and processes are detailed in ECSS-Q-ST-70-01."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.2a","Requirement","ECSS-Q-ST-20_0380128",1,"Created","Contamination-sensitive items shall be cleaned, controlled and maintained to the required cleanliness levels."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.2b","Requirement","ECSS-Q-ST-20_0380129",1,"Created","The required cleanliness levels for all levels of flight hardware shall be indicated on drawings, specifications, procedures, or other documents controlling the manufacture, assembly, integration and test of the items. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.3a","Requirement","ECSS-Q-ST-20_0380130",1,"Created","The supplier shall develop detailed methods for attaining the cleanliness levels specified for the hardware."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.4a","Requirement","ECSS-Q-ST-20_0380131",1,"Created","Contamination shall be minimized by operating in clean working areas and by proper handling, preservation, packaging and storage."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.4b","Requirement","ECSS-Q-ST-20_0380132",1,"Created","Contamination-sensitive items fabricated or processed in contamination-controlled environments shall be inspected, tested, modified or repaired in identical or cleaner environments, unless specific precautions are taken to protect the items concerned from contamination."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.4c","Requirement","ECSS-Q-ST-20_0380133",1,"Created","Specific protection measures, such as protective dust covers, shall be implemented to protect contamination-sensitive items when they are integrated in a higher level of assembly."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.7.5a","Requirement","ECSS-Q-ST-20_0380134",1,"Created","Fabrication, assembly and integration of contamination sensitive items shall be conducted in facilities that provide cleanliness levels compatible with the specified product cleanliness."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8a","Requirement","ECSS-Q-ST-20_0380135",1,"Created","Inspection and tests shall be planned at the points of the manufacturing, assembly and integration flow where maximum assurance for correct processing and prevention of unrecoverable or costly nonconformances can be obtained."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8b","Requirement","ECSS-Q-ST-20_0380136",1,"Created","All identified critical characteristics shall be inspected as defined in the critical-item control programme."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8c","Requirement","ECSS-Q-ST-20_0380137",1,"Created","Self-inspection by the operators performing the associated manufacturing, assembly and integration activities shall not be considered sufficient for critical characteristics."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8d","Requirement","ECSS-Q-ST-20_0380138",1,"Created","Among the inspections and tests as part of the manufacturing, assembly and integration flow, mandatory inspection points (MIPs) shall be performed with participation of the customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8e","Requirement","ECSS-Q-ST-20_0380139",1,"Created","MIPs shall be agreed with the customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8f","Requirement","ECSS-Q-ST-20_0380140",1,"Created","MIPs shall be selected in accordance with the criteria as defined below, when one or more of the following conditions apply:\n    1. When maximum visibility of quality is given.\n    2. When critical processes are performed.\n    3. Where the next step of the manufacturing sequence:\n        (a) is irreversible, or\n        (b) makes the item difficult and costly to disassemble for inspection, or\n        (c) renders the location inaccessible for inspection.\n    4. When the item, once installed in the next higher assembly damages by its failure the higher assembly.\n    5. When previous failure history of the item indicates a need for inspection.\n    6. When a potential adverse impact on the properties and integrity of the end product could result, owing to the criticality or complexity of the manufacturing step.\n    7. When testing or critical inspections cannot be accomplished by the supplier.\n        NOTE For example, environments or test equipment not available at supplier’s facility.\n    8. When verification tests are destructive in nature and the quality cannot be verified solely by inspection or test at the supplier’s facility.\n    9. When manufacturing and AIV of complex equipment or subsystems is planned.\n        NOTE For example, for payloads.\n    10. When past performance or quality history of the lower level supplier is marginal.\n    11. When an item is going to final inspection."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8g","Requirement","ECSS-Q-ST-20_0380141",1,"Created","Criteria 5.5.8f.7 to 10 shall be considered together with the criticality and complexity of the supplies and the supplier’s experience with the lower level supplier."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8h","Requirement","ECSS-Q-ST-20_0380142",1,"Created","A MIP shall require an invitation with the agreed notice before the event, and the participation of the customer, or their written agreement to proceed without their participation."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.8i","Requirement","ECSS-Q-ST-20_0380143",1,"Created","The supplier shall make provisions for a positive identification of the inspection and test status of any items at any stage of the manufacturing, assembly and integration cycle, starting from the incoming inspection up to shipping of the end item."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.1a","Requirement","ECSS-Q-ST-20_0380144",1,"Created","The supplier shall ensure the control of flight items which are temporarily removed or non-flight items which are temporarily installed to facilitate assembly, integration, testing, handling or preservation of the end item."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.1b","Requirement","ECSS-Q-ST-20_0380145",1,"Created","The control shall be initiated upon installation or removal of the first temporarily installed or removed item and be maintained through delivery and use of the end item."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.1c","Requirement","ECSS-Q-ST-20_0380146",1,"Created","The supplier shall establish and maintain records of temporary installations and removals."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.1d","Requirement","ECSS-Q-ST-20_0380147",1,"Created","Temporarily installed items shall be accounted for to prevent their being incorporated in the final flight configuration."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.2a","Requirement","ECSS-Q-ST-20_0380148",1,"Created","The supplier shall prepare and maintain system, subsystem and equipment logbooks in conformance with the DRD in Annex C for all operations and tests performed on the item during the period to be covered by the logbook."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.2b","Requirement","ECSS-Q-ST-20_0380149",1,"Created","Equipment logbooks shall start with the first qualification or acceptance test after assembly."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.2c","Requirement","ECSS-Q-ST-20_0380150",1,"Created","Subsystem and system logbooks shall follow-on from the individual equipment logbooks to form a full record."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.2d","Requirement","ECSS-Q-ST-20_0380151",1,"Created","The logbook shall accompany the hardware whenever it is placed in the custody of another organization"]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.9.2e","Requirement","ECSS-Q-ST-20_0380152",1,"Created","The receiving organization shall maintain the logbook up-to-date."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.5.10a","Requirement","ECSS-Q-ST-20_0380153",1,"Created","The supplier shall establish and maintain manufacturing, assembly and integration records to provide all manufacturing, assembly, integration and inspection data required for traceability."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.1a","Requirement","ECSS-Q-ST-20_0380154",1,"Created","The supplier shall ensure that test facilities, either internal or external, conform to specified requirements."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.2a","Requirement","ECSS-Q-ST-20_0380155",1,"Created","The supplier shall ensure that computer-aided testing techniques and data are validated prior to use and controlled during their use in testing."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.2b","Requirement","ECSS-Q-ST-20_0380156",1,"Created","The supplier shall ensure that provisions are made for testing, approval and configuration control of the software involved and prevention of its being tampered with."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.2c","Requirement","ECSS-Q-ST-20_0380157",1,"Created","The supplier shall ensure that test equipment are designed such that their correct operation can be verified without having to apply them to the test item."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.3.1a","Requirement","ECSS-Q-ST-20_0380158",1,"Created","The supplier shall ensure that tests are performed in accordance with documented procedures, which shall include, as a minimum:\n    1. scope of the test, including the identification of the requirement being verified,\n    2. identification of the test object,\n    3. applicable documents, with their revision status,\n    4. test flow,\n    5. test organization,\n    6. test conditions,\n    7. test equipment and set-up,\n    8. step-by-step procedure, including definition of specific steps to be witnessed by QA personnel,\n    9. recording of data,\n    10. pass or fail criteria and test data evaluation requirements, and\n    11. guidelines or criteria for deviation from test procedure and for retest."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.3.1b","Requirement","ECSS-Q-ST-20_0380159",1,"Created","The QA organization shall review and approve test procedures."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.3.2a","Requirement","ECSS-Q-ST-20_0380160",1,"Created","The supplier shall ensure that all tests are comprehensively documented in test reports, and that they include, as a minimum:\n    1. reference to the applicable test procedure, and description of the deviations from it during the actual testing,\n    2. test data records and evaluation, and\n    3. summary of test results."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.3.2b","Requirement","ECSS-Q-ST-20_0380161",1,"Created","The QA organization shall review and approve test reports."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4a","Requirement","ECSS-Q-ST-20_0380162",1,"Created","On the basis of an analysis of the test plan, the QA organization shall define within the test plan the most appropriate way to monitor the performance of test activities, to ensure the adherence to the test procedures, and that any deviations are properly documented and treated."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4b","Requirement","ECSS-Q-ST-20_0380163",1,"Created","Test witnessing by QA personnel shall be considered when manual intervention is performed, at the setting-up, start and end of continuous fully automated test sequences, or when no automatic recording of test parameters or results is available."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4c","Requirement","ECSS-Q-ST-20_0380164",1,"Created","All testing activities related to critical characteristics as identified in the critical-items control programme shall be certified."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4d","Requirement","ECSS-Q-ST-20_0380165",1,"Created","Self-certification by the operators performing the test activities shall not be considered sufficient for critical characteristics."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4e","Requirement","ECSS-Q-ST-20_0380166",1,"Created","Testing activities or results to be subject to QA certification shall be identified as such in the relevant test procedure."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4f","Requirement","ECSS-Q-ST-20_0380167",1,"Created","Testing shall be subject to the requirements for the control of hazardous operations.\n    NOTE Definition of hazardous operations is given in ECSS-Q-ST-40."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.4g","Requirement","ECSS-Q-ST-20_0380168",1,"Created","Where safety of personnel or damage to items or associated test equipment is possible, QA personnel shall have the authority to stop the test."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.5a","Requirement","ECSS-Q-ST-20_0380169",1,"Created","The supplier shall ensure that formal reviews are performed before and after major portions of qualification or acceptance tests."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.6.5b","Requirement","ECSS-Q-ST-20_0380170",1,"Created","The QA organization shall be represented in the formal boards established for the review of readiness for testing and testing accomplishment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.1a","Requirement","ECSS-Q-ST-20_0380171",1,"Created","The supplier shall establish a formal acceptance process for all deliverable items, at any contractual level, to ensure that conformance of the items to be delivered is fully assessed and documented."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.1b","Requirement","ECSS-Q-ST-20_0380172",1,"Created","The supplier shall ensure that the preparation of the items for delivery and the physical delivery itself are performed in such a way that quality degradation is prevented."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.2a","Requirement","ECSS-Q-ST-20_0380173",1,"Created","The supplier shall provide an EIDP for each deliverable end item in conformance with the DRD in Annex B."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.2b","Requirement","ECSS-Q-ST-20_0380174",1,"Created","The EIDP shall constitute the basis for formal acceptance reviews."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.2c","Requirement","ECSS-Q-ST-20_0380175",1,"Created","EIDPs shall be maintained and integrated into higher level EIDPs during subsystem or system integration and testing. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3a","Requirement","ECSS-Q-ST-20_0380176",1,"Created","The supplier shall ensure that a DRB is convened prior to the delivery of equipment, separately assembled subsystems, test equipment or handling equipment for higher level activities.\n    NOTE “Acceptance Review Board” (ARB) defined in ECSS-M-ST-10 is referred to as “Delivery Review Board” (DRB) in this document."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3b","Requirement","ECSS-Q-ST-20_0380177",1,"Created","The DRB functions at system level shall be fulfilled by the final acceptance review and chaired by the customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3c","Requirement","ECSS-Q-ST-20_0380178",1,"Created","The DRB shall be composed, at least, of the following members:\n    1. Representatives of the receiving organization:\n        (a) Project manager, or authorized representative, as chairman;\n        (b) PA manager, or authorized representative;\n        (c) Engineering or design manager, or authorized representative.\n    2. Submitting supplier’s representatives:\n        (a) Project manager, or authorized representative;\n        (b) PA manager, or authorized representative;\n        (c) Engineering or design manager, or authorized representative.\n    3. Higher level customers’ representative(s), as observers (not required for separate subsystems)."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3d","Requirement","ECSS-Q-ST-20_0380179",1,"Created","If the final customer reserves the right to attend DRBs at any lower level as an observer, he shall be given due notice of such a DRB meeting."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3e","Requirement","ECSS-Q-ST-20_0380180",1,"Created","The DRB shall be responsible for authorising the shipment of the items under acceptance, and certifying in writing that:\n    1. the items conform to the contractual requirements and to an approved design configuration;\n    2. the items are free from material and workmanship deficiencies;\n    3. all nonconformances are closed-out, or corresponding plans, compatible with the delivery, are accepted;\n    4. the relevant EIDP is complete and accurate."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3f","Requirement","ECSS-Q-ST-20_0380181",1,"Created","Delivery shall only be authorized by the unanimous agreement of the DRB members."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.3g","Requirement","ECSS-Q-ST-20_0380182",1,"Created","For the delivery a certificate of conformity, in conformance with Annex D, shall be made available and signed by the supplier."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.4.1a","Requirement","ECSS-Q-ST-20_0380183",1,"Created","The supplier shall ensure that packaging materials, methods, procedures and instructions provide for protection of items while at the supplier’s plant, during transportation, and after their arrival at destination."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.4.2a","Requirement","ECSS-Q-ST-20_0380184",1,"Created","The supplier shall ensure that appropriate marking and labelling for packaging, storage, transportation and shipping of items are performed in accordance with the applicable specifications."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.5.1a","Requirement","ECSS-Q-ST-20_0380185",1,"Created","The supplier shall ensure that the items to be shipped from his plant are inspected before release and found to be complete, adequately preserved and packaged, correctly marked and accompanied by all the required documentation."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.5.1b","Requirement","ECSS-Q-ST-20_0380186",1,"Created","Accompanying documentation shall include the EIDP and, attached to the outside of the shipping container, the handling and packing or unpacking procedure and any relevant safety procedures."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.7.5.2a","Requirement","ECSS-Q-ST-20_0380187",1,"Created","The supplier shall make provisions for the prevention of damage to items during transportation."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.1.1.1a","Requirement","ECSS-Q-ST-20_0380188",1,"Created","The supplier shall ensure that internal design and verification standards are used or developed corresponding with the techniques to be used and fitting with the level of complexity of the items to be developed."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.1.1.1b","Requirement","ECSS-Q-ST-20_0380189",1,"Created","The supplier shall ensure that development risks are identified and appropriate back-up solutions are identified."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.1.1.1c","Requirement","ECSS-Q-ST-20_0380190",1,"Created","The supplier shall ensure that the verification method and process are tailored to the:\n    1. complexity of the item to be verified;\n    2. criticality of the function to be implemented by the GSE item;\n    3. inherent criticality of the item itself."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.2a","Requirement","ECSS-Q-ST-20_0380191",1,"Created","The supplier shall ensure that GSE is configuration controlled."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.3.1a","Requirement","ECSS-Q-ST-20_0380192",1,"Created","The supplier shall ensure that selected GSE suppliers have a demonstrated ability to conform to requirements, through:\n    1. previous supply of items similar or more complex in the same field of techniques and technologies,\n    2. certification covering similar design, development and production as applicable for similar items in conformance with 5.4.1.2, or\n    3. evidence, documented by existing design, development, production and quality standards, of having similar experience associated with known success."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.3.1b","Requirement","ECSS-Q-ST-20_0380193",1,"Created","Procurement documents shall identify validation and receiving inspection requirements, and conform to the requirements in clause 5.4.2."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.3.2a","Recommendation","ECSS-Q-ST-20_0380228",1,"Created","The supplier and his lower level suppliers should not deviate from their standard practices when these are already documented and recognized for similar items."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.4.1a","Requirement","ECSS-Q-ST-20_0380195",1,"Created","The acceptance data package shall include :\n    1. information regarding interfaces,\n    2. deviations from contractual requirements,\n    3. certification of conformance to an identified baseline,\n    4. description of the functioning of the item, and instructions to operate and maintain it, and\n    5. safety data or safety certification(s)."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.5a","Requirement","ECSS-Q-ST-20_0380196",1,"Created","Acceptance shall be achieved through a formal review process \n    NOTE Review process is defined in ECSS-M-ST-10-01."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.5b","Requirement","ECSS-Q-ST-20_0380197",1,"Created","The acceptance process shall include:\n    1. acceptance plan,\n    2. inspection and test procedures, and\n    3. inspection and test reports."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.5c","Permission","ECSS-Q-ST-20_0380229",1,"Created","Acceptance may be achieved through a simple inspection process if agreed between customer and supplier."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.6a","Requirement","ECSS-Q-ST-20_0380199",1,"Created","The supplier shall propose GSE elements for which acceptance is granted by a delivery board and agree these with his customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.6b","Requirement","ECSS-Q-ST-20_0380200",1,"Created","The delivery board shall include QA representatives from the supplier and the customer."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.7a","Requirement","ECSS-Q-ST-20_0380201",1,"Created","The requirements of the following clauses shall be applied to the delivery of ground items and handling, storage, packing and shipping activities:\n    1. preparation for delivery, in conformance with 5.7.4,\n    2. delivery, in conformance with 5.7.5, and\n    3. handling, storage and preservation, in conformance with 5.2.7."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.8a","Requirement","ECSS-Q-ST-20_0380202",1,"Created","The following requirements shall be tailored in accordance with the complexity and criticality of the GSE item:\n    1. traceability requirements in 5.2.5, and\n    2. metrology and calibration requirements in 5.2.6."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.9a","Requirement","ECSS-Q-ST-20_0380203",1,"Created","The supplier shall ensure that maintenance activities are planned."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","5.8.9b","Requirement","ECSS-Q-ST-20_0380204",1,"Created","The supplier shall ensure that maintenance demonstration is performed in order to prove that maintainability requirements are satisfied in the real operational environment."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-20_0380205",1,"Created","The Quality Assurance Plan shall introduce the purpose, objective and the reason prompting its preparation "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<2>a","Requirement","ECSS-Q-ST-20_0380206",1,"Created","The Quality Assurance Plan shall list the applicable and reference documents in support of the generation of the document."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<3>a","Requirement","ECSS-Q-ST-20_0380207",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable quality assurance general requirements defined in ECSS-Q-ST-20 clause 5.1."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<4>a","Requirement","ECSS-Q-ST-20_0380208",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable Quality assurance requirements for design and verification defined in ECSS-Q-ST-20 clause 5.3."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<5>a","Requirement","ECSS-Q-ST-20_0380209",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable Quality assurance requirements for procurement defined in ECSS-Q-ST-20 clause 5.4"]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<6>a","Requirement","ECSS-Q-ST-20_0380210",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable Quality assurance requirements for manufacturing, assembly and integration defined in ECSS-Q-ST-20 clause 5.5."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<7>a","Requirement","ECSS-Q-ST-20_0380211",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable Quality assurance requirements for testing defined in ECSS-Q-ST-20 clause 5.6."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.1<8>a","Requirement","ECSS-Q-ST-20_0380212",1,"Created","The Quality Assurance Plan shall describe the activities to be applied to fulfil the applicable Quality assurance requirements for acceptance and delivery defined in ECSS-Q-ST-20 clause 5.7."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","A.2.2a","Permission","ECSS-Q-ST-20_0380230",1,"Created","The response to this DRD may be combined with the response to the product assurance plan, as defined in ECSS-Q-ST-10."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","B.2.1a","Requirement","ECSS-Q-ST-20_0380214",1,"Created","The EIDP shall include the following information and documentation:\n    1. The DRB minutes\n    2. The customer acceptance certificate if not covered in DRB minutes\n    3. Cover page\n        NOTE An example is given in Annex F.\n    4. Table of contents\n        NOTE An example is given in Annex G.\n    5. Change record\n    6. The product certificate of conformity in conformance with Annex D.\n    7. NCR list\n    8. ABCL\n    9. Summary and status of RFDs and RFWs raised and processed on the product\n    10. The product logbook\n    11. Product definition documents to be used for further integration, testing and operation in higher level assemblies including the software used to operate the item and the product user or operating manuals.\n    12. Procedures to be used for the proper handling of the product after its final delivery, including procedures for:\n        (a) packing,\n        (b) handling,\n        (c) storage,\n        (d) transportation,\n        (e) safety, and\n        (f) cleanliness.\n    13. Copies of the product test reports, or as a minimum the list of the documents with the identification of their location.\n    14. List of delivered ground support equipment (e.g.: MGSE, EGSE, FGSE, OGSE) with the reference to their corresponding EIDPs and software product.\n    15. List of EIDPs or logbooks of units and subsystem supplied by lower tier suppliers.\n    16. List of the loose items and not installed items supplied with the product.\n    17. Any additional useful information or data relevant to the product.\n        NOTE For example, cleanliness certification when cleanliness is a requirement."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1a","Requirement","ECSS-Q-ST-20_0380215",1,"Created","The logbook cover page shall contain the following:\n    1. general information,\n    2. contents,\n    3. approvals of the relevant authorities (QA, PA, PM), and\n    4. customer acceptance (if required by the business agreement).\n        NOTE An example of a logbook cover page is given in Annex E."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1b","Requirement","ECSS-Q-ST-20_0380216",1,"Created","The logbook shall contain the “hardware configuration and traceability” table, which reports all the identification references of single elements composing the CI. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1c","Requirement","ECSS-Q-ST-20_0380217",1,"Created","The logbook shall contain the “hardware configuration change and status” table, which reports for each singe element of the CI all the events relevant to integration, removal and replacement on the higher level."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1d","Requirement","ECSS-Q-ST-20_0380218",1,"Created","The logbook shall contain the summary list of the integration and test instructions, including for each entry, the action start date, action performed date and action close-out date shall also be reported.\n    NOTE Example: shop traveller"]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1e","Requirement","ECSS-Q-ST-20_0380219",1,"Created","The logbook shall contain the summary list of nonconformances with relevant identification references, issue date, closure dates, and status."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1f","Requirement","ECSS-Q-ST-20_0380220",1,"Created","The logbook shall contain all the electrical connector (or other limited cycles items) mate and demate cycles in order to ensure the conformance with the project requirements."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1g","Requirement","ECSS-Q-ST-20_0380221",1,"Created","The logbook shall contain the records of total operating hours for each limited-life element identified in the test procedures."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1h","Requirement","ECSS-Q-ST-20_0380222",1,"Created","The logbook shall contain, in chronological order, the events related to the integration and test activities performed on the relevant item (i.e. system, subsystem, and equipment), including the following:\n    1. Action requested form, reporting all the operations performed with the references to the applicable documents or procedures, start date, completion date and quality inspection stamps.\n    2. Step-by-step procedures and results, in which copies of the as-run procedures are included in a suitable format.\n    3. Procedures variation form, in which copies of modified procedures (red marked) identified with a procedure variation number and duly approved by responsible authorities, are included. "]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","C.2.1i","Requirement","ECSS-Q-ST-20_0380223",1,"Created","The logbook shall contain the list of open action or open test at the time of the product shipment to the customer, test facility or launch pad."]
["ECSS-Q-ST-20C","ECSS - Superseded v1.0","D.2.1a","Requirement","ECSS-Q-ST-20_0380224",1,"Created","The DoC shall contain the following elements:\n    1. Title including references to identify the product and the relevant applicable documents\n        NOTE Examples for references are item name, project, serial number, part number, customer, contract number.\n    2. Document no. in accordance with project configuration control rules;\n    3. EIDP reference number;\n    4. Intended use, specifying the item objective (i.e. BB, QM, FM)\n    5. Reference of conformity, calling for example the following documents:\n        (a) Business agreement requirements: reference number of design spec., ICD or other contractual documents;\n        (b) Operational documents: reference number of drawings, procedures, and electrical schemes;\n        (c) Deliverable documents: reference number of EIDP, logbooks, and manuals.\n    6. Statement of conformity.\n    7. List of waivers or deviations or other remarks."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.1.2a","Requirement","ECSS-Q-ST-70_0490001",1,"Created","The supplier shall prepare, maintain and implement a MMPP plan, as part of the overall PA plan in conformance to ECSS-Q-ST-10 and this Standard or as a separate document."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.1.2b","Requirement","ECSS-Q-ST-70_0490002",1,"Created","The MMPP plan shall be submitted to the customer for approval."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.1.3a","Requirement","ECSS-Q-ST-70_0490003",1,"Created","To obtain the validation status for materials and qualification status for parts and verification status for processes, the MMPP manager shall present to the customer those activities which were performed in order to comply with this Standard together with results obtained."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.1.3b","Requirement","ECSS-Q-ST-70_0490004",1,"Created","The MMPP manager shall organize technical review meetings with his suppliers at all levels."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2a","Requirement","ECSS-Q-ST-70_0490005",1,"Created","Each supplier and sub-supplier shall establish, collect, review and deliver the declared materials, mechanical parts and processes lists including all the items intended for use in the flight equipment."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2b","Requirement","ECSS-Q-ST-70_0490006",1,"Created","The lists shall reflect the current design at the time of issue."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2c","Requirement","ECSS-Q-ST-70_0490007",1,"Created","These lists shall contain the materials, mechanical parts and processes used in the current design in order to: \n    1. demonstrate compliance with all requirements of the programme;\n    2. verify the results of equipment supplier activities;\n    3. control and monitor the status of materials, mechanical parts and processes in accordance with programme milestones.\n        NOTE See Annex F."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2d","Recommendation","ECSS-Q-ST-70_0490194",1,"Created","The following constraints should apply:\n    1. maximum use of the materials and processes described in approved data sources and items already approved on similar projects;\n        NOTE For approved data sources see for example ECSS-Q-ST-70-71.\n    2. use of project related preferred lists, if available."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2e","Requirement","ECSS-Q-ST-70_0490009",1,"Created","The following constraints shall be taken into account: \n    1. requirements originating from the initial technical specification;\n    2. programmatic project requirements and conditions;"]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2f","Requirement","ECSS-Q-ST-70_0490010",1,"Created","An analysis of the criticality of these preliminary lists shall, after checking the conformity of the materials, mechanical parts and processes, against all the project requirements, allow them to be classified into three categories:\n    1. Critical items, subject to evaluation, validation, qualification, or verification programmes.\n    2. Items that are not critical but which do not conform to one or more project requirements (a justified deviation request should be drafted for this category).\n    3. Non-critical items."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.2g","Requirement","ECSS-Q-ST-70_0490011",1,"Created","For critical items a request for approval shall be submitted in conformance with Annex D."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3a","Requirement","ECSS-Q-ST-70_0490012",1,"Created","The supplier shall document all materials in the Declared materials list in conformance with Annex A."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3b","Requirement","ECSS-Q-ST-70_0490013",1,"Created","The supplier shall document all mechanical parts in the Declared mechanical parts list in conformance with Annex B."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3c","Requirement","ECSS-Q-ST-70_0490014",1,"Created","The supplier shall document all processes in the Declared process list in conformance with Annex C."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3d","Requirement","ECSS-Q-ST-70_0490015",1,"Created","The supplier shall process the lists of lower level suppliers to ensure exchangeabililty, searchability, sortability, storability and retrievability for that set of lists, before submitting it to the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3e","Requirement","ECSS-Q-ST-70_0490016",1,"Created","These lists shall be updated during the course of the project."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3f","Requirement","ECSS-Q-ST-70_0490017",1,"Created","The preliminary lists shall include the items from suppliers’ preliminary needs.\n    NOTE They are used to identify critical items (available for the PDR)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3g","Requirement","ECSS-Q-ST-70_0490018",1,"Created","The as-designed lists shall include the items from the baselines various design files (available for the CDR)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.3h","Requirement","ECSS-Q-ST-70_0490019",1,"Created","Any change after CDR or QR shall be reflected in the list and shall be in accordance with Figure 4-1 (Part 2).\n    NOTE 1 The MMPP manager is responsible within the programme to ensure that all the information needed is given and that the approval status is consistent with technical and scheduling objectives and data is exchangeable.\n    NOTE 2 Where no project requirements exist for a separate DMPL, the mechanical parts can be entered into a separate section of the DML.\n    NOTE 3 The materials of, for example, screws and nuts that are made up of a few materials can be listed in the DMPL. The materials (metals and plastics) of complex parts can be listed in the DML with, for example, outgassing, toxicity, flammability, corrosion and stress corrosion values and reference to the DMPL item."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.4a","Requirement","ECSS-Q-ST-70_0490020",1,"Created","The supplier shall perform the following tasks:\n    1. obtaining the correct and complete lists from lower level suppliers;\n    2. providing provisional and, later, definitive approval for each list;\n    3. submitting the project declared lists for approval prior to initiation of the hardware phase (before critical design review)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.4b","Requirement","ECSS-Q-ST-70_0490021",1,"Created","The lists established by the suppliers shall include all the information described in this Standard."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.4c","Requirement","ECSS-Q-ST-70_0490022",1,"Created","Amendments to the lists shall be implemented only through established change procedures."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.4d","Requirement","ECSS-Q-ST-70_0490023",1,"Created","The following documentation shall be delivered to the customer upon request:\n    1. RFA (reference and issue);\n    2. evaluation reports;\n    3. deviation requests."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.2.4e","Requirement","ECSS-Q-ST-70_0490024",1,"Created","The material, mechanical parts or process justification files shall be made available to the customer upon request either on the supplier site, or by any other process agreed by both parties.\n    NOTE For example, by non-disclosure agreement."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.3a","Requirement","ECSS-Q-ST-70_0490025",1,"Created","Parts and materials shall satisfy the mission’s functional constraints."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.3b","Requirement","ECSS-Q-ST-70_0490026",1,"Created","Parts and materials shall satisfy both ground environment constraints and flight constraints.\n    NOTE Examples are:\n        · Ground environment constraints: manufacture, tests, storage, maintenance, transport and integration\n        · Flight constraints: launch and orbit."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.3c","Requirement","ECSS-Q-ST-70_0490027",1,"Created","The technical criteria from clause 5.1 shall be taken into account, according to the mission."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.3d","Requirement","ECSS-Q-ST-70_0490028",1,"Created","The estimated availability of the parts and products obtained from materials and processes used shall be compatible with the final system’s life cycle (tests, storage and mission)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.4a","Requirement","ECSS-Q-ST-70_0490029",1,"Created","The supplier shall establish and maintain a contamination and cleanliness control programme including, as a minimum:\n    1. cleaning procedures, and\n    2. cleanliness monitoring procedures or methods."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.4b","Requirement","ECSS-Q-ST-70_0490030",1,"Created","The risks of chemical or particle pollution generated by parts, materials or processes used shall be identified and reduced in accordance with mission requirements (cleanliness or contamination analysis)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.4c","Requirement","ECSS-Q-ST-70_0490031",1,"Created","For cleanliness- or contamination-critical applications, a requirement specification (chemical and particle) and a specific cleanliness control plan and shall be established in conformance with Annex A (CRS DRD) and Annex B (C&CCP DRD) of ECSS-Q-ST-70-01."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.5a","Requirement","ECSS-Q-ST-70_0490032",1,"Created","Parts and materials with hazardous characteristics shall be identified, managed and processed in conformance with ECSS-Q-ST-40."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","4.6a","Requirement","ECSS-Q-ST-70_0490033",1,"Created","When optical, mechanical or electrical GSE materials are used in thermal vacuum or interfacing with flight hardware, possible degradation shall be taken into account.\n    NOTE For example, contamination, surface degradation, electro-mechanical and chemical effects."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.2a","Requirement","ECSS-Q-ST-70_0490034",1,"Created","Material properties shall be compatible with the thermal environment to which they are exposed."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.3a","Requirement","ECSS-Q-ST-70_0490035",1,"Created","Materials subject to thermal cycling shall be assessed for their ability to withstand induced thermal stress."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.3b","Requirement","ECSS-Q-ST-70_0490036",1,"Created","The following materials shall be tested in conformance with ECSS-Q-ST-70-04:\n    1. Materials susceptible to thermal vacuum effect.\n        NOTE For a non-exhaustive list of such materials, see ECSS-Q-ST-70-04 Clause 1.\n    2. Materials of unknown characteristics in respect to thermal vacuum."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.3c","Requirement","ECSS-Q-ST-70_0490037",1,"Created","Materials subject to thermal cycling other than those covered by 5.1.3b, shall be tested in accordance with a procedure approved by the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.4a","Requirement","ECSS-Q-ST-70_0490038",1,"Created","Materials selection shall be made in conformance with ECSS-Q-ST-70-71."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.4b","Requirement","ECSS-Q-ST-70_0490039",1,"Created","Outgassing tests shall be carried out in conformance with ECSS-Q-ST-70-02.\n    NOTE The need for retest of materials used for an extended period of time at a temperature higher than 50 °C should be mutually agreed with the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.5a","Requirement","ECSS-Q-ST-70_0490040",1,"Created","Spacecraft and associated equipment shall be manufactured from materials and by processes that do not cause a hazard to personnel or hardware, whether on the ground or in space."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.5b","Requirement","ECSS-Q-ST-70_0490041",1,"Created","ECSS-Q-ST-70-29 shall apply for the characterization of offgassing products.\n    NOTE MAPTIS and MIL-HDBK-454 test method is not space relevant."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.6a","Requirement","ECSS-Q-ST-70_0490042",1,"Created","The materials flammability resistance shall be evaluated in conformance with ECSS-Q-ST-70-21 for the most hazardous environment envisaged for their use.\n    NOTE For NASA STS payloads see NASA STD-6001."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.7a","Requirement","ECSS-Q-ST-70_0490043",1,"Created","Materials used on the spacecraft external surfaces shall be assessed in conformance with ECSS-Q-ST-70-06 in order to determine their resistance to the radiation dosage expected during the mission."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.8a","Requirement","ECSS-Q-ST-70_0490044",1,"Created","External surfaces of the spacecraft shall be sufficiently conductive, interconnected and grounded to the spacecraft structure to avoid the build-up of differential charges in conformance with ECSS-E-ST-20-06."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.9a","Requirement","ECSS-Q-ST-70_0490045",1,"Created","For all materials that come into contact with atmospheric gases, cleaning fluids or other chemicals, it shall be demonstrated that the degradation of properties during their anticipated service-life is acceptable in terms of the performance and integrity requirements."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.10a","Requirement","ECSS-Q-ST-70_0490046",1,"Created","Materials used for structural and load-bearing applications (subject to tensile stress) shall be chosen in conformance with ECSS-Q-ST-70-36."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.10b","Requirement","ECSS-Q-ST-70_0490047",1,"Created","Any material not covered by standard ECSS-Q-ST-70-36 shall be tested in conformance with ECSS-Q-ST-70-37."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.11a","Requirement","ECSS-Q-ST-70_0490048",1,"Created","Materials within the system exposed to liquid oxygen (LOX), gaseous oxygen (GOX) or other reactive fluids, both directly and as a result of single point failures when failure propagation effects cause hazardous operation of interfacing hardware shall be compatible with that fluid in their application."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.11b","Requirement","ECSS-Q-ST-70_0490049",1,"Created","The possibility of hydrogen embrittlement occurring during component manufacture or use shall be assessed, and an material evaluation be undertaken, including the assessment of adequate protection and control."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.12a","Requirement","ECSS-Q-ST-70_0490050",1,"Created","When bimetallic contacts are used, the choice of the pair of metallic materials used shall be agreed with the customer. \n    NOTE This also includes metal-to-conductive fibre-reinforced materials contacts."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.12b","Requirement","ECSS-Q-ST-70_0490051",1,"Created","Galvanic compatibilities shall be selected in conformance with Table 5-1."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.12c","Requirement","ECSS-Q-ST-70_0490052",1,"Created","Materials not listed in Table 5-1 shall be evaluated in a flight-simulated configuration using an accelerated environment to be agreed by the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.13a","Requirement","ECSS-Q-ST-70_0490053",1,"Created","All materials considered for use on the external surfaces of spacecraft intended for use in Low Earth Orbit (LEO) altitudes (between 200 km and 700 km) shall be evaluated for their resistance to atomic oxygen (ATOX)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.13b","Requirement","ECSS-Q-ST-70_0490054",1,"Created","Test procedures shall be subject to the approval of the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.14a","Requirement","ECSS-Q-ST-70_0490055",1,"Created","The effect of impacts by micrometeoroids and debris on materials shall\n    1. be reviewed and assessed on a case by case basis, and\n    2. their use comply with safety evaluation and assessment results concerning design and application criteria or details."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.15a","Requirement","ECSS-Q-ST-70_0490056",1,"Created","Precautions shall be taken to avoid moisture absorption during manufacture and storage of CFRP-type materials in conformance with ECSS-Q-ST-70-01 and ECSS-Q-ST-70-22."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.16a","Requirement","ECSS-Q-ST-70_0490057",1,"Created","For all solid surfaces in moving contact with other solid surfaces, it shall be demonstrated that the degradation of surface properties over the complete mission is acceptable from a performance point of view."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.1.17a","Requirement","ECSS-Q-ST-70_0490058",1,"Created","Materials shall be selected to ensure sufficient life with respect to the intended application."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-70_0490059",1,"Created","Materials shall be chosen giving preference to the following:\n    1. those successfully used for an identical application in other space programmes similar with respect to environment constraints and lifetime to the proposed application;\n    2. those for which satisfactory evaluation results are obtained on samples representative of the application with a sufficient margin as regards conditions of use;\n    3. those included in approved data sources.\n        NOTE For example: ECSS-Q-ST-70-71, ESA and NASA data banks."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-Q-ST-70_0490060",1,"Created","Whether the materials are already validated or remain to be validated, their selection shall take into account the following criteria:\n    1. continuity of supply;\n    2. reproducibility of characteristics."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-Q-ST-70_0490061",1,"Created","Pure tin finish with more than 97 % purity shall not be used.\n    NOTE This is due to the possibility of whisker growth and transformation to grey tin powder at low temperatures."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.2.2b","Requirement","ECSS-Q-ST-70_0490062",1,"Created","The incoming inspection of each component batch shall include the verification of the termination composition (to avoid assembly of pure tin finish)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.3a","Requirement","ECSS-Q-ST-70_0490063",1,"Created","The supplier shall establish and maintain a declared materials list in conformance with Annex A."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-70_0490064",1,"Created","The supplier shall analyse all the materials contained in his preliminary lists with respect to criticality and in correlation with the risk analysis performed. "]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.4.2b","Requirement","ECSS-Q-ST-70_0490065",1,"Created","Any material not meeting the project requirements shall be subject to a RFD to be submitted to the next customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.4.2c","Requirement","ECSS-Q-ST-70_0490066",1,"Created","Any critical material shall be subject to a RFA to be submitted to the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.4.2d","Requirement","ECSS-Q-ST-70_0490067",1,"Created","For any material not meeting the project requirements the supplier shall submit a RFA in conformance with Annex D.\n    NOTE Any material when specifically required, marking inks can be excluded."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-70_0490068",1,"Created","Depending on the results of the criticality analysis, the supplier shall perform an evaluation phase before the validation phase for all critical materials with unknown characteristics (new materials) or with major changes in the use or in the configuration"]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.1b","Permission","ECSS-Q-ST-70_0490195",1,"Created","In case of an extension of an existing application, the evaluation indicated in 5.5.1a need not be performed if so agreed with the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.1c","Requirement","ECSS-Q-ST-70_0490070",1,"Created","Guarantied characteristics of materials and material supplier inspection methods, together with associated documents, shall be available for review at the supplier’s premises before the start of evaluation or qualification phases."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-70_0490071",1,"Created","The evaluation shall consider the following as a minimum:\n    1. the limits of use;\n    2. the materials physical, chemical or functional characteristics along with their values and tolerances;\n    3. behavioural tendencies and degradation processes depending on environmental parameters (including sensitivity to pollution);\n    4. acceptance criteria."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.2b","Requirement","ECSS-Q-ST-70_0490072",1,"Created","When evaluation is performed, an evaluation programme (available at PDR, according to Figure 4-1) shall be drawn up, implemented and an evaluation report (available before CDR, according to Figure 4-1 and Table 4-1) shall be drawn up."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.3a","Requirement","ECSS-Q-ST-70_0490073",1,"Created","For all critical materials, a validation programme (available at PDR) shall be drawn up by the supplier and then implemented to check or confirm that the materials satisfy the mission requirements with appropriate margins as necessary to obtain validation status."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.3b","Requirement","ECSS-Q-ST-70_0490074",1,"Created","Validation status shall depend on the results obtained (validation report) and the review of corresponding documentation (available at CDR)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.4a","Requirement","ECSS-Q-ST-70_0490075",1,"Created","The material shall not receive an approval identification in the declared material list for the project unless the requirements in 5.5.2 and 5.5.3 are satisfied."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.4b","Requirement","ECSS-Q-ST-70_0490076",1,"Created","If approval is not granted, the supplier in charge of the item shall either:\n    1. select another material, or\n    2. propose a modified evaluation programme and resubmit for approval, or\n    3. if actions 5.5.4b.1 and 5.5.4b.2 fail to achieve positive results, initiate a deviation procedure."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.5.5a","Requirement","ECSS-Q-ST-70_0490077",1,"Created","For materials not conforming to project requirements, whether at the end of criticality analysis or of evaluation and validation tests, the supplier shall submit a request for deviation in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1a","Requirement","ECSS-Q-ST-70_0490078",1,"Created","All materials shall be procured to an internationally or nationally recognized specification or an in-house fully configured procurement specification which defines the materials properties, the materials requirements, the test methods, the acceptance criteria for the specific applications, source inspection (if any) and material supplier inspection."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1b","Requirement","ECSS-Q-ST-70_0490079",1,"Created","Where material suppliers do not accept specifications and procurement is by means of a datasheet the supplier shall introduce internal, in-house receipt inspection to ensure that the validation status of the material is maintained during the subsequent procurements."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1c","Requirement","ECSS-Q-ST-70_0490080",1,"Created","Materials with long lead times or long procurement delays (versus the project schedule) shall be identified before the formal subsystem PDR. "]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1d","Requirement","ECSS-Q-ST-70_0490081",1,"Created","Procurement shall be thoroughly planned, documented and implemented in a timely manner to obtain reliable product assurance provision at CDR. "]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1e","Requirement","ECSS-Q-ST-70_0490082",1,"Created","Back-up plans shall be prepared and initiated whenever there is evidence of delays or technical problems."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.1f","Requirement","ECSS-Q-ST-70_0490083",1,"Created","The material requirements shall be explicitly accepted by the material supplier or manufacturer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.2a","Requirement","ECSS-Q-ST-70_0490084",1,"Created","All materials shall be submitted to an incoming inspection."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.6.2b","Requirement","ECSS-Q-ST-70_0490085",1,"Created","An incoming inspection procedure shall define the inspections and tests to be carried out, particularly for materials that are known to be variable in their final properties."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.1a","Requirement","ECSS-Q-ST-70_0490086",1,"Created","The supplier shall verify that all critical materials are validated before being used in the manufacture of qualification or flight products."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.1b","Requirement","ECSS-Q-ST-70_0490087",1,"Created","Any modification, change of condition or configuration of application shall lead to a re-evaluation in conformance with the process shown in Figure 4-1."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.2a","Requirement","ECSS-Q-ST-70_0490088",1,"Created","The supplier shall apply the traceability rules defined in ECSS-Q-ST-20 to all materials."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.2b","Recommendation","ECSS-Q-ST-70_0490196",1,"Created","Materials should be identified by a unique reference number, code or a lot number to provide traceability should there be an incident or nonconformance, or a need for a technical investigation following failure or damage, to reconstruct the materials history, either individually (individual traceability) or by the manufacturing lot of which it was a part (lot traceability)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.3a","Requirement","ECSS-Q-ST-70_0490090",1,"Created","The supplier shall define provisions for packaging, storage and removal from storage for materials."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.3b","Requirement","ECSS-Q-ST-70_0490091",1,"Created","Measurements and inspections used to guarantee the material integrity and monitoring during storage and removal from storage shall be identified."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.4a","Requirement","ECSS-Q-ST-70_0490092",1,"Created","The supplier shall ensure that all materials which have limited-life characteristics have their date of manufacture (when available, otherwise date of delivery) and shelf-life expiry date accurately identified and clearly marked on each lot or batch."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.4b","Permission","ECSS-Q-ST-70_0490197",1,"Created","Materials which have exceeded their shelf-life expiry date may be re-certified only after the physical and chemical characteristics are inspected and the parameters, subject to deterioration, are evaluated for continued acceptability according to the accept and reject criteria in conformance with ECSS-Q-ST-70-22."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.5a","Requirement","ECSS-Q-ST-70_0490094",1,"Created","Materials with limited-life after implementation (such as propellant) shall be identified and controlled in conformance with ECSS-Q-ST-10-04.\n    NOTE Storage and mission life are criteria for the assessment and control of those materials."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.6a","Requirement","ECSS-Q-ST-70_0490095",1,"Created","Nonconformances and alerts shall be managed in conformance with ECSS-Q-ST-10."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","5.7.7a","Requirement","ECSS-Q-ST-70_0490096",1,"Created","Material safety data sheet or equivalent shall be available for all materials."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.1a","Requirement","ECSS-Q-ST-70_0490097",1,"Created","The supplier shall verify that all materials and processes used in the manufacture of parts satisfy the mission technical requirements."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.2a","Requirement","ECSS-Q-ST-70_0490098",1,"Created","Parts shall be chosen from those successfully used for an identical application in other space programmes similar with respect to environment constraints and lifetime whenever those parts exist."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.2b","Requirement","ECSS-Q-ST-70_0490099",1,"Created","Type reduction actions shall be implemented at all levels of the programme."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.2c","Requirement","ECSS-Q-ST-70_0490100",1,"Created","Whether the parts are already qualified or remain to be qualified, their selection shall take into account the following criteria:\n    1. durability of supply;\n    2. reproducibility of characteristics."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.3a","Requirement","ECSS-Q-ST-70_0490101",1,"Created","The supplier shall establish and maintain a declared mechanical parts list in conformance with Annex B."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.4.2a","Requirement","ECSS-Q-ST-70_0490102",1,"Created","The supplier shall analyse all the parts contained in their preliminary lists with respect to criticality and in correlation with the risk analyses performed in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.4.2b","Requirement","ECSS-Q-ST-70_0490103",1,"Created","Critical parts shall be identified in the DMPL and included in the critical items list."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.4.2c","Requirement","ECSS-Q-ST-70_0490104",1,"Created","Any critical part shall be the subject of a RFA."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.1a","Requirement","ECSS-Q-ST-70_0490105",1,"Created","Depending on the results of the criticality analysis, the supplier shall perform an evaluation phase before the validation phase for all critical parts with unknown characteristics or with major changes in the use or in the configuration."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.1b","Permission","ECSS-Q-ST-70_0490198",1,"Created","In case of an extension of an existing application, the evaluation indicated in 6.5.1a need not be performed if so agreed with the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.1c","Requirement","ECSS-Q-ST-70_0490107",1,"Created","Guarantied characteristics of materials and material supplier inspection methods, together with associated documents, shall be available for review at the suppliers premises before the start of evaluation or qualification phases.\n    NOTE Refer to Table 4-1 for an explanation of the steps involved."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.2a","Requirement","ECSS-Q-ST-70_0490108",1,"Created","The evaluation shall consider the following, as a minimum, for each critical part:\n    1. the limits of use,\n    2. the part’s physical or functional characteristics, along with its values and tolerances,\n    3. behavioural tendencies and degradation processes depending on environment parameters (including sensitivity to pollution), and\n    4. acceptance criteria."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.2b","Requirement","ECSS-Q-ST-70_0490109",1,"Created","When an evaluation is performed an evaluation programme (available at PDR) shall be drawn up, implemented, and an evaluation report (available before CDR) shall be drawn up."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.2c","Requirement","ECSS-Q-ST-70_0490110",1,"Created","The behaviour of the parameters to be monitored which were also recorded during the evaluation programme tests, shall serve as a reference for the analysis of qualification test results.\n    NOTE Example of such behaviour is variation and change over time."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.3a","Requirement","ECSS-Q-ST-70_0490111",1,"Created","For each critical part a qualification programme shall be drawn up by the supplier (of the equipment using the critical part) and then implemented to check or confirm whether the parts satisfy mission requirements with appropriate margins."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.3b","Requirement","ECSS-Q-ST-70_0490112",1,"Created","Qualification status shall depend on the results obtained (qualification report) and the reviews of corresponding documentation (available at CDR)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.4a","Requirement","ECSS-Q-ST-70_0490113",1,"Created","The mechanical parts shall not receive an approval identification in the declared mechanical parts list for the project unless the requirements in 6.5.2 and 6.5.3 are satisfied."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.4b","Requirement","ECSS-Q-ST-70_0490114",1,"Created","If approval is not granted, the supplier in charge of the item shall either:\n    1. select another mechanical part, or\n    2. propose a modified evaluation programme and resubmit for approval, or\n    3. if actions 6.5.4b.1 and 6.5.4b.2 fail to achieve positive results, initiate a deviation procedure."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.5.5a","Requirement","ECSS-Q-ST-70_0490115",1,"Created","For parts not conforming to project requirements, whether at the end of criticality analysis or of evaluation and qualification tests, the supplier shall submit a request for deviation in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.1a","Requirement","ECSS-Q-ST-70_0490116",1,"Created","Mechanical parts with long lead times or procurement delays (versus the project schedule) shall be identified before the subsystem PDR."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.1b","Requirement","ECSS-Q-ST-70_0490117",1,"Created","Procurement shall be planned, documented and implemented in a timely manner to obtain reliable product assurance provision at CDR."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.1c","Requirement","ECSS-Q-ST-70_0490118",1,"Created","Back-up plans shall be prepared and initiated whenever there is evidence of possible delays or technical problems."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.2a","Requirement","ECSS-Q-ST-70_0490119",1,"Created","Each part shall be covered by a procurement specification or a standard."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.2b","Requirement","ECSS-Q-ST-70_0490120",1,"Created","The procurement specifications shall define the part characteristics, requirements, tests methods, acceptance criteria, lot acceptance testing, source inspection (if any) and material supplier inspection."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.2c","Requirement","ECSS-Q-ST-70_0490121",1,"Created","The procurement specifications shall be explicitly accepted by the part supplier or manufacturer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.3a","Requirement","ECSS-Q-ST-70_0490122",1,"Created","For complex parts related to a specific project development, each supplier shall define the nature and frequency of their own source inspection points. "]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.3b","Requirement","ECSS-Q-ST-70_0490123",1,"Created","Source inspection shall be carried out by the customer on the premises of the supplier (part manufacturer) in conformance with ECSS-Q-ST-20."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.4a","Requirement","ECSS-Q-ST-70_0490124",1,"Created","Each part or batch of parts shall be submitted to an incoming inspection."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.6.4b","Requirement","ECSS-Q-ST-70_0490125",1,"Created","An incoming inspection procedure shall be established defining the inspections and tests to be carried out."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.1a","Requirement","ECSS-Q-ST-70_0490126",1,"Created","The supplier shall ensure that all critical parts are qualified before being used in the manufacture of qualification or flight products."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.1b","Requirement","ECSS-Q-ST-70_0490127",1,"Created","Any modification, change in condition or configuration of application shall lead to a re-evaluation in conformance with the process shown in Figure 4-1."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.2a","Requirement","ECSS-Q-ST-70_0490128",1,"Created","The supplier shall apply the traceability rules defined in ECSS-Q-ST-20 to his parts."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.2b","Recommendation","ECSS-Q-ST-70_0490199",1,"Created","Parts should be identified by a unique reference number or code and a lot number to provide traceability - where there is an incident or nonconformance, or for the purposes of technical investigations following failure or damage - to reconstruct the parts history, either individually (individual traceability) or by the manufacturing lot it was part of (lot traceability)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.3a","Requirement","ECSS-Q-ST-70_0490130",1,"Created","The supplier shall define provisions for packaging, storage and removal from storage for parts."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.3b","Requirement","ECSS-Q-ST-70_0490131",1,"Created","Measurements and inspections used to guarantee the part integrity and monitoring during storage and removal from storage shall be identified."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.4a","Requirement","ECSS-Q-ST-70_0490132",1,"Created","Limited-life parts after implementation or subject to wear out shall be identified and controlled, taking into account storage and mission life.\n    NOTE Examples of such parts are mechanisms, pyro initiators and O-rings."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.4b","Requirement","ECSS-Q-ST-70_0490133",1,"Created","Limited-life parts shall be assessed as candidates to the critical items list in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","6.7.5a","Requirement","ECSS-Q-ST-70_0490134",1,"Created","Management of nonconformances and alerts shall be in conformance with ECSS-Q-ST-10."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.1a","Requirement","ECSS-Q-ST-70_0490135",1,"Created","Each process to be used in the manufacturing or assembly of a product shall be identified by a specification or procedure."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.1b","Requirement","ECSS-Q-ST-70_0490136",1,"Created","Reference shall be made to accept and reject criteria."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.2a","Requirement","ECSS-Q-ST-70_0490137",1,"Created","The supplier shall verify that the materials and the mechanical parts used during the implementation of processes satisfy the requirements of this Standard."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.3a","Requirement","ECSS-Q-ST-70_0490138",1,"Created","Processes shall be chosen from those already verified according to the following order of preference and priority:\n    1. those covered by space agencies or other governmental organization certification for identical conditions of use;\n    2. those for which satisfactory evaluation and verification results are obtained on samples representative of the application with a sufficient margin as regards conditions of use;\n    3. those already successfully used by the same supplier for other space programmes in the same conditions of use."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.3b","Requirement","ECSS-Q-ST-70_0490139",1,"Created","Whether the processes are already verified or remain to be verified, their selection shall take into account the following criteria:\n    1. reliability;\n    2. inspectability;\n    3. re-workability of the process item;\n    4. reproducibility."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.4a","Requirement","ECSS-Q-ST-70_0490140",1,"Created","The supplier shall establish and maintain a declared processes list in conformance with Annex C."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2a","Requirement","ECSS-Q-ST-70_0490141",1,"Created","The supplier shall analyse all the processes contained in their preliminary lists with respect to criticality and in correlation with the risk analyses performed."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2b","Requirement","ECSS-Q-ST-70_0490142",1,"Created","Critical processes shall be identified in the DPL and included in the list of critical items."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2c","Requirement","ECSS-Q-ST-70_0490143",1,"Created","Any critical process shall be the subject of an RFA."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2d","Requirement","ECSS-Q-ST-70_0490144",1,"Created","Special processes shall be identified and controlled."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2e","Requirement","ECSS-Q-ST-70_0490145",1,"Created","Process control shall be ensured by means of procedures or personnel certification or inline process control."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.5.2f","Permission","ECSS-Q-ST-70_0490200",1,"Created","Whenever feasible a statistical process may be carried out."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.1a","Requirement","ECSS-Q-ST-70_0490147",1,"Created","Depending on the results of the criticality analysis, the supplier shall perform an evaluation phase before the validation phase for all critical processes which are new or with major changes in the use or in the configuration. "]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.1b","Permission","ECSS-Q-ST-70_0490201",1,"Created","In case of an extension of an existing application, the evaluation indicated in 7.6.1a need not be performed if so agreed with the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.1c","Requirement","ECSS-Q-ST-70_0490149",1,"Created","For confidential processes, the supplier shall prove that the process has been verified.\n    NOTE 1 For example, by presenting a verification certificate from space agencies or other governmental organization responsible to check the applicability of this verification.\n    NOTE 2 Refer to Table 4-1 for an explanation of the steps involved."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.2a","Requirement","ECSS-Q-ST-70_0490150",1,"Created","The evaluation shall consider the following as a minimum for each critical process:\n    1. the limits of use,\n    2. the values, determined by test samples or technology samples, of relevant parameters and their tolerances, and\n    3. acceptance criteria."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.2b","Requirement","ECSS-Q-ST-70_0490151",1,"Created","When an evaluation is performed, the supplier shall provide \n    1. an evaluation plan at PDR and\n    2. an evaluation report before CDR."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.3a","Requirement","ECSS-Q-ST-70_0490152",1,"Created","For each critical process, the supplier shall implement a verification programme."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.3b","Requirement","ECSS-Q-ST-70_0490153",1,"Created","The verification programme shall be defined in conformance with existing ECSS or national agency standards of verification."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.3c","Requirement","ECSS-Q-ST-70_0490154",1,"Created","The supplier shall ensure that the processes satisfy the mission requirements and that the parameters needed for the product design are defined so as to obtain verification status."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.3d","Requirement","ECSS-Q-ST-70_0490155",1,"Created","Verification status shall depend on the results obtained (verification report) and the review of corresponding documentation (available at CDR)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.4a","Requirement","ECSS-Q-ST-70_0490156",1,"Created","The processes shall not receive an approval identification in the declared processes list unless requirements in 7.6.2 and 7.6.3 are satisfied. If approval is not granted, the supplier in charge of the item shall either\n    1. select other processes, or\n    2. propose a modified evaluation programme and resubmit for approval, or\n    3. if actions 7.6.4a.1 and 7.6.4a.2 fail to achieve positive results, initiate a deviation procedure."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.6.5a","Requirement","ECSS-Q-ST-70_0490157",1,"Created","For processes not conforming to project requirements, whether at the end of criticality analysis or of evaluation and verification tests, the supplier shall submit a request for deviation in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.1a","Requirement","ECSS-Q-ST-70_0490158",1,"Created","The supplier shall confirm that all critical processes have been verified before being used in the manufacture of qualification or flight products."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.1b","Requirement","ECSS-Q-ST-70_0490159",1,"Created","Any modification, change of condition or configuration of application shall lead to a re-evaluation in conformance with the process shown in Figure 4-1."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.2a","Requirement","ECSS-Q-ST-70_0490160",1,"Created","When a process needs to be re-verified, a request for approval (RFA) shall be established and a re-verification programme shall be implemented.\n    NOTE Any prolonged stoppage in manufacturing, any major change of the facilities or procedures or any transfer of production to another entity can invalidate partially or completely the initial verification of a process."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.3a","Requirement","ECSS-Q-ST-70_0490161",1,"Created","Before implementation of a process, the supplier shall ensure that personnel are trained and that environment, means and documentation are adequate."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.3b","Requirement","ECSS-Q-ST-70_0490162",1,"Created","This verification shall ensure that: \n    1. manufacturing and quality control tools associated with the process are adequate, calibrated and properly maintained are used under appropriate environmental and cleanliness conditions, see clause 4.4,\n    2. personnel are properly trained and certified, and\n    3. the processes specifications, manufacturing and inspection procedures and workmanship standards including clear definition of manufacturing operations and clear acceptance criteria exist.\n        NOTE 1 Photographically documented if possible for visual acceptance criteria at the appropriate work and inspection stations.\n        NOTE 2 For planning of manufacturing, assembly and integration operation and inspection see ECSS-Q-ST-20."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.4a","Requirement","ECSS-Q-ST-70_0490163",1,"Created","Traceability of processes shall be ensured in conformance with ECSS-Q-ST-20."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.5a","Requirement","ECSS-Q-ST-70_0490164",1,"Created","Nonconformances and alerts shall be processed in conformance with ECSS-Q-ST-10."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.6a","Requirement","ECSS-Q-ST-70_0490165",1,"Created","MIPs shall be defined in conformance with ECSS-Q-ST-20."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","7.7.7a","Requirement","ECSS-Q-ST-70_0490166",1,"Created","The supplier shall define provisions for packaging, storage, and removal from storage for products or semi-finished products before and after implementation of processes."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-70_0490167",1,"Created","The DML shall contain the following statements:\n    1. “Materials are classified into 20 groups depending on their type or their main use, see Table A-1”.                                         \n    2. “Primers are classified in the group of their associated component.”\n    3. “Where no project requirement exists for a separate DMPL, mechanical parts are entered on the DML as a separate group with the corresponding numbers.”"]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","A.2.1<1>b","Requirement","ECSS-Q-ST-70_0490168",1,"Created","If new groups are created, for a given project, these shall have numbers over 21."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","A.2.1<2>a","Requirement","ECSS-Q-ST-70_0490169",1,"Created","The DML shall include the information stated in Figure A-1, where the header information identifies the list as the declared materials list and includes the issue number and date of issue, as follows:\n    1. Item number (applicable to equipment manufacturer level only)\n        (a) This consists of the material group identifier and the user code. It takes the form of:\n<group number>.<identifier within the group>.<running number>.<user code>\n            NOTE For example: 11.5.1.KOF.\n        (b) Characteristics of the item number are:\n              - The user, identified by an agreed user code for the project.\n              - One only per material type.\n              - Does not change during the life of the materials list (sub-items are permitted when deemed necessary).\n    2. Commercial identification or standardized designation\n        (a) Enter the correct and standard designation, such as the trade name plus number.\n        (b) If no trade name exists, enter the manufacturer’s name plus number.\n        (c) For metal alloys, the Aluminium Association (AA) system is recommended for aluminium alloys, and the American Iron and Steel Institute (AISI) system for steel. For other metals or alloys, the main constituent is entered first except in the case of a traditional name.\n            NOTE For example: brass or bronze.\n        (d) For each material, as designated in A.2.1<2>a2(a) to(c), use a unique item number. If several lines are used for different applications or processing, add sub-item numbers.\n    3. Chemical nature and product type\n        (a) For metallic materials, add the condition as procured if applicable.\n            NOTE Example of such conditions are rolled and heat treatment.\n        (b) Where a semi-finished product is procured, give the relevant state. \n            NOTE Example of such state are form, plate and sheet.\n        (c) Give the thickness of the material, that can be an important parameter.\n            NOTE Examples of chemical nature are: epoxy resin, polyurethane adhesive, Ti6Al4V.\n    4. Procurement information\n        (a) Manufacturer or distributor: name of the manufacturer and name of the distributor if different.\n        (b) Procurement specification: reference of the procurement specification with issue, revision and date. It may be replaced by a national or international specification or standard, if this exists, and identifies the source of procurement, if relevant. Indication of issue or date is not applicable when datasheets are used\n    5. Processing parameters\nList here a summary of the process parameters applied by the user of the process.\n        NOTE E.g. mixture proportions, cure temperature, special cleaning agent, surface treatment, thermal treatment and temperature, and reference to specification number.\n    6. Use and location\n        (a) Use codes able to define the location of the material with respect to the:\n            • subsystem;\n            • particular piece of equipment (box or item);\n            • use of the equipment, e.g. a structural element, thermal control, electrical insulation.\n            NOTE If the CI number is not included in the list header, then a suitable abbreviation of the relevant subsystem is included.\n        (b) Include any restrictions that apply to the use of a particular material in the corresponding comment column.\n    7. Environmental code\nThe environmental code is defined using Table A-2.\n    8. Size code\nThe size code is indicated by an alphanumeric combination, such as A5, V2 or M3, as in Table A-3.\n    9. Validation references, justification for approval and prime comments and prime approval\n        (a) Make reference to relevant test data that demonstrates the acceptability of the material under the environmental conditions and the application relevant to the particular project concerned. Specifically, in column 9.1, corrosion (CORR), stress corrosion (SCC), flammability (FLAM), offgassing (OFFG) and outgassing (OUTG) data or report-references are entered.\n        (b) Use standard abbreviations to summarize the acceptance status of a material for a particular property.\n        (c) Use the justification for approval (column 9.2) and prime approval (column 9.3) columns for any additional information to obtain customer approval.\n        (d) Standard abbreviations are used to summarize the acceptability or otherwise of a material for a specific property. These are defined for the project.\n        (e) Select the supplier approval status code from Table A-4.\n    10. Customer approval status code and comments\n        (a) Select this code from Table A-4.\n        (b) Include additional comments where appropriate."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","A.2.2a","Requirement","ECSS-Q-ST-70_0490170",1,"Created","The change record shall list the successive issues and their release dates since the first formal issue of the document."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","A.2.2b","Requirement","ECSS-Q-ST-70_0490171",1,"Created","The change record shall include a brief description of the updates which contributed to each issue or revision.\n    NOTE This DRD recommends the format and define the content within the framework of a project or a programme."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.1<1>a","Requirement","ECSS-Q-ST-70_0490172",1,"Created","The DMPL shall contain the following statements:\n“Mechanical parts are classified into 11 groups depending on their type or their main use” (see Table B-1)."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.1<1>b","Requirement","ECSS-Q-ST-70_0490173",1,"Created","If, for a given project it is considered necessary to create new groups, these shall have numbers over 61."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.1<1>c","Recommendation","ECSS-Q-ST-70_0490202",1,"Created","Items that appear in the EEE parts list should not be repeated here.\n    NOTE For example, heaters, some valves, thermostats, relays, transformer coils and solenoids."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.1<2>a","Requirement","ECSS-Q-ST-70_0490175",1,"Created","The DMPL shall include the information in Figure B-1, where the header information identifies the list as the declared mechanical parts list and includes the issue number and date of issue, as follows:\n    1. Item number (applicable at equipment supplier level only)\n        (a) This consists of the mechanical part identifier and the user code. It takes the form of:\n<group number>.<identifier within the group>.<running number>.<user code>\n            NOTE For example: 7.2.1.ACSA.\n        (b) Characteristics of the item number are:\n             - Identify the subcontractor by an agreed user code for the project.\n             - One only per mechanical part type.\n             - Does not change during the life of the mechanical parts list.\n    2. Commercial identification\n        (a) Enter the correct and standard designation, such as trade name plus number. \n        (b) If no trade name exists then enter the manufacturers’ name and number.\n    3. Type of part\nDescribe the material and surface treatment (if applicable).\n    4. Procurement information\n        (a) Manufacturer or distributor: name of the manufacturer and name of the distributor if different.\n        (b) Procurement specification: reference of the procurement specification with issue, revision and date. It may be replaced by a national or international specification or standard if this exists and identifies the source of procurement if relevant.\n    5. Elementary function, main characteristics\n        (a) Enter the function of the mechanical part.\n        (b) Enter the main characteristics of the mechanical part.\n            NOTE For example, number of revolutions per minute for a ball bearing.\n    6. Use and location\nUse codes able to define the location of the mechanical part with respect to the:\n        (a) subsystem;\n        (b) particular piece of equipment (box or item);\n        (c) use of the equipment.\n    7. Environmental code\nThe environmental code is defined using Table B-2.\n    8. Criticality\nEnter “C” for critical or “N” for non-critical. If a mechanical part is considered critical, describe the reason for the criticality and methods of control.\n    9. Supplier reference, prime comments and prime approval status \n        (a) Use the supplier reference, prime comments and approval columns to enter any additional information that can be necessary in order to obtain customer approval.\n        (b) This information comprises reference and issue of the RFA or approval, mechanical parts justification file, evaluation reports and deviation requests.\n        (c) Make reference to the relevant test data that demonstrates acceptability of the mechanical part under the environment conditions and the application relevant to the particular project concerned. \n        (d) Use standard abbreviations, defined by the customer, to summarize the acceptance status of a mechanical part for a particular property.\n        (e) In order to justify the use of a material for flammability resistance, list here the material thickness and height of oxygen share.\n        (f) Select the prime approval status code from Table B-3.\n    10. The customer approval status code and comments\n        (a) Select this code from Table B-3.   \n        (b) Include additional comments where appropriate."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.2a","Requirement","ECSS-Q-ST-70_0490176",1,"Created","The change record shall list the successive issues and their release dates since the first formal issue of the document."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","B.2.2b","Requirement","ECSS-Q-ST-70_0490177",1,"Created","This record shall include a brief description of the updates which contributed to each issue or revision.\n    NOTE This DRD recommends the format and defines the content within the framework of a project or a programme."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","C.2.1<1>a","Requirement","ECSS-Q-ST-70_0490178",1,"Created","The DPL shall contain the following statements:\nProcesses are classified into 17 groups depending on their type or their main use, see Table C-1."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","C.2.1<1>b","Requirement","ECSS-Q-ST-70_0490179",1,"Created","If, for a given project it is considered necessary to create new groups, these shall have numbers over 17."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","C.2.1<2>a","Requirement","ECSS-Q-ST-70_0490180",1,"Created","The DPL shall include the information in Figure C-1, where the header information identifies the list as the declared processes list and includes the issue number and date of issue, as follows\n    1. Item number (applicable to equipment supplier level only)\n        (a) This consists of the process identifier and the user code. It takes the form of \n<group number>.<identifier within the group>.<running number>.<user code>\n            NOTE For example: 1.2.1.SSEX\n        (b) Characteristics of the item number are:\n             - Identify the subcontractor by an agreed user code for the project.\n             - One only per process type.\n             - Does not change during the life of the process list.\n    2. Process identification\nIndicate the correct and standard identification of the process, e.g. the process name or title: bonding, coating or soldering.\n    3. Specification\n        (a) Identify the name or abbreviation of the process executor.\n        (b) Make a reference to the associated procedure, together with the issue, revision and date.\n            NOTE For example, national, international, EN, ISO, ECSS or company in-house.\n    4. Process description\nEnter here a short description of the process.\n    5. Use and location\nUse codes able to define the location of the process with respect to the:\n        (a) subsystem,\n        (b) particular piece of equipment (box or item),\n        (c) use of the equipment.\n            NOTE For example, a structural element, thermal control, electrical insulation).\n    6. This column number is not used.\n    7. Associated item numbers\nEnter the associated material list (DML) or mechanical parts list (DMPL) with the process.\n    8. Criticality\n        (a) Enter “C” for critical or “N” for non-critical.\n        (b) If a process is considered to be critical, Enter the references to the relevant RFA.\n    9. Supplier reference, prime comments and approval\n        (a) Use the supplier reference and approval columns to enter any additional information that can be necessary to obtain customer approval.\n        (b) Select the supplier approval status code from Table C-2.\n    10. The customer approval status code and comments\n        (a) Select this code from Table C-2.\n        (b) Include additional comments where appropriate."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","C.2.2a","Requirement","ECSS-Q-ST-70_0490181",1,"Created","The change record shall list the successive issues and their release dates since the first formal issue of the document."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","C.2.2b","Requirement","ECSS-Q-ST-70_0490182",1,"Created","This record shall include a brief description of the updates which contributed to each issue or revision.\n    NOTE This DRD recommends the format and define the content within the framework of a project or a programme."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","D.2.1a","Recommendation","ECSS-Q-ST-70_0490203",1,"Created","The RFA should contain the information in Figure D-1 (pages 1 and 2), as follows:\n    1. The header information, identifying the document as a request for approval together with the project logo and project name, RFA reference, issue revision and date.\n    2. Originator\nOriginator’s name and reference.\n    3. Location\nSubsystem and equipment codes.\n    4. Item description\nBrief description of the item.\n    5. PMP information\nThe DML, DMPL or DPL item number and list reference.\n    6. Item status, including the following information:\n        (a) manufacturers’ name and qualification reference;\n        (b) suppliers’ name and qualification status;\n        (c) product or material specification;\n        (d) procurement specification;\n        (e) process or handling specification;\n        (f) other related process or handling specifications;\n        (g) verification or qualification specification;\n        (h) report on verification or qualification.\n    7. Reason for RFA\nEnter the reason for the RFA.\n    8. Application and location details\nEnter here the details of the application and exact location of the item.\nGive the reference in the CIL.\n    9. Evaluation and validation programme\nReference and details of main tests.\n    10. Subcontractor supplier approval for the first issue of the RFA.\n    11. Customer initial decision, to be entered on first issue of the RFA providing:\n        (a) the decision concerning the proposed material,\n        (b) the requirement to perform tests (deviation request as necessary), and\n        (c) the decision concerning the proposed test programme.\n    12. Customer’s and final customer’s (if applicable) signature\n    13. Justification results obtained with reference to the supplier’s validation report and conclusion.\n    14. Subcontractor supplier approval on RFA final issue.\n    15. Final approval status of the RFA by the customer."]
["ECSS-Q-ST-70C","ECSS - Superseded v1.0","D.2.2a","Requirement","ECSS-Q-ST-70_0490184",1,"Created","The RFA shall be completed by the supplier (parts 1 to 10, 13 and 14) and the customer (parts 11 12 and 15)."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.1a","Requirement","ECSS-Q-ST-10_0360001",1,"Created","The supplier shall identify the personnel responsible for implementing and performing PA management and other PA disciplines."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.1b","Requirement","ECSS-Q-ST-10_0360002",1,"Created","The supplier shall assign a project PA manager reporting to the project manager and having unimpeded access to higher management."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.1c","Requirement","ECSS-Q-ST-10_0360003",1,"Created","The appointed project PA manager, irrespective of other responsibilities, shall have organizational authority to establish and implement a product assurance programme in accordance with the project product assurance requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.1d","Requirement","ECSS-Q-ST-10_0360004",1,"Created","The project PA Manager shall act as the focal point of contact within the project concerning Product Assurance matters.\n    NOTE The project PA manager is referred to as “PA manager” in the rest of this document."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.2a","Requirement","ECSS-Q-ST-10_0360005",1,"Created","The supplier shall define and document the responsibility, the authority and the interrelation of personnel who manage, perform and verify work affecting product assurance."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.2b","Requirement","ECSS-Q-ST-10_0360006",1,"Created","The supplier shall define and document the responsibilities and the interfaces of the PA functions, either external or internal, involved in a project."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.2c","Requirement","ECSS-Q-ST-10_0360007",1,"Created","When the supplier's PA organization delegates product assurance tasks to another organization it shall be done in a documented and controlled way monitored by the PA organization.\n    NOTE The supplier PA organization retains the responsibility towards the Customer"]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.3a","Requirement","ECSS-Q-ST-10_0360008",1,"Created","The supplier shall identify the PA resources needed to implement the PA programme."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.3b","Requirement","ECSS-Q-ST-10_0360009",1,"Created","The supplier shall provide resources capable to perform the PA tasks identified in the PA programme."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.1.3c","Requirement","ECSS-Q-ST-10_0360010",1,"Created","Reviews and audits of the product assurance programme, of processes or of product shall be carried out by personnel not directly involved in the work being performed."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.2a","Requirement","ECSS-Q-ST-10_0360011",1,"Created","The PA manager shall interface with project management, ensuring that the contractual provision and schedule planning for the definition and phasing of PA activities are met."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.2b","Requirement","ECSS-Q-ST-10_0360012",1,"Created","The PA manager shall interface with risk management, configuration management, engineering, procurement and AIV for the definition and execution of tasks in which PA activities are involved."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.2c","Requirement","ECSS-Q-ST-10_0360013",1,"Created","The PA manager shall interface with the customer regarding all Product Assurance matters."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.2d","Requirement","ECSS-Q-ST-10_0360014",1,"Created","The PA manager shall interface with lower-tier suppliers regarding all Product Assurance matters."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.3a","Requirement","ECSS-Q-ST-10_0360015",1,"Created","The supplier shall prepare, maintain and implement a plan of the PA activities in accordance with the customer PA requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.3b","Requirement","ECSS-Q-ST-10_0360016",1,"Created","The Product Assurance plan shall be prepared in conformance with DRD in Annex A."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.1.3c","Requirement","ECSS-Q-ST-10_0360017",1,"Created","The Product Assurance plan shall be submitted to the customer for approval.\n    NOTE 1 The Product Assurance plan can refer to Clauses of the Company Quality Manual and to in-house procedures.\n    NOTE 2 Information on the schedule for delivery of PA management documents is given in Annex C"]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-10_0360018",1,"Created","The PA manager shall ensure that PA disciplines are organized at the beginning of the project according to customer contractual requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-Q-ST-10_0360019",1,"Created","The PA manager shall ensure that the inputs used by the PA disciplines are consistent and complete, and available in line with the project schedule."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1c","Requirement","ECSS-Q-ST-10_0360020",1,"Created","The PA manager shall ensure that the PA disciplines perform the tasks described in the PA Plan in line with the project schedule."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1d","Requirement","ECSS-Q-ST-10_0360021",1,"Created","The PA manager shall ensure that the outputs produced by the PA disciplines are consistent and complete, and delivered in line with the project schedule."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1e","Requirement","ECSS-Q-ST-10_0360022",1,"Created","The PA manager shall ensure the application of processes defined in applicable project plans and documents. "]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1f","Requirement","ECSS-Q-ST-10_0360023",1,"Created","The PA manager shall control the quality of his supplier’s products by:\n    1. issuing product assurance requirements applicable to the supplier \n    2. ensuring the implementation of the PA requirements by the supplier."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1g","Requirement","ECSS-Q-ST-10_0360024",1,"Created","The PA manager shall ensure that PA contributions to verification are defined and provided."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1h","Requirement","ECSS-Q-ST-10_0360025",1,"Created","The PA manager shall ensure that a qualification programme is defined, approved and maintained by the relevant organization.\n    NOTE Requirement for the qualification programme are addressed in ECSS-Q-ST-20, ECSS-Q-ST-60, ECSS-Q-ST-70, ECSS-E-ST-10-02 and ECSS-E-ST-10-03."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1i","Requirement","ECSS-Q-ST-10_0360026",1,"Created","The PA manager shall ensure that the qualification programme is implemented and the qualification results are recorded, evaluated and documented."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1j","Requirement","ECSS-Q-ST-10_0360027",1,"Created","The PA manager shall ensure that a Qualification Status List of the programme items is maintained in conformance with Annex B."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1k","Requirement","ECSS-Q-ST-10_0360028",1,"Created","The PA manager shall review and approve the achieved qualification status."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.1l","Requirement","ECSS-Q-ST-10_0360029",1,"Created","The PA manager shall approve the product acceptance during the Acceptance or Delivery Review.\n    NOTE The PA manager approval is based on the outputs of the Acceptance or Delivery Review."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-Q-ST-10_0360030",1,"Created","The supplier shall report on the status and progress of the product assurance program implementation."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.2b","Requirement","ECSS-Q-ST-10_0360031",1,"Created","The PA report shall include at least the following items for the reporting period:\n    • Progress and accomplishment of each major product assurance task including resolved and new problems, future planning of major activities and events\n    • Status of PA reviews, Audits and MIPs, Waiver requests, Non conformances (minor and major), Critical items (including mitigation action plan status), Qualification status, EEE component status, Material and processes status, Alerts status."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.2c","Permission","ECSS-Q-ST-10_0360066",1,"Created","The PA progress report may be part of the project progress report. \n    NOTE The general contents of the project progress report are detailed in ECSS-M-ST-10 Annex E."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.3a","Requirement","ECSS-Q-ST-10_0360033",1,"Created","The supplier shall perform audits on his own performance to verify the implementation and effectiveness of the provisions defined in the PA plan.\n    NOTE 1 Audits can be performed by sampling on various projects or by periodic audits of the supplier quality system.\n    NOTE 2 The general contents of project audits are detailed in ECSS-M-ST-10 clause 5.2.3."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.3b","Requirement","ECSS-Q-ST-10_0360034",1,"Created","The supplier shall establish and maintain an audit plan for procurement activities on the project, designating the lower tier suppliers to be audited, the current status and the schedule for auditing."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.3c","Requirement","ECSS-Q-ST-10_0360035",1,"Created","In addition to the planned audits, extra audits shall be performed when necessary to overcome failure, consistent poor quality, or other problems. "]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.3d","Requirement","ECSS-Q-ST-10_0360036",1,"Created","The supplier shall plan and perform audits using established and maintained procedures."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-Q-ST-10_0360037",1,"Created","The supplier shall establish a critical items control programme in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.4b","Requirement","ECSS-Q-ST-10_0360038",1,"Created","The PA manager shall identify and evaluate critical items in support of the overall project risk management activities."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.4c","Requirement","ECSS-Q-ST-10_0360039",1,"Created","The PA manager shall ensure that a critical item control programme is implemented to eliminate or mitigate associated risks."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.5a","Requirement","ECSS-Q-ST-10_0360040",1,"Created","The PA manager shall ensure that the applicable issues of all documents and data are available at all locations where activities required for the implementation of the PA programme are performed."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.5b","Requirement","ECSS-Q-ST-10_0360041",1,"Created","The PA manager shall ensure that invalid or obsolete documents and data are removed from all points of issue or use, or assured against unintended use."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.5c","Requirement","ECSS-Q-ST-10_0360042",1,"Created","The PA manager shall ensure that obsolete documents and data retained for legal or knowledge preservation purposes are identified as such."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.5d","Requirement","ECSS-Q-ST-10_0360043",1,"Created","The PA manager shall identify the project documents requiring approval including those requiring approval by PA."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.6a","Requirement","ECSS-Q-ST-10_0360044",1,"Created","The supplier shall establish and maintain quality records to provide objective evidence of complete and successful performance of all PA discipline tasks and to demonstrate compliance with requirements.\n    NOTE Requirements for the storage, retrieval and archiving of quality records are addressed in ECSS-M-ST-40."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.7a","Requirement","ECSS-Q-ST-10_0360045",1,"Created","The PA manager shall verify during Configuration Control Boards the suitability for release of drawings, plans, specifications, procedures and changes thereto.\n    NOTE The operation of Configuration Control Boards is detailed in ECSS-M-ST-40"]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.7b","Requirement","ECSS-Q-ST-10_0360046",1,"Created","The PA manager shall ensure that:\n    1. the as designed status is defined and released prior to manufacturing;\n    2. the as-built documentation is properly defined, identified and maintained in order to reflect approved modifications; and\n    3. items delivered comply with the as-built documentation."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.8a","Requirement","ECSS-Q-ST-10_0360047",1,"Created","The supplier shall establish and maintain a nonconformance control system in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.9a","Requirement","ECSS-Q-ST-10_0360048",1,"Created","The supplier shall notify its customer of preliminary information on failures or problems that can result in an alert.\n    NOTE 1 The above is applicable to failure or problems detected by the supplier or by one of his lower tier suppliers.\n    NOTE 2 The above is only applicable to failures or problems meeting all of the following criteria:\n        · The item with the observed failure or problem has multiple applications, which can have implications for more than one project, thus requiring prompt action.\n        · The failure or problem has occurred in the application of an item within the specified design and usage limitations. \n        · Failures or problems due to usage within reasonably expected limits of performance, but where these limits were not specified precisely.\n        · A preliminary investigation has provided evidence of the root cause of the failure or problem.\n        · Failure or problems are confirmed not to be of a random nature."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.9b","Requirement","ECSS-Q-ST-10_0360049",1,"Created","The supplier shall investigate in cooperation with the originator of the failure or problem to define the immediate measures to be taken, to identify the causes, and to recommend corrective actions for similar items."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.9c","Requirement","ECSS-Q-ST-10_0360050",1,"Created","The PA manager shall ensure:\n    1. the assessment of any failure having the potential to lead to an alert by the customer,\n    2. the investigation, until disposition of the items subject of the potential alert, and\n    3. the assessment of incoming alerts for the definition, implementation and follow-up of necessary actions."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","5.2.9d","Requirement","ECSS-Q-ST-10_0360051",1,"Created","The supplier shall participate in the alert system organized by the customer or other sources, by:\n    1. assessment of the impact of incoming alerts to project work, and definition, implementation and follow-up of necessary corrective actions at any contractual level.\n    2. distribution of incoming alerts to the possible affected users within the project.\n        NOTE The alert system is set up for the prompt interchange of information on failures or problems which can affect more than one user, or can recur in other projects or circumstances, if no preventive actions are taken."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-10_0360052",1,"Created","The PAP shall introduce the purpose, objective and the reason prompting its preparation.\n    NOTE For example: programme or project reference and phase."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<2>a","Requirement","ECSS-Q-ST-10_0360053",1,"Created","The PAP shall list the applicable and reference documents in support of the generation of the document."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<3.1>a","Requirement","ECSS-Q-ST-10_0360054",1,"Created","The PAP shall describe the organization (including responsibilities and authorities), the activities, processes and procedures to be applied by the supplier to fulfil the applicable product assurance planning requirements defined in clause 5.1 of ECSS-Q-ST-10C."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<3.2>a","Requirement","ECSS-Q-ST-10_0360055",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable product assurance implementation requirements defined in clause 5.2 of ECSS-Q-ST-10C."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<4>a","Requirement","ECSS-Q-ST-10_0360056",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable quality assurance requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<5>a","Requirement","ECSS-Q-ST-10_0360057",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable dependability requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<6>a","Requirement","ECSS-Q-ST-10_0360058",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable safety requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<7>a","Requirement","ECSS-Q-ST-10_0360059",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable EEE Component requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<8>a","Requirement","ECSS-Q-ST-10_0360060",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable Material and Processes requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<9>a","Requirement","ECSS-Q-ST-10_0360061",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil the applicable Software product assurance requirements."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.1<10>a","Requirement","ECSS-Q-ST-10_0360062",1,"Created","The PAP shall describe the activities, processes and procedures to be applied by the supplier to fulfil all other applicable PA requirements not covered in the clause A.2.1<3> to clause A.2.1<9> (e.g. Security, Planetary Protection, Off-The-Shelf, Customer Furnished equipment).\n    NOTE The order of the sections is not mandatory."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.2a","Permission","ECSS-Q-ST-10_0360067",1,"Created","The response to this DRD may be combined with the response to the project management plan, as defined in ECSS-M-ST-10."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","A.2.2b","Permission","ECSS-Q-ST-10_0360068",1,"Created","The response to this DRD may be performed by reference to separate discipline plans addressing some of the above clauses of this DRD."]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","B.2.1a","Requirement","ECSS-Q-ST-10_0360065",1,"Created","The QSL shall include or refer to the following information:\n    1. Equipment designation:\n        (a) Identification of hardware by name, \n        (b) Configuration Item number and model.\n    2. Next higher assembly level :\n        (a) Identification of next higher assembly.\n    3. Manufacturer's name :\n        (a) Identification of Item Supplier.\n    4. Reference of requirements documents\n        (a) Reference numbers of applicable requirement specifications.\n    5. Design heritage:\n        (a) Specify if the design is “New”, otherwise identification of the project in which the design was used.\n        (b) Summary of current qualification status:\n            • Basis for qualification (qualification test results, heritage, and qualification on other projects) programme on which the qualification test was conducted;\n            • Project on which the test was conducted.\n    6. Proposed category A, B, C, or D (related to Design heritage):\n        NOTE Qualification approach as defined in the ECSS-E-ST-10-02.\n    7. Reference of Qualification plan document:\n        (a) Current qualification status/screening and applicability of qualification test versus requirements.\n        (b) Reference numbers of Qualification Plan(s).\n        (c) Identification of developments models (EM, EQM, QM, PFM) to be manufactured and tested for the project.\n    8. Reports:\n        (a) Reference to Verification Control Document and/or reference to Analyses, Test and Inspection Reports;\n        (b) Qualification Authority: Organization in charge of the item qualification (if any).\n    9. The qualification status:\n        • QUALIFIED,\n        • TO BE QUALIFIED,\n        • QUALIFICATION IN PROGRESS\n    10. Open Actions / Due dates/Remarks:\n        (a) For an open action: summary of missing qualification actions and planned dates for the closure of such actions.\n        (b) List of major NCRs and associated waivers to the qualification items"]
["ECSS-Q-ST-10C","ECSS - Superseded v1.0","B.2.2a","Permission","ECSS-Q-ST-10_0360069",1,"Created","The form may be a table which contains the here above information of B.2.1 or reference to separate document.\n    NOTE An example of such a table is shown in Figure B-1."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.1a","Requirement","ECSS-Q-ST-30_0410001",1,"Created","The dependability assurance shall be implemented by means of a systematic process for specifying requirements for dependability and demonstrating that these requirements are achieved. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.1b","Requirement","ECSS-Q-ST-30_0410002",1,"Created","The dependability assurance process shall be in conformance with the dependability assurance programme plan for the project."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.2a","Requirement","ECSS-Q-ST-30_0410003",1,"Created","The supplier shall coordinate, implement and integrate the dependability programme management with the PA programme management."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3a","Requirement","ECSS-Q-ST-30_0410004",1,"Created","The supplier shall develop, maintain and implement a dependability plan for all project phases in conformance with the DRD in Annex C."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3b","Requirement","ECSS-Q-ST-30_0410005",1,"Created","The plan shall address the applicable requirements of this document.\n    ","NOTE The plan can be included in the PA programme plan."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3c","Requirement","ECSS-Q-ST-30_0410006",1,"Created","The extent that dependability assurance is applied shall take account of the severity (as defined in Table 5-1) of the consequences of failures."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3d","Requirement","ECSS-Q-ST-30_0410007",1,"Created","The establishment and implementation of the dependability programme plan shall be considered in conjunction with the safety aspects of the programme. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3e","Requirement","ECSS-Q-ST-30_0410008",1,"Created","The Supplier shall ensure that any potential conflict between dependability and safety requirements are managed. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.3f","Requirement","ECSS-Q-ST-30_0410009",1,"Created","Responsibilities for carrying out all dependability tasks within each phase of the lifecycle shall be defined."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.4a","Requirement","ECSS-Q-ST-30_0410010",1,"Created","As part of the risk management process implemented on the project, the Dependability engineer shall be responsible for identifying and reporting dependability associated risks .\n    ","NOTE ECSS-M-ST-80 describes the risk management process."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.4b","Requirement","ECSS-Q-ST-30_0410011",1,"Created","Dependability risk analysis reduction and control shall include the following steps:\n    1. identification and classification of undesirable events according to the severity of their consequences;\n    2. analysis of failure scenarios, determination of related failure modes, failure origins or causes;\n    3. classification of the criticality of the functions and associated products according to the severity of relevant failure consequences;\n    4. definition of actions and recommendations for detailed risk assessment, risk elimination, or risk reduction and control to an acceptable level;\n    5. status of risk reduction and risk acceptance;\n    6. implementation of risk reduction;\n    7. verification of risk reduction and assessment of residual risks.\n        ","NOTE The process of risk identification and assessment implies both qualitative and quantitative approaches."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.4c","Requirement","ECSS-Q-ST-30_0410012",1,"Created","Risk reduction measures that are proposed for dependability shall be assessed at system level in order to select the optimum solution to reduce the system level risk."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.5a","Requirement","ECSS-Q-ST-30_0410013",1,"Created","Dependability critical items shall be identified by dependability analyses performed to support the risk reduction and control process performed on the project. \n    ","NOTE The criteria for identifying dependability critical items are given in clause 6.5."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.5b","Requirement","ECSS-Q-ST-30_0410014",1,"Created","Dependability critical items, as part of the Critical Items List, shall be subject to risk assessment and critical items control in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.5c","Requirement","ECSS-Q-ST-30_0410015",1,"Created","The control measures shall include:\n    1. a review of all design, manufacturing and test documentation related to critical functions, critical items and procedures;\n    2. dependability representation on relevant Review Boards to ensure that the disposition takes account of their criticality level."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.5d","Requirement","ECSS-Q-ST-30_0410016",1,"Created","The dependability aspects shall be considered during the entire verification process for dependability critical items until closeout."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.6a","Requirement","ECSS-Q-ST-30_0410017",1,"Created","The supplier shall ensure that all dependability data for a design review are presented to the customer in accordance with the project review schedule. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.6b","Requirement","ECSS-Q-ST-30_0410018",1,"Created","All dependability data submitted shall indicate the design baseline and shall be coherent with all other supporting technical documentation."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.6c","Requirement","ECSS-Q-ST-30_0410019",1,"Created","All design changes shall be assessed for their impact on dependability and a reassessment of the dependability shall be performed"]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.7a","Requirement","ECSS-Q-ST-30_0410020",1,"Created","Dependability lessons learnt shall be collected during the project life cycle including operational and disposal phases.\n    ","NOTE Dependability lessons learnt consider:\n        · the impact of newly imposed requirements;\n        · assessment of all malfunctions, anomalies, deviations and waivers;\n        · effectiveness of strategies of the project;\n        · new dependability tools and methods that have been developed or demonstrated;\n        · effective versus ineffective verifications that have been performed."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.8a","Requirement","ECSS-Q-ST-30_0410021",1,"Created","The supplier shall report dependability progress to the customer as part of product assurance activities in conformance with ECSS-Q-ST-10."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","4.9a","Requirement","ECSS-Q-ST-30_0410022",1,"Created","The supplier shall maintain all data used for the dependability programme."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.1a","Requirement","ECSS-Q-ST-30_0410023",1,"Created","Dependability shall be integrated as part of the design process. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.1b","Requirement","ECSS-Q-ST-30_0410024",1,"Created","The dependability characteristics shall be traded off with other system attributes such as mass, size, cost and performance during the optimization of the design in all phases of the project. \n    ","NOTE Dependability is an inherent characteristic of a system or product."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.1c","Requirement","ECSS-Q-ST-30_0410025",1,"Created","Manufacture, assembly, integration, test and operations shall not degrade dependability attributes introduced into the design."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.2a","Requirement","ECSS-Q-ST-30_0410026",1,"Created","The dependability requirement specification shall be part of the overall project requirements."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.2b","Requirement","ECSS-Q-ST-30_0410027",1,"Created","Dependability requirements shall be apportioned, in a top-down process, to establish dependability requirements for lower level elements. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.2c","Requirement","ECSS-Q-ST-30_0410028",1,"Created","Dependability requirements shall be applied during the preparation and review of design and test specifications. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.2d","Requirement","ECSS-Q-ST-30_0410029",1,"Created","The dependability requirements shall be included into the technical specifications. \n    ","NOTE The technical specifications typically include:\n        · functional, operational and environmental requirements,\n        · test requirements including stress levels, test parameters, and accept or reject criteria,\n        · design performance margins, derating factors, quantitative dependability requirements, and qualitative dependability requirements (identification and classification of undesirable events), under specified environmental conditions,\n        · the identification of human factors and how they can influence dependability during the project lifecycle,\n        · the identification of external, internal and installation factors that can influence dependability during the project lifecycle, \n        · the degree of tolerance to hardware failures or software malfunctions, \n        · the detection, isolation, diagnosis, and recovery of the system from failures and its restoration to an acceptable state,\n        · the requirement for the prevention of failures crossing interfaces with unacceptable consequences,\n        · definition of the maintenance concept,\n        · maintenance tasks and requirements for special skills, \n        · requirements for preventive maintenance, special tools, and special test equipment,\n        · requirements for process and technology margin demonstration and qualification,\n        · requirement on sampling strategy in serial production and for periodical demonstration of qualification preservation."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.1a","Requirement","ECSS-Q-ST-30_0410030",1,"Created","The identification of critical areas of design and the assessment of the severity of failure consequences shall be interpreted by the level at which the analysis is made. \n    ","NOTE The Space System level can be broken down into Space Segment and Ground Segment where separate requirements can be provided. The Space Segment and Ground Segment can be further broken down, dependant on particular contractual requirements, into lower levels elements (e.g. subsystem, equipment…). "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.1b","Requirement","ECSS-Q-ST-30_0410031",1,"Created","The success criteria (sometimes referred to as “mission success criteria”) shall be defined at each level to be analysed. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.2a","Requirement","ECSS-Q-ST-30_0410032",1,"Created","A severity classification (either severity name or level) shall be assigned in accordance with Table 5-1 to each identified failure mode analysed according to the failure effect (consequence). "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.2b","Requirement","ECSS-Q-ST-30_0410033",1,"Created","Severity categories shall be assigned without consideration of existing compensating provisions to provide a qualitative measure of the worst potential consequences resulting from item failure."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.2c","Requirement","ECSS-Q-ST-30_0410034",1,"Created","For analyses lower than system level, the severity due to possible failure propagation shall be identified as level 1 for dependability. \n    ","NOTE For example, for analysis at subsystem, and equipment level"]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.2d","Requirement","ECSS-Q-ST-30_0410035",1,"Created","The number identifying the severity category shall be followed by a suffix to indicate either redundancy (R) single point failures (SP) or safety hazards (SH)."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.2e","Requirement","ECSS-Q-ST-30_0410036",1,"Created","An understanding to these criteria identified in table 1 shall be agreed between customer and supplier."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.3a","Requirement","ECSS-Q-ST-30_0410037",1,"Created","Failure tolerance requirements shall be defined in the performance specifications."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.3b","Requirement","ECSS-Q-ST-30_0410038",1,"Created","The verification of the failure tolerance shall address all failure modes whose severity of consequence is classified as catastrophic, critical and major."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.4a","Requirement","ECSS-Q-ST-30_0410039",1,"Created","The supplier shall confirm that reliability is built into the design using fault tolerance and design margins. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.4b","Requirement","ECSS-Q-ST-30_0410040",1,"Created","The supplier shall analyse the failure characteristics of systems in order to identify areas of design weakness and propose corrective solutions. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.3.4c","Requirement","ECSS-Q-ST-30_0410041",1,"Created","In order to implement dependability aspects into the design, the following approaches shall apply:\n    1. functional design:\n        (a) the preferred use of software designs or methods that have performed successfully in similar applications\n        (b) the implementation of failure tolerance;\n        (c) the implementation of fault detection, isolation and recovery, allowing proper failure processing by dedicated flight and ground measures, and considering detection or reconfiguration times in relation with propagation times of events under worst case conditions;\n        (d) the implementation of monitoring of the parameters that are essential for mission performance, considering the failure modes of the system in relation to the actual capability of the detection devices, and considering the acceptable environmental conditions to be maintained on the product.\n    2. physical design:\n        (a) the application of proven design rules;\n        (b) the selective use of designs that have performed successfully in the same intended mission environment;\n        (c) the selection of parts having a quality level in accordance with project specification;\n        (d) the use of EEE parts derating and stress margins for mechanical parts;\n        (e) the use of design techniques for optimising redundancy (while keeping system design complexity as low as possible);\n        (f) the assurance that built-in equipment can be inspected and tested;\n        (g) the provision of accessibility to equipment.\n            ","NOTE Functional design is intended to imply non-physical design which includes software. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.4a","Requirement","ECSS-Q-ST-30_0410042",1,"Created","During the preliminary design phase, the contractor shall classify functions, operations and products in accordance with their criticality level."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.4b","Requirement","ECSS-Q-ST-30_0410043",1,"Created","Classification shall be approved by the customer."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.4c","Requirement","ECSS-Q-ST-30_0410044",1,"Created","The criticality of functions (hardware and/or software) and operations shall be directly related to the severity of the consequences resulting from failure of the function as defined in Table 5-1.\n    ","NOTE For example, a function whose failure induces a catastrophic consequence is required to be classified with the highest criticality level."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.4d","Requirement","ECSS-Q-ST-30_0410045",1,"Created","The criticality of a product (hardware and software) shall be identified at the highest criticality of the functions associated to that product."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.4e","Requirement","ECSS-Q-ST-30_0410046",1,"Created","The classification shall be used to focus efforts on the most critical areas during the project phases."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.5a","Requirement","ECSS-Q-ST-30_0410047",1,"Created","The supplier shall ensure that dependability aspects are covered in all development, qualification and acceptance test planning and reviews, including the preparation of test specifications and procedures and the evaluation of test results. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.5b","Requirement","ECSS-Q-ST-30_0410048",1,"Created","The dependability discipline shall support:\n    1. definition of test characteristics and test objectives,\n    2. selection of measurement parameters, and\n    3. statistical evaluation of test results."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.6a","Requirement","ECSS-Q-ST-30_0410049",1,"Created","The supplier shall ensure that dependability cognizant and qualified staff:\n    1. contribute to definition of operations manual and procedures, \n    2. review operations manual and procedures for verification of consistency with dependability analyses."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.6b","Requirement","ECSS-Q-ST-30_0410050",1,"Created","Procedures for operations shall be analysed to identify and assess the risks associated with operations, sequences and situations that can affect dependability performance."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.6c","Requirement","ECSS-Q-ST-30_0410051",1,"Created","The analyses mentioned in 5.6b shall take into account the technical and human environment, and verify that the procedures:\n    1. include dispositions to face abnormal situations and supply the necessary safeguard measures;\n    2. do not compromise equipment reliability;\n    3. are in accordance with established maintenance dispositions; \n    4. include dispositions to minimize failures due to human errors."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.7a","Requirement","ECSS-Q-ST-30_0410052",1,"Created","The supplier shall establish and maintain a system to track the dependability recommendations, in order to support the risk reduction process. \n    ","NOTE These recommendations are derived from the dependability analyses, and trade-off studies (typically during Phases A and B). The dependability recommendations can be tracked in combination with safety recommendations."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.7b","Requirement","ECSS-Q-ST-30_0410053",1,"Created","All recommendations from 5.7a shall be justified, documented and tracked."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.7c","Requirement","ECSS-Q-ST-30_0410054",1,"Created","Formal evidence of acceptance or rejection of the recommendation by the supplier’s management shall be provided."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","5.7d","Requirement","ECSS-Q-ST-30_0410055",1,"Created","An accepted dependability recommendation shall be implemented into the relevant corresponding documentation .\n    ","NOTE Example of corresponding documentation are: design documents, and operation manuals."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.1a","Requirement","ECSS-Q-ST-30_0410056",1,"Created","The supplier shall identify undesirable events that lead to the loss or degradation of product performances, together with their classification into categories related to the severity of their failures consequences (see Table 5-1)."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.1b","Requirement","ECSS-Q-ST-30_0410057",1,"Created","Preliminary identification and classification of undesirable events shall be determined from analysis of criteria for mission success, during conceptual and preliminary design phases. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.1c","Requirement","ECSS-Q-ST-30_0410058",1,"Created","All undesirable events, whose occurrence can jeopardize, compromise, or degrade the mission success shall be assessed at the highest product level (overall system including space and ground segments). "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.1d","Requirement","ECSS-Q-ST-30_0410059",1,"Created","The undesirable events, at lower levels of the product tree, shall be the product failure effects which can induce the undesirable events identified for the highest product level. \n    ","NOTE For example, at space segment, ground segment, subsystem, and equipment level."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.1e","Requirement","ECSS-Q-ST-30_0410060",1,"Created","Identification and classification of undesirable events shall be finalised after assessment of failure scenarios (see clause 6.2)."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.2a","Requirement","ECSS-Q-ST-30_0410061",1,"Created","The supplier shall analyse the possible scenarios leading to the occurrence of undesirable events, "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.2b","Requirement","ECSS-Q-ST-30_0410062",1,"Created","The supplier shall identify failure modes, failure origins and causes, detailed failure effects leading to undesirable events."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.3a","Requirement","ECSS-Q-ST-30_0410063",1,"Created","Dependability analyses shall be performed on all space projects throughout the project life cycle to support the tasks and requirements specified in clause 5."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.3b","Requirement","ECSS-Q-ST-30_0410064",1,"Created","Dependability analyses shall be performed initially to contribute to the definition of the conceptual design and the system requirements. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.3c","Requirement","ECSS-Q-ST-30_0410065",1,"Created","The analyses shall be performed to support the conceptual, preliminary and detailed development and optimization of the design, including the testing phase that leads to design qualification. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.3d","Requirement","ECSS-Q-ST-30_0410066",1,"Created","Dependability analyses shall be implemented in order to:\n    1. ensure conformance to reliability, availability and maintainability requirements, and\n    2. identify all potential failure modes and technical risks with respect to functional requirements that can lead to non-compliance to the dependability requirements, \n    3. provide inputs to risk assessment and risk reduction and their control measures in line with the risk management process implemented on the project."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.3e","Requirement","ECSS-Q-ST-30_0410067",1,"Created","The results of dependability analyses shall be incorporated into the design justification file in order to support improvements to the design."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.1a","Requirement","ECSS-Q-ST-30_0410068",1,"Created","Dependability analyses shall be conducted on all levels of the space system and be performed in respect of the level that is being assessed i.e. System, Subsystem and Equipment levels.\n    ","NOTE The main purpose of all dependability analyses is to improve the design by providing timely feedback to the designer, to reduce risks within the processes used to realize the products and to verify conformance to the specified dependability requirement."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.1b","Requirement","ECSS-Q-ST-30_0410069",1,"Created","The analyses identified in clauses 6.4.2 to 6.4.4 shall be:\n    1. conducted as required by the contract, \n    2. tailored to match the generic requirements on each project, \n    3. taking into account the hardware, software and human functions comprising the system. \n        ","NOTE As it is not possible to quantitatively assess the software functions, only a qualitative assessment can be made as the dependability of software is influenced by the software development process."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.1c","Requirement","ECSS-Q-ST-30_0410070",1,"Created","A set of analyses selected from clauses 6.4.2 to 6.4.4 shall be defined as part of the contract requirement."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.1a","Requirement","ECSS-Q-ST-30_0410071",1,"Created","Reliability prediction techniques shall be used with the following objectives:\n    1. to optimize the reliability of a design against competing constraints such as cost and mass, \n    2. to predict the in–service reliability of a product,\n    3. to provide failure probability data for purposes such as risk assessment. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.1b","Requirement","ECSS-Q-ST-30_0410072",1,"Created","The reliability data sources and methods used in reliability predictions shall be as specified by the customer. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.1c","Requirement","ECSS-Q-ST-30_0410073",1,"Created","If the reliability data sources and methods are not specified by the customer, the supplier shall justify the selected data sources and methods used, for customer approval. \n    ","NOTE ECSS-Q-HB-30-08 is a guideline for the selection of reliability data sources and their use."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.1d","Requirement","ECSS-Q-ST-30_0410074",1,"Created","Reliability models shall be prepared to support predictions and FMEA/FMECA. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2a","Requirement","ECSS-Q-ST-30_0410075",1,"Created","Failure Modes and Effects Analysis (FMEA) / Failure Modes, Effects and Criticality Analysis (FMECA) shall be performed on the functional and physical design (Functional FMECA and Product FMECA respectively) and, if required by the contract, the processes used to realize the final product (Process FMECA). "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2b","Requirement","ECSS-Q-ST-30_0410076",1,"Created","All potential failure modes shall be identified and classified according to the severity (FMEA) or criticality (FMECA) of their consequences."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2c","Requirement","ECSS-Q-ST-30_0410077",1,"Created","Measures shall be proposed in the analysis and introduced in the product design and in the control of processes to render all such consequences acceptable to the project."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2d","Requirement","ECSS-Q-ST-30_0410078",1,"Created","When any design or process changes are made, the FMEA/FMECA shall be updated and the effects of new failure modes introduced by the changes shall be assessed."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2e","Requirement","ECSS-Q-ST-30_0410079",1,"Created","Provisions for failure detection and recovery actions shall be identified as part of the FMEA/FMECA."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2f","Requirement","ECSS-Q-ST-30_0410080",1,"Created","The FMEA/FMECA shall be used to support the verification of the reliability modelling, the reliability and safety analyses, maintainability analysis, logistic support activity, test and maintenance planning, and the Failure Detection, Isolation and Recovery (FDIR) policy."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.2g","Requirement","ECSS-Q-ST-30_0410081",1,"Created","As part of the FMEA/FMECA, potential failure propagation shall be assessed.\n    ","NOTE For FMEA/FMECA refer to ECSS-Q-ST-30-02."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.3a","Requirement","ECSS-Q-ST-30_0410082",1,"Created","HSIA shall be performed to ensure that the software reacts in an acceptable way to hardware failure. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.3b","Requirement","ECSS-Q-ST-30_0410083",1,"Created","HSIA shall be performed at the level of the technical specification of the software. \n    ","NOTE HSIA can be included in the FMEA/FMECA (refer to ECSS-Q-ST-30-02)."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.4a","Requirement","ECSS-Q-ST-30_0410084",1,"Created","Contingency analysis shall be performed in conformance with Annex D in order to:\n    1. identify the failure, identify the cause, control the effect and indicate how recovery of the mission integrity can be achieved\n    2. identify the methods of recovery of the nominal or degraded functionalities, with respect to project dependability policy,\n        ","NOTE 1 For example, availability targets.\nNOTE 2 The contingency analysis is typically a system level task.\nNOTE 3 FMEA/FMECA is an input to contingency analysis."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.5a","Requirement","ECSS-Q-ST-30_0410085",1,"Created","A Fault Tree Analysis shall be performed to ensure that the design conforms to the failure tolerance requirements for combinations of failures. \n    ","NOTE 1 ECSS-Q-ST-40-12 is a guideline for FTA.\nNOTE 2 The system supplier performs FTA to identify possible event combinations leading to the undesirable end event (e.g. “loss of mission”). Subsystem supplier provides input to this activity by establishing FTA at subsystem level with respect to the top events:\n        · loss of function of the subsystem, and\n        · inadvertent activation of the subsystem function."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.6a","Requirement","ECSS-Q-ST-30_0410086",1,"Created","Common-cause analyses shall be performed on reliability and safety critical items in conformance with Annex I, to identify the root cause of failures that have a potential to negate failure tolerance levels (see clause 5.3.3). \n    ","NOTE 1 The analyses can be accomplished as part of FMEA/FMECA or FTA. \nNOTE 2 An example of check list of generic common-cause parameters is provided in Annex L                                                 "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.7a","Requirement","ECSS-Q-ST-30_0410087",1,"Created","Worst case analysis shall be performed on electrical equipment in conformance with Annex J, to demonstrate that it performs within specification despite variations in its constituent part parameters and the imposed environment."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.7b","Requirement","ECSS-Q-ST-30_0410088",1,"Created","The WCA report shall contain all baseline information (assumptions, methods and techniques) used for the preparation of the analysis, the results obtained and a comparison of the specified parameters as derived from the specification of the equipment or module."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.7c","Requirement","ECSS-Q-ST-30_0410089",1,"Created","If not specified in the project requirement, the supplier shall propose the component aging parameter drifts for customer approval.\n    ","NOTE 1 The document ECSS-Q-TM-30-12 is a source for component aging parameter drifts, but is to be complemented with others inputs as it does not cover exhaustively the EEE parts.\nNOTE 2 ECSS-Q-HB-30-01 describes the WCA methodology."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.8a","Requirement","ECSS-Q-ST-30_0410090",1,"Created","Part derating shall be implemented in conformance with ECSS-Q-ST-30-11 to assure that the stress levels applied to all EEE parts are within the limits. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.8b","Requirement","ECSS-Q-ST-30_0410091",1,"Created","Part stress analyses shall be performed at part level to verify that the derating rules have been implemented."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.9a","Requirement","ECSS-Q-ST-30_0410092",1,"Created","Zonal analysis shall be performed in conformance with Annex G, in order to evaluate the consequences due to potential subsystem-to-subsystem interactions inherent in the system installation."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.2.10a","Requirement","ECSS-Q-ST-30_0410093",1,"Created","FDIR analysis shall be performed at System level in conformance with Annex F, to ensure that the autonomy and failure tolerance requirements are fulfilled.\n    ","NOTE ECSS-E-ST-70-11 provides the description of FDIR process."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.3a","Requirement","ECSS-Q-ST-30_0410094",1,"Created","Maintainability requirements shall be apportioned to set maintainability requirements for lower level products to conform to the maintenance concept and maintainability requirements of the system."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.3b","Requirement","ECSS-Q-ST-30_0410095",1,"Created","Maintainability prediction shall be performed at system level in conformance with Annex H, and used as a design tool to assess and compare design alternatives with respect to specified maintainability quantitative requirements:\n    1. the time to diagnose (i.e. detect and isolate) item failures,\n    2. the time to remove and replace the defective item, \n    3. the time to return the system or subsystem to its nominal configuration and to perform the necessary checks, and\n    4. the item failure rates. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.3c","Requirement","ECSS-Q-ST-30_0410096",1,"Created","Preventive maintenance analysis shall be performed at system level to determine the maintenance plan. \n    ","NOTE Each preventive maintenance action is based on the results of the application of systematic decision logic approved by the customer."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.3d","Requirement","ECSS-Q-ST-30_0410097",1,"Created","The maintainability analysis shall identify maintainability critical items.\n    ","NOTE Maintainability critical items include:\n        · products that cannot be checked and tested after integration, \n        · limited-life products, \n        · products that do not meet, or cannot be validated as compliant to the maintainability requirements."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.4a","Requirement","ECSS-Q-ST-30_0410098",1,"Created","The supplier shall perform availability analysis or simulations in order to assess the availability of the system. \n    ","NOTE The results are used to:\n        · optimize the system concept with respect to design, operations and maintenance,\n        · verify conformance to availability requirements, \n        · provide inputs to estimate the overall cost of operating the system."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.4b","Requirement","ECSS-Q-ST-30_0410099",1,"Created","The supplier shall perform an analysis of outages in order to supply input data for availability analysis. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.4c","Requirement","ECSS-Q-ST-30_0410100",1,"Created","The availability analysis output shall include a list of all potential outages identified (as defined in the project), their causes, probabilities of occurrence and duration. \n    ","NOTE Instead of outage probabilities, failure rates associated with outages can be provided."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.4d","Requirement","ECSS-Q-ST-30_0410101",1,"Created","The means of outage detection and the recovery methods shall be identified in the analysis."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.4.4e","Requirement","ECSS-Q-ST-30_0410102",1,"Created","The availability analysis shall be carried out at system level using the system reliability and maintainability models as well as the data from the outages. \n    ","NOTE For availability analysis, refer to ECSS-Q-ST-30-09."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5a","Requirement","ECSS-Q-ST-30_0410103",1,"Created","The Dependability critical items identified by the dependability analyses shall be documented in conformance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5b","Requirement","ECSS-Q-ST-30_0410104",1,"Created","Items identified as single-point failure with at least a failure consequence severity classified as catastrophic, critical or major, shall be included in the dependability critical items list."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5c","Requirement","ECSS-Q-ST-30_0410105",1,"Created","Items that have a criticality number greater than or equal to 6 shall be included in the dependability critical items list in conformance with ECSS-Q-ST-30-02."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5d","Requirement","ECSS-Q-ST-30_0410106",1,"Created","All items that have failure consequences classified as catastrophic shall be included in the dependability critical items list."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5e","Requirement","ECSS-Q-ST-30_0410107",1,"Created","Products that cannot be checked and tested after integration, limited–life products, products that do not meet - or cannot be verified as meeting - applicable maintainability requirements, shall be included in the dependability critical items list."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","6.5f","Requirement","ECSS-Q-ST-30_0410108",1,"Created","The documentation for each dependability critical item shall include a justification for retention of that item and be subject to approval by the customer.\n    ","NOTE Further criteria for the classification of dependability critical items can be specified by the customer in line with the risk management policy defined on the project."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","7.1a","Requirement","ECSS-Q-ST-30_0410109",1,"Created","Reliability testing and demonstration shall be performed according to the project requirements in order to:\n    1. validate failure modes and effects,\n    2. check failure tolerance, failure detection and recovery,\n    3. obtain statistical failure data to support predictions and risk assessment,\n    4. consolidate reliability assessments,\n    5. validate the capability of the hardware to operate with software or to be operated by a human being in accordance with the specifications,\n    6. demonstrate the reliability of critical items, and\n    7. validate or justify data bases used for theoretical demonstrations."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","7.2a","Requirement","ECSS-Q-ST-30_0410110",1,"Created","Availability testing and demonstration shall be performed according to the project requirements in order to validate or justify data bases used for theoretical demonstrations (duration of outages and probability of occurrence)."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","7.3a","Requirement","ECSS-Q-ST-30_0410111",1,"Created","Maintainability demonstration shall be performed by performing the verification of the applicable maintainability requirements and by ensuring that preventive and corrective maintenance activities are successfully performed within the scope of the maintenance concept. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","7.3b","Requirement","ECSS-Q-ST-30_0410112",1,"Created","“The maintainability demonstration” shall verify the ability to:\n    1. detect, diagnose and isolate each faulty line replaceable unit or orbit replaceable unit;\n    2. remove and replace each line replaceable unit or orbit replaceable unit;\n    3. perform mission-essential repairs on units that are not intended to be replaced;\n    4. check that the product is fully functional after maintenance actions have been completed;\n    5. demonstrate that no safety hazard is introduced as a result of maintenance actions;\n    6. demonstrate that the maintenance operations can be performed within the applicable constraints, including the operations necessary to prepare a system during the launch campaign \n        ","NOTE 1 xample of such a constraints are time and volume or accessibility. \nNOTE 2 Example of such operations are “remove-before-flight” items or replacement of batteries. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","7.4a","Requirement","ECSS-Q-ST-30_0410113",1,"Created","Dependability data as specified in the contract, shall be collected for a period agreed with the customer from sources such as non-conformance and problem or failure reports, and maintenance reports. \n    ","NOTE Dependability data can be used for dependability performances monitoring through agreed or specified models. "]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","C.7a","Requirement","ECSS-Q-ST-30_0410114",1,"Created","The dependability plan shall include as a minimum:\n    • list of the applicable and reference documents,\n    • applicable dependability requirements,\n    • description of the dependability organisation and management,\n    • contractor / supplier management,\n    • details of the dependability tasks for each phase,\n    • dependability activities status reporting."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","D.7a","Requirement","ECSS-Q-ST-30_0410115",1,"Created","The contingency analysis document shall include:\n    • a description of the system,\n    • a description of the method to perform contingency analysis,\n    • details of the failure detection method,\n    • details of the diagnostics,\n    • details of the recovery actions or procedures,\n    • actions and recommendations for project team."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","E.7a","Requirement","ECSS-Q-ST-30_0410116",1,"Created","The reliability prediction document shall include:\n    • a clear identification of the design being analysed,\n    • reliability block diagrams,\n    • the methodology used with rationales,\n    • an analysis of the results,\n    • recommendations for project decision."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","F.7a","Requirement","ECSS-Q-ST-30_0410117",1,"Created","The FDIR analysis document shall include:\n• a description of the system\n• a description of the method to perform FDIR (e.g. FMEA/FMECA synthesis, FDIR reviews),\n• details of considered failures,\n• symptoms of failures (e.g. TM, observables),\n• detailed failure impact on the system,\n• the recovery actions (e.g. TC, automatic on board mechanism),\n• actions and recommendations for project team."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","G.7a","Requirement","ECSS-Q-ST-30_0410118",1,"Created","The zonal analysis document shall include:\n    • an identification of the perimeter under investigation, \n    • a detailed definition of the interface(s),\n    • the description of the potential interaction(s),\n    • the list of actions and recommendations for project decision."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","H.7a","Requirement","ECSS-Q-ST-30_0410119",1,"Created","The document shall contain, as a minimum:\n    • maintenance levels: for corrective and preventive actions,\n    • identification of FDIR policy,\n    • mathematical model description,\n    • the maintenance indicators (e.g. MTTR, maintenance time per year, maintenance frequency),\n    • the sparing recommendations (e.g. number of spares, weight and volume of up and downloading spares),\n    • identification of Maintainability Critical Items."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","I.7a","Requirement","ECSS-Q-ST-30_0410120",1,"Created","The common-cause analysis document shall include:\n    • a description of the perimeter of the design being analysed,\n    • the list of the ‘common-cause’ parameters and their effects,\n    • actions and recommendations for project team.\n\t","NOTE See check lists parameters examples in Annex L."]
["ECSS-Q-ST-30C","ECSS - Superseded v1.0","J.7a","Requirement","ECSS-Q-ST-30_0410121",1,"Created","The WCA document shall include:\n    • assumptions applicable to the environmental condition,\n    • a list of the selected parts database with the worst case parameters,\n    • a description of the general methodology, \n    • an explanation of the numerical analysis technique, \n    • results and conclusion of the WCA."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.1a","Requirement","ECSS-Q-ST-40_0440001",1,"Created","The supplier shall establish and maintain a safety programme to assure conformance with project safety policy and requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.1b","Requirement","ECSS-Q-ST-40_0440002",1,"Created","The safety programme shall establish a safety management system to implement provisions of this Standard - commensurate with the programme requirements and tailored by the customer \n    NOTE 1 For tailoring, refer to clause 1                                         \n    NOTE 2 The system safety programme requirements are subject to tailoring, without diminishing the intent to protect flight and ground personnel, the launch vehicle, associated payloads, ground support equipment, the general public, public and private property, the space system and associated segments and the environment from hazards associated with space systems.\n    NOTE 3 As support to tailoring, informative Annex F provides a guideline for determining the applicability of this standard depending on the type of project."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.2a","Requirement","ECSS-Q-ST-40_0440003",1,"Created","The supplier shall establish and maintain a safety programme plan in conformance with the DRD in Annex B.\n    NOTE The plan can either be included as part of an overall project product assurance plan or as a separate safety programme plan."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.2b","Requirement","ECSS-Q-ST-40_0440004",1,"Created","The supplier shall cover, in his safety programme plan, the safety tasks for the project phases in conformance with 5.7.1."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.3a","Requirement","ECSS-Q-ST-40_0440005",1,"Created","The supplier shall comply with all applicable national or international safety regulations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.3b","Requirement","ECSS-Q-ST-40_0440006",1,"Created","The launch site safety regulations and rules shall be applied."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.3c","Requirement","ECSS-Q-ST-40_0440007",1,"Created","The implementation of safety requirements shall not be compromised by other requirements.\n    NOTE For example: security requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.1a","Requirement","ECSS-Q-ST-40_0440008",1,"Created","Each supplier shall appoint a safety manager who has appropriate training or experience."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.1b","Requirement","ECSS-Q-ST-40_0440009",1,"Created","The safety manager shall have organisational authority and independence to:\n    1. establish and maintain a safety programme in accordance with the project safety requirements,\n    2. manage all safety assurance aspects of the design of the system (including software) and its operation in accordance with the Safety Plan,\n    3. coordinate the interfaces:\n        (a) with the relevant bodies involved in the project in accordance with the safety plan,\n        (b) with the safety launcher authority.\n            NOTE Depending on the project safety criticality, the safety manager can be combined with other functions (e.g. PA manager) when agreed with the customer."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.2.1a","Requirement","ECSS-Q-ST-40_0440010",1,"Created","The safety manager shall:\n    1. have the right of access to safety-related data relevant to project safety in conformance with ECSS-M-ST-40, \n    2. have unimpeded access to any management level without organizational constraint on any aspect of project safety."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.2.2a","Requirement","ECSS-Q-ST-40_0440011",1,"Created","The safety manager or safety relevant authority shall have the authority to:\n    1. reject any project document, or to stop any project activity that does not conform to approved safety requirements or procedures,\n    2. interrupt hazardous operations when it becomes clear by the Safety Manager that the operation does not conform to the agreed measures defined in the corresponding hazard report and derived approved hazard procedure."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.3a","Requirement","ECSS-Q-ST-40_0440012",1,"Created","The supplier shall perform safety audits or reviews to verify compliance to project safety policy and requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.3b","Requirement","ECSS-Q-ST-40_0440013",1,"Created","The safety audits shall be in accordance with ECSS-M-ST-10 and ECSS-Q-ST-10.\n    NOTE The safety audits can be part of the project audits."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.3c","Requirement","ECSS-Q-ST-40_0440014",1,"Created","The customer shall be informed of the audit schedule."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.4a","Requirement","ECSS-Q-ST-40_0440015",1,"Created","Documentation related to safety shall be approved by the safety manager upon his verification of completeness, compliance with stated safety requirements and formal closeout of open safety verification items (as defined and agreed during safety audits and reviews)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.5a","Requirement","ECSS-Q-ST-40_0440016",1,"Created","The safety manager (or a designated representative) shall have concluded the review of, and approved, any hazardous operation before it is executed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.6a","Requirement","ECSS-Q-ST-40_0440017",1,"Created","The safety manager or designated delegate shall be represented at configuration control boards (CCBs), nonconformance review boards (NRBs), test review board (TRBs), and at qualification, and acceptance reviews, where safety requirements and safety-critical functions are involved."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.6b","Requirement","ECSS-Q-ST-40_0440018",1,"Created","The safety function shall be further represented at all boards dealing with health matters where exposure or endurance limits are defined for flight and ground crews."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.4.7a","Requirement","ECSS-Q-ST-40_0440019",1,"Created","The safety approval authority shall:\n    1. review and disposes the safety data submittals,\n    2. approve the close-out of hazards,\n    3. decide on deviations and waivers, and finally\n    4. accept the statement of safety compliance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.5a","Requirement","ECSS-Q-ST-40_0440020",1,"Created","The safety risk identification, reduction and control shall be part of the project's risk management process as specified in ECSS-M-ST-80."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.5b","Requirement","ECSS-Q-ST-40_0440021",1,"Created","Safety risk identification, reduction and control shall be a continuous and iterative process throughout the project life cycle, encompassing\n    1. allocation of safety requirements;\n    2. hazard and safety risk identification;\n    3. evaluation (including categorisation) of consequence severity;\n    4. hazard and safety risk reduction and control;\n    5. close out and acceptance of residual risk."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.5c","Requirement","ECSS-Q-ST-40_0440022",1,"Created","For the identification of hazards and associated safety risks, consideration shall be given to past experience, studies, ground and flight tests, reviews, the industrial process as well as the operational use."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.6a","Requirement","ECSS-Q-ST-40_0440023",1,"Created","The safety critical items shall be part of the project's overall critical items control programme as specified in ECSS-Q-ST-10-04."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.1a","Requirement","ECSS-Q-ST-40_0440024",1,"Created","Safety analysis shall support the identification of sources of safety risk as well as the performance of preliminary trade-off analyses between alternative system concepts."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.1b","Requirement","ECSS-Q-ST-40_0440025",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Analyse safety requirements and lessons-learnt associated with similar previous missions;\n    2. Perform preliminary hazard analysis of the proposed system and operations concept to support concept trade-offs;\n    3. Perform comparative safety risk assessment of the concept options;\n    4. Identify the relevant project safety requirements;\n    5. Plan safety activities for the feasibility phase;\n    6. Support the mission definition review.\n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.2a","Requirement","ECSS-Q-ST-40_0440026",1,"Created","Safety analysis shall support trade-off analyses in arriving at the concept that has acceptable safety risk considering the project and mission constraints. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.2b","Requirement","ECSS-Q-ST-40_0440027",1,"Created","The design technology selected and the operational concept to be implemented shall be selected based on the analysis data for the safest system architecture to eliminate or reduce hazards to acceptable levels."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.2c","Requirement","ECSS-Q-ST-40_0440028",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Commence hazard analyses of the design and operations concepts in order to identify applicable system level hazards, hazardous conditions, and potential hazardous events and consequences; \n    2. Support concept trades by identifying safety critical aspects of the concept options;\n    3. Apply hazard elimination and minimization and make safety recommendations; \n    4. Perform comparative safety risk assessments of the concept options; \n    5. Identify system level safety critical functions;\n    6. Identify system level project specific safety requirements; \n    7. Plan safety activities for the project definition phase; \n    8. Support the preliminary requirements review. \n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.3a","Requirement","ECSS-Q-ST-40_0440029",1,"Created","The safety analysis shall support a continued and more detailed safety optimization of the system design and operations and the identification of technical safety requirements and their applicability."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.3b","Requirement","ECSS-Q-ST-40_0440030",1,"Created","The analysis shall also provide inputs to safety risk assessment in support of safety risk evaluation, the identification of risk contributors in the design and in the operational concept."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.3c","Requirement","ECSS-Q-ST-40_0440031",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Update hazard analysis in support of design and mission concept definition activities; identify additional project specific safety requirements; \n    2. Update safety critical functions identification, and define the failure tolerance requirements; \n    3. Identify emergency, warning, and caution situations;\n    4. Update the system safety risk assessment as part of the contribution provided by the safety domain to the risk management process;\n    5. Identify project safety requirements; \n    6. Ensure that project requirement documentation and activities comply with project safety requirements;\n    7. Support a system requirements review and preliminary design review; \n    8. Plan verification of safety requirements implementation; \n    9. Prepare the safety plan for the detailed definition, production and qualification phase. \n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.4a","Requirement","ECSS-Q-ST-40_0440032",1,"Created","Safety analysis shall support detailed design, production, qualification, testing."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.4b","Requirement","ECSS-Q-ST-40_0440033",1,"Created","Safety analysis shall also support operational safety optimization, safety requirements implementation evaluation, risk reduction verification, and hazard and risk acceptance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.4c","Requirement","ECSS-Q-ST-40_0440034",1,"Created","Analysis of operations shall also support the identification of emergency and contingency response planning and training requirements, and the development of procedures."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.4d","Requirement","ECSS-Q-ST-40_0440035",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Perform detailed system level hazard analysis; \n    2. Perform supporting safety analysis;\n    3. Update the project technical safety requirements to incorporate the results of safety analyses; \n    4. Ensure that the project implementation and verification programme covers identified hazard control verification activities; \n        NOTE For example: reviews, inspections, analyses and tests.\n    5. Update safety critical functions identification, failure tolerance requirements, and identify safety critical items; \n    6. Implement control programme for safety critical items; \n    7. Perform safety risk assessment in support of design improvement, project resource apportionment, control programme for safety critical items and project reviews; \n    8. Monitor verification of safety requirements implementation; \n    9. Verify and document hazard control implementation; \n    10. Check that all open verification items are recorded and agreed procedures are in place;\n    11. Support the critical design review, the qualification review and the acceptance review;\n    12. Perform project internal safety reviews and internal audits; \n    13. Identify, monitor and control project assembly, integration, testing and handling operations which are potentially hazardous to personnel or hardware; \n    14. Review and approve hazardous and safety critical operational procedures;\n    15. Perform accident-incident reporting and investigation; \n    16. Support customer safety reviews at defined programme milestones;\n    17. Prepare a project safety “lessons-learned” report; \n    18. Prepare operational phase safety plan. \n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.5a","Requirement","ECSS-Q-ST-40_0440036",1,"Created","Safety analysis shall evaluate design and operational changes for impact to safety, assuring that safety margins are maintained and that operations are conducted within accepted risk."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.5b","Requirement","ECSS-Q-ST-40_0440037",1,"Created","The analysis shall also support the evaluation of operational anomalies for impact to safety, and the continued evaluation of risk trends."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.5c","Requirement","ECSS-Q-ST-40_0440038",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Issue the operational phase safety plan;\n    2. Review operational procedures; \n    3. Approve safety critical operational procedures; \n    4. Identify and monitor hazardous operations; \n    5. Support the flight readiness review, operational readiness review, launch readiness review and flight qualification reviews;\n    6. Support ground and flight operations; \n    7. Perform safety critical items control; \n    8. Monitor and assess evolution of the system configuration and operations resulting from design fixes and updates;\n    9. Update hazard analyses and implement additional hazard controls as necessary; \n    10. Investigate safety related flight anomalies and trends; \n    11. Update safety risk assessment as necessary to support operational decisions;\n    12. Prepare disposal phase safety plan. \n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.6a","Requirement","ECSS-Q-ST-40_0440039",1,"Created","Safety analysis shall evaluate all disposal operations and associated hazards. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.6b","Requirement","ECSS-Q-ST-40_0440040",1,"Created","Disposal solutions shall be identified which meet the project's safety requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.1.6c","Requirement","ECSS-Q-ST-40_0440041",1,"Created","The following safety programme tasks shall apply for human spaceflight programmes and safety critical systems:\n    1. Perform hazard analysis with respect to the disposal operations;\n    2. Check that the disposal operation conforms to international safety regulations by performing the necessary safety analysis;\n    3. Review the procedures of the disposal operations;\n    4. Support the mission close-out review.\n        NOTE These tasks should also serve as a guideline for other space programmes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.2a","Requirement","ECSS-Q-ST-40_0440042",1,"Created","The supplier shall hold regular safety status and progress meetings with the customer and his lower tier suppliers as part of the project progress meetings as specified in ECSS-M-ST-10. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.2b","Requirement","ECSS-Q-ST-40_0440043",1,"Created","The relevant customer and supplier specialists shall attend the meetings."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.3a","Requirement","ECSS-Q-ST-40_0440044",1,"Created","The customer shall define, conduct and chair the safety reviews to ensure satisfactory implementation of safety programme and technical safety requirements. \n    NOTE A supplier is considered as a customer vis-à-vis its lower tier suppliers (as defined in ECSS-S-ST-00)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.3b","Requirement","ECSS-Q-ST-40_0440045",1,"Created","The supplier shall support safety reviews by the customer and the relevant safety approval authority, as specified in the relevant review plans. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.3c","Requirement","ECSS-Q-ST-40_0440046",1,"Created","Each supplier participating in a safety review shall prepare, and submit for review, the safety data package."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.7.3d","Requirement","ECSS-Q-ST-40_0440047",1,"Created","Safety reviews shall be performed, and the review objectives achieved, in conformance with clause 5.7.1."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.8a","Requirement","ECSS-Q-ST-40_0440048",1,"Created","The supplier shall provide a statement of safety compliance to demonstrate that the space system elements conform to stated safety requirements. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.8b","Requirement","ECSS-Q-ST-40_0440049",1,"Created","The supplier shall include in his statement of compliance a statement that open verifications are followed up in the safety verification tracking log (SVTL), as defined in clause 8.5.1, and do not affect further safe processing."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.8c","Requirement","ECSS-Q-ST-40_0440050",1,"Created","The project shall provide to the safety approval authority all safety-related information for their acceptance of the statement of safety compliance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.1a","Requirement","ECSS-Q-ST-40_0440051",1,"Created","Safety training shall be part of the overall training in accordance with ECSS-Q-ST-20."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.1b","Requirement","ECSS-Q-ST-40_0440052",1,"Created","All safety related training of any personnel working - permanently or occasionally - with system elements that can have hazardous properties shall have three major aspects:\n    1. general awareness briefings on safety measures to be taken at a given location or working environment;\n    2. basic technical training in the required safety techniques and skills which is a prerequisite to fulfil the job function under consideration;\n        NOTE For example: inspection, test, maintenance or integration.\n    3. product specific training that focuses on the hazards related to the specific system element."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.2a","Requirement","ECSS-Q-ST-40_0440053",1,"Created","The supplier shall identify the need for product specific safety training and implement the corresponding safety training programme for all relevant parties. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.2b","Requirement","ECSS-Q-ST-40_0440054",1,"Created","The supplier shall inform the customer of any safety training identified by him as necessary for the flight operations crew or mission control personnel, together with a definition of the type of training required and its scope."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.2c","Requirement","ECSS-Q-ST-40_0440055",1,"Created","The supplier shall support the implementation of the customer's training programme for the flight operations crew or mission control personnel."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.3a","Requirement","ECSS-Q-ST-40_0440056",1,"Created","All personnel accessing the area where the product is processed shall participate previously in the general safety awareness briefing."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.4a","Requirement","ECSS-Q-ST-40_0440057",1,"Created","The supplier shall provide basic technical training to all project engineering and safety personnel working with hazardous products."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.9.5a","Requirement","ECSS-Q-ST-40_0440058",1,"Created","The supplier shall maintain records of personnel having received safety training in accordance with ECSS-Q-ST-20."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10a","Requirement","ECSS-Q-ST-40_0440059",1,"Created","The supplier shall report to the customer all accidents and incidents occurred during project activities under the control of the supplier or his lower tier suppliers that affect the system element. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10b","Requirement","ECSS-Q-ST-40_0440060",1,"Created","The supplier shall support - at request - project related accident and incident investigations that occur outside of the supplier’s control or facility."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10c","Requirement","ECSS-Q-ST-40_0440061",1,"Created","The supplier shall coordinate the investigation activities in cooperation with other supplier functional departments and lower tier suppliers."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10d","Requirement","ECSS-Q-ST-40_0440062",1,"Created","The accident or incident investigation report shall be formally closed by the supplier upon approval by the customer."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10e","Requirement","ECSS-Q-ST-40_0440063",1,"Created","If the conclusion of the assessment is that the accident-incident has had an effect on the project, i.e. the safety of the product or its operation, the organisations safety representative shall be informed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.10f","Requirement","ECSS-Q-ST-40_0440064",1,"Created","In case of 5.10e., the accident-incident report shall become part of the project's safety data and is documented in the safety data package."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.1a","Requirement","ECSS-Q-ST-40_0440065",1,"Created","The supplier shall maintain, as part of the project documentation, all safety-related data to support reviews and safety compliance demonstration."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.1b","Requirement","ECSS-Q-ST-40_0440066",1,"Created","The customer shall be given access to this data on request during audits, safety reviews and meetings held at the supplier’s premises in accordance with ECSS-M-ST-40."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2a","Requirement","ECSS-Q-ST-40_0440067",1,"Created","The supplier shall submit a safety data package (SDP) to support reviews.\n    NOTE This can be a stand-alone package or be integrated into the overall data package if the safety review is part of an overall project review."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2b","Requirement","ECSS-Q-ST-40_0440068",1,"Created","The safety data package shall contain at least the following safety related documentation:\n    1. Safety analysis report (in accordance with Annex D);\n    2. Supporting analysis (if applicable);\n    3. Safety risk assessment (if applicable);\n    4. Hazardous ground operations list and procedures;\n    5. Safety verification tracking log (SVTL, in accordance with Annex C)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2c","Requirement","ECSS-Q-ST-40_0440069",1,"Created","The contents of the safety data packages for the planned safety reviews of a project or programme shall be specified by the Safety Approval Authority to assure they support the objectives of the safety reviews for which they are delivered (in conformance with clause 5.7.2). "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2d","Requirement","ECSS-Q-ST-40_0440070",1,"Created","The supplier shall use the actual configuration baseline, as defined by ECSS-M-ST-40, as the design and operational baseline that is the subject of the safety data package."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2e","Requirement","ECSS-Q-ST-40_0440071",1,"Created","The supplier shall integrate safety data related to the various subsystems or equipment that makes up the system into the safety data package that is presented at the review."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.2f","Requirement","ECSS-Q-ST-40_0440072",1,"Created","All safety data shall be traceable from the safety data package and available for review."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.1a","Requirement","ECSS-Q-ST-40_0440073",1,"Created","Safety requirements that cannot be met shall be identified as specified in ECSS-M-ST-40."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.1b","Requirement","ECSS-Q-ST-40_0440074",1,"Created","A request for deviation or waiver shall be generated and tracked according to the requirements of ECSS-M-ST-40. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.2a","Requirement","ECSS-Q-ST-40_0440075",1,"Created","All RFD/RFW shall be assessed in order to identify those which impact safety. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.2b","Requirement","ECSS-Q-ST-40_0440076",1,"Created","The accumulated deviations and waivers that affect safety shall be assessed to ensure that the effects of individual deviations do not invalidate the rationale used for the acceptance of other deviations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.3a","Requirement","ECSS-Q-ST-40_0440077",1,"Created","Safety deviations and waivers shall be subject to safety approval authority acceptance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.3.4a","Requirement","ECSS-Q-ST-40_0440078",1,"Created","Deviations and waivers that affect project safety requirements or safety-critical functions which the supplier considers acceptable shall be subject of review and disposition by the customer and the safety approval authority."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.4a","Requirement","ECSS-Q-ST-40_0440079",1,"Created","Safety lessons learned shall be collected during the project and used during the project, as far as they are relevant.\n    NOTE Safety lessons learned should consider as a minimum:\n        a. the impact of newly imposed requirements;\n        b. assessment of all malfunctions, accidents, anomalies, deviations and waivers;\n        c. effectiveness of safety strategies of the project;\n        d. new safety tools and methods that have been developed or demonstrated;\n        e. effective versus ineffective verifications that have been performed;\n        f. changes proposed to safety policy, strategy or technical requirements with rationale."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.4b","Requirement","ECSS-Q-ST-40_0440080",1,"Created","The safety lessons learned information shall be made available to the customer and suppliers, particularly to project and safety managers as well as design and safety engineers upon request for use on other projects. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","5.11.5a","Requirement","ECSS-Q-ST-40_0440081",1,"Created","The safety critical items identified by the safety analysis shall be documented in accordance with ECSS-Q-ST-10-04."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.2a","Requirement","ECSS-Q-ST-40_0440082",1,"Created","Safety requirements shall be identified and traced from the system level into the design and then allocated to the lower levels."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.2b","Requirement","ECSS-Q-ST-40_0440083",1,"Created","When specified by the project, the identified safety requirements shall be justified in the design and presented in an appropriate document."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.2a","Requirement","ECSS-Q-ST-40_0440084",1,"Created","Appropriate design features shall be selected to ensure inherent safety.\n    NOTE Such features are fail safe design solutions, damage control, containment and isolation of potential hazards. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.1a","Requirement","ECSS-Q-ST-40_0440085",1,"Created","The following sequence of activities shall be applied to identified hazards, hazardous conditions, and functions whose failures have hazardous consequences:\n    1. Hazard elimination\n    2. Hazard minimization\n    3. Hazard control."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.2a","Requirement","ECSS-Q-ST-40_0440086",1,"Created","Hazards and hazardous conditions shall, consistent with the project constraints and mission objectives, be eliminated from the design and operational concepts by the selection of design technology, architecture and operational characteristics. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.3a","Requirement","ECSS-Q-ST-40_0440087",1,"Created","Where hazards and hazardous conditions are not eliminated, the severity of the associated hazardous events and consequences shall, consistent with the project constraints and mission objectives, be reduced to an accepted level through the change of the design architecture, technologies, and operational characteristics allowing the substitution of those hazards by other hazards with lower potential threat."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.1a","Requirement","ECSS-Q-ST-40_0440088",1,"Created","Hazards that have not been eliminated and have been subjected to hazard minimization (as defined in 6.3.3.3a) shall be controlled through preventative or mitigation measures, associated to hazard scenarios, which are introduced into the system design and operation to avoid the events or to interrupt their propagation to consequences."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.1b","Requirement","ECSS-Q-ST-40_0440089",1,"Created","The following measures shall be applied in order of precedence:\n    1. Design selection\n    2. Automatic safety devices\n    3. Warning devices\n    4. Special procedures."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.2a","Requirement","ECSS-Q-ST-40_0440090",1,"Created","Failure tolerance is the basic safety requirement that shall be used to control most hazards. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.2b","Requirement","ECSS-Q-ST-40_0440091",1,"Created","The design shall tolerate a minimum number of credible failures and/or operator errors determined by the hazard consequence."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.2c","Requirement","ECSS-Q-ST-40_0440092",1,"Created","The supplier shall establish the list of failures to be considered as \"non credible\" for customer approval as early as possible in development."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.3a","Requirement","ECSS-Q-ST-40_0440093",1,"Created","Hazard which cannot be controlled by compliance to failure tolerance shall be reduced to an accepted level by compliance with specific safety related properties and characteristics of the design. \n    NOTE Examples are: structures, pressures vessels, mechanisms, material compatibility, flammability."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.4a","Requirement","ECSS-Q-ST-40_0440094",1,"Created","Hazards that are not eliminated through design selection shall be reduced and made controllable through the use of automatic safety devices as part of the system, subsystem or equipment. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.4b","Requirement","ECSS-Q-ST-40_0440095",1,"Created","The safety devices, specified in 6.3.3.4.4a, shall not be dependant on human performance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.4c","Recommendation","ECSS-Q-ST-40_0440320",1,"Created","Use of software in automatic safety devices should be avoided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.4d","Requirement","ECSS-Q-ST-40_0440097",1,"Created","If software is used in automatic safety devices, justification shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.5a","Requirement","ECSS-Q-ST-40_0440098",1,"Created","When it is not practical to preclude the existence or occurrence of known hazards or to use automatic safety devices, devices shall be used for the timely detection of the condition and the generation of a warning signal."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.5b","Requirement","ECSS-Q-ST-40_0440099",1,"Created","This shall be coupled with emergency controls of corrective action for operators to safe or shut down the affected subsystem."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.6a","Requirement","ECSS-Q-ST-40_0440100",1,"Created","When it is not possible to reduce the magnitude of a hazard through the design, the use of safety devices or the use of warning devices, special procedures shall be developed to control the hazardous conditions for the enhancement of safety."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.6b","Requirement","ECSS-Q-ST-40_0440101",1,"Created","Special procedures shall be verified by test and appropriate training be provided for personnel."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.6c","Requirement","ECSS-Q-ST-40_0440102",1,"Created","Hazard detection shall be implemented if alternative means cannot be used."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.3.4.6d","Requirement","ECSS-Q-ST-40_0440103",1,"Created","To permit the use of real time monitoring, hazard detection and safing systems for hazard control, the availability of sufficient response time shall be verified and corresponding safing procedures be developed and verified and the personnel trained.\n    NOTE Special procedures are the least effective of the hazard control and risk reduction measures available. They can include emergency and contingency procedures, procedural constraints, or the application of a controlled maintenance programme. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.4a","Requirement","ECSS-Q-ST-40_0440104",1,"Created","The system design shall meet the safety requirements under the worst-case natural and induced environments defined for the project."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.4b","Requirement","ECSS-Q-ST-40_0440105",1,"Created","Design and performance margins shall be established and applied for worst-case combinations of induced and natural environments and operating characteristics."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.5a","Requirement","ECSS-Q-ST-40_0440106",1,"Created","Loss, malfunctioning, and sudden restoration of external services shall be defined as an input to the development phase."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.5b","Requirement","ECSS-Q-ST-40_0440107",1,"Created","The system design shall be defined so that catastrophic or critical consequences are not induced by loss, malfunctioning, and sudden restoration of external services."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6a","Requirement","ECSS-Q-ST-40_0440108",1,"Created","Safety monitoring, display, alarm and safing capabilities shall be incorporated for manned space systems."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6b","Requirement","ECSS-Q-ST-40_0440109",1,"Created","These capabilities shall provide the information to allow the crew and system operators to take actions to protect personnel from the consequences of failures within safety-critical functions and the failure of hazard control measures."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6c","Requirement","ECSS-Q-ST-40_0440110",1,"Created","The system design shall provide the capability for detecting failures that result in degradation of failure tolerance with respect to the hazard detection, signalling and safing function."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6d","Requirement","ECSS-Q-ST-40_0440111",1,"Created","The performance of these functions shall be verifiable during flight and ground operational phases."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6e","Requirement","ECSS-Q-ST-40_0440112",1,"Created","The emergency, caution and warning function shall detect and notify the crew and system operators of emergency, warning and caution situations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6f","Requirement","ECSS-Q-ST-40_0440113",1,"Created","Safing functions and capabilities shall be included that provide for the containment or control of emergency, warning and caution situations. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6g","Requirement","ECSS-Q-ST-40_0440114",1,"Created","Provisions shall be included for the monitoring of safing function execution. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6h","Requirement","ECSS-Q-ST-40_0440115",1,"Created","Dedicated safing functions shall be provided for emergency situations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6i","Requirement","ECSS-Q-ST-40_0440116",1,"Created","Control of warning and caution situations shall be acceptable by system reconfiguration or by dedicated safing functions."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6j","Requirement","ECSS-Q-ST-40_0440117",1,"Created","A single failure shall not cause loss of the emergency and warning function."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6k","Requirement","ECSS-Q-ST-40_0440118",1,"Created","Where the operation of a safing system introduces a new hazard, inadvertent activation of the safing system shall be controlled in accordance with the failure tolerance requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6l","Requirement","ECSS-Q-ST-40_0440119",1,"Created","A single failure shall not cause loss of the emergency and warning functions together with the monitored functions. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6m","Requirement","ECSS-Q-ST-40_0440120",1,"Created","Emergency, warning and caution data, out of limit annunciation and safing commands shall be given priority over other data processing and command functions."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6n","Requirement","ECSS-Q-ST-40_0440121",1,"Created","When systems or elements are integrated into, or docked with the other systems or elements, the emergency, warning, caution, and safing function shall enable the areas of control responsibility to monitor and display the applicable parameters, and to control the related safing functions. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6o","Requirement","ECSS-Q-ST-40_0440122",1,"Created","Emergency, warning, and caution parameter status information shall be available and displayed at the launch control and mission control centres in “near real time” during the operational phases. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.6p","Requirement","ECSS-Q-ST-40_0440123",1,"Created","It shall be possible for the crew to ascertain and monitor in “real time” the status of emergency, warning and caution parameters of non-crewed systems or elements prior to docking with crewed systems."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.7a","Requirement","ECSS-Q-ST-40_0440124",1,"Created","The design and the operational characteristics of the space system shall be such that the generation of space debris is minimized consistent with the project constraints and mission objectives."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.8a","Requirement","ECSS-Q-ST-40_0440125",1,"Created","The space vehicle shall be designed and operated (post-mission disposal manoeuvres) such that, where applicable, the risk of a catastrophic event does not exceed the level of acceptable risk specified by the project and by the launch base safety authority.\n    NOTE Hardware of a space system that is returned from orbit presents a potential threat to the Earth's population due to the risk of debris entering the atmosphere in an uncontrolled manner."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.9a","Requirement","ECSS-Q-ST-40_0440126",1,"Created","Biological contamination (including organic-constituents) resulting from the introduction of extraterrestrial matter shall be avoided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.9b","Requirement","ECSS-Q-ST-40_0440127",1,"Created","The introduction of extraterrestrial matter shall not affect the environmental conditions on Earth."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.9c","Requirement","ECSS-Q-ST-40_0440128",1,"Created","Extraterrestrial matter shall be treated as hazardous substances until proven otherwise."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.9d","Requirement","ECSS-Q-ST-40_0440129",1,"Created","A containment function for hazardous substances of the spacecraft, which prevents release in case of accidents until recovery or arrival at a dedicated containment facility, shall be provided. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.9e","Requirement","ECSS-Q-ST-40_0440130",1,"Created","If containment cannot be verified, the hazardous substances (and any part of the space system that has potentially been exposed) shall not be returned to Earth (unless sterilized in space)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10a","Requirement","ECSS-Q-ST-40_0440131",1,"Created","A mission abort capability shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10b","Requirement","ECSS-Q-ST-40_0440132",1,"Created","Safing and safe heaven functions shall be provided. \n    NOTE These functions can be implemented through measures such as resource conservation, increased shielding (solar flares, meteoroids and radiation), vehicle or systems reconfiguration and trajectory changes. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10c","Requirement","ECSS-Q-ST-40_0440133",1,"Created","Escape and rescue functions shall be provided. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10d","Requirement","ECSS-Q-ST-40_0440134",1,"Created","The capability to reconfigure the system to restore the functional capability of safety critical functions in case of failures or accidents shall be provided. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10e","Requirement","ECSS-Q-ST-40_0440135",1,"Created","The capability to monitor, detect and assess hazards and effects of slow insidious events with hazardous consequences shall be detailed according to project constraints and mission objectives.\n    NOTE Such hazards include fatigue, corrosion, micro-organisms, aging, deterioration, contamination. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.10f","Requirement","ECSS-Q-ST-40_0440136",1,"Created","The space system shall provide an on-board medical facility and the capability for handling a permanently impaired or deceased crewmember."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.3.11a","Requirement","ECSS-Q-ST-40_0440137",1,"Created","System shall be designed such that any required access to system elements during flight or ground operations can be accomplished with an accepted level of risk to personnel. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1a","Requirement","ECSS-Q-ST-40_0440138",1,"Created","The severity of potential consequences of identified hazardous events shall be categorized as shown in Table 6-1."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1b","Requirement","ECSS-Q-ST-40_0440139",1,"Created","An understanding of the criteria defined in Table 6-1 shall be agreed between customer and supplier."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1c","Requirement","ECSS-Q-ST-40_0440140",1,"Created","Detrimental environmental effects, from the point of view of severe hazardous consequences to the global public, shall be included in the consequence severity evaluation.\n    NOTE 1 Table 6-1 is used both in ECSS-Q-ST-30 and ECSS-Q-ST-40.\n    NOTE 2 This impact can be immediate and personal. It also can be on a broader scale not limited to a single person only. The hazardous consequences can be short term or long term.\n    NOTE 3 In space flight, the environment concerned can be outer space, including the Moon and the planets, geostationary orbit (GEO), low Earth orbit (LEO) as well as the Earth’s atmosphere."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1d","Requirement","ECSS-Q-ST-40_0440141",1,"Created","The availability of the following shall not be used as rationale for the reduction of the severity: \n    1. design features which reduce the probability of a hazardous event occurring, but which do not affect its severity; \n    2. warning devices, crew safe haven, or crew escape capabilities. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1e","Requirement","ECSS-Q-ST-40_0440142",1,"Created","For international programmes, a coherent set of consequence severity shall be established for joint operational phases."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1f","Requirement","ECSS-Q-ST-40_0440143",1,"Created","These categories shall not violate the safety policy and principles as defined in clause 4.2.1 for the protection of human life or the principles of categorization in accordance with the definition of consequence severity categories in Table 6-1."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1g","Requirement","ECSS-Q-ST-40_0440144",1,"Created","The expert assessment on determining limits for exposures that do not create a hazard, those that create critical hazards and those that create catastrophic hazards shall be performed by the responsible authority, early in the design process.\n    NOTE Examples of responsible authority are medical boards or radiation protection committees."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.1h","Requirement","ECSS-Q-ST-40_0440145",1,"Created","The detailed safety requirements and measures shall be derived from allowed exposure levels.\n    NOTE For example: maximum allowable concentrations, maximum emission concentrations or radiation doses."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.1a","Requirement","ECSS-Q-ST-40_0440146",1,"Created","Failure tolerance shall be the basic safety requirement used to control hazards."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.1b","Requirement","ECSS-Q-ST-40_0440147",1,"Created","No single system failure or single operator error shall have critical or catastrophic consequences. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.1c","Requirement","ECSS-Q-ST-40_0440148",1,"Created","No combination of two independent system failures or operator errors shall have catastrophic consequences."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.1d","Requirement","ECSS-Q-ST-40_0440149",1,"Created","Safety inhibits shall be independent, verifiable, stable and stay in a safe position even in case of energy failure."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.1e","Requirement","ECSS-Q-ST-40_0440150",1,"Created","Multiple failures, which result from common-cause or common-mode failure mechanisms, shall be analysed as single failures for determining failure tolerance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.2a","Requirement","ECSS-Q-ST-40_0440151",1,"Created","The system design shall:\n    1. include the capability for on-board redundancy management of safety-critical functions, \n    2. provide failure tolerance and redundancy status information to the flight and ground crews, including immediate crew notification in the case of failure detection, redundancy switch-over, or loss of operational redundancy,\n    3. include failure detection, failure isolation and switching of redundant items."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.2b","Requirement","ECSS-Q-ST-40_0440152",1,"Created","The capability shall be provided to the flight crew and mission control to override automatic safing and redundancy switch-over."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.2c","Requirement","ECSS-Q-ST-40_0440153",1,"Created","Alternate or redundant safety-critical functions shall be physically and functionally separated or protected in such a way that any event that causes the loss of one path does not result in the loss of alternative or redundant paths."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.2.3a","Requirement","ECSS-Q-ST-40_0440154",1,"Created","Hardware failures or software errors shall not cause additional failures with hazardous effects or propagate to cause the hazardous operation of interfacing hardware."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.1a","Requirement","ECSS-Q-ST-40_0440155",1,"Created","Technical requirements for areas of design for minimum risk shall be identified and approved by the relevant safety approval authorities\n    NOTE “Design for minimum risk” is a safety requirement used to control hazards by specifying safety-related properties and characteristics of the design."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.2a","Requirement","ECSS-Q-ST-40_0440156",1,"Created","Structural safety factors shall be defined and applied in accordance with ECSS-E-ST-32-10 or higher safety factor where applicable."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.2b","Requirement","ECSS-Q-ST-40_0440157",1,"Created","Safety margins shall be based on worst credible combinations of environmental conditions."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.3a","Requirement","ECSS-Q-ST-40_0440158",1,"Created","For manned systems, where structural failure can have catastrophic or critical consequences, structures, pressure vessels, fasteners and load-bearing paths within mechanisms shall be designed in accordance with ECSS-E-ST-32-01."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.3b","Requirement","ECSS-Q-ST-40_0440159",1,"Created","For unmanned systems, only pressure vessels shall be designed in accordance with ECSS-E-ST-32-01, when required by launch site safety authority."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.4a","Requirement","ECSS-Q-ST-40_0440160",1,"Created","Materials shall be selected and controlled in accordance with ECSS-Q-ST-70."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.4b","Requirement","ECSS-Q-ST-40_0440161",1,"Created","Material selection shall assure that hazards associated with material characteristics are either eliminated or controlled.\n    NOTE Examples of these material properties to be characterized are: toxicity, flammability, resistance to stress corrosion, outgassing, offgassing, resistance to radiation, resistance to thermal cycling, arc tracking, thermal degradation, resistance to cleaning fluid and microbiological growth."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.3.4c","Requirement","ECSS-Q-ST-40_0440162",1,"Created","If requirement 6.4.3.4b. is not feasible, the system design shall include the necessary provisions to control hazardous events associated with material characteristics in accordance with the requirements of this Standard.\n    NOTE An example of provisions to be included by the system design is containment of hazardous substances. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.4a","Requirement","ECSS-Q-ST-40_0440163",1,"Created","When given, the probabilistic safety targets shall be used for\n    1. identifying and ranking major risk contributors,\n    2. making the acceptable risk decision for each identified hazard,\n    3. supporting the disposition making for those cases where nonconformance to the qualitative requirements is identified.\n        NOTE Probabilistic safety targets can be established by the customer for hazardous consequences at system level for each project or programme. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.4.4b","Requirement","ECSS-Q-ST-40_0440164",1,"Created","Probabilistic safety targets shall conform to the requirements given by launch safety authorities and national and international regulations.\n    NOTE Informative Annex E provides criteria for the establishing of probabilistic safety targets."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.1a","Requirement","ECSS-Q-ST-40_0440165",1,"Created","A safety critical function that, if lost or degraded, or through incorrect or inadvertent operation, can result in a catastrophic or critical hazardous consequence, shall be identified as a safety-critical function.\n    NOTE As an example, a series of operational events that can result in a hazard if they occur inadvertently or are operated out of order."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.1b","Requirement","ECSS-Q-ST-40_0440166",1,"Created","Identification shall be done without taking into account hazards controls to be or already implemented."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.2a","Requirement","ECSS-Q-ST-40_0440167",1,"Created","Inadvertent operation of a safety-critical function shall be prevented by\n    1. two independent inhibits, if it induces critical consequences, or\n    2. three independent inhibits, if it induces catastrophic consequences."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.3a","Requirement","ECSS-Q-ST-40_0440168",1,"Created","The system shall provide failure tolerance and redundancy status information of safety-critical functions."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.3b","Requirement","ECSS-Q-ST-40_0440169",1,"Created","The system shall provide the status of at least two inhibits on functions that, if inadvertently operated, can lead to catastrophic consequences, including\n    1. notification in real time in case of failure detection,\n    2. announcement of any loss of operational redundancy, \n    3. notification of redundancy switch-over, or \n    4. changes of inhibit status."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.4a","Requirement","ECSS-Q-ST-40_0440170",1,"Created","The design shall either provide the capability for the safe shutdown of safety-critical functions prior to in-flight maintenance operations or conform to the failure tolerance requirements during maintenance operations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.5a","Requirement","ECSS-Q-ST-40_0440171",1,"Created","Electronic, electrical, electromechanical (EEE) components used to support safety-critical functions in flight standard hardware shall be selected and procured in accordance with the applicable programme requirements of ECSS-Q-ST-60."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.1a","Requirement","ECSS-Q-ST-40_0440172",1,"Created","Safety aspects associated with the software function shall be an integral part of the overall system safety efforts and not be assessed in isolation."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.1b","Requirement","ECSS-Q-ST-40_0440173",1,"Created","A software component shall be considered safety-critical if the loss or degradation of its function, or its incorrect or inadvertent operation, can result in catastrophic or critical consequences. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.2a","Requirement","ECSS-Q-ST-40_0440174",1,"Created","During the project life cycle, safety analysis shall be carried out to:\n    1. identify the criticality of software components in accordance with the severity of the consequences as defined in Table 6-1,\n    2. determine where and under what conditions the system can trigger hazardous events caused by the software,\n    3. define verification methods for hazard controls involving software,\n    4. provide verification evidence of hazard control implementation. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.3a","Requirement","ECSS-Q-ST-40_0440175",1,"Created","The criticality of a software component shall be evaluated taking into account the overall system design which can provide for, e.g. back-up or emergency procedures, hardware inhibits and certain time to effect."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.4a","Requirement","ECSS-Q-ST-40_0440176",1,"Created","A safety-critical software component shall be designed, implemented, verified and operated according to the engineering and product assurance requirements defined in ECSS-E-ST-40 and ECSS-Q-ST-80."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.4b","Requirement","ECSS-Q-ST-40_0440177",1,"Created","Safety-critical software shall be analysed for the identification and verification of adequate software controls and inhibits and validated accordingly. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.5.6.4c","Requirement","ECSS-Q-ST-40_0440178",1,"Created","The level of required software product assurance effort shall be determined in accordance with the criticality of the software component."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1a","Requirement","ECSS-Q-ST-40_0440179",1,"Created","Safety involvement in the operational phase shall be planned."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1b","Requirement","ECSS-Q-ST-40_0440180",1,"Created","Responsibilities, rules and contingency procedures shall be established prior to operation for hazardous “limit” conditions that can occur during ground and in-flight operations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1c","Requirement","ECSS-Q-ST-40_0440181",1,"Created","Operating ranges and performance limits for safe operation shall be established and specified."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1d","Requirement","ECSS-Q-ST-40_0440182",1,"Created","The design shall not require continuous active control by personnel in order to stay within the established operating ranges and performance limits."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1e","Requirement","ECSS-Q-ST-40_0440183",1,"Created","Man-machine interfaces shall be designed and the personnel tasks shall be scoped to reduce the potential for hazardous events resulting from human error to an accepted level."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.1f","Requirement","ECSS-Q-ST-40_0440184",1,"Created","Limits for crew exposure to natural and system-induced environments shall be established and maintained by design features or operational constraints that cover nominal, contingency, and emergency operational modes, in order to preclude crew injury or inability to perform safety-critical functions."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.1a","Requirement","ECSS-Q-ST-40_0440185",1,"Created","Hazards to the humans, public and private property and the environment, resulting from launcher system operation or malfunction shall be precluded by compliance with the regulations of the launch safety authority."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.2a","Requirement","ECSS-Q-ST-40_0440186",1,"Created","Normal or abort operations shall not result in contamination of the Earth’s environment that endangers human health, crops or natural resources or that exceed limits set by national or international regulations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.3a","Requirement","ECSS-Q-ST-40_0440187",1,"Created","Flight rules shall be prepared for each mission that outline pre-planned decisions in case of off-nominal situations and consistent with safety requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.4a","Requirement","ECSS-Q-ST-40_0440188",1,"Created","Hazardous commanding control shall ensure that all hazardous commands are identified."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.4b","Requirement","ECSS-Q-ST-40_0440189",1,"Created","Hazardous commanding control shall ensure that failure modes, associated with flight and ground operation - including hardware, software and procedures - used in commanding from control centres or other ground equipment, are included in the safety assessment."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.4c","Requirement","ECSS-Q-ST-40_0440190",1,"Created","Hazardous commanding control shall ensure that the system design provides protection to avoid the erroneous acceptance of commands that can result in catastrophic or critical consequences."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.4d","Requirement","ECSS-Q-ST-40_0440191",1,"Created",".Hazardous commanding control shall ensure that commands, which can result in catastrophic or critical hazardous consequences, are not performed until they are authorized and verified."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.5a","Requirement","ECSS-Q-ST-40_0440192",1,"Created","Mission operation change control shall ensure that all changes, which are desired or become necessary during mission, are reviewed for safety impact."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.5b","Requirement","ECSS-Q-ST-40_0440193",1,"Created","Mission operation change control shall ensure that the responsible safety approval authority approves all operational change requests with safety impact."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.6a","Requirement","ECSS-Q-ST-40_0440194",1,"Created","Safety status parameters shall be identified."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.6b","Requirement","ECSS-Q-ST-40_0440195",1,"Created","Safety status parameters shall be monitored."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.6c","Requirement","ECSS-Q-ST-40_0440196",1,"Created","Deviation from specified limits shall be managed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.7a","Requirement","ECSS-Q-ST-40_0440197",1,"Created","In the case of a deviation from the planned launch trajectory during ascent, launch vehicle stages shall be remotely destroyed or have their propulsion engines shut off to prevent stages or debris from falling outside pre-defined safe areas."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.7b","Requirement","ECSS-Q-ST-40_0440198",1,"Created","The launch vehicle and spent stage trajectories shall be monitored to determine vehicle, stage or debris impact points."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.2.7c","Requirement","ECSS-Q-ST-40_0440199",1,"Created","Residual propellants contained in spent or aborted suborbital stages shall be safely dispersed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.1a","Requirement","ECSS-Q-ST-40_0440200",1,"Created","Safety requirements of the clause shall be applied during the following ground operations:\n    1. development, qualification or acceptance testing;\n    2. assembly, integration or test operations;\n    3. launch site operations;\n    4. servicing or turn-around operations; and\n    5. transportation or handling operations,"]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.2a","Requirement","ECSS-Q-ST-40_0440201",1,"Created","The supplier shall establish procedures to perform safety readiness reviews and inspections prior to the performance of any applicable operation."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.3a","Requirement","ECSS-Q-ST-40_0440202",1,"Created","To verify conformance to safety requirements, readiness reviews and inspections shall include safety review and assessment of facilities, equipment (incl. GSE), test articles, operating, test and contingency procedures, access controls, and personnel capabilities to comply with the safety requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.4a","Requirement","ECSS-Q-ST-40_0440203",1,"Created","Hazardous operations shall be monitored for conforming to safety requirements and procedures, and for the possible development of unforeseen hazardous situations. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.4b","Requirement","ECSS-Q-ST-40_0440204",1,"Created","Where necessary, contingency and emergency plans or procedures shall be established and verified prior to the commencement of the operation. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.4c","Requirement","ECSS-Q-ST-40_0440205",1,"Created","The safety manager or safety relevant authority shall have the authority to stop any operation that does not conform to safety requirements. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.5a","Requirement","ECSS-Q-ST-40_0440206",1,"Created","Launch, landing, turn-around and mission operations shall be subject to hazard analysis."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.5b","Requirement","ECSS-Q-ST-40_0440207",1,"Created","For ground operations, the analysis shall address the:\n    1. potential hazardous consequences of human error and procedural deficiencies;\n    2. adequacy and maintenance of operational margins;\n    3. potential for human exposure to hazards and hazardous effects;\n    4. requirements for operator and flight crew training;\n    5. adequacy of information and data provided by the flight hardware, ground support equipment (GSE), or test equipment, as appropriate, to support the performance of the operations in accordance with all applicable safety requirements (including all safety regulations)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.6a","Requirement","ECSS-Q-ST-40_0440208",1,"Created","All Ground support equipment (GSE) shall be subjected to hazard analysis."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.6b","Requirement","ECSS-Q-ST-40_0440209",1,"Created","All GSE shall conform to the ‘Essential Health & Safety Requirements’ of all applicable EU ‘New Approach directives’. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.6c","Requirement","ECSS-Q-ST-40_0440210",1,"Created","Conformance to 6.6.3.6b. shall be shown by the addition of the ‘CE’ mark to the product and the issuing of a ‘Declaration of Conformity’."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","6.6.3.6d","Requirement","ECSS-Q-ST-40_0440211",1,"Created","Conformance to any other product related directives shall be demonstrated.\n    NOTE Further guidance is given in Annex G."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.2a","Requirement","ECSS-Q-ST-40_0440212",1,"Created","Safety analysis shall be performed in a systematic manner as a basis for all applicable phases and to ensure that hazards are identified, eliminated or minimized and controlled and safety risks are assessed and reduced."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.2b","Requirement","ECSS-Q-ST-40_0440213",1,"Created","Safety analyses shall be initiated early in the design process and provide concurrent support to project engineering in the selection of the least hazardous design and operational options that are compatible with the project mission and programme constraints and conform to the requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.2c","Requirement","ECSS-Q-ST-40_0440214",1,"Created","The results of safety analyses shall also be used to support project management in the assessment of the overall risks, verification of risk reduction, ranking of risk sources, support to project resource allocation, monitoring of risk trends, and residual risk acceptance. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.2d","Requirement","ECSS-Q-ST-40_0440215",1,"Created","Analysis shall always be made with reference to a defined configuration baseline as defined by ECSS-M-ST-40."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.1a","Requirement","ECSS-Q-ST-40_0440216",1,"Created","The supplier shall respond to and comply with the applicable safety requirements for the project."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.2a","Requirement","ECSS-Q-ST-40_0440217",1,"Created","The supplier shall identify additional safety requirements, where applicable, through the use of lessons learned from previous projects and the safety analyses performed during the project."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.3a","Requirement","ECSS-Q-ST-40_0440218",1,"Created","The supplier shall define the safety requirements for the various functions of the system."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.4a","Requirement","ECSS-Q-ST-40_0440219",1,"Created","The supplier shall define the safety requirements associated with the various subsystems and lower levels."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.5a","Requirement","ECSS-Q-ST-40_0440220",1,"Created","The supplier shall justify to the customer the proposed allocation of safety requirements at the latest at the end of the detailed definition phase."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.3.6a","Requirement","ECSS-Q-ST-40_0440221",1,"Created","The supplier shall ensure that the function and subsystem safety requirements are included in the relevant functional and subsystem specification."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.4a","Requirement","ECSS-Q-ST-40_0440222",1,"Created","Safety analysis shall be refined and updated in an iterative manner as the design process proceeds, to ensure that hazards and hazardous events are assessed, and that the relevant detailed design and operational requirements, hazard controls, and verification activities are defined and implemented.\n    NOTE Refer to 5.7 for detailed safety programme tasks in the different project phases"]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.1a","Requirement","ECSS-Q-ST-40_0440223",1,"Created","The safety analysis report shall be established in conformance with the DRD in Annex D in order to gather results of safety analyses, which use deterministic and probabilistic methods which are described in the clauses 7.5.2 to 7.5.4."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2a","Requirement","ECSS-Q-ST-40_0440224",1,"Created","Hazard analysis shall be performed in a systematic manner, beginning in the concept phase and continuing through the operational phase, including end-of-life and disposal."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2b","Requirement","ECSS-Q-ST-40_0440225",1,"Created","Hazard analysis shall support the hazard reduction process."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2c","Requirement","ECSS-Q-ST-40_0440226",1,"Created","Hazard analysis shall identify and evaluate:\n    1. hazards associated with system design, its operation (both on ground and in flight) and the operation environment; \n    2. the hazardous effects resulting from the physical and functional propagation of initiator events;\n    3. the hazardous events resulting from the failure of system functions and functional components;\n    4. time critical situations. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2d","Requirement","ECSS-Q-ST-40_0440227",1,"Created","The following potential initiator events shall be considered:\n    1. hardware failure (random or time dependent);\n    2. latent software error;\n    3. operator error;\n    4. design inadequacies, including:\n        (a) inadequate margins;\n        (b) unintended operating modes caused by sneak-circuits;\n        (c) material inadequacies and incompatibilities;\n        (d) hardware-software interactions;\n    5. natural and induced environmental effects;\n    6. procedural deficiencies."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2e","Requirement","ECSS-Q-ST-40_0440228",1,"Created","Hazard analysis includes a systematic analysis of the “system” operations and operating procedures that shall be performed in the detailed design and operational stages of a project. \n    NOTE This analysis evaluates the capability of the system to be operated safely, to determine the safest operating modes, and to evaluate the acceptability of the operating procedures."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.2f","Requirement","ECSS-Q-ST-40_0440229",1,"Created","The systematic analysis of system operation and operating procedures shall be repeated as the design and operational detail evolves, including the system’s operational modes and man-machine interfaces."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.3a","Requirement","ECSS-Q-ST-40_0440230",1,"Created","Safety risk assessment shall \n    1. comprise the identification, classification and ranking of safety risks and their contributors,\n    2. be based on deterministic hazard analysis by combining the consequence severity and the likelihood of occurrence of the consequence,\n    3. be used to facilitate effective and efficient safety risk reduction and control, \n    4. support project risk management as defined in ECSS-M-ST-80, \n    5. assess compliance with probabilistic safety targets.\n        NOTE 1 The estimation of event likelihoods is based on the use of different sources of data i.e.: \n            · previous experience on the particular system (i.e. measured or observed directly relevant test or experience data), \n            · data from other systems or projects (i.e. extrapolation from generic data, similarity data, or physical models), and \n            · expert judgment (i.e. direct estimation of likelihoods by domain specialists).\n        NOTE 2 The determination of likelihood is not a mean to downgrade the severity of function (see 6.4.1d)                                                     "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.3b","Requirement","ECSS-Q-ST-40_0440231",1,"Created","Safety risk assessment shall be started early in the design process and performed in progressive steps during the implementation of the safety programme. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.1a","Requirement","ECSS-Q-ST-40_0440232",1,"Created","Following supporting assessment and analysis methods shall be used as necessary (tailored by project) to support hazards analysis and safety risk assessment.\n    NOTE 1 Example of tailoring by project is when the supporting assessment and analysis methods are not applicable in e.g. unmanned missions.\n    NOTE 2 Assessments and analyses from ECSS-Q-ST-30 can be used to support safety assessment."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.1b","Requirement","ECSS-Q-ST-40_0440233",1,"Created","Supporting analyses shall be agreed with all relevant parties."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.2a","Requirement","ECSS-Q-ST-40_0440234",1,"Created","Warning time analysis shall be performed during the concept definition phase and the design and development phase in order to evaluate time-critical situations identified in the hazard analysis and to support the implementation of hazardous-situation detection and warning devices or contingency procedures. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.2b","Requirement","ECSS-Q-ST-40_0440235",1,"Created","The analysis shall determine the\n    1. time interval during which the event is detected and the response action taken; \n    2. detection capability of the proposed design with respect to detection sensitivity and detection time; \n    3. resultant time available for response;\n    4. adequacy of the proposed design or contingency procedures, including emergency evacuation, rescue, system reconfiguration, redundancy switching, and maintenance."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.2c","Requirement","ECSS-Q-ST-40_0440236",1,"Created","The detection times shall be determined from the\n    1. occurrence of the initiating event to the time when a hazardous consequence occurs (propagation time); \n    2. occurrence of the initiating event to the time of earliest detection or annunciation; and \n    3. time taken for corrective action to be implemented."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.3a","Requirement","ECSS-Q-ST-40_0440237",1,"Created","Caution and warning analysis shall be performed during the concept definition phase and the design and development phase of human space flight programmes in order to identify\n    1. emergency, warning, and caution parameters;\n    2. the required safing functions and capabilities;\n    3. limit sensing requirements;\n    4. the applicability of the individual “caution and warning” functions to the different mission phases. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.3b","Requirement","ECSS-Q-ST-40_0440238",1,"Created","The caution and warning analysis shall utilize the results of the warning time and hazards analyses as appropriate."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.1a","Requirement","ECSS-Q-ST-40_0440239",1,"Created","Multiple failures, which result from common-cause or common-mode failure mechanisms, shall be analysed as single failures for determining failure tolerance. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.2a","Requirement","ECSS-Q-ST-40_0440240",1,"Created","The supplier shall identify the requirement for and the scope of dedicated common-cause and common-mode analyses by means of the review of the results of the other safety analyses, such as FTA and hazard analysis, and of the characteristic of the system and of its environment."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.3a","Requirement","ECSS-Q-ST-40_0440241",1,"Created","The supplier shall identify potential common-cause failures by assessment of the effects of common-causes. \n    NOTE For example: radiation, thermal environment and fires."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.3b","Requirement","ECSS-Q-ST-40_0440242",1,"Created","The common-cause failure analysis shall be performed in coordination with the FTA and the hazard analysis.\n    NOTE The analysis of common-cause failures can require that use be made of the result of dedicated engineering analyses, e.g. thermal analyses, meteorite or debris impact analysis."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.4a","Requirement","ECSS-Q-ST-40_0440243",1,"Created","Common-mode failures shall be analysed by means of the use of check-lists (to be established by the supplier) that list potential common-modes for system components during the manufacturing, integration, test, operation and maintenance phases. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.4b","Requirement","ECSS-Q-ST-40_0440244",1,"Created","The common-mode analysis shall be coordinated with the FMEA/FMECA."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.4.5a","Requirement","ECSS-Q-ST-40_0440245",1,"Created","Results of common-cause and common-mode analysis shall be integrated with the results of the system level safety analyses (fault tree analysis, hazard analysis)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.5a","Requirement","ECSS-Q-ST-40_0440246",1,"Created","The fault tree analysis shall be used to establish the systematic link between the system-level hazard and the contributing hazardous events and subsystem, equipment or piece part failure."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.5b","Requirement","ECSS-Q-ST-40_0440247",1,"Created","A fault tree analysis, or its equivalent, shall be performed to verify the failure tolerance requirements.\n    NOTE Refer to ECSS-Q-ST-40-12 “Fault tree analysis - Adoption notice ECSS/IEC 61025” for further instructions on fault tree analyses."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.6a","Requirement","ECSS-Q-ST-40_0440248",1,"Created","Whenever safety analyses identify operator errors as a cause of catastrophic or critical hazards, a dedicated analysis shall be carried out."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.6b","Requirement","ECSS-Q-ST-40_0440249",1,"Created","The human error analysis shall be used to support the safety analysis for the identification of human operator error modes and their effects and for the definition of adequate countermeasures to prevent or control human operator errors."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.6c","Requirement","ECSS-Q-ST-40_0440250",1,"Created","The human error analysis shall be developed from the early phases of the project onwards in order to define recommendations for the hardware and software design, procedure development and training preparation programme."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.7a","Requirement","ECSS-Q-ST-40_0440251",1,"Created","The results of failure modes and effects analysis (FMEA) or failure modes, effects and criticality analysis (FMECA) shall be used to support the hazard analysis in the evaluation of the effects of failures. FMEA/FMECA and hazard analysis are complementary analyses.\n    NOTE Refer to ECSS-Q-ST-30-02 for further instructions on FMEA/FMECA."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.8a","Requirement","ECSS-Q-ST-40_0440252",1,"Created","Zonal analysis shall be performed where redundancy is used to reduce the probability of losing a function or of inadvertently actuating a safety-critical function."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","7.5.4.8b","Requirement","ECSS-Q-ST-40_0440253",1,"Created","The objectives of the zonal analysis shall ensure that equipment installation meets the adequate safety requirements regarding:\n    1. basic installation rules and space practices;\n    2. interaction between subsystems;\n    3. implication of operator errors;\n    4. effects of external events.\n        NOTE Zonal analysis is the systematic inspection of the topology of a system, the evaluation of potential component-to-component interactions with and without failure, and the assessment of the severity of potential hazards inherent in the system installation."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.1a","Requirement","ECSS-Q-ST-40_0440254",1,"Created","A system shall be in place that tracks all hazards and related risks, to relate all verifications of the corresponding hazard uniquely to unambiguous causes and controls."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.1b","Requirement","ECSS-Q-ST-40_0440255",1,"Created","For common techniques for verification of design features used to control hazards, the requirements of ECSS-E-ST-10 shall apply. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.1c","Requirement","ECSS-Q-ST-40_0440256",1,"Created","To successfully complete the safety process, positive feedback shall be provided on completion results for all verification items associated with a given hazard."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.1a","Requirement","ECSS-Q-ST-40_0440257",1,"Created","The supplier shall establish a hazard reporting system for tracking the status of all identified hazards."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.1b","Requirement","ECSS-Q-ST-40_0440258",1,"Created","The system shall be applied for all hazards with potentially catastrophic or critical consequences."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.1c","Requirement","ECSS-Q-ST-40_0440259",1,"Created","The supplier shall report, and provide evidence, that\n    1. controls are defined and agreed;\n    2. verification methods are defined and agreed; \n    3. verification is completed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.1d","Requirement","ECSS-Q-ST-40_0440260",1,"Created","If verification cannot be completed, the supplier shall establish a Safety Verification Tracking Log (SVTL) (refer to clause 8.5.1a.)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.2a","Requirement","ECSS-Q-ST-40_0440261",1,"Created","Status of hazard control and risk reduction activities shall be reviewed at safety progress meetings and project safety reviews for compliance with decisions taken and achievement of intended results."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.2.3a","Requirement","ECSS-Q-ST-40_0440262",1,"Created","All hazard documentation shall be formally issued for each safety review and major project review, as specified in clause 5.11). "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.1a","Requirement","ECSS-Q-ST-40_0440263",1,"Created","Verification engineering shall select the verification methods consistent:\n    1. with the verification requirements documented in the hazard report,\n    2. with the launch base safety rules."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.1b","Requirement","ECSS-Q-ST-40_0440264",1,"Created","Verification planning shall commence in an integrated manner upon selection of the control method."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.2a","Requirement","ECSS-Q-ST-40_0440265",1,"Created","Safety verification methods shall include alternatively or in combination review of design, analysis, inspection and test."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.2b","Requirement","ECSS-Q-ST-40_0440266",1,"Created","For all safety verifications traceability shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.3a","Requirement","ECSS-Q-ST-40_0440267",1,"Created","All relevant technical safety and engineering analyses performed or updated with analysis in respect to the as-built configuration shall be used for verification. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.3b","Requirement","ECSS-Q-ST-40_0440268",1,"Created","When similarity analysis is provided, for tracking purposes it shall contain a copy of (or a unique reference to) the referenced previous verification, verification procedure and requirement valid at the time of the first verification."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.1a","Requirement","ECSS-Q-ST-40_0440269",1,"Created","Inspections which are considered as necessary in order to meet safety requirements of the system shall be identified and included in user manuals and procedures."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2a","Requirement","ECSS-Q-ST-40_0440270",1,"Created","All preflight safety inspections shall be assessed for inclusion in the MIP list. \n    NOTE If preflight safety inspections are included on the MIP list, closeout is feasible by MIP reporting or individual reporting as appropriate."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2b","Requirement","ECSS-Q-ST-40_0440271",1,"Created","Launch preparation inspections shall be entered into the launch base procedure. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2c","Requirement","ECSS-Q-ST-40_0440272",1,"Created","The closeout shall be given by the approved launch authority procedure."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2d","Requirement","ECSS-Q-ST-40_0440273",1,"Created","Late access procedures shall be the subject of training and be performed by qualified personnel. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2e","Requirement","ECSS-Q-ST-40_0440274",1,"Created","Training for flight crew and mission operation teams shall be performed, including specific safety briefing, training and mission simulation. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.2f","Requirement","ECSS-Q-ST-40_0440275",1,"Created","Close-out shall be by safety-approved procedure, documented training session and simulations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.4.3a","Requirement","ECSS-Q-ST-40_0440276",1,"Created","Inflight inspections shall be entered into flight procedures and operation manuals."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.5a","Requirement","ECSS-Q-ST-40_0440277",1,"Created","The supplier shall select, and propose to the safety approval authority, the safety verification methods to be used in conformance to the applicable safety requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.3.5b","Requirement","ECSS-Q-ST-40_0440278",1,"Created","The results of safety verification shall be submitted for approval to the relevant safety approval authority."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.1a","Requirement","ECSS-Q-ST-40_0440279",1,"Created","Safety-critical functions shall be verified by testing which include application of the operating procedures, the “man-in-the-loop”, and the verification of the effectiveness of applicable failure tolerance requirements."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.1b","Requirement","ECSS-Q-ST-40_0440280",1,"Created","The tests shall include the demonstration of nominal, contingency and emergency operational modes."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.2a","Requirement","ECSS-Q-ST-40_0440281",1,"Created","The safety-critical characteristics of all safety-critical functions shall be qualified by test."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.2b","Requirement","ECSS-Q-ST-40_0440282",1,"Created","Safety-critical function qualification testing shall include the determination of performance margins considering worst case combinations of induced and natural environments and operating conditions. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.2c","Requirement","ECSS-Q-ST-40_0440283",1,"Created","Qualification “by similarity” shall not be applied except after customer approval on a case-by-case basis. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.3a","Requirement","ECSS-Q-ST-40_0440284",1,"Created","Induced failure tests shall be performed when required by safety analysis for evaluating failure effects, and for demonstrating failure tolerance conformance in safety-critical functions. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.4a","Requirement","ECSS-Q-ST-40_0440285",1,"Created","Verification of unique safety required design or operational characteristics shall form part of the development, qualification or acceptance testing programmes as appropriate. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.5a","Requirement","ECSS-Q-ST-40_0440286",1,"Created","Where full-scale testing is not performed, equivalent safety verification method based on technically representative hardware or models shall be justified, approved and performed. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.4.5b","Requirement","ECSS-Q-ST-40_0440287",1,"Created","For the verification of hazard controls in catastrophic hazards where non-flight equipment replaces part of the flight equipment to test a flight function the verification shall be performed independently by a third party which was not involved in the design and qualification of the flight model (FM)."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.5.1a","Requirement","ECSS-Q-ST-40_0440288",1,"Created","A safety verification tracking log (SVTL) shall be established, in conformance with the DRD in Annex C, to collect all the open verification items of the different hazard reports from the safety analysis."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.5.1b","Requirement","ECSS-Q-ST-40_0440289",1,"Created","In time for acceptance by the customer, and in preparation of transfer to the next stage of system integration, the safety manager shall verify that: \n    1. hazard close-outs performed so far by the responsible engineer are still valid; \n    2. the verifications reflect the as-built or as-modified status of the hardware;\n    3. all open verifications at this time are acceptable for transfer to the next stage of system integration; \n    4. all open verifications are entered into the verification tracking log (SVTL);\n    5. the verification tracking log is maintained to reflect the current status."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.5.1c","Requirement","ECSS-Q-ST-40_0440290",1,"Created","If the safety verification constrains any ground operations, the safety manager shall give notification to the safety review panel."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.5.2a","Requirement","ECSS-Q-ST-40_0440291",1,"Created","The safety manager shall assure that each hazard considered for closure has the approval by the safety approval authority, verifying that\n    1. hazards not eliminated are controlled in accordance with the applicable requirements and associated verification activities are successfully completed, or, when applicable,\n    2. deviations from, or waivers of requirements, are granted by the safety approval authority."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","8.6a","Requirement","ECSS-Q-ST-40_0440292",1,"Created","All ground equipment that falls into the scope of an applicable ‘New Approach directive’ shall be ‘CE’ marked and supplied with a supporting ‘Declaration of Conformity’ and User Manual detailing all safety warnings.\"\n    NOTE Additional information is provided in Informative Annex G. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.1<1>a","Requirement","ECSS-Q-ST-40_0440293",1,"Created","The safety programme plan shall include a description of the project safety organization, responsibilities, and its working relationship and interfaces with product assurance disciplines (reliability, maintainability, software product assurance, parts, materials and processes and quality assurance according to ECSS-Q-ST-10, -20, -30, -60, -70 and -80), with configuration management according to ECSS-M-ST-40, system engineering according to ECSS-E-ST-10, design and other project functions and departments of organizations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.1<1>b","Requirement","ECSS-Q-ST-40_0440294",1,"Created","The safety programme plan shall describe how the provisions of ECSS-Q-ST-40 are implemented:\n    1. Safety programme and organization;\n    2. Safety engineering;\n    3. Safety analysis requirements and techniques;\n    4. Safety verification;\n    5. Operational safety."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.1<2>a","Requirement","ECSS-Q-ST-40_0440295",1,"Created","The plan shall show how the project safety organization implements concurrent safety and project engineering activities in continuous support of the project design and development process."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.1<3>a","Requirement","ECSS-Q-ST-40_0440296",1,"Created","The plan shall describe how safety-related activities and requirements are defined for and controlled at suppliers’ and lower tier suppliers’ premises."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.1<4>a","Requirement","ECSS-Q-ST-40_0440297",1,"Created","The plan shall make provisions for assuring conformance to safety requirements and regulations that are applicable to any other facilities and service that are utilized during the course of the project. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","B.2.2a","Permission","ECSS-Q-ST-40_0440321",1,"Created","The safety programme plan may be incorporated within the Product Assurance Plan when agreed between the relevant parties."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<1>a","Requirement","ECSS-Q-ST-40_0440299",1,"Created","The SVTL shall identify the following general information:\n    1. name of the project for which it has been established;\n    2. project documentation identification number;\n    3. applicability for flight or ground safety verifications;\n    4. indication of the specific page number followed by the total number of pages;\n    5. name of the equipment, payload or experiment for which the SVTL has been established;\n    6. mission or flight to which the equipment, payload or experiment has been manifested;\n    7. dates of issue and update."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<2>a","Requirement","ECSS-Q-ST-40_0440300",1,"Created","For each verification item to be tracked a unique identifier shall be used."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<2>b","Requirement","ECSS-Q-ST-40_0440301",1,"Created","The SVTL shall use the designations assigned by the safety manager."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<3>a","Requirement","ECSS-Q-ST-40_0440302",1,"Created","The identification number of the hazard report containing the verification item shall be indicated."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<4>a","Requirement","ECSS-Q-ST-40_0440303",1,"Created","The verification method or the verification means shall be transferred from the hazard report including the procedures by number and title."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<5>a","Requirement","ECSS-Q-ST-40_0440304",1,"Created","The input of “yes” or “no” shall indicate whether this safety verification constrains any ground operations."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<5>b","Requirement","ECSS-Q-ST-40_0440305",1,"Created","If “yes” for flight tracking log: an attachment shall be provided that identifies which ground operation is constrained."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<5>c","Requirement","ECSS-Q-ST-40_0440306",1,"Created","If “yes” for ground tracking log: the ground operation constrained by this verification shall be indicated specifically in the user manual and included as a step in a procedure."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<6>a","Requirement","ECSS-Q-ST-40_0440307",1,"Created","The input of \"yes\" or \"no\" shall indicate whether the verification has to be performed independently (in accordance with 8.4.5b). "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<7>a","Requirement","ECSS-Q-ST-40_0440308",1,"Created","The planned date for the completion of the verification shall be indicated."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<8>a","Requirement","ECSS-Q-ST-40_0440309",1,"Created","The SVTL log shall indicate the title and serial number of the tests, review of designs, inspections and analyses by which this verification is formally closed."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","C.2.1<8>b","Permission","ECSS-Q-ST-40_0440322",1,"Created","Any appropriate information or remarks may be added."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<1>a","Requirement","ECSS-Q-ST-40_0440311",1,"Created","Title - The title of the safety analysis report shall identify the applicable project. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<1>b","Requirement","ECSS-Q-ST-40_0440312",1,"Created","Title page - A title page shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<1>c","Requirement","ECSS-Q-ST-40_0440313",1,"Created","Contents - A contents list shall be provided. "]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<1>d","Requirement","ECSS-Q-ST-40_0440314",1,"Created","Foreword - A foreword shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<1>e","Requirement","ECSS-Q-ST-40_0440315",1,"Created","Introduction - An introduction shall be provided."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<2>a","Requirement","ECSS-Q-ST-40_0440316",1,"Created","The safety analysis report shall identify the following general information:\n    1. the project documentation identification number, the title of the safety analysis report, date of release and release authority;\n    2. the project phase;\n    3. identification of which organizational entity prepared the document;\n    4. information regarding the approval of the document;\n    5. a statement of effectivity identifying which other documents have been cancelled and replaced in whole or in part."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<2>b","Requirement","ECSS-Q-ST-40_0440317",1,"Created","The safety analysis report shall contain the following analysis specific information:\n    1. objective of safety analysis;\n    2. applicable requirements relevant to the safety analysis;\n    3. description of system design & operation from a safety point of view;\n    4. description of safety analysis process and methods;\n    5. detailed results of safety analysis documented in form of a set of hazard reports (see D.2.1<2>c.);\n    6. list of safety critical functions;\n    7. safety critical item list;\n    8. safety input to risk management;\n    9. support analyses used (e.g. FTA, FMEA/FMECA);\n    10. overall conclusions from safety assessment."]
["ECSS-Q-ST-40C","ECSS - Superseded v1.0","D.2.1<2>c","Requirement","ECSS-Q-ST-40_0440318",1,"Created","Each hazard report shall contain as a minimum the following data:\n    1. title;\n    2. types of hazards and description of their manifestation in the system design and operational configuration and environment;\n    3. identified hazard scenario with description of causes (associated with the hazard manifestation), hazardous events (physical and functional propagation) and consequences; \n    4. consequence severity category;\n    5. propagation time from cause to consequence;\n    6. likelihood of hazard scenario and magnitude of safety risk (optional);\n    7. applicable safety requirements;\n    8. hazard reduction measures (implementation of safety requirements, hazard elimination or minimization and control);\n    9. verification measures;\n    10. safety risk trend after hazard reduction (optional); \n    11. status (safety verification actions open or closed, non-conformances and waivers);\n    12. approval;\n    13. acceptance of safety risk (optional).\n        NOTE Example of formats that can be used for “Hazard and safety risk register”, and “Ranked hazard and safety risk log” are given in the annexes of ECSS-Q-ST-40-02. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.2a","Requirement","ECSS-Q-ST-70-26_0130001",1,"Created","The supplier shall provide cleaning services for production facilities of high reliability crimping."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.2b","Requirement","ECSS-Q-ST-70-26_0130002",1,"Created","The areas, in which crimping is carried out, shall be maintained in an orderly fashion."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.2c","Requirement","ECSS-Q-ST-70-26_0130003",1,"Created","Loose material that can cause contamination of the crimped connection shall be removed. \n    NOTE For example: Dirt, dust, oils and clipped wires."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.2d","Requirement","ECSS-Q-ST-70-26_0130004",1,"Created","Furniture shall be kept to a minimum in the work areas and be arranged to allow easy and thorough cleaning of the floor."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.2e","Requirement","ECSS-Q-ST-70-26_0130005",1,"Created","Working surfaces shall be covered with an easily cleaned hard top or have a replaceable surface of clean, non-corrosive silicone-free paper."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.3a","Requirement","ECSS-Q-ST-70-26_0130006",1,"Created","The crimping area shall have a controlled environment, which limits entry of contamination. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.3b","Requirement","ECSS-Q-ST-70-26_0130007",1,"Created","The area shall be continuously controlled as follows:\n    1. room temperature:(22 ± 3) °C;\n    2. relative humidity: (55 ± 10) %."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.3c","Requirement","ECSS-Q-ST-70-26_0130008",1,"Created","The workstations shall not be exposed to draughts."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.3d","Requirement","ECSS-Q-ST-70-26_0130009",1,"Created","Fresh air shall be supplied to the room through a filtering system with positive pressure difference with regard to adjacent rooms."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.3e","Requirement","ECSS-Q-ST-70-26_0130010",1,"Created","The exhaust air shall be suitably restricted."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.4a","Requirement","ECSS-Q-ST-70-26_0130011",1,"Created","The supplier shall ensure adequate illumination conditions of the crimp workstations."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.4b","Requirement","ECSS-Q-ST-70-26_0130012",1,"Created","The light intensity shall be 1 080 lux on the work surface. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.1.4c","Requirement","ECSS-Q-ST-70-26_0130013",1,"Created","90 % of the work area shall be shadowless and without severe reflections."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-70-26_0130014",1,"Created","The supplier shall provide the tooling necessary for continued high quality crimping."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1b","Requirement","ECSS-Q-ST-70-26_0130015",1,"Created","Tools used shall employ an integral mechanism, which controls the crimping operation in conformance to MIL-DTL-22520G.\n    NOTE The mechanism ensures that, once the operation is started, the tool cannot be opened until the crimping cycle is complete."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1c","Requirement","ECSS-Q-ST-70-26_0130016",1,"Created","Tools shall be marked to show the size and type of termination for which it is calibrated."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1d","Requirement","ECSS-Q-ST-70-26_0130017",1,"Created","Tool calibration shall be verified once each shift in conformance with the clause 5.5.5 requirements."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1e","Requirement","ECSS-Q-ST-70-26_0130018",1,"Created","Proper operation of the integral ratcheting mechanism or the positive stops on pneumatic tools shall be verified as defined in clause 5.5.6."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1f","Requirement","ECSS-Q-ST-70-26_0130019",1,"Created","Before starting a crimping process on a new terminal size and wire type, tools used for crimping of the previous wire type shall be returned to the tool facility."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1g","Requirement","ECSS-Q-ST-70-26_0130020",1,"Created","If the tool settings seals are broken, the tool shall be returned immediately for recalibration."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.1h","Requirement","ECSS-Q-ST-70-26_0130021",1,"Created","Tools used in the crimping operation shall be clean; excess lubricants shall be removed before crimping starts."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.2a","Requirement","ECSS-Q-ST-70-26_0130022",1,"Created","The supplier shall provide the tooling necessary to avoid damage to the conductor."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.2b","Requirement","ECSS-Q-ST-70-26_0130023",1,"Created","The selection of thermal or precision cutting devices, manual or automatic power-driven, shall provide protection of the conductor strands. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.2c","Requirement","ECSS-Q-ST-70-26_0130024",1,"Created","Wire stretching by use of mechanical strippers shall be avoided."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.2d","Requirement","ECSS-Q-ST-70-26_0130025",1,"Created","The conductor shall not be twisted, ringed, nicked, cut or scored by stripping operation."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.2e","Requirement","ECSS-Q-ST-70-26_0130026",1,"Created","Both thermal and mechanical stripping tools shall be calibrated periodically on sample evaluation during a production run."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.3a","Requirement","ECSS-Q-ST-70-26_0130027",1,"Created","The supplier shall provide the tooling necessary for precision wire trimming and cutting."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.3b","Requirement","ECSS-Q-ST-70-26_0130028",1,"Created","The cutter used for trimming conductor wire shall shear sharply and consistently produce a clean, flat, smooth-cut surface along the entire cutting edge. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.3c","Requirement","ECSS-Q-ST-70-26_0130029",1,"Created","Twisting action during cutting operation shall be avoided. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.3d","Requirement","ECSS-Q-ST-70-26_0130030",1,"Created","Smooth, long-nose pliers or tweezers shall be used for attaching or removing conductor wire."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.3e","Requirement","ECSS-Q-ST-70-26_0130031",1,"Created","The cutting edges of pliers shall be regularly checked for damage and maintained in a sharp condition."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.1.2.4a","Requirement","ECSS-Q-ST-70-26_0130032",1,"Created","The supplier shall provide the equipment specified in Table 5-1 necessary for verification activities specified in clauses 5.4.2 and 5.4.3. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-70-26_0130033",1,"Created","The supplier shall visually examine wire, terminal and connector contacts for cleanliness, absence of oil films and freedom from tarnish or corrosion before assembly."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-Q-ST-70-26_0130034",1,"Created","The supplier shall perform cleaning of the work pieces in conformance with ECSS-Q-ST-70-08. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1c","Requirement","ECSS-Q-ST-70-26_0130035",1,"Created","Further cleaning or other treatment shall not be carried out."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1d","Requirement","ECSS-Q-ST-70-26_0130036",1,"Created","The supplier shall handle work pieces with clean lint free gloves or finger cots."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1e","Requirement","ECSS-Q-ST-70-26_0130037",1,"Created","Before a crimping activity, tools at the operator’s station shall be verified to conform to those selected in accordance with the applicable PID."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1f","Requirement","ECSS-Q-ST-70-26_0130038",1,"Created","All conductor strands shall be inserted cleanly into the barrel without any buckling. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1g","Requirement","ECSS-Q-ST-70-26_0130039",1,"Created","Strands shall not be left outside or cut back to reduce the conductor diameter to fit an undersized barrel. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1h","Requirement","ECSS-Q-ST-70-26_0130040",1,"Created","The supplier shall use tools specified in MIL-DTL-22520.\n    NOTE Examples of crimping parameters are given in Table A-2 and Table A-3"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1i","Requirement","ECSS-Q-ST-70-26_0130041",1,"Created","The supplier shall take provisions to avoid degradation of the silver plated wire caused by tarnish during storage. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.1j","Requirement","ECSS-Q-ST-70-26_0130042",1,"Created","In cases when the same wire is joined later by soldering, the solder fluxes prescribed in ECSS-Q-ST-70-08 shall be used to avoid degradation.\n    NOTE For shift performance inspection requirements see clause 5.5.5."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-Q-ST-70-26_0130043",1,"Created","The supplier shall use silver plated copper multi stranded wire and braided shield cable in crimp type connectors. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2b","Requirement","ECSS-Q-ST-70-26_0130044",1,"Created","Exceptional cases when nickel- or tin-plated wires are used shall be approved by the customer through a request for approval (RFA), in conformance with ECSS-Q-ST-70, clause 5.1.4."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2c","Requirement","ECSS-Q-ST-70-26_0130045",1,"Created","The supplier shall use high strength copper alloy wire for 24 AWG, 26 AWG and 28 AWG crimped joints.\n    NOTE Soft or annealed copper wire are not acceptable for crimped joints of 24 AWG, 26 AWG and 28 AWG size. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2d","Requirement","ECSS-Q-ST-70-26_0130046",1,"Created","The supplier shall use space-qualified components having gold plated terminals in conformance with ECSS-Q-ST-60."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2e","Requirement","ECSS-Q-ST-70-26_0130047",1,"Created","Specific terminals such as ferrules, splices and lugs shall be purchased to MIL or SAE-AS-7928 specifications. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2f","Requirement","ECSS-Q-ST-70-26_0130048",1,"Created","When gold plating is not available the finish shall be in conformance with ECSS-Q-ST-70-71."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.2g","Requirement","ECSS-Q-ST-70-26_0130049",1,"Created","Cadmium, chromate-coated cadmium and non-fused tin-plating shall not be used."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.3a","Requirement","ECSS-Q-ST-70-26_0130050",1,"Created","The supplier shall perform a review of all the materials, tools and techniques planned to be used to ensure conformance to requirements of this standard and as a means of identifying potential problems.\n    NOTE Type of wire includes number of strands, plating metal, type and thickness of insulation."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.3b","Requirement","ECSS-Q-ST-70-26_0130051",1,"Created","Dies, setting of controls for the length of strip in automatic stripping machines and the selection of specific locators or positioners, shall be selected to meet process requirements.\n    NOTE The requirement is valid for power driven and manual crimping processes as well as for size and tolerance for crimping tools"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.3c","Requirement","ECSS-Q-ST-70-26_0130052",1,"Created","The results of the review shall be documented in a PID in conformance with DRD of ECSS-Q-ST-70-38."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-Q-ST-70-26_0130053",1,"Created","The supplier shall give preference to the selection of single wire interconnections."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4b","Requirement","ECSS-Q-ST-70-26_0130054",1,"Created","The supplier shall not use strands of wire doubled backed to increase the conductor diameter."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4c","Requirement","ECSS-Q-ST-70-26_0130055",1,"Created","The supplier shall use additional stranded wires to increase the cross-sectional area up to a selected barrel size; \n    NOTE The requirement is applied for cases where the insulation is prepared as normal and transparent “shrink-fit insulation” to cover the loose end of the wire to prevent any risk of a short circuit."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4d","Requirement","ECSS-Q-ST-70-26_0130056",1,"Created","For 28 AWG up to 16 AWG wire sizes, the maximum insulation clearance shall be equal to the outside diameter (over the insulation) of the wire being used. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4e","Requirement","ECSS-Q-ST-70-26_0130057",1,"Created","The gaps for larger size wires shall not exceed 2 mm.\n    NOTE No minimum gap is specified except that the conductor wire shall be visible to permit inspection."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.4f","Requirement","ECSS-Q-ST-70-26_0130058",1,"Created","Where the terminal or contact is supplied with insulation support, the wire insulation shall enter the support to the extent that no bare wire is exposed. \n    NOTE An example of a typical connector barrel and single wire crimping is shown Figure 5-1."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5a","Requirement","ECSS-Q-ST-70-26_0130059",1,"Created","Requirements of this clause shall be applied when single wire crimping cannot be used."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5b","Requirement","ECSS-Q-ST-70-26_0130060",1,"Created","The maximum number of wires in one crimp barrel shall be two."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5c","Requirement","ECSS-Q-ST-70-26_0130061",1,"Created","The sum of the two nominal conductor sections shall be compatible with the crimp barrel used \n    NOTE 2 ´ 24 AWG is approximately equal to 1 ´ 20 AWG."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5d","Requirement","ECSS-Q-ST-70-26_0130062",1,"Created","Both conductors shall be of the same material and support the same plating finish.\n    NOTE 1 For example: Both are silver and not a combination of silver and nickel\n    NOTE 2 Before introduction into the barrel wires or conductors can be twisted to obtain a “single” conductor."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5e","Requirement","ECSS-Q-ST-70-26_0130063",1,"Created","Axial strength measurements shall be performed on the two associated wires and the axial strength shall be 75 % of the sum of the two wires axial strength requirements."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.5f","Requirement","ECSS-Q-ST-70-26_0130064",1,"Created","For separate conductors introduced into the barrel the following shall apply: \n    1. the actual strength measurement is performed on one of the wires (the smaller, if two different sizes are used);\n    2. the axial strength requirement is as quoted in Table 5-3 for the actual size of wire pulled, assuming a barrel size equal to that wire’s gauge.\n        NOTE Examples of crimping parameters are given in Table A-1 and an example of a typical connector barrel and multi-wire crimping is shown in Figure 5-2."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.6a","Requirement","ECSS-Q-ST-70-26_0130065",1,"Created","The shielded wires on coaxial cables shall be braided."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.6b","Requirement","ECSS-Q-ST-70-26_0130066",1,"Created","Axial strength measurements shall be performed only on the shield after removal of the core dielectric."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.6c","Requirement","ECSS-Q-ST-70-26_0130067",1,"Created","Following crimping, the assembly shall be protected by shrink tubing.\n    NOTE Examples of crimping parameters are given in Table A-3 and an example of a typical ferrule shield crimping is shown in Figure 5-3."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7a","Requirement","ECSS-Q-ST-70-26_0130068",1,"Created","Tools specified by the manufacturer of the terminals shall be used."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7b","Requirement","ECSS-Q-ST-70-26_0130069",1,"Created","The maximum number of wires shall be ten."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7c","Requirement","ECSS-Q-ST-70-26_0130070",1,"Created","Seven wires maximum shall be on the same side."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7d","Requirement","ECSS-Q-ST-70-26_0130071",1,"Created","All conductors shall be of the same material and within a size range of 4 wire gauges on the same side."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7e","Requirement","ECSS-Q-ST-70-26_0130072",1,"Created","All conductors shall be positioned parallel in the terminal before crimping."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7f","Requirement","ECSS-Q-ST-70-26_0130073",1,"Created","Axial strength measurements shall be performed on \n    1. all of the grouped wires for groups with equal wire sizes\n    2. on the smallest wire for groups with different wire sizes."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7g","Requirement","ECSS-Q-ST-70-26_0130074",1,"Created","In the case where opposed wires are tested a specifically designed test fixture shall be used. \n    NOTE A typical test fixture is shown in Figure A-6."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.2.7h","Requirement","ECSS-Q-ST-70-26_0130075",1,"Created","Following crimping, the assembly shall be protected by shrink tubing.\n    NOTE Examples of typical lug and splice wire crimping are shown in Figure 5-4."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.1a","Requirement","ECSS-Q-ST-70-26_0130076",1,"Created","Requirement of this clause shall be applied to crimp configurations that are not specified in clauses 5.2.4 to 5.2.7"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.1b","Requirement","ECSS-Q-ST-70-26_0130077",1,"Created","The supplier shall document the data of successful process qualification in the PID format to ensure continued high quality of production performance."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.1c","Requirement","ECSS-Q-ST-70-26_0130078",1,"Created","An approved PID and additional relevant data from a previous project shall be presented to substantiate a RFA."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.2a","Requirement","ECSS-Q-ST-70-26_0130079",1,"Created","The supplier shall perform tensile strength and voltage drop tests on samples prepared at a number of tool settings, in conformance with the methods defined in clause 5.4 and in conformance with the following process:\n    1. Ten samples prepared at the point specified by the crimping tool manufacturer as a starting point for calibrating tools and pulled (in conformance with Table A-1, Table A-2 and Table A-3).\n    2. The tool indenter opening is then adjusted in convenient increments above and below this point, and ten samples pulled at each increment. \n    3. Voltage drop tests are then performed on five samples for each tool setting.\n    4. A plot is made with increments being close enough together to obtain a smooth curve.\n    5. The minimum in voltage drop and maximum in tensile strength is then determined and evaluated as per Table 5-2 and Table 5-3.\n    6. The design value or operating point should lie approximately in the middle of the flat top portion of the tensile-strength plot, as per Figure 5-5"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.2b","Requirement","ECSS-Q-ST-70-26_0130080",1,"Created","The supplier shall validate satisfactory results achieved from the final tool setting at the operating point in conformance with the methods defined in clause 5.4 and according to the following process: \n    1. Tensile strength tests are performed on five samples corresponding to the operating point.\n    2. Voltage drop tests are performed on five samples corresponding to the operating point.\n    3. Metallographic tests are performed on a minimum of three of these samples corresponding to the operating point.\n    4. Not tested samples are retained for reference.\n        NOTE This approach is conducted from the variation of the main parameter involved to the relevant terminal crimping.\n            a. Connector barrel crimping: selector setting;\n            b. Ferrule crimping: die selection;\n            c. Lug and splice crimping: total cross-section of stranded wires."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.2c","Requirement","ECSS-Q-ST-70-26_0130081",1,"Created","Test data shall be recorded for PID justification."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.3.3a","Requirement","ECSS-Q-ST-70-26_0130082",1,"Created","The supplier shall seal and mark calibrated tools in conformance with clause 5.5.6.3 requirements."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.1a","Requirement","ECSS-Q-ST-70-26_0130083",1,"Created","The supplier shall submit samples to the tests detailed below. \n    NOTE The number of samples is dependent on the specific process requirement (in conformance with clauses 5.3.2 , 5.5.5 and 5.5.6.2 requirements). "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.1b","Requirement","ECSS-Q-ST-70-26_0130084",1,"Created","Test samples shall meet the requirements of clause 5.5.4.1. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.1c","Requirement","ECSS-Q-ST-70-26_0130085",1,"Created","Records of all results shall be tabulated in conformance with 5.5.7. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-70-26_0130086",1,"Created","The supplier shall measure the voltage drop from a point on the positioning shoulder of the contact to another point 14 mm distant on the attached wire (in conformance with the Table 5-2). "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.2b","Requirement","ECSS-Q-ST-70-26_0130087",1,"Created","In cases of two or more wires being crimped in the same contact, lug or splice, the voltage drop measurement shall be performed on each wire. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.2c","Requirement","ECSS-Q-ST-70-26_0130088",1,"Created","The voltage drop of the contact crimp joint shall not exceed the value specified in Table 5-2 for each wire tested."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.1a","Requirement","ECSS-Q-ST-70-26_0130089",1,"Created","The supplier shall use a tensile testing device with characteristics in conformance with Table 5-1. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.1b","Requirement","ECSS-Q-ST-70-26_0130090",1,"Created","The connections shall be loaded until failure occurs. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.1c","Requirement","ECSS-Q-ST-70-26_0130091",1,"Created","The value at failure shall be recorded, together with the information as to whether the failure was “pull-out”, “broke in crimp” or “break in wire”. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.1d","Requirement","ECSS-Q-ST-70-26_0130092",1,"Created","The required ultimate axial strengths for compacted and dispersive crimped joints shall be as shown in Table 5-3 and in clauses 5.4.3.2 and 5.4.3.3.\n    NOTE 1 The insulation may be stripped approximately 2 cm on test specimens to promote visual inspection of the mode of failure in the tensile test.\n    NOTE 2 The required ultimate axial strength values for crimped copper alloy wire are calculated based on the requirement of a minimum wire strength of 343 N/mm\n    NOTE 3 A typical test fixture for testing lug and splice crimps is shown in Figure A-6"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.2a","Requirement","ECSS-Q-ST-70-26_0130093",1,"Created","The required axial strength shall be 75 % of the wire strength."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.2b","Requirement","ECSS-Q-ST-70-26_0130094",1,"Created","Axial strength for copper and copper-alloy wires having either silver-, tin- or nickel-plated finishes shall be as specified in Table 5-3."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.3.3a","Requirement","ECSS-Q-ST-70-26_0130095",1,"Created","The required axial strength shall be:\n    1. 70 % of the shield strength,\n    2. 70 % of one of the smallest gauge wires within the connection if pulled individually, or\n    3. 70 % of the sum of all the wires axial strength requirements if all wires are pulled together."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4a","Requirement","ECSS-Q-ST-70-26_0130096",1,"Created","The supplier shall employ a certified laboratory to perform the metallographic tests described below."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4b","Requirement","ECSS-Q-ST-70-26_0130097",1,"Created","The customer shall approve the certification status of the laboratory."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4c","Requirement","ECSS-Q-ST-70-26_0130098",1,"Created","The joint to be sectioned shall be mounted in a low exotherm resin capable of being moulded without the application of external pressure. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4d","Requirement","ECSS-Q-ST-70-26_0130099",1,"Created","The joint shall be oriented that the wire is perpendicular to the polishing surface. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4e","Requirement","ECSS-Q-ST-70-26_0130100",1,"Created","The specimen shall be ground with the aid of appropriate grades of silicon carbide papers, in order to expose the mid-section of the joint. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4f","Requirement","ECSS-Q-ST-70-26_0130101",1,"Created","This section shall then be polished with successively finer grades of diamond paste down to 1 µm. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4g","Requirement","ECSS-Q-ST-70-26_0130102",1,"Created","To aid microscopic examination, the polished section shall be very lightly etched with an accepted chemical reagent specific to the composition of the materials being crimped."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4h","Requirement","ECSS-Q-ST-70-26_0130103",1,"Created","The section shall be examined in both as-polished and etched states using a metallographic microscope at a magnification up to ´400."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.4.4i","Requirement","ECSS-Q-ST-70-26_0130104",1,"Created","The following acceptance criteria shall be met:\n    1. Each micro section is free from contamination;\n    2. The crimp barrel is evenly deformed;\n    3. Voids occupy less than 10 % of the cross sectioned area of the wire volume;\n    4. The wires and barrel appear as a gas-tight joint and conform to the workmanship sample prepared during qualification;\n    5. All wires are deformed from their circular cross section;\n    6. There are no indentations or fracturing of the deformed receptacle barrel or its plated finish.\n        NOTE 1 For ferrule shield crimping the requirements of 5.4.4i.3. and 5. are not applicable.\n        NOTE 2 For wire barrel contact size 20 - 18 the requirement 5.4.4i.3. is not applicable due to localized voiding at the crimp corners."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-70-26_0130105",1,"Created","The supplier shall install a Quality Assurance (QA) function in conformance with the requirements as defined in ECSS-Q-ST-20. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.1b","Requirement","ECSS-Q-ST-70-26_0130106",1,"Created","The quality control process shall be as specified in Figure 5-7."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.1a","Requirement","ECSS-Q-ST-70-26_0130107",1,"Created","The supplier shall employ trained and competent personnel for all crimping operations. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.1b","Requirement","ECSS-Q-ST-70-26_0130108",1,"Created","The supplier shall develop, maintain and implement a training programme, in conformance with ECSS-Q-ST-20. \n    NOTE The aim of the training programme is to provide for excellence of workmanship and personnel skills, careful and safe operations, and improvement of the quality of crimped joints."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.2a","Requirement","ECSS-Q-ST-70-26_0130109",1,"Created","Trained personnel, performing crimping operations, shall be certified according to a customer approved process "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.2b","Requirement","ECSS-Q-ST-70-26_0130110",1,"Created","The certification of personnel shall be based upon objective evidence of crimp quality, resulting from test and inspection of the crimped joints. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.2c","Requirement","ECSS-Q-ST-70-26_0130111",1,"Created","Operators or inspectors shall be re-certified in cases of repeatedly unacceptable quality levels and changes in crimping techniques, parameters or required skills."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.2d","Requirement","ECSS-Q-ST-70-26_0130112",1,"Created","The supplier shall perform training and certification at a school authorized by the customer."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.2.3a","Requirement","ECSS-Q-ST-70-26_0130113",1,"Created","The supplier shall maintain records of the training and certification status of crimping operators and inspection personnel."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.3a","Requirement","ECSS-Q-ST-70-26_0130114",1,"Created","The supplier shall prepare standards consisting of satisfactory work samples (in conformance with the Figure 5-8 and Figure 5-9)"]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.3b","Requirement","ECSS-Q-ST-70-26_0130115",1,"Created","The supplier shall have readily available visual aids, which clearly illustrate the quality characteristics of all crimped connections utilized. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.3c","Requirement","ECSS-Q-ST-70-26_0130116",1,"Created","Defects such as those listed in clause 5.5.4.2 and shown in Figure 5-8 shall be included as examples."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.3d","Requirement","ECSS-Q-ST-70-26_0130117",1,"Created","The operator shall discard production crimps which in his judgement are defective."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.3e","Requirement","ECSS-Q-ST-70-26_0130118",1,"Created","Defective test samples shall not be discarded."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.1a","Requirement","ECSS-Q-ST-70-26_0130119",1,"Created","The operator shall examine the wire for nicks, rings, broken strands, untwisted lay or not-removed insulation in the area of the crimp before the stripped wire is inserted into the contact or terminal barrel. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.1b","Requirement","ECSS-Q-ST-70-26_0130120",1,"Created","Damaged wires where the base material is exposed shall not be used. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.1c","Requirement","ECSS-Q-ST-70-26_0130121",1,"Created","Contacts and terminal barrels that show evidence of the presence of tarnish, corrosion or physical damage, including bent contacts, shall not be used."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.1d","Requirement","ECSS-Q-ST-70-26_0130122",1,"Created","Inspection shall verify that wire size and type, the contact and terminal are as specified in the drawing or control document."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.2a","Requirement","ECSS-Q-ST-70-26_0130123",1,"Created","The QA inspector shall carry out inspection with the aid of a binocular microscope having an initial linear magnification of ´7. \n    NOTE Further examination of surface characteristics can be performed at higher magnifications. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.2b","Requirement","ECSS-Q-ST-70-26_0130124",1,"Created","The inspector shall not physically disturb parts and conductor leads to aid inspection. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.2c","Requirement","ECSS-Q-ST-70-26_0130125",1,"Created","The following acceptance criteria shall be met; \n    1. Insulation is not damaged by the crimping tool or the terminal;\n    2. The conductor is visible in the inspection hole when an inspection hole is provided;\n    3. The crimp barrel has no unintentional sharp edges, peeled metal, burrs, cracked platings or cuts after crimping;\n    4. All functional parts, including all retention clips or locking devices, are operational after the crimp has been made;\n    5. No tarnished or corroded contacts are present;\n    6. No misplaced crimps, as determined by marks found on areas not designed to take crimping, are present;\n    7. No undercrimps or overcrimps are present;\n        NOTE An undercrimp is detected by a loose conductor and an overcrimp by broken strands or deformed wire at end of terminal.\n    8. If undercrimps or overcrimps are detected this is cause to stop \n        · operations at that station, \n        · reject all production crimps made since the last verification or pull test, \n        · investigate tool, wire and terminals for the cause of failure.\n    9. No bent contacts are present."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.4.2d","Requirement","ECSS-Q-ST-70-26_0130126",1,"Created","Failure to meet the acceptance criteria of 5.5.4.2c shall be cause for rejection."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5a","Requirement","ECSS-Q-ST-70-26_0130127",1,"Created","Each operator shall prepare four samples at the beginning of a shift or before a series of crimping operations."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5b","Requirement","ECSS-Q-ST-70-26_0130128",1,"Created","At the end of the operation four further samples shall be crimped. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5c","Requirement","ECSS-Q-ST-70-26_0130129",1,"Created","Alternatively the supplier shall keep a logbook for each tool. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5d","Requirement","ECSS-Q-ST-70-26_0130130",1,"Created","The logbook shall show the quantity of parts crimped since each calibration and since each go/no-go operation. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5e","Requirement","ECSS-Q-ST-70-26_0130131",1,"Created","Four samples shall be crimped after each 100 crimping operations have been performed."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5f","Requirement","ECSS-Q-ST-70-26_0130132",1,"Created","A tool shall be changed whenever a wire size or contact size is changed. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5g","Requirement","ECSS-Q-ST-70-26_0130133",1,"Created","The operator shall prepare four samples at the start of the operation after such a change.\n    NOTE This can be omitted if samples have already been prepared by the tool during the shift."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5h","Requirement","ECSS-Q-ST-70-26_0130134",1,"Created","In each case, the operator shall submit three samples to the tensile strength test detailed in clause 5.4.3. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5i","Requirement","ECSS-Q-ST-70-26_0130135",1,"Created","The fourth sample shall be retained for reference and traceability purposes (in conformance with clause 5.5.6.2 requirements)."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.5j","Requirement","ECSS-Q-ST-70-26_0130136",1,"Created","The supplier shall perform an analysis of shift performance test results, in comparison with initial tool calibration results, to determine any drift in tool performance."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.1a","Requirement","ECSS-Q-ST-70-26_0130137",1,"Created","The QA organization of the supplier shall ensure that each crimping tool and piece of measuring equipment is calibrated as indicated in the subsequent sub clauses. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.1b","Requirement","ECSS-Q-ST-70-26_0130138",1,"Created","The QA organization of the supplier shall record any suspected and actual equipment failure as a project nonconformance report \n    NOTE Based on past nonconformance reports previous results can be examined to ascertain whether or not re-inspection or retesting is required. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.1c","Requirement","ECSS-Q-ST-70-26_0130139",1,"Created","The QA organization of the supplier shall notify the customer of the nonconformance details."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.1d","Requirement","ECSS-Q-ST-70-26_0130140",1,"Created","The supplier’s calibration procedure shall include the requirements specified in this clause for tool calibration."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.2a","Requirement","ECSS-Q-ST-70-26_0130141",1,"Created","The QA organization of the supplier shall ensure that crimping tools, both manual and powered, are calibrated when initially set up for each specific wire size, connection size and type prior to first use. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.2b","Requirement","ECSS-Q-ST-70-26_0130142",1,"Created","Calibration shall be verified in conformance with the following check-list:\n    1. cleanliness control of the active part of the tool (e.g. indenters);\n    2. set up with the aid of the “go/no-go” gauge in conformance with specified conditions;\n    3. tests in conformance with the clause 5.4 requirements on not less than four samples."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.2c","Requirement","ECSS-Q-ST-70-26_0130143",1,"Created","After satisfactory calibration the tool status shall be documented in a “tool calibration sheet” to ensure tool traceability."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.2d","Requirement","ECSS-Q-ST-70-26_0130144",1,"Created","This traceability shall be established by periodic analysis of the corresponding data from the shift performance inspection and tests (in conformance with clause 5.5.5 requirements), \n    NOTE The frequency of analysis is defined in relation to production activity such as six months or 2 500 crimping operations."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.2e","Requirement","ECSS-Q-ST-70-26_0130145",1,"Created","A significant drift in test results shall result in tool rejection.\n    NOTE Such a tool is generally labelled \"out-of-calibration tool\" (in conformance with clause 5.5.6.4 requirements)."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.3a","Requirement","ECSS-Q-ST-70-26_0130146",1,"Created","The supplier shall provide sealing for calibrated crimping tools to ensure against unauthorized alteration of adjustment settings. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.3b","Requirement","ECSS-Q-ST-70-26_0130147",1,"Created","A wire and lead seal method shall be used if the tool has provisions for it; "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.3c","Requirement","ECSS-Q-ST-70-26_0130148",1,"Created","Alternatively, the tool shall be sealed by a non-reusable decal seal, which, if the calibrated setting is altered, is visibly damaged. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.3d","Requirement","ECSS-Q-ST-70-26_0130149",1,"Created","Seals shall be placed on all external adjustment points of the tool."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.4a","Requirement","ECSS-Q-ST-70-26_0130150",1,"Created","Tools that are out of calibration shall be returned to the tool facility for readjustment and calibration. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.6.4b","Requirement","ECSS-Q-ST-70-26_0130151",1,"Created","Tools that are worn or damaged shall be identified as rejected and removed from the fabrication area."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.7a","Requirement","ECSS-Q-ST-70-26_0130152",1,"Created","The supplier shall maintain traceability throughout the process from incoming inspection to final test, including details of test equipment, tools and personnel employed in performing the task."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.7b","Requirement","ECSS-Q-ST-70-26_0130153",1,"Created","Quality records and logbooks shall be retained for at least ten years "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.7c","Requirement","ECSS-Q-ST-70-26_0130154",1,"Created","Quality records and logbooks shall contain the following information:\n    1. the as-built and test configuration list (waiver and deviation summary);\n    2. non conformance reports and corrective actions;\n    3. copy of the visual inspection and shift performance test results with reference to the relevant procedure, personnel and tools used;\n    4. records of the training, testing and certification status of crimping operators (in conformance with clause 5.5.3 requirements) and ECSS-Q-ST-70-08."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.8a","Requirement","ECSS-Q-ST-70-26_0130155",1,"Created","The QA organization of the supplier shall disposition any nonconformance which is observed in respect of the process in conformance with the quality assurance requirements, in conformance with ECSS-Q-ST-20-09. "]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.5.8b","Requirement","ECSS-Q-ST-70-26_0130156",1,"Created","Failure of a crimping tool to pass any requirement specified in clause 5.1.2.1 shall require rejection of all crimps made by that tool since it was last tested successfully for acceptance."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.6a","Requirement","ECSS-Q-ST-70-26_0130157",1,"Created","The supplier shall produce documentation for: \n    1. Process identification, PID and RFA,\n    2. Inspection,\n    3. Traceability,\n    4. Testing, both procedures and records,\n    5. Logbooks, and\n    6. Calibration."]
["ECSS-Q-ST-70-26C","ECSS - Superseded v1.0","5.6b","Requirement","ECSS-Q-ST-70-26_0130158",1,"Created","The format of the documents shall be in accordance with the deliverables item list defined in the business agreement.\n    NOTE No specific DRD requirements emerge from this Standard."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.1a","Requirement","ECSS-Q-ST-80_0720001",1,"Created","The supplier shall ensure that an organizational structure is defined for software development, and that individuals have defined tasks and responsibilities."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-80_0720002",1,"Created","The responsibility, the authority and the interrelation of personnel who manage, perform and verify work affecting software quality shall be defined and documented.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.2.2a","Requirement","ECSS-Q-ST-80_0720003",1,"Created","The responsibilities and the interfaces of each organisation, either external or internal, involved in a project shall be defined and documented.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.2.3a","Requirement","ECSS-Q-ST-80_0720004",1,"Created","The delegation of software product assurance tasks by a supplier to a lower level supplier shall be done in a documented and controlled way, with the supplier retaining the responsibility towards the customer.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.3.1a","Requirement","ECSS-Q-ST-80_0720005",1,"Created","The supplier shall provide adequate resources to perform the required software product assurance tasks.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.3.2a","Requirement","ECSS-Q-ST-80_0720006",1,"Created","Reviews and audits of processes and of products shall be carried out by personnel not directly involved in the work being performed."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.4.1a","Requirement","ECSS-Q-ST-80_0720007",1,"Created","The supplier shall identify the personnel responsible for software product assurance for the project (SW PA manager/engineer).\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.4.2a","Requirement","ECSS-Q-ST-80_0720008",1,"Created","The software product assurance manager/engineer shall\n    1. report to the project manager (through the project product assurance manager, if any);\n    2. have organisational authority and independence to propose and maintain a software product assurance programme in accordance with the project software product assurance requirements;\n    3. have unimpeded access to higher management as necessary to fulfil his/her duties."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.5.1a","Requirement","ECSS-Q-ST-80_0720009",1,"Created","The supplier shall review the project requirements to establish and make timely provision for acquiring or developing the resources and skills for the management and technical staff.\n","EXPECTED OUTPUT: Training plan [MGT, -; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.5.2a","Requirement","ECSS-Q-ST-80_0720010",1,"Created","The supplier shall maintain training records.\n","EXPECTED OUTPUT: Records of training and experience [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.5.3a","Requirement","ECSS-Q-ST-80_0720011",1,"Created","The supplier shall ensure that the right composition and categories of appropriately trained personnel are available for the planned activities and tasks in a timely manner."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.1.5.4a","Requirement","ECSS-Q-ST-80_0720012",1,"Created","The supplier shall determine the training subjects based on the specific tools, techniques, methodologies and computer resources to be used in the development and management of the software product. \n    NOTE Personnel can undergo training to acquire skills and knowledge relevant to the specific field with which the software is to deal."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.1a","Requirement","ECSS-Q-ST-80_0720013",1,"Created","The supplier shall develop a software product assurance plan in response to the software product assurance requirements in conformance with DRD in annex B."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.1b","Requirement","ECSS-Q-ST-80_0720014",1,"Created","The software product assurance plan shall be either a standalone document or a section of the supplier overall product assurance plan.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.2a","Requirement","ECSS-Q-ST-80_0720015",1,"Created","Any internal manuals, standards or procedures referred to by the software product assurance plan shall become an integral part of the supplier’s software product assurance programme."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.3a","Requirement","ECSS-Q-ST-80_0720016",1,"Created","The software product assurance plan shall be revisited and updated as needed at each milestone to ensure that the activities to be undertaken in the following phase are fully defined.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.4a","Requirement","ECSS-Q-ST-80_0720017",1,"Created","Before acceptance review, the supplier shall either supplement the software product assurance plan to specify the quality measures related to the operations and maintenance processes, or issue a specific software product assurance plan. \n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.5a","Requirement","ECSS-Q-ST-80_0720018",1,"Created","The supplier shall provide with the software product assurance plan a compliance matrix documenting conformance with the individual software product assurance requirements applicable for the project or business agreement.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.1.5b","Requirement","ECSS-Q-ST-80_0720019",1,"Created","For each software product assurance requirement, the compliance matrix shall provide a reference to the document where the expected output of that requirement is located.\n    NOTE For compliance with the required DRDs a general statement of compliance is acceptable.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.2.1a","Requirement","ECSS-Q-ST-80_0720020",1,"Created","The supplier shall report on a regular basis on the status of the software product assurance programme implementation, if appropriate as part of the overall product assurance reporting of the project.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.2.2a","Requirement","ECSS-Q-ST-80_0720021",1,"Created","The software product assurance report shall include:\n    1. an assessment of the current quality of the product and processes, based on measured properties, with reference to the metrication as defined in the software product assurance plan;\n    2. verifications undertaken;\n    3. problems detected;\n    4. problems resolved. \n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-80_0720022",1,"Created","The supplier shall deliver at each milestone review a software product assurance milestone report, covering the software product assurance activities performed during the past project phases.\n","EXPECTED OUTPUT: Software product assurance milestone report [PAF, SPAMR; SRR, PDR, CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.3a","Requirement","ECSS-Q-ST-80_0720023",1,"Created","For software audits, ECSS-Q-ST-10 clause 5.2.3 shall apply.\n","EXPECTED OUTPUT: Audit plan and schedule [PAF, -; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-Q-ST-80_0720024",1,"Created","For software alerts, ECSS-Q-ST-10 clause 5.2.9 shall apply.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Preliminary alert information [PAF, -; -];\n          b.Alert information [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.5.1a","Requirement","ECSS-Q-ST-80_0720025",1,"Created","The supplier shall define and implement procedures for the logging, analysis and correction of all software problems encountered during software development.\n","EXPECTED OUTPUT: Software problem reporting procedures [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.5.2a","Requirement","ECSS-Q-ST-80_0720026",1,"Created","The software problem report shall contain the following information:\n    1. identification of the software item;\n    2. description of the problem;\n    3. recommended solution;\n    4. final disposition;\n    5. modifications implemented (e.g. documents, code, and tools);\n    6. tests re-executed.\n","EXPECTED OUTPUT: Software problem reporting procedures [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.5.3a","Requirement","ECSS-Q-ST-80_0720027",1,"Created","The procedures for software problems shall define the interface with the nonconformance system (i.e. the circumstances under which a problem qualifies as a nonconformance).\n","EXPECTED OUTPUT: Software problem reporting procedures [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.5.4a","Requirement","ECSS-Q-ST-80_0720028",1,"Created","The supplier shall ensure the correct application of problem reporting procedures."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.6.1a","Requirement","ECSS-Q-ST-80_0720029",1,"Created","For software nonconformance handling, ECSS-Q-ST-10-09 shall apply \n","EXPECTED OUTPUT: The following outputs are expected:\n          a.NCR SW procedure as part of the Software product assurance plan [PAF, SPAP; SRR];\n          b.Nonconformance reports [DJF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.6.1b","Requirement","ECSS-Q-ST-80_0720030",1,"Created","When dealing with software nonconformance, the NRB shall include, at least, a representative from the software product assurance and the software engineering organizations.\n","EXPECTED OUTPUT: Identification of SW experts in NRB [MGT, -; SRR]"]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.6.2a","Requirement","ECSS-Q-ST-80_0720031",1,"Created","The software product assurance plan shall specify the point in the software life cycle from which the nonconformance procedures apply.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.7.1a","Requirement","ECSS-Q-ST-80_0720032",1,"Created","Quality models shall be used to specify the software quality requirements.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.2.7.2a","Requirement","ECSS-Q-ST-80_0720033",1,"Created","The following characteristics shall be used to specify the quality model:\n    1. functionality;\n    2. reliability;\n    3. maintainability;\n    4. reusability;\n    5. suitability for safety;\n    6. security;\n    7. usability;\n    8. efficiency;\n    9. portability;\n    10. software development effectiveness.\n        NOTE 1 Quality models are the basis for the identification of process metrics (see clause 6.2.5) and product metrics (see clause 7.1.4).\n        NOTE 2 quality models are also addressed by ISO/IEC 9126 or ECSS-Q-HB-80-04.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.3.1a","Requirement","ECSS-Q-ST-80_0720034",1,"Created","Risk management for software shall be performed by cross-reference to the project risk policy, as specified in ECSS-M-ST-80."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.3.2.1a","Requirement","ECSS-Q-ST-80_0720035",1,"Created","For critical item control, ECSS-Q-ST-10-04 shall apply."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.3.2.2a","Requirement","ECSS-Q-ST-80_0720036",1,"Created","The supplier shall identify the characteristics of the software items that qualify them for inclusion in the Critical Item List."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.1.1a","Requirement","ECSS-Q-ST-80_0720037",1,"Created","For supplier selection ECSS-Q-ST-20 clause 5.4.1 shall apply.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Results of pre-award audits and assessments [PAF, -; -];\n          b.Records of procurement sources [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.1.2a","Requirement","ECSS-Q-ST-80_0720038",1,"Created","For the selection of suppliers of existing software, including software contained in OTS equipments and units, the expected output of clauses 6.2.7.2 to 6.2.7.6 shall be made available.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.2.1a","Requirement","ECSS-Q-ST-80_0720039",1,"Created","The supplier shall establish software product assurance requirements for the next level suppliers, tailored to their role in the project, including a requirement to produce a software product assurance plan.\n","EXPECTED OUTPUT: Software product assurance requirements for suppliers [PAF, -; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.2.2a","Requirement","ECSS-Q-ST-80_0720040",1,"Created","The supplier shall provide the software product assurance requirements applicable to the next level suppliers for customer’s acceptance.\n","EXPECTED OUTPUT: Software product assurance requirements for suppliers [PAF, -; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.3.1a","Requirement","ECSS-Q-ST-80_0720041",1,"Created","The supplier shall monitor the next lower level suppliers’ conformance to the product assurance requirements. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.3.2a","Requirement","ECSS-Q-ST-80_0720042",1,"Created","The monitoring process shall include the review and approval of the next lower level suppliers’ product assurance plans, the continuous verification of processes and products, and the monitoring of the final validation of the product."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.3.3a","Requirement","ECSS-Q-ST-80_0720043",1,"Created","The supplier shall ensure that software development processes are defined and applied by the next lower level suppliers in conformance with the software product assurance requirements for suppliers.\n","EXPECTED OUTPUT: Next level suppliers’ software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.3.4a","Requirement","ECSS-Q-ST-80_0720044",1,"Created","The supplier shall provide the next lower level suppliers’ software product assurance plan for customer’s acceptance.\n","EXPECTED OUTPUT: Next level suppliers’ software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.4.4a","Requirement","ECSS-Q-ST-80_0720045",1,"Created","The supplier shall provide the lower level suppliers with the relevant results of the safety and dependability analyses performed at higher and his level (ref. clauses 6.2.2.1 and 6.2.2.2), including:\n    1. the criticality classification of the software products to be developed;\n    2. information about the failures that can be caused at higher level by the software products to be developed.\n","EXPECTED OUTPUT: Safety and dependability analyses results for lower level suppliers [RB, -; SRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-80_0720046",1,"Created","For procurement documents, ECSS-Q-ST-20 clause 5.4.2 shall apply."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-80_0720047",1,"Created","The choice of procured software shall be described and submitted for customer review.\n","EXPECTED OUTPUT: Software development plan [MGT, SDP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.3a","Requirement","ECSS-Q-ST-80_0720048",1,"Created","For each of the software items the following data shall be provided:\n    1. ordering criteria\n        NOTE For example: versions, options and extensions.\n    2. receiving inspection criteria;\n    3. back-up solutions if the product becomes unavailable;\n    4. contractual arrangements with the supplier for the development, maintenance and upgrades to new releases.\n","EXPECTED OUTPUT: Procurement data [MGT, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.4a","Requirement","ECSS-Q-ST-80_0720049",1,"Created","All the procured software shall be identified and registered by configuration management."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.5a","Requirement","ECSS-Q-ST-80_0720050",1,"Created","The supplier shall subject the procured software to a planned receiving inspection, in accordance with ECSS-Q-ST-20 clause 5.4.4, and the receiving inspection criteria as required by clause 5.5.3.\n","EXPECTED OUTPUT: Receiving inspection report [PAF, -; PDR, CDR, QR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.5.6a","Requirement","ECSS-Q-ST-80_0720051",1,"Created","Exportability constraints shall be identified."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.1.1a","Requirement","ECSS-Q-ST-80_0720052",1,"Created","Methods and tools to be used for all the activities of the development cycle, (including requirements analysis, software specification, modelling, design, coding, validation, testing, configuration management, verification and product assurance) shall be identified by the supplier and agreed by the customer.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.1.2a","Requirement","ECSS-Q-ST-80_0720053",1,"Created","The choice of development methods and tools shall be justified by demonstrating through testing or documented assessment that:\n    1. the development team has appropriate experience or training to apply them,\n    2. the tools and methods are appropriate for the functional and operational characteristics of the product, and\n    3. the tools are available (in an appropriate hardware environment) throughout the development and maintenance lifetime of the product.\n","EXPECTED OUTPUT: Software product assurance milestone report [PAF, SPAMR; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.1.3a","Requirement","ECSS-Q-ST-80_0720054",1,"Created","The correct use of methods and tools shall be verified and reported. \n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.2.1a","Requirement","ECSS-Q-ST-80_0720055",1,"Created","The software development environment shall be selected according to the following criteria:\n    1. availability;\n    2. compatibility;\n    3. performance;\n    4. maintenance;\n    5. durability and technical consistency with the operational equipment;\n    6. the assessment of the product with respect to requirements, including the criticality category;\n    7. the available support documentation;\n    8. the acceptance and warranty conditions;\n    9. the conditions of installation, preparation, training and use;\n    10. the maintenance conditions, including the possibilities of evolutions;\n    11. copyright and intellectual property rights constraints;\n    12. dependence on one specific supplier.\n","EXPECTED OUTPUT: Software development plan [MGT, SDP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.2.2a","Requirement","ECSS-Q-ST-80_0720056",1,"Created","The suitability of the software development environment shall be justified.\n","EXPECTED OUTPUT: Software development plan [MGT, SDP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.6.2.3a","Requirement","ECSS-Q-ST-80_0720057",1,"Created","The availability of the software development environment to developers and other users shall be verified before the start of each development phase."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.1a","Requirement","ECSS-Q-ST-80_0720058",1,"Created","The supplier shall monitor and control the effectiveness of the processes used during the development of the software, including the relevant processes corresponding to the services called from other organizational entities outside the project team.\n    NOTE The process assessment and improvement performed at organization level can be used to provide evidence of compliance for the project.\n","EXPECTED OUTPUT: Software process assessment records: Overall assessments and improvement programme plan [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.2.1a","Requirement","ECSS-Q-ST-80_0720059",1,"Created","The process assessment model and method to be used when performing any software process assessment shall be documented. \n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software process assessment record: assessment model [PAF, -; -];\n          b.Software process assessment record: assessment method [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.2.2a","Requirement","ECSS-Q-ST-80_0720060",1,"Created","Assessments performed and process assessment models used shall be in conformance with ISO/IEC 15504 (Part 2).\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software process assessment record: evidence of conformance of the process assessment model [PAF, -; -];\n          b.Software process assessment record: assessment method [PAF, -; -]. \n    NOTE 1 The model and method documented in ECSS-Q-HB-80-02 are conformant to ISO/IEC 15504 (Part 2).\n    NOTE 2 Currently the CMMI model is not fully conformant to ISO/IEC 15504, however it can be used, provided that the SCAMPI A method is applied."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.2.3a","Requirement","ECSS-Q-ST-80_0720061",1,"Created","The process assessment model, the method, the assessment scope, the results and the assessors shall be verified as complying with the project requirements.\n    NOTE 1 Examples of assessment scopes are: organizational unit evaluated, and processes evaluated.\n    NOTE 2 ECSS-Q-HB-80-02 provides space specific process reference model and their indicators.\n","EXPECTED OUTPUT: Software process assessment record: Software process assessment recognition evidence [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.2.4a","Requirement","ECSS-Q-ST-80_0720062",1,"Created","Assessments, carried out in accordance with ECSS-Q-HB-80-02, shall be performed by a competent assessor, whereas the other assessment team members can be either competent assessor or provisional assessor.\n    NOTE 1 For other assessment schemes conformant to ISO/IEC 15504 (Part 2), assessors certified under INTRSA are competent assessors.\n    NOTE 2 When using CMMI/SCAMPI A, SEI authorized lead appraisers are competent assessors.\n","EXPECTED OUTPUT: Software process assessment record: competent assessor justification [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.3.1a","Requirement","ECSS-Q-ST-80_0720063",1,"Created","The results of the assessment shall be used as feedback to improve as necessary the performed processes, to recommend changes in the direction of the project, and to determine technology advancement needs."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.3.1b","Requirement","ECSS-Q-ST-80_0720064",1,"Created","The suppliers shall ensure that the results of previous assessments are used in its project activity \n","EXPECTED OUTPUT: Software process assessment records: improvement plan [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.3.2a","Requirement","ECSS-Q-ST-80_0720065",1,"Created","The process improvement shall be conducted according to a documented process improvement process.\n    NOTE 1 For the definition of the process improvement process, see ECSS-Q-HB-80-02.\n    NOTE 2 For CMMI, the process improvement is described in the OPF (Organizational Process Focus) process area.\n","EXPECTED OUTPUT: Software process assessment records: improvement process [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","5.7.3.3a","Requirement","ECSS-Q-ST-80_0720066",1,"Created","Evidence of the improvement in performed processes or in project documentation shall be provided.\n    NOTE See ECSS-Q-HB-80-02.\n","EXPECTED OUTPUT: Software process assessment records: evidence of improvements [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.1a","Requirement","ECSS-Q-ST-80_0720067",1,"Created","The software development life cycle shall be defined or referenced in the software product assurance plan."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.1b","Requirement","ECSS-Q-ST-80_0720068",1,"Created","The following characteristics of the software life cycle shall be defined:\n    1. phases;\n    2. input and output of each phase;\n    3. status of completion of phase output;\n    4. milestones;\n    5. dependencies;\n    6. responsibilities;\n    7. role of the customer at each milestone review, in conformance with ECSS-M-ST-10 and ECSS-M-ST-10-01.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.2a","Requirement","ECSS-Q-ST-80_0720069",1,"Created","In the definition of the life cycle and associated milestones and documents, the quality objectives shall be used."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.3a","Requirement","ECSS-Q-ST-80_0720070",1,"Created","The software life cycle shall be reviewed against the contractual software engineering and product assurance requirements. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.4a","Requirement","ECSS-Q-ST-80_0720071",1,"Created","The software life cycle shall be reviewed for suitability and for the availability of resources to implement it by all functions involved in its application."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.1.5a","Requirement","ECSS-Q-ST-80_0720072",1,"Created","A milestone (SW TRR as defined in ECSS-E-ST-40 clause 5.3.5.1) shall be scheduled immediately before the software validation process starts, to check that:\n    1. the software status is compatible with the commencement of validation activities;\n    2. the necessary resources, software product assurance plans, test and validation documentation, simulators or other technical means are available and ready for use.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.1a","Requirement","ECSS-Q-ST-80_0720073",1,"Created","The following activities shall be covered either in software-specific plans or in project general plans:\n    1. development;\n    2. specification, design and customer documents to be produced;\n    3. configuration and documentation management;\n    4. verification, testing and validation activities;\n    5. maintenance.\n","EXPECTED OUTPUT: Software project plans [MGT, MF, DJF]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.2a","Requirement","ECSS-Q-ST-80_0720074",1,"Created","All plans shall be finalized before the start of the related activities.\n","EXPECTED OUTPUT: Software project plans [MGT, MF, DJF]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.3a","Requirement","ECSS-Q-ST-80_0720075",1,"Created","All plans shall be updated for each milestone to reflect any changes during development.\n","EXPECTED OUTPUT: Software project plans [MGT, MF, DJF]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.4a","Requirement","ECSS-Q-ST-80_0720076",1,"Created","The software product assurance plan shall identify all plans to be produced and used, the relationship between them and the time-scales for their preparation and update.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.5a","Requirement","ECSS-Q-ST-80_0720077",1,"Created","Each plan shall be reviewed against the relevant contractual requirements. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.6a","Requirement","ECSS-Q-ST-80_0720078",1,"Created","Procedures and project standards shall address all types of software products included in the project.\n","EXPECTED OUTPUT: Procedures and standards [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.7a","Requirement","ECSS-Q-ST-80_0720079",1,"Created","All procedures and project standards shall be finalized before starting the related activities.\n","EXPECTED OUTPUT: Procedures and standards [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.8a","Requirement","ECSS-Q-ST-80_0720080",1,"Created","Each procedure or standard shall be reviewed against the relevant plans and contractual requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.1.9a","Requirement","ECSS-Q-ST-80_0720081",1,"Created","Before any activity is started, each procedure or standard for that activity shall be reviewed by all functions involved in its application, for suitability and for the availability of resources to implement it."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.1a","Requirement","ECSS-Q-ST-80_0720082",1,"Created","For the system-level analyses leading to the criticality classification of software products based on the severity of failures consequences, ECSS-Q-ST-40 Table 6-1, and ECSS-Q-ST-30 Table 5-1, shall apply.\n","EXPECTED OUTPUT: Criticality classification of software products [PAF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.2a","Requirement","ECSS-Q-ST-80_0720083",1,"Created","The supplier shall perform a software dependability and safety analysis of the software products, in accordance with the requirements of ECSS-Q-ST-30 and ECSS-Q-ST-40 and using the results of system-level safety and dependability analyses, in order to determine the criticality of the individual software components.\n","EXPECTED OUTPUT: Software dependability and safety analysis report [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.3a","Requirement","ECSS-Q-ST-80_0720084",1,"Created","The supplier shall identify the methods and techniques for the software dependability and safety analysis to be performed at technical specification and design level."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.3b","Requirement","ECSS-Q-ST-80_0720085",1,"Created","Methods and techniques for software dependability and safety analysis shall be agreed between the supplier and customer.\n    NOTE ECSS-Q-HB-80-03 provides indication on methods and techniques that can be applied such as: \n        · software failure modes, effects and criticality analysis (for the performing of this analysis, see also ECSS-Q-ST-30-02);\n        · software fault tree analysis;\n        · software common cause failure analysis.\n","EXPECTED OUTPUT: Criticality classification of software components [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.4a","Requirement","ECSS-Q-ST-80_0720086",1,"Created","Based on the results of the software criticality analysis, the supplier shall apply engineering measures to reduce the number of critical software components and mitigate the risks associated with the critical software (ref. clause 6.2.3)."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.5a","Requirement","ECSS-Q-ST-80_0720087",1,"Created","The supplier shall report on the status of the implementation and verification of the SW dependability and safety analysis recommendations.\n","EXPECTED OUTPUT: Software dependability and safety analysis report [PAF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.6a","Requirement","ECSS-Q-ST-80_0720088",1,"Created","The supplier shall update the software dependability and safety analysis at each software development milestone, to confirm the criticality category of software components.\n","EXPECTED OUTPUT: Software dependability and safety analysis report [PAF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.7a","Requirement","ECSS-Q-ST-80_0720089",1,"Created","The supplier shall provide the results of the software dependability and safety analysis for integration into the system-level dependability and safety analyses, addressing in particular:\n    1. additional failure modes identified at software design level;\n    2. recommendations for system-level activities.\n        NOTE For example: introduction of hardware inhibits, and modifications of the system architecture.\n","EXPECTED OUTPUT: Software dependability and safety analysis report [PAF, -; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.8a","Requirement","ECSS-Q-ST-80_0720090",1,"Created","As part of the software requirements analysis activities (ref. clause 6.3.2), the supplier shall contribute to the Hardware-Software Interaction Analysis (HSIA) by identifying, for each hardware failure included in the HSIA, the requirements that specify the software behaviour in the event of that hardware failure."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.2.9a","Requirement","ECSS-Q-ST-80_0720091",1,"Created","During the verification and validation of the software requirements resulting from the Hardware-Software Interaction Analysis, the supplier shall verify that the software reacts correctly to hardware failures, and no undesired software malfunctions occur that may lead to system failures."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.1a","Requirement","ECSS-Q-ST-80_0720092",1,"Created","The supplier shall define and implement measures to avoid propagation of failures between software components of different criticality.\n    NOTE This can be achieved by design measures such as separate hardware platforms, isolation of software processes or prohibition of shared memory (segregation and partitioning). "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.1b","Requirement","ECSS-Q-ST-80_0720093",1,"Created","Software components whose malfunction may cause failures of higher criticality components shall be classified in accordance with the consequences of those failures.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software product assurance plan [PAF, SPAP; PDR, CDR];\n          b.Software dependability and safety analysis report [PAF, -; PDR, CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.2a","Requirement","ECSS-Q-ST-80_0720094",1,"Created","The supplier shall define, justify and apply measures to assure the dependability and safety of critical software.\n    NOTE These measures can include:\n        · use of software design or methods that have performed successfully in a similar application;\n        · insertion of features for failure isolation and handling (ref. ECSS-Q-HB-80-03, software failure modes, effects and criticality analysis);\n        · defensive programming techniques, such as input verification and consistency checks;\n        · use of a “safe subset” of programming language;\n        · use of formal design language for formal proof;\n        · 100 % code branch coverage at unit testing level;\n        · full inspection of source code;\n        · witnessed or independent testing;\n        · gathering and analysis of failure statistics;\n        · removing deactivated code or showing through a combination of analysis and testing that the means by which such code can be inadvertently executed are prevented, isolated, or eliminated.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.3a","Requirement","ECSS-Q-ST-80_0720095",1,"Created","The application of the chosen measures to handle the critical software shall be verified.\n","EXPECTED OUTPUT: Software product assurance milestone report [PAF, SPAMR; PDR, CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.4a","Requirement","ECSS-Q-ST-80_0720096",1,"Created","Critical software shall be subject to regression testing after:\n    1. any change of functionality of the underlying platform hardware;\n        NOTE For example: instruction set of a processor.\n    2. any change of the tools that affect directly or indirectly the generation of the executable code.\n        NOTE In case of minor changes in tools that affect the generation of the executable code, a binary comparison of the executable code generated by the different tools can be used to verify that no modifications are introduced.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.5a","Requirement","ECSS-Q-ST-80_0720097",1,"Created","The need for additional verification and validation of critical software shall be analysed after:\n    1. any change of functionality or performance of the underlying platform hardware;\n    2. any change in the environment in which the software or the platform hardware operate.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.6a","Requirement","ECSS-Q-ST-80_0720098",1,"Created","Identified unreachable code shall be removed and the need for re-verification and re-validation shall be analysed. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.7a","Requirement","ECSS-Q-ST-80_0720099",1,"Created","Unit and integration testing shall be (re-)executed on non-instrumented code."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.3.8a","Requirement","ECSS-Q-ST-80_0720100",1,"Created","Validation testing shall be (re-)executed on non-instrumented code."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.1a","Requirement","ECSS-Q-ST-80_0720101",1,"Created","ECSS-M-ST-40 shall be applied for software configuration management, complemented by the following requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.2a","Requirement","ECSS-Q-ST-80_0720102",1,"Created","The software configuration management system shall allow any reference version to be re-generated from backups.\n","EXPECTED OUTPUT: Software configuration management plan [MGT, SCMP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.3a","Requirement","ECSS-Q-ST-80_0720103",1,"Created","The software configuration file and the software release document shall be provided with each software delivery.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software configuration file [DDF, SCF; -];\n          b.Software release document [DDF, SRelD; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.4a","Requirement","ECSS-Q-ST-80_0720104",1,"Created","The software configuration file shall be available and up to date for each project milestone.\n","EXPECTED OUTPUT: Software configuration file [DDF, SCF; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.5a","Requirement","ECSS-Q-ST-80_0720105",1,"Created","Any components of the code generation tool that are customizable by the user shall be put under configuration control."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.5b","Requirement","ECSS-Q-ST-80_0720106",1,"Created","The change control procedures defined for the project shall address the specific aspects of these components.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software configuration file [DDF, SCF; CDR, QR, AR, ORR];\n          b.Software configuration management plan [MGT, SCMP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.6a","Requirement","ECSS-Q-ST-80_0720107",1,"Created","The supplier shall ensure that all authorized changes are implemented in accordance with the software configuration management plan.\n","EXPECTED OUTPUT: Authorized changes - Software configuration file [DDF, SCF; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.7a","Requirement","ECSS-Q-ST-80_0720108",1,"Created","The following documents shall be controlled (see ECSS-Q-ST-10 clause 5.2.5):\n    1. procedural documents describing the quality system to be applied during the software life cycle;\n    2. planning documents describing the planning and progress of the activities;\n    3. documents describing a particular software product, including:\n        (a) development phase inputs,\n        (b) development phase outputs,\n        (c) verification and validation plans and results,\n        (d) test case specifications, test procedures and test reports,\n        (e) traceability matrices,\n        (f) documentation for the software and system operators and users, and\n        (g) maintenance documentation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.8a","Requirement","ECSS-Q-ST-80_0720109",1,"Created","The supplier shall identify a method and tool to protect the supplied software against corruption.\n    NOTE For example: source, executable and data.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software product assurance plan [PAF, SPAP; SRR, PDR]; \n          b.Software configuration file [DDF, SCF; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.9a","Requirement","ECSS-Q-ST-80_0720110",1,"Created","The supplier shall define a checksum-type key calculation for the delivered operational software.\n    NOTE For example: executable binary, database. \n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.10a","Requirement","ECSS-Q-ST-80_0720111",1,"Created","The checksum value shall be provided in the software configuration file with each software delivery.\n","EXPECTED OUTPUT: Software configuration file [DDF, SCF; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.4.11a","Requirement","ECSS-Q-ST-80_0720112",1,"Created","The media through which the software is delivered to the customer shall be marked by the supplier indicating the following information as a minimum:\n    1. the software name;\n    2. the version number;\n    3. the reference to the software configuration file.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software product assurance plan [PAF, SPAP; SRR, PDR];\n          b.Labels [DDF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.5.1a","Requirement","ECSS-Q-ST-80_0720113",1,"Created","Metrics shall be used to manage the development and to assess the quality of the development processes. \n    NOTE Process metrics are based on quality models (see clause 5.2.7).\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.5.2a","Requirement","ECSS-Q-ST-80_0720114",1,"Created","Process metrics shall be collected, stored and analysed on a regular basis by applying quality models and procedures. \n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.5.3a","Requirement","ECSS-Q-ST-80_0720115",1,"Created","The following basic process metrics shall be used within the supplier’s organization: \n    1. duration: how phases and tasks are being completed versus the planned schedule;\n    2. effort: how much effort is consumed by the various phases and tasks compared to the plan.\n","EXPECTED OUTPUT: Internal metrics report."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.5.4a","Requirement","ECSS-Q-ST-80_0720116",1,"Created","Process metrics shall be used within the supplier’s organization and reported to the customer, including:\n    1. number of problems detected during verification;\n    2. number of problems detected during integration and validation testing and use. \n        NOTE See also software problem reporting described in clause 5.2.5.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.5.5a","Requirement","ECSS-Q-ST-80_0720117",1,"Created","Metrics reports shall be included in the software product assurance reports.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.1a","Requirement","ECSS-Q-ST-80_0720118",1,"Created","Activities for the verification of the quality requirements shall be specified in the definition of the verification plan. \n    NOTE Verification includes various techniques such as review, inspection, testing, walk-through, cross-reading, desk-checking, model simulation, and many types of analysis such as traceability analysis, formal proof or fault tree analysis. \n","EXPECTED OUTPUT: Software verification plan [DJF, SVerP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.2a","Requirement","ECSS-Q-ST-80_0720119",1,"Created","The outputs of each development activity shall be verified for conformance against pre-defined criteria."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.2b","Requirement","ECSS-Q-ST-80_0720120",1,"Created","Only outputs which have been subjected to planned verifications shall be used as inputs for subsequent activities.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.3a","Requirement","ECSS-Q-ST-80_0720121",1,"Created","A summary of the assurance activities concerning the verification process and their findings shall be included in software product assurance reports.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.4a","Requirement","ECSS-Q-ST-80_0720122",1,"Created","The completion of actions related to software problem reports generated during verification shall be verified and recorded.\n","EXPECTED OUTPUT: Software problem reports [DJF, -; SRR, PDR, CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.5a","Requirement","ECSS-Q-ST-80_0720123",1,"Created","Software containing deactivated code shall be verified specifically to ensure that the deactivated code cannot be activated or that its accidental activation cannot harm the operation of the system.\n","EXPECTED OUTPUT: Software verification report [DJF, SVR; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.6a","Requirement","ECSS-Q-ST-80_0720124",1,"Created","Software containing configurable code shall be verified specifically to ensure that any unintended configuration cannot be activated at run time or included during code generation.\n","EXPECTED OUTPUT: Software verification report [DJF, SVR; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.7a","Requirement","ECSS-Q-ST-80_0720125",1,"Created","The supplier shall ensure that:\n    1. the planned verification activities are adequate to confirm that the products of each phase are conformant to the applicable requirements;\n    2. the verification activities are performed according to the plan. \n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.8a","Requirement","ECSS-Q-ST-80_0720126",1,"Created","Reviews and inspections shall be carried out according to defined criteria, and according to the defined level of independence of the reviewer from the author of the reviewed item. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.9a","Requirement","ECSS-Q-ST-80_0720127",1,"Created","Each review and inspection shall be based on a written plan or procedure.\n    NOTE For projects reviews, ECSS-E-ST-40 clause 5.3.3.3, bullet b and Annex P are applicable.\n","EXPECTED OUTPUT: Review and inspection plans or procedures [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.10a","Requirement","ECSS-Q-ST-80_0720128",1,"Created","The review or inspection plans or procedures shall specify: \n    1. the reviewed or inspected items;\n    2. the person in charge;\n    3. the participants;\n    4. the means of review or inspection (e.g. tools or check list);\n    5. the nature of the report.\n","EXPECTED OUTPUT: Review and inspection plans or procedures [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.11a","Requirement","ECSS-Q-ST-80_0720129",1,"Created","Review and inspection reports shall:\n    1. refer to the corresponding review/inspection procedure or plan; \n    2. identify the reviewed item, the author, the reviewer, the review criteria and the findings of the review.\n","EXPECTED OUTPUT: Review and inspection reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.12a","Requirement","ECSS-Q-ST-80_0720130",1,"Created","Traceability matrices (as defined in ECSS-E-ST-40 clause 5.8) shall be verified at each milestone.\n","EXPECTED OUTPUT: Software product assurance milestone report [PAF, SPAMR; SRR, PDR, CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.13a","Requirement","ECSS-Q-ST-80_0720131",1,"Created","Independent software verification shall be performed by a third party."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.6.13b","Requirement","ECSS-Q-ST-80_0720132",1,"Created","Independent software verification shall be a combination of reviews, inspections, analyses, simulations, testing and auditing.\n    NOTE This requirement is applicable where the risks associated with the project justify the costs involved. The customer can consider a less rigorous level of independence, e.g. an independent team in the same organization.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.ISVV plan [DJF, -; SRR, PDR];\n          b.ISVV report [DJF, -; PDR, CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.2a","Requirement","ECSS-Q-ST-80_0720133",1,"Created","Analyses of the advantages to be obtained with the selection of existing software (ref. 3.2.11) instead of new development shall be carried out.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software reuse approach, including approach to delta qualification [PAF, SPAP; SRR, PDR];\n          b.Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.3a","Requirement","ECSS-Q-ST-80_0720134",1,"Created","The existing software shall be assessed with regards to the applicable functional, performance and quality requirements.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software reuse approach, including approach to delta qualification [PAF, SPAP; SRR, PDR];\n          b.Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.4a","Requirement","ECSS-Q-ST-80_0720135",1,"Created","The quality level of the existing software shall be analysed with respect to the project requirements, according to the criticality of the system function implemented, taking into account the following aspects:\n    1. software requirements documentation;\n    2. software architectural and detailed design documentation;\n    3. forward and backward traceability between system requirements, software requirements, design and code;\n    4. unit tests documentation and coverage;\n    5. integration tests documentation and coverage;\n    6. validation documentation and coverage;\n    7. verification reports;\n    8. performance;\n        NOTE For example: memory occupation, CPU load.\n    9. operational performances;\n    10. residual nonconformances and waivers;\n    11. user operational documentation;\n        NOTE For example: user manual.\n    12. code quality (adherence to coding standards, metrics).\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software reuse approach, including approach to delta qualification [PAF, SPAP; SRR, PDR];\n          b.Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.5a","Requirement","ECSS-Q-ST-80_0720136",1,"Created","The results of the reused software analysis shall be recorded in the software reuse file, together with an assessment of the possible level of reuse and a description of the assumptions and the methods applied when estimating the level of reuse.\n    NOTE Results of the reused software analysis, such as detailed reference to requirement and design documents, test reports and coverage results.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software reuse approach, including approach to delta qualification [PAF, SPAP; SRR, PDR];\n          b.Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.6a","Requirement","ECSS-Q-ST-80_0720137",1,"Created","The analysis of the suitability of existing software for reuse shall be complemented by an assessment of the following aspects:\n    1. the acceptance and warranty conditions;\n    2. the available support documentation; \n    3. the conditions of installation, preparation, training and use; \n    4. the identification and registration by configuration management; \n    5. maintenance responsibility and conditions, including the possibilities of changes; \n    6. the durability and validity of methods and tools used in the initial development, that are envisaged to be used again; \n    7. the copyright and intellectual property rights constraints (modification rights); \n    8. the licensing conditions;\n    9. exportability constraints.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.7a","Requirement","ECSS-Q-ST-80_0720138",1,"Created","Corrective actions shall be identified, documented in the reuse file and applied to the reused software not meeting the applicable requirements related to the aspects as specified in clauses 6.2.7.2 to 6.2.7.6.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.8a","Requirement","ECSS-Q-ST-80_0720139",1,"Created","Reverse engineering techniques shall be applied to generate missing documentation and to reach the required verification and validation coverage."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.8b","Requirement","ECSS-Q-ST-80_0720140",1,"Created","For software products whose life cycle data from previous development are not available and reverse engineering techniques are not fully applicable, the following methods shall be applied:\n    1. generation of validation and verification documents based on the available user documentation (e.g. user manual) and execution of tests in order to achieve the required level of test coverage;\n    2. use of the product service history to provide evidence of the product’s suitability for the current application, including information about:\n        (a) relevance of the product service history for the new operational environment;\n        (b) configuration management and change control of the software product;\n        (c) effectiveness of problem reporting;\n        (d) actual error rates and maintenance records;\n        (e) impact of modifications.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.9a","Requirement","ECSS-Q-ST-80_0720141",1,"Created","The software reuse file shall be updated at project milestones to reflect the results of the identified corrective actions for reused software not meeting the project requirements.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.10a","Requirement","ECSS-Q-ST-80_0720142",1,"Created","All the reused software shall be kept under configuration control."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.7.11a","Requirement","ECSS-Q-ST-80_0720143",1,"Created","The detailed configuration status of the reused software baseline shall be provided to the customer in the reuse file for acceptance.\n","EXPECTED OUTPUT: Software reuse file [DJF, SRF; SRR, PDR, CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.1a","Requirement","ECSS-Q-ST-80_0720144",1,"Created","For the selection of tools for automatic code generation, the supplier shall evaluate the following aspects:\n    1. evolution of the tools in relation to the tools that use the generated code as an input;\n        NOTE For example: compilers or code management systems.\n    2. customization of the tools to comply with project standards; \n    3. portability requirements for the generated code; \n    4. collection of the required design and code metrics; \n    5. verification of software components containing generated code; \n    6. configuration control of the tools including the parameters for customisation;\n    7. compliance with open standards."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.2a","Requirement","ECSS-Q-ST-80_0720145",1,"Created","The requirements on testing applicable to the automatically generated code shall ensure the achievement of the same objectives as those for manually generated code.\n","EXPECTED OUTPUT: Validation and testing documentation [DJF, SValP; PDR], [DJF, SVS; CDR, QR, AR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.3a","Requirement","ECSS-Q-ST-80_0720146",1,"Created","The required level of verification and validation of the automatic generation tool shall be at least the same as the one required for the generated code, if the tool is used to skip verification or testing activities on the target code."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.4a","Requirement","ECSS-Q-ST-80_0720147",1,"Created","Modelling standards for automatic code generation tools shall be defined and applied.\n","EXPECTED OUTPUT: Modelling standards [PAF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.5a","Requirement","ECSS-Q-ST-80_0720148",1,"Created","Adherence to modelling standards shall be verified.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.6a","Requirement","ECSS-Q-ST-80_0720149",1,"Created","Clause 6.3.4 shall apply to automatically generated code, unless the supplier demonstrates that the automatically generated code does not need to be manually modified."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.2.8.7a","Requirement","ECSS-Q-ST-80_0720150",1,"Created","The verification and validation documentation shall address separately the activities to be performed for manually and automatically generated code.\n","EXPECTED OUTPUT: Validation and testing documentation [DJF, SValP; PDR], [DJF, SVS; CDR, QR, AR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.1.1a","Requirement","ECSS-Q-ST-80_0720151",1,"Created","For the definition of the software related system requirements to be specified in the requirements baseline, ECSS-E-ST-40 clause 5.2 shall apply."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.1.2a","Requirement","ECSS-Q-ST-80_0720152",1,"Created","The requirements baseline shall be subject to documentation control and configuration management as part of the development documentation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.1.3a","Requirement","ECSS-Q-ST-80_0720153",1,"Created","For the definition of the requirements baseline, all results from the safety and dependability analyses (including results from the HSIA ECSS-Q-ST-30 clause 6.4.2.3) shall be used."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.2.1a","Requirement","ECSS-Q-ST-80_0720154",1,"Created","The requirements baseline shall be analyzed to fully and unambiguously define the software requirements in the technical specification."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.2.2a","Requirement","ECSS-Q-ST-80_0720155",1,"Created","The technical specification shall be subject to documentation control and configuration management as part of the development documentation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.2.3a","Requirement","ECSS-Q-ST-80_0720156",1,"Created","For the definition of the technical specification, all results from the safety and dependability analyses (including results from the HSIA ECSS-Q-ST-30 clause 6.4.2.3) shall be used."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.2.4a","Requirement","ECSS-Q-ST-80_0720157",1,"Created","In addition to the functional requirements, the technical specification shall include all non-functional requirements necessary to satisfy the requirements baseline, including, as a minimum, the following:\n    1. performance,\n    2. safety,\n    3. reliability,\n    4. robustness,\n    5. quality,\n    6. maintainability,\n    7. configuration management,\n    8. security,\n    9. privacy,\n    10. metrication, and\n    11. verification and validation.\n        NOTE Performance requirements include requirements on numerical accuracy.\n","EXPECTED OUTPUT: Software requirements specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.2.5a","Requirement","ECSS-Q-ST-80_0720158",1,"Created","Prior to the technical specification elaboration, customer and supplier shall agree on the following principles and rules as a minimum:\n    1. assignment of persons (on both sides) responsible for establishing the technical specification;\n    2. methods for agreeing on requirements and approving changes;\n    3. efforts to prevent misunderstandings such as definition of terms, explanations of background of requirements;\n    4. recording and reviewing discussion results on both sides."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.1a","Requirement","ECSS-Q-ST-80_0720159",1,"Created","The design definition file shall be subject to documentation control and configuration management. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.2a","Requirement","ECSS-Q-ST-80_0720160",1,"Created","Mandatory and advisory design standards shall be defined and applied.\n","EXPECTED OUTPUT: Design standards [PAF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.3a","Requirement","ECSS-Q-ST-80_0720161",1,"Created","For software in which numerical accuracy is relevant to mission success specific rules on design and code shall be defined to ensure that the specified level of accuracy is obtained.\n    NOTE For example: for an attitude and orbit control subsystem, scientific data generation components.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.4a","Requirement","ECSS-Q-ST-80_0720162",1,"Created","Adherence to design standards shall be verified.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.5a","Requirement","ECSS-Q-ST-80_0720163",1,"Created","The supplier shall define means, criteria and tools to ensure that the complexity and modularity of the design meet the quality requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.5b","Requirement","ECSS-Q-ST-80_0720164",1,"Created","The design evaluation shall be performed in parallel with the design process, in order to provide feedback to the software design team.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.6a","Requirement","ECSS-Q-ST-80_0720165",1,"Created","Synthesis of the results obtained in the software complexity and modularity evaluation and corrective actions implemented shall be described in the software product assurance reports.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.3.7a","Requirement","ECSS-Q-ST-80_0720166",1,"Created","The supplier shall review the design documentation to ensure that it contains the appropriate level of information for maintenance activities.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software product assurance plan [PAF, SPAP; PDR];\n          b.Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.1a","Requirement","ECSS-Q-ST-80_0720167",1,"Created","Coding standards (including consistent naming conventions and adequate commentary rules) shall be specified and observed.\n","EXPECTED OUTPUT: Coding standards [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.2a","Requirement","ECSS-Q-ST-80_0720168",1,"Created","The standards shall be consistent with the product quality requirements.\n    NOTE Coding standards depend on the software quality objectives (see clause 5.2.7).\n","EXPECTED OUTPUT: Coding standards [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.3a","Requirement","ECSS-Q-ST-80_0720169",1,"Created","The tools to be used in implementing and checking conformance with coding standards shall be identified in the product assurance plan before coding activities start.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.4a","Requirement","ECSS-Q-ST-80_0720170",1,"Created","Coding standards shall be reviewed with the customer to ensure that they reflect product quality requirements.\n","EXPECTED OUTPUT: Coding standards and description of tools [PAF, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.5a","Requirement","ECSS-Q-ST-80_0720171",1,"Created","Use of low-level programming languages shall be justified.\n","EXPECTED OUTPUT: Software development plan [MGT, SDP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.6a","Requirement","ECSS-Q-ST-80_0720172",1,"Created","The supplier shall define measurements, criteria and tools to ensure that the software code meets the quality requirements.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.6b","Requirement","ECSS-Q-ST-80_0720173",1,"Created","The code evaluation shall be performed in parallel with the coding process, in order to provide feedback to the software programmers."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.7a","Requirement","ECSS-Q-ST-80_0720174",1,"Created","Synthesis of the code analysis results and corrective actions implemented shall be described in the software product assurance reports.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.4.8a","Requirement","ECSS-Q-ST-80_0720175",1,"Created","The code shall be put under configuration control immediately after successful unit testing."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.1a","Requirement","ECSS-Q-ST-80_0720176",1,"Created","Testing shall be performed in accordance with a strategy for each testing level (i.e. unit, integration, validation against the technical specification, validation against the requirements baseline, acceptance), which includes:\n    1. the types of tests to be performed;\n        NOTE For example: functional, boundary, performance, and usability tests.\n    2. the tests to be performed in accordance with the plans and procedures;\n    3. the means and organizations to perform assurance function for testing and validation.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.2a","Requirement","ECSS-Q-ST-80_0720177",1,"Created","Based on the criticality of the software, test coverage goals for each testing level shall be agreed between the customer and the supplier and their achievement monitored by metrics: \n    1. for unit level testing;\n    2. for integration level testing;\n    3. for validation against the technical specification and validation against the requirements baseline.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.3a","Requirement","ECSS-Q-ST-80_0720178",1,"Created","The supplier shall ensure through internal review that the test procedures and data are adequate, feasible and traceable and that they satisfy the requirements.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.4a","Requirement","ECSS-Q-ST-80_0720179",1,"Created","Test readiness reviews shall be held before the commencement of test activities, as defined in the software development plan.\n","EXPECTED OUTPUT: Test readiness review reports [DJF, -; TRR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.5a","Requirement","ECSS-Q-ST-80_0720180",1,"Created","Test coverage shall be checked with respect to the stated goals.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.5b","Requirement","ECSS-Q-ST-80_0720181",1,"Created","Feedback from the results of test coverage evaluation shall be continuously provided to the software developers."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.6a","Requirement","ECSS-Q-ST-80_0720182",1,"Created","The supplier shall ensure that nonconformances and software problem reports detected during testing are properly documented and reported to those concerned.\n","EXPECTED OUTPUT: Nonconformance reports and software problem reports [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.7a","Requirement","ECSS-Q-ST-80_0720183",1,"Created","The test coverage of configurable code shall be checked to ensure that the stated requirements are met in each tested configuration.\n","EXPECTED OUTPUT: Statement of compliance with test plans and procedures [PAF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.8a","Requirement","ECSS-Q-ST-80_0720184",1,"Created","The completion of actions related to software problem reports generated during testing and validation shall be verified and recorded.\n","EXPECTED OUTPUT: Software problem reports [DJF, -; SRR, PDR, CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.9a","Requirement","ECSS-Q-ST-80_0720185",1,"Created","Provisions shall be made to allow witnessing of tests by the customer."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.10a","Requirement","ECSS-Q-ST-80_0720186",1,"Created","Provisions shall be made to allow witnessing of tests by supplier personnel independent of the development.\n    NOTE For example: specialist software product assurance personnel."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.11a","Requirement","ECSS-Q-ST-80_0720187",1,"Created","The supplier shall ensure that:\n    1. tests are conducted in accordance with approved test procedures and data, \n    2. the configuration under test is correct, \n    3. the tests are properly documented, and \n    4. the test reports are up to date and valid. \n","EXPECTED OUTPUT: Statement of compliance with test plans and procedures [PAF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.12a","Requirement","ECSS-Q-ST-80_0720188",1,"Created","The supplier shall ensure that tests are repeatable by verifying the storage and recording of tested software, support software, test environment, supporting documents and problems found.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.13a","Requirement","ECSS-Q-ST-80_0720189",1,"Created","The supplier shall confirm in writing that the tests are successfully completed.\n","EXPECTED OUTPUT: Testing and validation reports [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.14a","Requirement","ECSS-Q-ST-80_0720190",1,"Created","Review boards looking to engineering and product assurance aspects shall be convened after the completion of test phases, as defined in the software development plan."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.15a","Requirement","ECSS-Q-ST-80_0720191",1,"Created","Areas affected by any modification shall be identified and re-tested (regression testing)."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.16a","Requirement","ECSS-Q-ST-80_0720192",1,"Created","In case of re-testing, all test related documentation (test procedures, data and reports) shall be updated accordingly.\n","EXPECTED OUTPUT: Updated test documentation [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.17a","Requirement","ECSS-Q-ST-80_0720193",1,"Created","The need for regression testing and additional verification of the software shall be analysed after any change of the platform hardware.\n","EXPECTED OUTPUT: Updated test documentation [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.18a","Requirement","ECSS-Q-ST-80_0720194",1,"Created","The need for regression testing and additional verification of the software shall be analysed after a change or update of any tool used to generate it.\n    NOTE For example: source code or object code.\n","EXPECTED OUTPUT: Updated test documentation [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.19a","Requirement","ECSS-Q-ST-80_0720195",1,"Created","Validation shall be carried out by staff who have not taken part in the design or coding of the software being validated.\n    NOTE This can be achieved at the level of the whole software product, or on a component by component basis."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.20a","Requirement","ECSS-Q-ST-80_0720196",1,"Created","Validation of the flight software against the requirement baseline on the flight equipment model shall be performed on a software version without any patch. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.21a","Requirement","ECSS-Q-ST-80_0720197",1,"Created","The supplier shall review the test documentation to ensure that it is up to date and organized to facilitate its reuse for maintenance."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.22a","Requirement","ECSS-Q-ST-80_0720198",1,"Created","Tests shall be organized as activities in their own right in terms of planning, resources and team composition. \n","EXPECTED OUTPUT: Test and validation documentation [DJF, SValP; PDR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.23a","Requirement","ECSS-Q-ST-80_0720199",1,"Created","The necessary resources for testing shall be identified early in the life cycle, taking into account the operating and maintenance requirements. \n","EXPECTED OUTPUT: Test and validation documentation [DJF, SValP; PDR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.24a","Requirement","ECSS-Q-ST-80_0720200",1,"Created","Test tool development or acquisition (hardware and software) shall be planned for in the overall project plan.\n","EXPECTED OUTPUT: Test and validation documentation [DJF, SValP; PDR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.25a","Requirement","ECSS-Q-ST-80_0720201",1,"Created","The supplier shall establish and review the test procedures and data before starting testing activities and also document the constraints of the tests concerning physical, performance, functional, controllability and observability limitations.\n","EXPECTED OUTPUT: Test and validation documentation [DJF, SValP; PDR], [DJF, SVS; CDR, QR, AR], [DJF, SUITP; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.26a","Requirement","ECSS-Q-ST-80_0720202",1,"Created","Before offering the product for delivery and customer acceptance, the supplier shall validate its operation as a complete product, under conditions similar to the application environment as specified in the requirements baseline."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.27a","Requirement","ECSS-Q-ST-80_0720203",1,"Created","When testing under the operational environment is performed, the following concerns shall be addressed:\n    1. the features to be tested in the operational environment;\n    2. the specific responsibilities of the supplier and customer for carrying out and evaluating the test;\n    3. restoration of the previous operational environment (after test).\n","EXPECTED OUTPUT: Test and validation documentation [DJF, -; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.28a","Requirement","ECSS-Q-ST-80_0720204",1,"Created","Independent software validation shall be performed by a third party.\n    NOTE This requirement is applicable where the risks associated with the project justify the costs involved. The customer can consider a less rigorous level of independence, e.g. an independent team in the same organization.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.ISVV plan [DJF, -; SRR, PDR];\n          b.ISVV report [DJF, -; PDR, CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.29a","Requirement","ECSS-Q-ST-80_0720205",1,"Created","The validation shall include testing in the different configurations possible or in a representative set of them when it is evident that the number of possible configurations is too high to allow validation in all of them.\n","EXPECTED OUTPUT: Test and validation documentation [DJF, SValP; PDR], [DJF, SVS; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.30a","Requirement","ECSS-Q-ST-80_0720206",1,"Created","Software containing deactivated code shall be validated specifically to ensure that the deactivated code cannot be activated or that its accidental activation cannot harm the operation of the system.\n","EXPECTED OUTPUT: Testing and validation reports [DJF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.31a","Requirement","ECSS-Q-ST-80_0720207",1,"Created","Software containing configurable code shall be validated specifically to ensure that unintended configuration cannot be activated at run time or included during code generation.\n","EXPECTED OUTPUT: Testing and validation reports [DJF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.5.32a","Requirement","ECSS-Q-ST-80_0720208",1,"Created","Activities for the validation of the quality requirements shall be specified in the definition of the validation specification. \n","EXPECTED OUTPUT: Software validation specification [DJF, SVS; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.1a","Requirement","ECSS-Q-ST-80_0720209",1,"Created","The roles, responsibilities and obligations of the supplier and customer during installation shall be established.\n","EXPECTED OUTPUT: Installation procedure [DDF, SCF; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.2a","Requirement","ECSS-Q-ST-80_0720210",1,"Created","The installation shall be performed in accordance with the installation procedure."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.3a","Requirement","ECSS-Q-ST-80_0720211",1,"Created","The customer shall establish an acceptance test plan specifying the intended acceptance tests including specific tests suited to the target environment (see ECSS-E-ST-40 clause 5.7.3.1).\n    NOTE 1 The acceptance tests can be partly made up of tests used during previous test activities.\n    NOTE 2 The acceptance test plan takes into account the requirement for operational demonstration, either as part of acceptance or after acceptance.\n","EXPECTED OUTPUT: Acceptance test plan [DJF, -; QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.4a","Requirement","ECSS-Q-ST-80_0720212",1,"Created","The customer shall ensure that the acceptance tests are performed in accordance with the approved acceptance test plan (see ECSS-E-ST-40 clause 5.7.3.2)."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.5a","Requirement","ECSS-Q-ST-80_0720213",1,"Created","Before the software is presented for customer acceptance, the supplier shall ensure that:\n    1. the delivered software complies with the contractual requirements (including any specified content of the software acceptance data package);\n    2. the source and object code supplied correspond to each other;\n    3. all agreed changes are implemented;\n    4. all nonconformances are either resolved or declared."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.6a","Requirement","ECSS-Q-ST-80_0720214",1,"Created","The customer shall verify that the executable code was regenerated from configuration managed source code components and installed in accordance with predefined procedures on the target environment."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.7a","Requirement","ECSS-Q-ST-80_0720215",1,"Created","Any discovered problems shall be documented in nonconformance reports.\n","EXPECTED OUTPUT: Nonconformance reports [DJF, -; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.8a","Requirement","ECSS-Q-ST-80_0720216",1,"Created","On completion of the acceptance tests, a report shall be drawn up and be signed by the supplier’s representatives, the customer’s representatives, the software quality engineers of both parties and the representative of the organization charged with the maintenance of the software product.\n","EXPECTED OUTPUT: Acceptance test report [DJF, -; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.6.9a","Requirement","ECSS-Q-ST-80_0720217",1,"Created","The customer shall certify conformance to the procedures and state the conclusion concerning the test result for the software product under test (accepted, conditionally accepted, rejected).\n","EXPECTED OUTPUT: Acceptance test report [DJF, -; AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.7.1a","Requirement","ECSS-Q-ST-80_0720218",1,"Created","During operations, the quality of the mission products related to software shall be agreed with the customer and users.\n    NOTE Quality of mission products can include parameters such as: error-free data, availability of data and permissible outages; permissible information degradation.\n","EXPECTED OUTPUT: Software operation support plan [OP, -; ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.7.2a","Requirement","ECSS-Q-ST-80_0720219",1,"Created","During the demonstration that the software conforms to the operational requirements, the following shall be covered as a minimum:\n    1. availability and maintainability of the host system (including reboot after maintenance interventions);\n    2. safety features;\n    3. human-computer interface;\n    4. operating procedures;\n    5. ability to meet the mission product quality requirements.\n","EXPECTED OUTPUT: Validation of the operational requirements [PAF, -; ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.7.3a","Requirement","ECSS-Q-ST-80_0720220",1,"Created","The product assurance plan for system operations shall include consideration of software.\n","EXPECTED OUTPUT: Input to product assurance plan for systems operation [PAF, -; ORR]"]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.1a","Requirement","ECSS-Q-ST-80_0720221",1,"Created","The organization responsible for maintenance shall be identified to allow a smooth transition into the operations and maintenance.\n    NOTE An organization, with representatives from both supplier and customer, can be set up to support the maintenance activities. Attention is drawn to the importance of the flexibility of this organization to cope with the unexpected occurrence of problems and the identification of facilities and resources to be used for the maintenance activities.\n","EXPECTED OUTPUT: Maintenance plan [MF, -; QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.2a","Requirement","ECSS-Q-ST-80_0720222",1,"Created","The maintenance organization shall specify the assurance, verification and validation activities applicable to maintenance interventions.\n","EXPECTED OUTPUT: Maintenance plan [MF, -; QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.3a","Requirement","ECSS-Q-ST-80_0720223",1,"Created","The maintenance plans shall be verified against specified requirements for maintenance of the software product.\n    NOTE The maintenance plans and procedures can address corrective, improving, adaptive and preventive maintenance, differentiating between “routine” and “emergency” maintenance activities."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.4a","Requirement","ECSS-Q-ST-80_0720224",1,"Created","The maintenance plans and procedures shall include the following as a minimum:\n    1. scope of maintenance;\n    2. identification of the first version of the software product for which maintenance is to be done;\n    3. support organization;\n    4. maintenance life cycle;\n    5. maintenance activities;\n    6. quality measures to be applied during the maintenance;\n    7. maintenance records and reports.\n","EXPECTED OUTPUT: Maintenance plan [MF, -; QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.5a","Requirement","ECSS-Q-ST-80_0720225",1,"Created","Rules for the submission of maintenance reports shall be established and agreed as part of the maintenance plan.\n","EXPECTED OUTPUT: Maintenance plan [MF, -; QR, AR, ORR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.6a","Requirement","ECSS-Q-ST-80_0720226",1,"Created","All maintenance activities shall be logged in predefined formats and retained. \n","EXPECTED OUTPUT: Maintenance records [MF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","6.3.8.7a","Requirement","ECSS-Q-ST-80_0720227",1,"Created","Maintenance records shall be established for each software product, including, as a minimum, the following information,:\n    1. list of requests for assistance or problem reports that have been received and the current status of each;\n    2. organization responsible for responding to requests for assistance or implementing the appropriate corrective actions;\n    3. priorities assigned to the corrective actions;\n    4. results of the corrective actions;\n    5. statistical data on failure occurrences and maintenance activities.\n        NOTE The record of the maintenance activities can be utilized for evaluation and enhancement of the software product and for improvement of the quality system itself.\n","EXPECTED OUTPUT: Maintenance records [MF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.1a","Requirement","ECSS-Q-ST-80_0720228",1,"Created","The software quality requirements (including safety and dependability requirements) shall be derived from the requirements defined at system level.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Requirement baseline [RB, SSS; SRR];\n          b.Technical specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.2a","Requirement","ECSS-Q-ST-80_0720229",1,"Created","Quality requirements shall be expressed in quantitative terms or constraints.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Requirement baseline [RB, SSS; SRR];\n          b.Technical specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.3a","Requirement","ECSS-Q-ST-80_0720230",1,"Created","The supplier shall define assurance activities to ensure that the product meets the quality requirements as specified in the technical specification.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.4a","Requirement","ECSS-Q-ST-80_0720231",1,"Created","In order to verify the implementation of the product quality requirements, the supplier shall define a metrication programme based on the identified quality model (see clause 5.2.7), specifying:\n    1. the metrics to be collected and stored;\n    2. the means to collect metrics (measurements);\n    3. the target values, with reference to the product quality requirements;\n    4. the analyses to be performed on the collected metrics, including the ones to derive:\n        (a) descriptive statistics;\n            NOTE For example: the number of units at each level of complexity.\n        (b) trend analysis (such as trends in software problems).\n    5. how the results of the analyses performed on the collected metrics are fed back to the development team and used to identify corrective actions;\n    6. the schedule of metrics collection, storing, analysis and reporting, with reference to the whole software life cycle.\n        NOTE Guidance for software metrication programme implementation can be found in ECSS-Q-HB-80-04. \n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.5a","Requirement","ECSS-Q-ST-80_0720232",1,"Created","The following basic products metrics shall be used:\n    1. size (code);\n    2. complexity (design, code);\n    3. fault density and failure intensity;\n    4. test coverage;\n    5. number of failures.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.6a","Requirement","ECSS-Q-ST-80_0720233",1,"Created","The results of metrics collection and analysis shall be included in the software product assurance reports, in order to provide the customer with an insight into the level of quality obtained.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.7a","Requirement","ECSS-Q-ST-80_0720234",1,"Created","Numerical accuracy shall be estimated and verified.\n","EXPECTED OUTPUT: Numerical accuracy analysis [DJF, SVR; PDR, CDR, QR]. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.1.8a","Requirement","ECSS-Q-ST-80_0720235",1,"Created","The supplier shall define the organization and means implemented to collect and analyse data required for the study of software maturity.\n    NOTE For example: failures, corrections, duration of runs.\n","EXPECTED OUTPUT: Software product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.1.1a","Requirement","ECSS-Q-ST-80_0720236",1,"Created","The software quality requirements shall be documented in the requirements baseline and technical specification.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Requirement baseline [RB, SSS; SRR];\n          b.Technical specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.1.2a","Requirement","ECSS-Q-ST-80_0720237",1,"Created","The software requirements shall be: \n    1. correct;\n    2. unambiguous;\n    3. complete;\n    4. consistent;\n    5. verifiable;\n    6. traceable."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.1.3a","Requirement","ECSS-Q-ST-80_0720238",1,"Created","For each requirement the method for verification and validation shall be specified.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Requirement baseline [RB, SSS; SRR];\n          b.Technical specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.2.1a","Requirement","ECSS-Q-ST-80_0720239",1,"Created","The software design shall meet the non-functional requirements as documented in the technical specification."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.2.2a","Requirement","ECSS-Q-ST-80_0720240",1,"Created","The software shall be designed to facilitate testing."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.2.3a","Requirement","ECSS-Q-ST-80_0720241",1,"Created","Software with a long planned lifetime shall be designed with minimum dependency on the operating system and the hardware, in order to aid portability.\n    NOTE This requirement is applicable to situations where the software lifetime can lead to the obsolescence and non-availability of the original operating system and/or hardware, thereby jeopardizing the maintainability the software.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software product assurance plan [PAF, SPAP; SRR, PDR];\n          b.Justification of design choices [DDF, SDD; PDR, CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.1a","Requirement","ECSS-Q-ST-80_0720242",1,"Created","Detailed test and validation documentation (data, procedures and expected results) defined in the ECSS-E-ST-40 DJF shall be consistent with the defined test and validation strategy (see clause 6.3.5 and ECSS-E-ST-40 clauses 5.5.3, 5.5.4, 5.6 and 5.8)."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.2a","Requirement","ECSS-Q-ST-80_0720243",1,"Created","The test documentation shall cover the test environment, tools and test software, personnel required and associated training requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.3a","Requirement","ECSS-Q-ST-80_0720244",1,"Created","The criteria for completion of each test and any contingency steps shall be specified."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.4a","Requirement","ECSS-Q-ST-80_0720245",1,"Created","Test procedures, data and expected results shall be specified."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.5a","Requirement","ECSS-Q-ST-80_0720246",1,"Created","The hardware and software configuration shall be identified and documented as part of the test documentation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.2.3.6a","Requirement","ECSS-Q-ST-80_0720247",1,"Created","For any requirements not covered by testing a verification report shall be drawn up documenting or referring to the verification activities performed.\n","EXPECTED OUTPUT: Software verification report [DJF, SVR; CDR, QR, AR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.1a","Requirement","ECSS-Q-ST-80_0720248",1,"Created","For the development of software intended for reuse, ECSS-E-ST-40 clauses 5.2.4.7 and 5.4.3.6 shall apply."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.2a","Requirement","ECSS-Q-ST-80_0720249",1,"Created","The information related to the components developed for reuse shall be separated from the others in the technical specification, design justification file, design definition file and product assurance file. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.3a","Requirement","ECSS-Q-ST-80_0720250",1,"Created","The information related to components developed for reuse in the technical specification, the design justification file, the design definition file and the product assurance file shall be self-contained."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.4a","Requirement","ECSS-Q-ST-80_0720251",1,"Created","The technical specification of components developed for reuse shall include requirements for maintainability, portability and verification of those components.\n","EXPECTED OUTPUT: Technical specification for reusable components [TS, -; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.5a","Requirement","ECSS-Q-ST-80_0720252",1,"Created","The configuration management system shall include provisions for handling specific aspects of software developed for reuse, such as:\n    • longer lifetime of the components developed for reuse compared to the other components of the project;\n    • evolution or change of the development environment for the next project that intends to use the components;\n    • transfer of the configuration and documentation management information to the next project reusing the software.\n","EXPECTED OUTPUT: Software configuration management plan [MGT, SCMP; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.6a","Requirement","ECSS-Q-ST-80_0720253",1,"Created","Where the components developed for reuse are developed to be reusable on different platforms, the testing of the software shall be performed on all those platforms. \n","EXPECTED OUTPUT: Verification and validation documentation for reusable components [DJF, -; CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.3.7a","Requirement","ECSS-Q-ST-80_0720254",1,"Created","The supplier shall provide a certificate of conformance that the tests have been successfully completed on all the relevant platforms.\n    NOTE In case not all platforms are available, the certificate of conformance states the limitations of the validation performed.\n","EXPECTED OUTPUT: Verification and validation documentation for reusable components [DJF, -; CDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.4.1a","Requirement","ECSS-Q-ST-80_0720255",1,"Created","The subcontracting and procurement of hardware shall be carried out according to the requirements of ECSS-Q-ST-20 clause 7.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Justification of selection of operational ground equipment [DJF, -; SRR, PDR];\n          b.Receiving inspection reports [PAF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.4.2a","Requirement","ECSS-Q-ST-80_0720256",1,"Created","The procurement of support services to be used in operational phases shall be justified as covering service level agreements, quality of services and escalation procedures, as needed for system exploitation and maintenance.\n","EXPECTED OUTPUT: Justification of selection of operational support services [DJF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.4.3a","Requirement","ECSS-Q-ST-80_0720257",1,"Created","The choice of procured hardware and services shall address the constraints associated with both the development and the actual use of the software.\n","EXPECTED OUTPUT: Justification of selection of operational ground equipment [DJF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.4.4a","Requirement","ECSS-Q-ST-80_0720258",1,"Created","The ground computer equipment and supporting services for implementing the final system shall be selected according to the project requirements regarding:\n    1. performance;\n    2. maintenance;\n    3. durability and technical consistency with the operational equipment;\n    4. the assessment of the product with respect to requirements, including the criticality category;\n    5. the available support documentation;\n    6. the acceptance and warranty conditions;\n    7. the conditions of installation, preparation, training and use;\n    8. the maintenance conditions, including the possibilities of evolutions;\n    9. copyright constraints;\n    10. availability;\n    11. compatibility;\n    12. site operational constraints.\n","EXPECTED OUTPUT: Justification of selection of operational ground equipment [DJF, -; SRR, PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.4.5a","Requirement","ECSS-Q-ST-80_0720259",1,"Created","Taking account of the provider’s maintenance and product policy, it shall be ensured that the hardware and support services can be maintained throughout the specified life of the software product within the operational constraints."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.5.1a","Requirement","ECSS-Q-ST-80_0720260",1,"Created","The supplier shall establish procedures for firmware device programming and duplication of firmware devices.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.5.2a","Requirement","ECSS-Q-ST-80_0720261",1,"Created","The firmware device shall be indelibly marked to allow the identification (by reference) of the hardware component and of the software component.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","7.5.3a","Requirement","ECSS-Q-ST-80_0720262",1,"Created","The supplier shall ensure that the firmware programming equipment is calibrated."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<1>a","Requirement","ECSS-Q-ST-80_0720263",1,"Created","The SPAP shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<2>a","Requirement","ECSS-Q-ST-80_0720264",1,"Created","The SPAP shall list the applicable and reference documents to support the generation of the document."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<3>a","Requirement","ECSS-Q-ST-80_0720265",1,"Created","The SPAP shall include any additional terms, definition or abbreviated terms used."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<4>a","Requirement","ECSS-Q-ST-80_0720266",1,"Created","The SPAP shall include or refer to a description of the system and software products being developed."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.1>a","Requirement","ECSS-Q-ST-80_0720267",1,"Created","The SPAP shall describe the organization of software product assurance activities, including responsibility, authority and the interrelation of personnel who manage, perform and verify work affecting software quality."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.1>b","Requirement","ECSS-Q-ST-80_0720268",1,"Created","The following topics shall be included:\n    1. organizational structure;\n    2. interfaces of each organisation, either external or internal, involved in the project; \n    3. relationship to the system level product assurance and safety;\n    4. independence of the software product assurance function;\n    5. delegation of software product assurance tasks to a lower level supplier, if any."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.2>a","Requirement","ECSS-Q-ST-80_0720269",1,"Created","The SPAP shall describe the responsibilities of the software product assurance function."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.3>a","Requirement","ECSS-Q-ST-80_0720270",1,"Created","The SPAP shall describe the resources to be used to perform the software product assurance function."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.3>b","Requirement","ECSS-Q-ST-80_0720271",1,"Created","The description in B.2.1<5.3>a shall include human resources and skills, hardware and software tools."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.4>a","Requirement","ECSS-Q-ST-80_0720272",1,"Created","The SPAP shall describe the reporting to be performed by software product assurance."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.5>a","Requirement","ECSS-Q-ST-80_0720273",1,"Created","The SPAP shall describe the quality models applicable to the project and how they are used to specify the quality requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.6>a","Requirement","ECSS-Q-ST-80_0720274",1,"Created","The SPAP shall describe the contribution of the software product assurance function to the project risk management."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.7>a","Requirement","ECSS-Q-ST-80_0720275",1,"Created","The SPAP shall describe the contribution of the software product assurance function to the next level suppliers selection and control."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.8>a","Requirement","ECSS-Q-ST-80_0720276",1,"Created","The SPAP shall describe the methods and tools used for all the activities of the development cycle, and their level of maturity."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.9>a","Requirement","ECSS-Q-ST-80_0720277",1,"Created","1.The SPAP shall state the scope and objectives of process assessment."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.9>b","Requirement","ECSS-Q-ST-80_0720278",1,"Created","2.The SPAP shall describe the methods and tools to be used for process assessment and improvement."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<5.10>a","Requirement","ECSS-Q-ST-80_0720279",1,"Created","The SPAP shall specify the quality measures related to the operations and maintenance processes (alternatively, a separate SPAP is produced)."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.1>a","Requirement","ECSS-Q-ST-80_0720280",1,"Created","The SPAP shall refer to the software development cycle description in the software development plan. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.1>b","Requirement","ECSS-Q-ST-80_0720281",1,"Created","If not covered in the software development plan, the life cycle shall be described."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.1>c","Requirement","ECSS-Q-ST-80_0720282",1,"Created","The life cycle shall include a milestone immediately before the starting of the software validation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.2>a","Requirement","ECSS-Q-ST-80_0720283",1,"Created","The SPAP shall describe all plans to be produced and used in the project."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.2>b","Requirement","ECSS-Q-ST-80_0720284",1,"Created","The relationship between the project plans and a timely planning for their preparation and update shall be described."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.3>a","Requirement","ECSS-Q-ST-80_0720285",1,"Created","The SPAP shall contain a description and justification of the measures to be applied for the handling of critical software, including the analyses to be performed and the standards applicable for critical software."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.4>a","Requirement","ECSS-Q-ST-80_0720286",1,"Created","The SPAP shall describe the contribution of the software product assurance function to the proper implementation of documentation and configuration management."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.4>b","Requirement","ECSS-Q-ST-80_0720287",1,"Created","The nonconformance control system shall be described or referenced. The point in the software life cycle from which the nonconformance procedures apply shall be specified."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.4>c","Requirement","ECSS-Q-ST-80_0720288",1,"Created","The SPAP shall identify method and tool to protect the supplied software, a checksum-type key calculation for the delivered operational software, and a labelling method for the delivered media."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.5>a","Requirement","ECSS-Q-ST-80_0720289",1,"Created","The SPAP shall describe the process metrics derived from the defined quality models, the means to collect, store and analyze them, and the way they are used to manage the development processes."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.6>a","Requirement","ECSS-Q-ST-80_0720290",1,"Created","The SPAP shall describe the approach for the reuse of existing software, including delta qualification. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.7>a","Requirement","ECSS-Q-ST-80_0720291",1,"Created","The following processes and activities shall be covered, taking into account the project scope and life cycle:\n    1. software requirements analysis;\n    2. software architectural design and design of software items;\n    3. coding;\n    4. testing and validation (including regression testing);\n    5. verification;\n    6. software delivery and acceptance;\n    7. operations and maintenance."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.8>a","Requirement","ECSS-Q-ST-80_0720292",1,"Created","The SPAP shall describe or list by reference all procedures and standards applicable to the development of the software in the project."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.8>b","Requirement","ECSS-Q-ST-80_0720293",1,"Created","The software product assurance measures to ensure adherence to the project procedures and standards shall be described. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<6.8>c","Requirement","ECSS-Q-ST-80_0720294",1,"Created","The standards and procedures to be described or listed in accordance with B.2.1<6.8>a shall be as a minimum those covering the following aspects:\n    1. project management;\n    2. risk management;\n    3. configuration and documentation management;\n    4. verification and validation;\n    5. requirements engineering;\n    6. design;\n    7. coding;\n    8. metrication;\n    9. nonconformance control;\n    10. audits;\n    11. alerts;\n    12. procurement;\n    13. reuse of existing software;\n    14. use of methods and tools;\n    15. numerical accuracy;\n    16. delivery, installation and acceptance;\n    17. operations;\n    18. maintenance;\n    19. device programming and marking."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<7>a","Requirement","ECSS-Q-ST-80_0720295",1,"Created","The SPAP shall describe the approach taken to ensure the quality of the software product. "]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<7>b","Requirement","ECSS-Q-ST-80_0720296",1,"Created","The description of the approach specified in B.2.1<7>a shall include the:\n    1. specification of the product metrics, their target values and the means to collect them;\n    2. definition of a timely metrication programme;\n    3. analyses to be performed on the collected metrics;\n    4. way the results are fed back to the development team;\n    5. documentation quality requirements;\n    6. assurance activities meant to ensure that the product meets the quality requirements."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<8>a","Requirement","ECSS-Q-ST-80_0720297",1,"Created","The SPAP shall include the compliance matrix to the applicable software product assurance requirements (e.g. ECSS-Q-ST-80 clauses, as tailored by a product assurance requirements document), or provide a reference to it."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","B.2.1<8>b","Requirement","ECSS-Q-ST-80_0720298",1,"Created","For each software product assurance requirement, the following information shall be provided:\n    1. requirement identifier;\n    2. compliance (C = compliant, NC = non–compliant, NA = not applicable);\n    3. reference to the project documentation covering the requirement (e.g. section of the software product assurance plan);\n    4. remarks."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<1>a","Requirement","ECSS-Q-ST-80_0720299",1,"Created","The SPAMR shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<2>a","Requirement","ECSS-Q-ST-80_0720300",1,"Created","The SPAMR shall list the applicable and reference documents to support the generation of the document."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<3>a","Requirement","ECSS-Q-ST-80_0720301",1,"Created","The SPAMR shall include any additional terms, definition or abbreviated terms used."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<4>a","Requirement","ECSS-Q-ST-80_0720302",1,"Created","The SPAMR shall contain reporting on verification activities performed by the product assurance function, including:\n    1. reviews;\n    2. inspections;\n    3. walk-throughs;\n    4. review of traceability matrices;\n    5. documents reviewed."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<4>b","Requirement","ECSS-Q-ST-80_0720303",1,"Created","The SPAMR shall contain reporting on the verification of the measures applied for the handling of critical software."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<5>a","Requirement","ECSS-Q-ST-80_0720304",1,"Created","The SPAMR shall include or reference a justification of the suitability of the methods and tools applied in all the activities of the development cycle, including requirements analysis, software specification, design, coding, validation, testing, configuration management, verification and product assurance."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<5>b","Requirement","ECSS-Q-ST-80_0720305",1,"Created","The SPAMR shall include reporting on the correct use of methods and tools."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<6>a","Requirement","ECSS-Q-ST-80_0720306",1,"Created","The SPAMR shall include reporting on the adherence of software products to the applicable modelling, design and coding standards, including:\n    1. reporting on the application of measures meant to ensure that the design complexity and modularity meet the quality requirements;\n    2. reporting on design documentation w.r.t. suitability for maintenance."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<7>a","Requirement","ECSS-Q-ST-80_0720307",1,"Created","The SPAMR shall include reporting on the collected product and process metrics, the relevant analyses performed, the corrective actions undertaken and the status of these actions."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<7>b","Requirement","ECSS-Q-ST-80_0720308",1,"Created","The results of the software maturity analysis shall also be reported."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<8>a","Requirement","ECSS-Q-ST-80_0720309",1,"Created","The SPAMR shall include reporting on adequacy of the testing and validation documentation (including feasibility, traceability repeatability), and on the achieved test coverage w.r.t. stated goals."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<9>a","Requirement","ECSS-Q-ST-80_0720310",1,"Created","The SPAMR shall include reporting on the status of software problem reports and nonconformances relevant to software."]
["ECSS-Q-ST-80C","ECSS - Superseded v1.0","C.2.1<10>a","Requirement","ECSS-Q-ST-80_0720311",1,"Created","Whenever relevant and up-to-date information has been already delivered as part of the regular PA progress reporting, a representative summary shall be provided, together with a detailed reference to the progress report(s) containing that information."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1a","Requirement","ECSS-Q-ST-10-09_0350001",1,"Created","The supplier’s project PA representative shall perform an immediate preliminary assessment of the nonconformance to establish its extent and cause when it is detected."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1b","Requirement","ECSS-Q-ST-10-09_0350002",1,"Created","Based on the preliminary assessment the supplier’s project PA representative shall take the following actions without delay:\n    1. Provisions for the safety of the personnel and of the equipment.\n    2. Prevention of unauthorized use of the nonconforming items, by marking and, unless otherwise determined by the PA representative, segregation until their disposition.\n    3. Prevention of the recurrence of the nonconformances on similar or identical items under processing or testing at that time.\n        NOTE This can lead to the suspension of manufacturing or testing."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1c","Requirement","ECSS-Q-ST-10-09_0350003",1,"Created","The supplier shall apply the following actions to the segregation of nonconforming articles:\n    1. Establish a clearly marked holding area for nonconforming items pending NRB disposition.\n    2. Limit the access to this area to NRB members or personnel authorized by the NRB.\n    3. Make provisions to prevent unauthorized removal of any item."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1d","Requirement","ECSS-Q-ST-10-09_0350004",1,"Created","For items whose segregation in the holding area is not practicable the supplier shall perform the following actions:\n    1. Mark the item as “not to be used”.\n    2. Make sure that the item can not be used by unauthorized personnel."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1e","Requirement","ECSS-Q-ST-10-09_0350005",1,"Created","The supplier shall complete the nonconformance report in conformance with Annex A, and submit it to the internal NRB. "]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1f","Requirement","ECSS-Q-ST-10-09_0350006",1,"Created","The supplier shall describe the nonconformance clear, unambiguous and sufficiently detailed that it can be understood by personnel not involved in its detection."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.1g","Requirement","ECSS-Q-ST-10-09_0350007",1,"Created","The supplier shall ensure traceability between the NCR and the quality and manufacturing records related to the nonconforming item."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-Q-ST-10-09_0350008",1,"Created","The NRB shall be the sole technical authority for the treatment of nonconformances occurring in the frame of a business agreement."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-Q-ST-10-09_0350009",1,"Created","All NRB members shall make dispositions and decisions by consensus."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.1c","Requirement","ECSS-Q-ST-10-09_0350010",1,"Created","The NRB chairman shall involve higher management levels in case of conflict."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.1a","Requirement","ECSS-Q-ST-10-09_0350011",1,"Created","The supplier shall nominate and authorize the internal NRBs core members for the business agreement."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.1b","Requirement","ECSS-Q-ST-10-09_0350012",1,"Created","The responsibilities and authorities of each member shall be assigned."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.1c","Requirement","ECSS-Q-ST-10-09_0350013",1,"Created","The internal NRB shall include, at least, core members from the following areas:\n    1. Project PA (chairman),\n    2. Engineering.\n        NOTE Additional members, or experts, depending on the NCR subject can be nominated by the chairman."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.1d","Requirement","ECSS-Q-ST-10-09_0350014",1,"Created","Immediately after the reporting of a nonconformance, the chairman shall convene an internal NRB."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.2a","Requirement","ECSS-Q-ST-10-09_0350015",1,"Created","The internal NRB shall classify nonconformances as major or minor, based on the severity of their consequences. \n    NOTE Classification of nonconformances is not based on their consequences on cost and schedule."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.2b","Requirement","ECSS-Q-ST-10-09_0350016",1,"Created","In case of several different minor nonconformances on the same item, the internal NRB shall evaluate whether the nonconformances remain minor or reclassified as “major”."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.2c","Requirement","ECSS-Q-ST-10-09_0350017",1,"Created","In case of doubt, the internal NRB shall classify nonconformances as major."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-10-09_0350018",1,"Created","The internal NRB shall investigate the cause(s) of the nonconformance.\n    NOTE If necessary, a separate group of experts can be assigned for the investigation."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3b","Requirement","ECSS-Q-ST-10-09_0350019",1,"Created","The supplier shall carry out physical operation of an irreversible nature on the nonconforming item only with prior approval by the customer.\n    NOTE Non-destructive testing can be used, if the techniques involved have previously been approved by the customer."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3c","Requirement","ECSS-Q-ST-10-09_0350020",1,"Created","The internal NRB shall analyse whether human error or poor workmanship are the primary or secondary cause for the nonconformance."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3d","Requirement","ECSS-Q-ST-10-09_0350021",1,"Created","In case that human error or poor workmanship are the primary or secondary cause for the nonconformance, the supplier shall review all related documents and the competence level of personnel in order to prevent recurrence."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3e","Requirement","ECSS-Q-ST-10-09_0350022",1,"Created","The internal NRB shall investigate the consequences of the nonconformance.\n    NOTE This can be supported, where appropriate, by dependability experts or by documentation such as FMECA, CIL, or DJF."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.2.3f","Requirement","ECSS-Q-ST-10-09_0350023",1,"Created","The internal NRB shall document the results of the investigation in the nonconformance report."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.2.3.5a","Requirement","ECSS-Q-ST-10-09_0350041",1,"Created","The responsible NRB shall identify and recommend the need for a waiver or deviation."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","5.5.1b","Requirement","ECSS-Q-ST-10-09_0350057",1,"Created","The supplier shall maintain a list covering minor and major NCRs, providing a complete representation of the status of all nonconformances occurring in the frame of a business agreement, for each product, at any time."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","6.3.3a","Requirement","ECSS-Q-ST-10-09_0350090",1,"Created","The operator shall adapt the basic requirements defined in clause 5 to the reporting and processing of operational nonconformances and anomalies, by establishing and maintaining documented procedures to be agreed with the relevant parties."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","A.2.1<22>a","Requirement","ECSS-Q-ST-10-09_0350115",1,"Created","The NCR shall describe the basic fact or circumstance which causes the nonconformance."]
["ECSS-Q-ST-10-09C","ECSS - Superseded v1.0","A.2.1<31>a","Requirement","ECSS-Q-ST-10-09_0350124",1,"Created","The NCR shall contain “Yes” or “No” based on customer NRB disposition and the identification number of the RFW in case of “Yes”."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","6.2b","Requirement","ECSS-Q-ST-70-10_0590015",1,"Created","The qualification programme shall identify:\n    1. the key personnel involved;\n    2. the test houses;\n    3. the test procedure and test sequence;\n    4. the proposed schedule of testing."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","6.4e","Requirement","ECSS-Q-ST-70-10_0590026",1,"Created","A qualification test report shall be prepared in conformance with Annex B and submitted to the qualification authority for review and approval together with all prepared microsections.\n    NOTE The qualification authority can request the delivery of the inspected qualification PCBs."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","6.5.14a","Requirement","ECSS-Q-ST-70-10_0590048",1,"Created","The following measurements shall be performed on test pattern X:\n    1. Evaluation of continuity of conductors after exposing the pattern to bending cycles.\n    2. Evaluation of adhesion between conductors and insulating material after exposing the pattern to bending cycles.\n        NOTE See example in Figure 6-15."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.2.3d","Requirement","ECSS-Q-ST-70-10_0590073",1,"Created","The nonconformance criteria for the substrate shall be as follows:\n1.\tNot in conformance with PCB manufacturer’s \ntrademark and required quality\tM\n2.\tScratches cutting glass fibre or leaving marks in the \ndielectric laminate that are affecting reliability\tM\n3.\tScratches not affecting reliability\tm\n4.\tDents, crazing and haloing:\n(a)\tVisible to the naked eye\tM\n(b)\tOnly visible with magnification aids\t\t          m\n5.\tNon­homogeneity regarding colouring and opacity\tm/M\n6.\tDiscoloured copper oxide layer on internal layer is acceptable;\n7.\tInclusion of foreign matter, blistering or air bubbles:\n(a)\tVisible to the naked eye\tM\n(b)\tOnly visible with magnification aids\tm\n8.\tDelamination\tM\n9.\tMeasling:\n(a)\tGeneral measling spread over the whole PCB \nsurface\tM\n(b)\tLocal measling that causes reduction of the \ninsulation distance in the outer layer to below the requirement\tM\n(c)\tLocal measling that does not cause reduction \nof the insulation distance in the outer layer to \nbelow the requirement\t                                              m\n10.\tFungus growth\tM\n11.\tDelamination of cover layer (only for flexible PCB)\t        m/M\n"]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.2.8.3c","Requirement","ECSS-Q-ST-70-10_0590108",1,"Created","The voltage shall be applied between two ground planes or between one ground plane and one conductor that are superimposed, i.e. on two separate adjacent layers."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.3.3.1a","Requirement","ECSS-Q-ST-70-10_0590141",1,"Created","The test shall be carried out in conformance with test 10a of IEC 60326-2-am 2 (1992-06)."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.3.3.3g","Requirement","ECSS-Q-ST-70-10_0590166",1,"Created","For the test the alternating movement shall be continued until an electrical discontinuity appears or until 500 cycles are completed without defect."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.3.4.1d","Requirement","ECSS-Q-ST-70-10_0590175",1,"Created","After 10 s, the tape shall be quickly pulled off perpendicular to the coating surface."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.3.5.1.3a","Requirement","ECSS-Q-ST-70-10_0590212",1,"Created","Same initial conditions as in clause 7.3.5.1.2 with application of a voltage to the circuit terminals such that the current varies by successive steps:\n    1. I0 = 2 A for 3 min.\n    2. I1 = 4 A for 3 min;\n    3. Further increments of 2 A every 3 min until destruction (open circuit) or if for I = 18 A circuit discontinuity is not achieved."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.4.1b","Requirement","ECSS-Q-ST-70-10_0590232",1,"Created","PCB manufacturer and the qualification authority shall agree on omission of any of these tests.\n    NOTE The solder bath test is to simulate solder wave assembly of PCBs and is followed by the vapour phase solder test to simulate solder reflow assembly of PCBs. The rework test simulates hand solder assembly, rework and repair of PCBs."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.4.2.2d","Requirement","ECSS-Q-ST-70-10_0590241",1,"Created","The other side compared to the procedure in 10.2.1.2a of the same test board shall be coated with flux or a solder paste with flux and baked."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","7.5i","Requirement","ECSS-Q-ST-70-10_0590266",1,"Created","The nonconformance criteria shall be as follows:\n    1. Peel strength < requirement \t\t\t\tM\n    2. Increase in resistance > +10 % \t\t\t\tM\n    3. Intralayer insulation resistance < 103 MΩ \t\t\tM\n    4. Interlayer insulation resistance < 104 MΩ \t\t\tM\n    5. Evidence of flashover, breakdown, sparking \t\t\tM\n    6. Microsectioning: broken metallization \t\t\tM\n    7. Technological and functional defects \t\t\tM"]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","8.5a","Requirement","ECSS-Q-ST-70-10_0590299",1,"Created","The PCB manufacturer shall calibrate any electrical and mechanical manufacturing equipment to traceable reference standards."]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","9.5b","Requirement","ECSS-Q-ST-70-10_0590332",1,"Created","The limits for the dimensional characteristics shall be as follows:\n1.\tExternal dimension tolerance \t±0,2 mm;\n2.\tThickness tolerance: ±10 %;\n3.\tMaximum active board size: supplier’s specification;\n4.\tMaximum board thickness: 3,2 mm;\n5.\tPositioning between registration mark and edge of circuit: ±0,2 mm;\n6.\tConductor width:\n(a)\tInternal: 120 mm minimum;\n(b)\tExternal: 200 mm minimum (for fine pitch 120 mm width is tolerated if less than 5 mm from component pad);\n7.\tConductor spacing:\n(a)\tInternal: 150 mm minimum;\n(b)\tExternal: 300 mm minimum (for fine pitch 150 mm spacing is tolerated if less than 5 mm from component pad);\n8.\tConductor tolerance (minimum/maximum): supplier’s specification;\n9.\tTolerance on diameter of terminal pads: supplier’s specification;\n10.\tMinimum drilled hole diameter:\n(a)\tComponent hole: in conformance with ECSS-Q-ST-70-08;\n(b)\tVia hole: 0,25 mm minimum \nand maximum aspect ratio t/d = 6;\n11.\tTolerance on diameter of plated­through holes:\n(a)\tNominal Æ ³ 0,7: D maximum 0,15 mm for component hole;\n(b)\tNominal Æ < 0,7: D maximum 0,20 mm;\n12.\tTolerance on diameter of non­plated­through holes: \nD maximum 0,20 mm;\n13.\tPositioning of holes with respect to reference mark: ±0,1 mm;\n14.\tRelative misregistration pad/hole: £ 0,15 mm;\n15.\tMisalignment determined by measuring minimum annular ring:\n(a)\tExternal layers: solder side: 0,20 mm\n(b)\tExternal layers: component side (reduced pads): 0,10 mm\n(c)\tExternal layers: non­soldering hole: 0,10 mm\n(d)\tInternal layers: 50 mm;\n16.\tLayer to layer registration: ±100 mm;\n17.\tNumber of layers: 18 maximum.\n"]
["ECSS-Q-ST-70-10C","ECSS - Superseded v1.0","9.6d","Requirement","ECSS-Q-ST-70-10_0590339",1,"Created","The limits for the mechanical characteristics shall be as follows:\n1.\tWarp and twist: \n£ 1,1 % for board thickness ³ 1,6 mm, \n£ 1,5 % for board thickness < 1,6 mm;\n2.\tConductor adhesion/peel strength:\n(a)\tOn epoxy with Tg < 160 °C: ³ 16 N/cm;\n(b)\tOn epoxy with Tg > 180 °C: ³ 12 N/cm;\n(c)\tOn polyimide: ³ 12 N/cm;\n(d)\tOn bismaleimide/trazine modified epoxy HTg: ³ 12 N/cm;\n(e)\tAramide/polyimide: ³ 6 N/cm;\n3.\tBond strength/pull strength:\n(a)\tFor terminal pads 4 mm Æ on epoxy Tg < 160 °C: ³ 140 N;\n(b)\tFor terminal pads 4 mm Æ on epoxy Tg > 180 °C: ³ 80 N;\n(c)\tFor terminal pads 4 mm Æ on polyimide: ³ 80 N;\n(d)\tFor terminal pads 4 mm Æ on bismaleimide/trazine modified epoxy HTg: ³ 60 N;\n(e)\tFor terminal pads 4 mm Æ on aramide/polyimide: ³ 60 N;\n(f)\tFor terminal pads 2 mm Æ on epoxy Tg < 160 °C: ³ 35 N;\n(g)\tFor terminal pads 2 mm Æ on epoxy Tg > 180 °C: ³ 20 N;\n(h)\tFor terminal pads 2 mm Æ on polyimide: ³ 20 N;\n(i)\tFor terminal pads 2 mm Æ on bismaleimide/trazine modified epoxy HTg: ³ 12 N;\n(j)\tFor terminal pads 2 mm Æ aramide/polyimide: ³ 12 N."]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","5.1.2i","Requirement","ECSS-Q-ST-70-11_0600011",1,"Created","The PCB manufacturer shall define during the design together with the supplier the amount of copper and its distribution.\n    NOTE An even distribution is preferred."]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","5.2.3.4f","Requirement","ECSS-Q-ST-70-11_0600036",1,"Created","If tin-lead plating is applied together with gold plating on the same PCB, a tin-lead overlap on gold of minimum 200 mm shall be used on the surface of the PCB.\n    NOTE This is done in order to ensure protection of the plated copper layer."]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","5.5.1d","Requirement","ECSS-Q-ST-70-11_0600069",1,"Created","The supplier shall retain the associated test coupon for at least 10 years or as otherwise specified in the project requirements.\n    NOTE The associated test coupon can be used for supplementary testing."]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","6.2.2d","Requirement","ECSS-Q-ST-70-11_0600078",1,"Created","The nonconformance criteria for the substrate shall be as follows:\n1.\tNot in conformance with PCB manufacturer’s \ntrademark and required quality\t.........................................M\n2.\tScratches cutting glass fibre or leaving marks in the dielectric laminate that are affecting reliability................................M\n3.\tScratches not affecting reliability\t........................................m\n4.\tDents, crazing and haloing:\n(a)\tVisible to the naked eye...................................................................................................................................M\n(b)\tOnly visible with magnification aids...................................................................................................................m\n5.\tNon­homogeneity regarding colouring and opacity......................................................................................................m/M\n6.\tDiscoloured copper oxide layer on internal layer is acceptable\n7.\tInclusion of foreign matter, blistering or air bubbles:\n(a)\tVisible to the naked eye....................................................................................................................................M\n(b)\tOnly visible with magnification aids....................................................................................................................m\n8.\tDelamination..........................................................................................................................................................M\n9.\tMeasling:\n(a)\tGeneral measling spread over the whole PCB surface..........................................................................................M\n(b)\tLocal measling that causes reduction of the insulation distance in the outer layer to below the requirement..............M\n(c)\tLocal measling that does not cause reduction of the insulation distance in the outer layer to below the requirement..m\n10.\tFungus growth;......................................................................................................................................................M\n11.\tDelamination of cover layer (only for flexible PCB)......................................................................................................m/M"]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","6.3.2c","Requirement","ECSS-Q-ST-70-11_0600105",1,"Created","The nonconformance criteria for the thickness of copper plating on external layers shall be as follows:\n1.\tBasic copper:\n(a)\tThickness not conforming to the \nsupplier’s specification\tM\n2.\tBasic copper plus electrolytic copper on non­soldering areas:\n(a)\tThickness < requirement\tM\n3.\tBasic copper plus electrolytic copper soldering pads (see Figure 6-7 number 2):\n(a)\tThickness < 40 mm\tM"]
["ECSS-Q-ST-70-11C","ECSS - Superseded v1.0","7.3e","Requirement","ECSS-Q-ST-70-11_0600138",1,"Created","The limits for the electrical characteristics shall be as follows:\n1.\tInsulation resistance:\n(a)\tIntralayer: ³ 104 MW;\n(b)\tInterlayer: ³ 105 MW;\n(c)\tWith temperature at 80 °C: ³ 102 MW;\n2.\tWithstanding voltage per mm spacing between conductors: 1 000 V r.m.s.;\n3.\tShort time overload: 7 A for 4 s;\n4.\tLong time overload, destructive current: ³ 8 A.\n"]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","6.4a","Requirement","ECSS-Q-ST-70-38_0210020",1,"Created","ECSS-Q-ST-70-08 shall apply for “Precautions against static charges”."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","6.8.2b","Requirement","ECSS-Q-ST-70-38_0210044",1,"Created","Equipment shall apply pastes of a viscosity and quantity such that the positioned device is retained on the board before and during soldering operations, ensuring self-centring and solder fillet formation."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","6.8.7c","Requirement","ECSS-Q-ST-70-38_0210053",1,"Created","The resolution of the X-ray equipment shall be able to detect solder balls having a diameter of 0,03 mm. "]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","7.8.1c","Requirement","ECSS-Q-ST-70-38_0210078",1,"Created","The warp and twist of the printed circuit multilayer board shall be in accordance with ECSS-Q-ST-70-11.\n    NOTE Symmetrical board design reduces warp and twist of the printed circuit board."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","8.1.1a","Requirement","ECSS-Q-ST-70-38_0210111",1,"Created","ECSS-Q-ST-70-08, clause “Preparation of conductors, terminals and solder cups” shall apply."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","8.5c","Requirement","ECSS-Q-ST-70-38_0210120",1,"Created","Baking times and temperatures shall be documented.\n    NOTE 1 Typical baking conditions are from 6 h to 24 h at 125 C depending on the JEDEC classification, except for components delivered in reels for which a lower temperature and longer time are used. \n    NOTE 2 It is good practice to store components under nitrogen, dry air (20 % RH maximum) or partial vacuum."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","9.7.9a","Requirement","ECSS-Q-ST-70-38_0210147",1,"Created","Staking compounds shall be selected in conformance with clause 7.10."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","11.8a","Permission","ECSS-Q-ST-70-38_0210284",1,"Created","Underfill beneath area arrays may be applied if it does not restrict the possibility of device removal.\n    NOTE 1 For power dissipation thermal adhesive can be used provided that it does not contravene the requirement of this standard (see ESA STM-265 for suitable silicone product) [2].\n    NOTE 2 Underfill has been observed to promote thermal fatigue of soldered connections during thermal cycling (see ESA STM-266 [4])."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","14.2h","Requirement","ECSS-Q-ST-70-38_0210210",1,"Created","Side-brazed, top-brazed and bottom-brazed packages shall be considered as different families."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","14.10b","Requirement","ECSS-Q-ST-70-38_0210235",1,"Created","In the case of visual failures, an analysis shall be performed to identify the cause: component or soldering process."]
["ECSS-Q-ST-70-38C","ECSS - Superseded v1.0","14.11d","Requirement","ECSS-Q-ST-70-38_0210244",1,"Created","Reference to the summary table number shall be made on each space project declared processes list in order to assist in achieving project approval. \n    NOTE See ECSS-Q-ST-70, Table D-3."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-Q-ST-20_0380008",1,"Unchanged","The supplier shall implement a nonconformance control system in conformance with ECSS-Q-ST-10-09."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.2.7.2b","Requirement","ECSS-Q-ST-20_0380041",2,"Normative Change","The supplier shall place the following items in designated segregated areas:\n1.\tlimited life materials,\n2.\tsuspended limited life materials,\n3.\tnonconforming items awaiting NRB disposition,\n4.\tscrapped items,\n5.\titems designated to be stored separately for health or safety reasons."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.3.2.4.2c","Requirement","ECSS-Q-ST-20_0380068",1,"Unchanged","The need for complementary qualification tests shall be analysed and the decision justified and submitted to the customer for approval."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.3.2.4.4a","Requirement","ECSS-Q-ST-20_0380072",1,"Unchanged","The supplier shall report the qualification status in conformance with the “Qualification status list” DRD as defined in ECSS-Q-ST-10."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.5.3.1b","Requirement","ECSS-Q-ST-20_0380105",2,"Informative Change","The supplier shall ensure that all manufacturing processes are covered by documented process specifications or standards.\nNOTE \tThe definition of manufacturing process specifications is given in ECSS-Q-ST-70."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.5.7.3a","Requirement","ECSS-Q-ST-20_0380130",1,"Unchanged","The supplier shall develop detailed methods for attaining the cleanliness levels specified for the hardware."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.6.3.2a","Requirement","ECSS-Q-ST-20_0380160",1,"Unchanged","The supplier shall ensure that all tests are comprehensively documented in test reports, and that they include, as a minimum:\n1.\treference to the applicable test procedure, and description of the deviations from it during the actual testing,\n2.\ttest data records and evaluation, and\n3.\tsummary of test results."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.6.5a","Requirement","ECSS-Q-ST-20_0380169",2,"Normative Change","The supplier shall ensure that reviews are performed before  and after defined points during qualification or acceptance tests.\nNOTE \t1\tTest Reviews are defined in ECSS-E-ST-10-03.\nNOTE \t2\tReviews before tests are called Test Readiness Reviews and reviews after tests are called Post Test Reviews or Test Review Boards."]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","5.8.1.1.1b","Requirement","ECSS-Q-ST-20_0380235",1,"Created","<< deleted, requirement moved to 5.8.1b >>"]
["ECSS-Q-ST-20C Rev.1","ECSS - Superseded v1.0","C.2.1b","Requirement","ECSS-Q-ST-20_0380216",1,"Unchanged","The logbook shall contain the “hardware configuration and traceability” table, which reports all the identification references of single elements composing the CI. "]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","4.1.2a","Requirement","ECSS-Q-ST-70_0490001",2,"Normative Change","The supplier shall prepare, maintain and implement a MMPP plan, as part of the overall PA plan in conformance with DRD from Annex A of ECSS-Q-ST-10 and this Standard or as a separate document."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","4.2.3g","Requirement","ECSS-Q-ST-70_0490018",2,"Normative Change","The as­designed lists shall include the items from the baselines various design files, available for CDR."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","5.1.5c","Requirement","ECSS-Q-ST-70_0490209",1,"Created","For materials for the use in manned compartments of a spacecraft or space segment elements, offgassing and toxicity analysis shall be performed."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","5.1.14c","Requirement","ECSS-Q-ST-70_0490220",1,"Created","Micrometeoroids and debris analysis and test procedures shall be subject to the approval by the customer."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","5.4.2a","Requirement","ECSS-Q-ST-70_0490064",1,"Unchanged","The supplier shall analyse all the materials contained in his preliminary lists with respect to criticality and in correlation with the risk analysis performed. "]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","5.7.2a","Requirement","ECSS-Q-ST-70_0490088",2,"Normative Change","The supplier shall apply the traceability rules specified in the requirements from clause 5.2.5 of ECSS-Q-ST-20 to all materials."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","5.7.7a","Requirement","ECSS-Q-ST-70_0490096",1,"Unchanged","Material safety data sheet or equivalent shall be available for all materials."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","6.7.1a","Requirement","ECSS-Q-ST-70_0490126",1,"Unchanged","The supplier shall ensure that all critical parts are qualified before being used in the manufacture of qualification or flight products."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","7.3n","Requirement","ECSS-Q-ST-70_0490263",1,"Created","Standards relating to the occupational health of operators working with processes resulting in exposure to vapours, dust or debris shall be implemented and controlled."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","7.6.1b","Permission","ECSS-Q-ST-70_0490275",1,"Created","In case of an extension of an existing application, the evaluation specified in requirement 7.6.1a need not be performed if so agreed with the customer."]
["ECSS-Q-ST-70C Rev.1","ECSS - Superseded v1.0","C.2.1<1>a","Requirement","ECSS-Q-ST-70_0490178",1,"Unchanged","The DPL shall contain the following statements:\nProcesses are classified into 17 groups depending on their type or their main use, see Table C-1."]
["ECSS-Q-ST-70-05C","ECSS - Superseded v1.0","5.1.5.2b","Requirement","ECSS-Q-ST-70-05_0540018",1,"Created","The sample holder shall be aligned so that the infrared beam is positioned in the centre of the IR transparent window."]
["ECSS-Q-ST-70-05C","ECSS - Superseded v1.0","5.2.3.3i","Requirement","ECSS-Q-ST-70-05_0540035",1,"Created","The Petri dish containing the contaminated solvent shall be processed in conformance with 5.2.3.2.\n    NOTE For details of the wiping process see Annex F."]
["ECSS-Q-ST-70-05C","ECSS - Superseded v1.0","5.4.3.2d","Requirement","ECSS-Q-ST-70-05_0540059",1,"Created","Each point shall be measured at least three times, possibly with different windows in order to eliminate systematic errors."]
["ECSS-Q-ST-70-05C","ECSS - Superseded v1.0","5.4.5.3c","Requirement","ECSS-Q-ST-70-05_0540084",1,"Created","Once the positioning or transfer of the solution can be performed within the accepted limits, the trainee operator shall start to produce the calibration curves.\n    NOTE For the calibration curves see Annex C.3."]
["ECSS-Q-ST-70-31C","ECSS - Superseded v1.0","4.2.2.3b","Requirement","ECSS-Q-ST-70-31_0660021",1,"Created","These samples shall be of the same material and be surface treated in the same manner as the workpiece."]
["ECSS-Q-ST-70-31C","ECSS - Superseded v1.0","4.3.1.2b","Requirement","ECSS-Q-ST-70-31_0660046",1,"Created","Surfaces shall be free of dust and grease.\n    ","NOTE This can be achieved by standard cleaning procedures or by the manufacturer cleaning method."]
["ECSS-Q-ST-70-31C","ECSS - Superseded v1.0","4.3.1.3f","Requirement","ECSS-Q-ST-70-31_0660055",1,"Created","Adhesive bonding on surfaces to be coated shall be completed before paint application."]
["ECSS-Q-ST-70-31C","ECSS - Superseded v1.0","4.4f","Requirement","ECSS-Q-ST-70-31_0660100",1,"Created","Outgassing properties shall be measured according to ECSS-Q-ST-70-02."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.2c","Requirement","ECSS-Q-ST-70-71_1260005",1,"Created","Long-term manned structures, shall not use aluminium alloys 2024-T6, 7079-T6 and 7178-T6 in structural applications."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.9e","Requirement","ECSS-Q-ST-70-71_1260038",1,"Created","The design of parts made of beryllium alloys shall include the material’s low impact resistance, notch sensitivity, its anisotropy and sensitivity to surface finish requirements."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.10c","Requirement","ECSS-Q-ST-70-71_1260047",1,"Created","When organic glasses are used, a radiation resistance assessment shall be performed."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.12j","Requirement","ECSS-Q-ST-70-71_1260071",1,"Created","Surfaces that have had tapes removed for reworking or for temporary reasons shall be cleaned after the tape is removed. \n","NOTE\tAdhesives, in particular silicone ones, can leave a residue which prevents adhesion of other systems onto that surface."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.17b","Requirement","ECSS-Q-ST-70-71_1260104",1,"Created","Polysulphide materials shall not be used in the space environment."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.18n","Requirement","ECSS-Q-ST-70-71_1260128",1,"Created","Polyamide films shall be assessed for moisture-related effects."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.2.20d","Requirement","ECSS-Q-ST-70-71_1260141",1,"Created","The materials for coaxial cable assembly shall be selected in conformance with requirements from clause 5 of ECSS-Q-ST-70-18."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.3.6d","Requirement","ECSS-Q-ST-70-71_1260169",1,"Created","The selection of welding techniques shall be performed in conformance with the requirement from clause 5 to 13 of ECSS-Q-ST-70-39."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.3.9.2c","Requirement","ECSS-Q-ST-70-71_1260194",1,"Created","Anodized layers shall be sealed and be continuous when used as the final surface finish of a part."]
["ECSS-Q-ST-70-71C","ECSS - Superseded v1.0","4.3.15.3a","Requirement","ECSS-Q-ST-70-71_1260227",1,"Created","Design of printed circuit board shall conform to the requirements from clause 5 to 15 of ECSS-Q-ST-70-12."]
["ECSS-Q-ST-60-14C","ECSS - Superseded v1.0","4.1.7a","Requirement","ECSS-Q-ST-60-14_0470010",1,"Created","The storage responsible entity shall establish and document the following:\n    1. Prohibited materials\n    2. Personnel access rules\n    3. Prohibited personnel actions\n    4. Measures and facilities to segregate and protect components during receiving, inspection, storage and delivery\n    5. Control measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60-14C","ECSS - Superseded v1.0","6.1.1b","Requirement","ECSS-Q-ST-60-14_0470019",1,"Created","Component families not covered in Table 6-1 shall be subject to special procedures to be defined by the program.\n    ","NOTE The relifing procedure can be applied on a sub-lot containing only the quantity of components immediately needed for production. In this case, the relifing date-code is applicable only to parts actually tested. The time limits specified in Table 5-1 remain applicable for the residual sub-lot."]
["ECSS-Q-ST-60-14C","ECSS - Superseded v1.0","6.1.5b","Requirement","ECSS-Q-ST-60-14_0470037",1,"Created","The measurement values of leaks on non-conforming components shall be recorded in the relifing report."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.2.1b","Requirement","ECSS-Q-ST-60_0480491",1,"Created","The selection, evaluation and approval of commercial EEE components for class 1 programmes shall be performed in conformance with clause 4.2 from ECSS-Q-ST-60-13."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.2.2.2c","Requirement","ECSS-Q-ST-60_0480030",2,"Normative Change","With respect to health and safety, beryllium oxide (except if identified in the procurement specification), cadmium, lithium, magnesium, mercury, zinc, radioactive material and all material which can cause safety hazards shall not be used."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.2.3.3b","Requirement","ECSS-Q-ST-60_0480063",1,"Unchanged","The Constructional Analysis shall comprise destructive and non-destructive inspections, analyses, and testing, to identify:\n    1. Design and construction technology,\n    2. Materials used,\n    3. Inherent reliability aspects,\n    4. Quality of workmanship,\n    5. Potential hazards."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.3.3b","Requirement","ECSS-Q-ST-60_0480087",2,"Normative Change","The screening test requirements shall be defined such that accumulated stress does not jeopardize component reliability. "]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.3.9g","Permission","ECSS-Q-ST-60_0480499",1,"Created","Independent laboratories may perform DPA when approved by the customer."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.5.4e","Requirement","ECSS-Q-ST-60_0480141",2,"Normative Change","If the as built DCL has not yet been delivered, the supplier shall be able to provide this information (part type actually installed with its relevant lot/date code number) within one week."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","4.6.4b","Requirement","ECSS-Q-ST-60_0480148",1,"Unchanged","The PAD shall allow traceability to the information related to the procurement of blank parts, the programming process and the acceptance of the programmed parts.","NOTE The programming process and the acceptance of the programmed parts are under the authority of the PCB if not otherwise determined in the PAD."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.2.2.1d","Requirement","ECSS-Q-ST-60_0480179",1,"Unchanged","When selecting items, the supplier shall check the current data, applicability of the basis of qualification, problem notifications and alerts, and adequacy of specifications. "]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.2.3.1f","Requirement","ECSS-Q-ST-60_0480204",1,"Unchanged","Omission of any of these elements, or the introduction of alternative activities, shall be justified."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.2.3.4a","Requirement","ECSS-Q-ST-60_0480213",1,"Unchanged","The evaluation shall determine which inspections or tests are required to provide the confidence that the component type under evaluation, when assembled and tested in accordance with the procurement specification, successfully meets the project requirements."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.3.5b","Requirement","ECSS-Q-ST-60_0480459",2,"Normative Change","The sample size for lot acceptance which may be reduced in some cases, shall be submitted to the customer for approval through the PAD process (see clause 5.2.4)."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.3.10b","Requirement","ECSS-Q-ST-60_0480267",1,"Unchanged","For components meeting the above criteria, and which have a lot / date code exceeding the period defined in ECSS-Q-ST-60-14 clause 5, the relifing procedure ECSS-Q-ST-60-14 shall apply."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","5.5.3b","Requirement","ECSS-Q-ST-60_0480281",1,"Unchanged","If alerts become available at a later stage, the supplier shall analyse the alerts, analyse the project risk and propose an action plan for customer approval. "]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.2.2.2b","Requirement","ECSS-Q-ST-60_0480321",1,"Unchanged","The supplier shall evaluate the robustness of selected EEE components against the stresses induced by the assembly techniques to be employed."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.2.2.4b","Requirement","ECSS-Q-ST-60_0480330",1,"Unchanged","The supplier who is responsible for the design of the piece of hardware shall demonstrate the compliance of its components selection with the radiation constraints of the project. "]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.3.1b","Requirement","ECSS-Q-ST-60_0480363",1,"Unchanged","Class 3 components shall meet the quality levels and supplementary conditions specified in Table 7-3."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.3.7c","Requirement","ECSS-Q-ST-60_0480384",1,"Unchanged","The incoming inspection shall be documented by a procedure to be presented, on request, to the customer for review."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.3.9b","Permission","ECSS-Q-ST-60_0480516",1,"Created","DPA may be carried out on representative samples of the components families when the following three conditions are met:\n    1. procured from the same manufacturer and same package without major change in the process,\n    2. with a limited datecode range of 13 weeks,\n    3. approved by the customer through the PAD (or Justification document) process.","NOTE In complement of above conditions, for series of integrated circuits, series of thermal switches, series of active discrete and series of passive components (e.g. 54xxxx, 1N63xx, …), representative samples can be from the same family considering technology limit and their complexity."]
["ECSS-Q-ST-60C Rev. 2","ECSS - Superseded v1.0","6.5.4a","Requirement","ECSS-Q-ST-60_0480418",1,"Unchanged","The traceability of individual components during manufacturing and testing shall be maintained as required by the procurement specifications."]
["ECSS-Q-ST-70-07C","ECSS - Superseded v1.0","5.1.2b","Requirement","ECSS-Q-ST-70-07_0560004",1,"Created","The supplier shall maintain a solder joint discrepancy log in conformance with the DRD in Annex A.\n    NOTE This is an aid to process control, optimization of parameters and repeatability."]
["ECSS-Q-ST-70-07C","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-70-07_0560040",1,"Created","A new verification test programme shall be carried out whenever a change to the PID is proposed."]
["ECSS-Q-ST-70-07C","ECSS - Superseded v1.0","A.2.1a","Requirement","ECSS-Q-ST-70-07_0560065",1,"Created","The solder joint discrepancy log shall contain, for each PCB assembly that has been wave soldered with the soldering machine, the measurements of the following process control parameters: \n    1. the preheat temperature,\n    2. the conveyer speed,\n    3. the solder temperature and, \n    4. the height of the wave."]
["ECSS-Q-ST-70-07C","ECSS - Superseded v1.0","B.2.1h","Requirement","ECSS-Q-ST-70-07_0560074",1,"Created","As part of the technology sample documentation, the following information shall be provided: \n    1. type of components,\n    2. list of used materials, \n    3. description of processes including machine parameters,\n    4. summary of cleanliness test results in conformance with clause 11 of ECSS-Q-ST-70-08 or equivalent method."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","5.5.2b","Requirement","ECSS-Q-ST-70-08_0570023",1,"Created","The working bench shall have a static dissipative top resistance to ESD protected area ground (Rg) in the range 7,5 ´ 105 Ω to 1 ´ 109 Ω."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","5.6.3d","Requirement","ECSS-Q-ST-70-08_0570048",1,"Created","Cutting edges shall be checked for damage and maintained in a sharp condition."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","5.6.6.3b","Permission","ECSS-Q-ST-70-08_0570546",1,"Created","The enamel may be removed by mechanical means provided that visual inspection using a minimum magnification of x40 is carried out to ensure that the conductor is undamaged."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","6.1c","Permission","ECSS-Q-ST-70-08_0570550",1,"Created","Electrical/electronic components identified as having plated or metallized external surfaces with a tin finish containing more than 97 % tin may be pretinned with a tin-lead solder in accordance with 6.2.2b.\n    NOTE Tin whisker mitigation (barrier methods such as coating or sleeving) is addressed in the framework of an NRB or Approval Authority."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","6.5b","Permission","ECSS-Q-ST-70-08_0570554",1,"Created","The following flexible insulation materials may be used in a space environment:\n    1. ETFE, FEP and PTFE.\n    2. Polyolefin and Kynar® sleeving for heat-shrinkable wire terminations.\n    3. Irradiated polyethylene, fluorinated resin and polyimide."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","7.2.1.1a","Requirement","ECSS-Q-ST-70-08_0570147",1,"Created","Stripping tools or machines shall be in accordance with clause 5.6.6."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","7.2.3.2.2a","Requirement","ECSS-Q-ST-70-08_0570172",1,"Created","Solder baths used for degolding and pretinning shall be in accordance with Table 7-2."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","7.2.3.2.4b","Requirement","ECSS-Q-ST-70-08_0570181",1,"Created","Solder shall be wicked-out using stranded wire."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","7.3.2b","Requirement","ECSS-Q-ST-70-08_0570206",1,"Created","Plated tips shall be examined for cracking.\n    NOTE Cracked platings allow the liquid solder to alloy with and erode the underlying copper, forming intermetallics which reduce heat transfer and lead to unacceptable joints."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","7.7.3a","Requirement","ECSS-Q-ST-70-08_0570231",1,"Created","The demoisturization process shall be carried out again according to clause 7.7.2 when prepared PCBs are stored in ambient conditions for more than 8 hours prior to soldering."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","8.1.5c","Requirement","ECSS-Q-ST-70-08_0570247",1,"Created","The assembly of TO-39, TO-59 and CKR-06 packages shall be performed in accordance with Figure 8-1 when assembled without stress relief."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","8.3c","Requirement","ECSS-Q-ST-70-08_0570272",1,"Created","The PCB shall not be damaged by the swaging process."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","9.1.2b","Requirement","ECSS-Q-ST-70-08_0570305",1,"Created","Terminals shall be selected to fit the conductors."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","9.4.6a","Requirement","ECSS-Q-ST-70-08_0570338",1,"Created","The bottom route conductor shall be installed before the side route conductor."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","9.9.2c","Requirement","ECSS-Q-ST-70-08_0570363",1,"Created","Pretinning shall be in accordance with clauses 7.2.5 and 7.2.6 ."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","9.9.4.1b","Requirement","ECSS-Q-ST-70-08_0570372",1,"Created","The sleeving shall be cut to a length that covers the finished soldered joint and extends over the remaining insulation of each conductor for a distance of 5 mm ±2 mm."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","10.2.2a","Requirement","ECSS-Q-ST-70-08_0570404",1,"Created","A concave fillet of solder shall be present between the terminal and the sides of the conductor."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","10.4a","Requirement","ECSS-Q-ST-70-08_0570429",1,"Created","Soldering aids shall be used to restrict the wicking of flux or solder under insulation in accordance with clause 5.6.8.4."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","11.2a","Requirement","ECSS-Q-ST-70-08_0570438",1,"Created","Ultrasonic cleaning shall not be used for PCBs populated with components."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","13.2b","Requirement","ECSS-Q-ST-70-08_0570463",1,"Created","The PCB design and mounting (including fittings such as stiffeners, frames or spacers) shall be representative of the flight model."]
["ECSS-Q-ST-70-08C","ECSS - Superseded v1.0","14.8a","Requirement","ECSS-Q-ST-70-08_0570496",1,"Created","Trained and certified personnel shall be employed for soldering operations and inspections."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","5.4.2e","Requirement","ECSS-Q-ST-30-11_0140016",1,"Created","As an exception in case clause 5.4.2c is not compatible for specific repeated and incessant transient use conditions, for the parts types and parameters listed, load ratio shall not exceed the steady state derated values +10 % or 80 % of the steady state rated values, which ever is lower:\n\t1.\tConnectors: voltage, current\n\t2.\tCeramic Capacitors: voltage\n\t3.\tResistors: current \n\t4.\tDiodes: current\n\t5.\tTransistors_ bipolar , MOSFETs, power FETs: current."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","6.3.2a","Requirement","ECSS-Q-ST-30-11_0140027",1,"Created","Parameters of capacitors from family-group code 01-03 shall be derated as per Table 6-2."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","6.10.1a","Recommendation","ECSS-Q-ST-30-11_0140173",1,"Created","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature. Where ESR is not known at the frequency of a ripple current, an extrapolation of the ESR value and resonance (from manufacturer’s or test data) should be made where possible."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","6.17.3c","Requirement","ECSS-Q-ST-30-11_0140080",1,"Created","The power supply shall be capable of delivering three times the specified fuse rated current in order to obtain short fusing times."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","6.26.2.8b","Requirement","ECSS-Q-ST-30-11_0140127",1,"Created","Parameters of heaters shall be derated as per Table 6-31."]
["ECSS-Q-ST-30-11C Rev.1","ECSS - Superseded v1.0","6.30.2a","Requirement","ECSS-Q-ST-30-11_0140137",1,"Created","Parameters of Transistors from family-group code 12-10 and 12-13 shall be derated as per Table 6-35."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.1.3b","Requirement","ECSS-Q-ST-60-13_0460008",1,"Created","At supplier's level, the Parts Control Board (PCB) shall be composed as follows:\n    1. chaired by a member of the supplier’s PA team with designated responsibility for components management,\n    2. include, as a minimum, in addition the suppliers’ parts engineer, the customer’s representative and the lower tier subcontractor parts engineers."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.2.2.4b","Requirement","ECSS-Q-ST-60-13_0460040",1,"Created","The supplier who is responsible for the design of the piece of hardware shall demonstrate the compliance of its components selection with the radiation constraints of the project."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.2.3.3b","Requirement","ECSS-Q-ST-60-13_0460063",1,"Created","The Construction analysis shall be documented by a procedure to be sent to the customer for approval.","NOTE Annex H provides guidelines for such procedure."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.3.3d","Requirement","ECSS-Q-ST-60-13_0460089",1,"Created","For commercial parts, screening tests shall be performed in accordance with Table 4-2."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.3.7b","Requirement","ECSS-Q-ST-60-13_0460101",1,"Created","The incoming inspection shall include the following items:\n    1. For any part:\n        (a) Marking control,\n        (b) Quantity verification,\n        (c) Packing checking,\n        (d) Review of the manufacturer delivered documentation,\n        (e) Additional tests based on the type of component, criticality and heritage with the manufacturer (e.g. solderability tests, electrical tests),\n        (f) In case of not golden termination finish, check the lead finish as per ESCC 25500 basic specification.\n    2. For the non-space qualified parts, when the final customer source inspection has not been performed, the following additional items: \n        (a) External visual inspection by sampling (AQL 0,65% level II or 20 parts min) \n        (b) Electrical measurements at room temperature on 20 parts or 100% (if lot size < 20 parts), or a datapackage review. "]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","4.4d","Requirement","ECSS-Q-ST-60-13_0460128",1,"Created","As a minimum, the following areas shall be covered:\n    1. Control of the environment in accordance with ESCC Basic Specification No. 24900.\n    2. Measures and facilities to segregate and protect components during receiving inspection, storage, and delivery to manufacturing. \n    3. Control measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.1.3d","Requirement","ECSS-Q-ST-60-13_0460164",1,"Created","Depending on the progress of the program, the main PCB activities shall be:\n    1. Review and approval of the supplier's compliance matrix to the clause of section 5 of this standard and any associated documents\n    2. Parts approval including evaluation activities,\n    3. Problem assessment (e.g. alerts, nonconformances, RFD, RFW and  delivery delays).\n    4. Upon customer’s request, assessment activities (by sampling) including: \n        (a) conformity of procurement conditions, \n        (b) conformity of procurement data,\n        (c) post-procurement data, and\n        (d) application of alerts recommendations","NOTE 1 Customer request depends on from the criticality of the equipment or supplier.\nNOTE 2 For (a) to (c), assessment of the procurement conditions, conformity of procurement and post-procurement data is performed versus approval document."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.1.5a","Requirement","ECSS-Q-ST-60-13_0460173",1,"Created","EEE components used in GSE, which are physically and directly interfacing to flight hardware, shall be:\n    1. Fit Form and Function compatible, \n    2. manufactured from materials identical to the flight opposite part, and\n    3. ensured to be visibly clean before each connection to flight hardware."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.2.3.1b","Requirement","ECSS-Q-ST-60-13_0460200",1,"Created","The supplier shall plan and carry out the evaluation."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.2.4d","Requirement","ECSS-Q-ST-60-13_0460218",1,"Created","Prior to procurement of components (or before equipment CDR at the latest), the approval process by the customer shall be organized as follows:\n    1. A Justification Document is required in accordance with annex F."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.3.3j","Requirement","ECSS-Q-ST-60-13_0460519",1,"Created","If modification of 5.3.3f is proposed to the customer, it shall meet the following similarity criteria:\n1.\tFor EFR, either:\n(a) \tthe data are as the same die revision, wafer fab, process and package.\n(b) \tthe data are not provided, but in this case the data on the same part type is not older than two years w.r.t date code.\n2.\tFor lifetest, either:\n(a)\tthe data are as the same die revision, wafer fab, process and pacakge.\n(b) \tthe data are not provided, but in this case the data on the same part type is not older thant two years w.r.t date code.\n3.  For thermal cycles the data are on same package."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.4e","Requirement","ECSS-Q-ST-60-13_0460531",1,"Created","Plastic encapsulated devices shall be stored in one of the following conditions:\n1.\tDry Nitrogen\n2.\tDry and ionised air with RH in a range of 15% to 20%\n3. \tDry packs as specified in J-STD-033 for dry pack inspection and control"]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","5.5.4b","Requirement","ECSS-Q-ST-60-13_0460283",1,"Created","The traceability shall be maintained through incoming, storage, and installation at the procurer and user of the component in accordance with programme PA requirements. "]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.1.4g","Requirement","ECSS-Q-ST-60-13_0460312",1,"Created","The content of the DCL shall be in conformance with the DRD in Annex B."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.2.3.1a","Requirement","ECSS-Q-ST-60-13_0460340",1,"Created","For class 3 components, the evaluation shall be limited to construction analysis and radiation tests."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.3.1g","Requirement","ECSS-Q-ST-60-13_0460543",1,"Created","Each trace code shall be maintained as is through the entire supply chain including distributor.","NOTE As far as possible, commercial parts should be ordered in the manufacturer’s standard packing quantities or multiples thereof to avoid distributor re-packing and handling and to preserve the traceability information usually included on the original manufacturer packaging."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.3.3c","Requirement","ECSS-Q-ST-60-13_0460375",1,"Created","All screening tests shall be performed at the component manufacturer’s premises or at a facility approved either by the qualification approval authority, where applicable (e.g. ESCC), or otherwise by the supplier ."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.4c","Requirement","ECSS-Q-ST-60-13_0460409",1,"Created","On request, handling and storage procedures shall be sent to the customer for review."]
["ECSS-Q-ST-60-13C","ECSS - Superseded v1.0","6.7a","Requirement","ECSS-Q-ST-60-13_0460436",1,"Created","Any result from inspection or control shall be documented (including lot acceptance, incoming, relifing and complementary tests)."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","6.1a","Requirement","ECSS-Q-ST-70-38_0210017",2,"Normative Change","The supplier shall maintain records of tool calibration and verification."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","6.6.4a","Requirement","ECSS-Q-ST-70-38_0210025",2,"Normative Change","Requirements from clause 5.6.5 from ECSS-Q-ST-70-08 shall apply \"Clinching tools\"."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","6.8.6a","Requirement","ECSS-Q-ST-70-38_0210050",1,"Unchanged","Clause 13.1 shall apply."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","7.8c","Requirement","ECSS-Q-ST-70-38_0210290",1,"Created","Printed Circuit Boards shall be procured in conformance with the requirements of clauses 5 and 6 of ECSS-Q-ST-70-11."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","7.9.2b","Requirement","ECSS-Q-ST-70-38_0210094",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","7.10a","Requirement","ECSS-Q-ST-70-38_0210103",2,"Normative Change","Adhesives shall be dispensable, non-stringing, and have a reproducible dot profile after application. "]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","9.5a","Requirement","ECSS-Q-ST-70-38_0210125",2,"Normative Change","Requirements from clause 8.5 from ECSS-Q-ST-70-08 shall apply for \"Mounting of components to terminals\"."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","9.7.7a","Requirement","ECSS-Q-ST-70-38_0210145",2,"Normative Change","Surface mounting of leaded (round or rectangular cross section) devices shall be parallel to the board surface."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","11.5.3a","Requirement","ECSS-Q-ST-70-38_0210167",2,"Normative Change","Devices having metallized terminations on the bottom side only  shall meet the dimensional and solder fillet requirements of Table 11-2 and Figure 11-2."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","11.5.8a","Requirement","ECSS-Q-ST-70-38_0210172",2,"Normative Change","The outer row of solder joints to area array devices shall be visually inspected by looking from the side in accordance with the requirements in 11.5.1 and Table 11-8 and with the rejection criteria specified in clauses 13.3 and 13.4."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","13.1d","Requirement","ECSS-Q-ST-70-38_0210184",2,"Normative Change","Devices and conductors shall not be physically moved to aid inspection."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.1u","Requirement","ECSS-Q-ST-70-38_0210364",1,"Created","Sensitive devices shall be submitted to re-verification every four years to monitor the stability of the assembly."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.3c","Requirement","ECSS-Q-ST-70-38_0210375",1,"Created","Removal and replacement shall be verified on the repair assembly method."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.3l","Requirement","ECSS-Q-ST-70-38_0210383",1,"Created","The supplier shall organise a Mandatory inspection point (MIP1) with the Approval Authority prior to any conformal coating with five days notification.","NOTE\tThe Approval Authority can delegate the MIP1 to the supplier.\n"]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.6c","Requirement","ECSS-Q-ST-70-38_0210220",2,"Normative Change","The monitoring temperature sensor shall be attached to the surface of the printed circuit board."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.8a","Requirement","ECSS-Q-ST-70-38_0210227",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.10a","Requirement","ECSS-Q-ST-70-38_0210234",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.13f","Requirement","ECSS-Q-ST-70-38_0210461",1,"Created","A delta-verification programme in accordance with the DRD from Annex G shall be submitted for approval to the Approval Authority."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","14.15.2a","Requirement","ECSS-Q-ST-70-38_0210469",1,"Created","The technology sample shall be inspected by the Approval Authority in accordance with the requirements from clause 13."]
["ECSS-Q-ST-70-38C Rev.1 Corr.1","ECSS - Superseded v1.0","F.2.1<4>a","Requirement","ECSS-Q-ST-70-38_0210485",1,"Created","The PID shall contain the following information about Organisation:\n1.\tRepresented as a flow chart: organization of the company, organization of production department and organization of the quality Department,\n2.\tFocal point and PID responsible,\n3.\tOperators and inspectors’ certification methodology."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.1.4f","Requirement","ECSS-Q-ST-60_0480016",2,"Unchanged","Any change of parts during equipment manufacturing (e.g. type and manufacturer) shall be handled through RFWs submitted to the customer for approval before mounting."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.2.1b","Requirement","ECSS-Q-ST-60_0480491",1,"Unchanged","The selection, evaluation and approval of commercial EEE components for class 1 programmes shall be performed in conformance with clause 4.2 from ECSS-Q-ST-60-13."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.2.2.4f","Requirement","ECSS-Q-ST-60_0480044",1,"Unchanged","The supplier shall identify components which are not compliant with the radiation requirements as critical radiation sensitive components. "]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.2.3.3c","Requirement","ECSS-Q-ST-60_0480064",1,"Unchanged","The findings of the analysis shall be contained within a Constructional Analysis Report and shall be included in the Evaluation Report."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.3.3d","Requirement","ECSS-Q-ST-60_0480089",2,"Unchanged","The quality levels defined in Table 7-1 shall apply."]
["ECSS-Q-ST-60-13C Rev.1","ECSS - Superseded v1.0","4.3.8f","Requirement","ECSS-Q-ST-60-13_0460495",2,"Normative Change"]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.3.9i","Requirement","ECSS-Q-ST-60_0480118",1,"Unchanged","For health and safety reasons, any test producing beryllium oxide dust shall be omitted."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","4.6.4b","Requirement","ECSS-Q-ST-60_0480148",1,"Unchanged","The PAD shall allow traceability to the information related to the procurement of blank parts, the programming process and the acceptance of the programmed parts.","NOTE \tThe programming process and the acceptance of the programmed parts are under the authority of the PCB if not otherwise determined in the PAD.\n"]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.1.4h","Requirement","ECSS-Q-ST-60_0480172",1,"Unchanged","The content of the DCL shall be in conformance with its DRD in Annex B."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.2.2.2i","Requirement","ECSS-Q-ST-60_0480534",1,"Created","The customer shall specify either requirement 5.2.2.2j, or requirements 5.2.2.2k and 5.2.2.2l to handle risks linked with pure-tin terminations."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.2.3.1a","Requirement","ECSS-Q-ST-60_0480199",1,"Unchanged","The supplier shall perform a component evaluation in absence of an approved demonstration that a component has the ability to conform to the requirements for functional performance, quality, dependability, and environmental resistance as required for the project."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.2.4d","Requirement","ECSS-Q-ST-60_0480218",3,"Deleted","The approval process by the customer depends on the part qualification status and shall be organized as follows:\n1.\tSpace qualified parts : Space qualified parts listed in the DCL are approved through the DCL review except in the following cases where a PAD in conformance with ECSS-Q-ST-60 Annex D is delivered for customer's approval:\n(a)\tadditional controls are required (e.g. precap, buy-off, LAT or LVT, RVT, DPA),\n(b)\tused outside the specified limits,\n(c)\tspecific tests are required during procurement as per Table 7-1,\n2.\tOther HiRel parts: A PAD in accordance with ECSS-Q-ST-60 Annex D is delivered to customer for approval.\n3.\tCommercial parts: A Justification Document in accordance with ECSS-Q-ST-60-13 Annex F is delivered to customer for approval.\n4.\t<<deleted>>"]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.3.5b","Requirement","ECSS-Q-ST-60_0480459",2,"Unchanged","The sample size for lot acceptance which may be reduced in some cases, shall be submitted to the customer for approval through the PAD process (see clause 5.2.4)."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.3.9i","Requirement","ECSS-Q-ST-60_0480265",1,"Unchanged","The results of DPA shall be documented by a report sent to the customer, on request, for information."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.4d","Requirement","ECSS-Q-ST-60_0480274",1,"Unchanged","As a minimum, the following areas shall be covered:\n1.\tControl of the environment in accordance with ESCC Basic Specification No. 24900.\n2.\tMeasures and facilities to segregate and protect components during receiving inspection, storage, and delivery to manufacturing. \n3.\tControl measures to ensure that electrostatic discharge susceptible components are identified and handled only by trained personnel using anti static packaging and tools."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","5.6.4e","Requirement","ECSS-Q-ST-60_0480295",3,"Normative Change","For one time programmable FPGA and PROM  without a clear and defined heritage, a post-programming burn-in shall be applied, in conformance with ESCC9000 subclause 8.16, for a minimum duration of 160 h.","NOTE \tFPGA and PROM  with defined heritage are documented in these reports: ESCC REP 010 and ESCC REP011, available on https://escies.org.\n"]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","6.2.2.2e","Requirement","ECSS-Q-ST-60_0480324",2,"Normative Change","For limited life duration, known instability, safety hazard or reliability risk reasons, the use of EEE components listed below shall not be used for new designs:\n1.\tRNC90 > 100 kOhm,\n2.\tTO3 and DO4/DO5 packages,\n3.\tWire link fuses."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","6.2.2.3a","Requirement","ECSS-Q-ST-60_0480318",1,"Unchanged","Preference shall be given to components which necessitate the least evaluation or qualification effort."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","6.2.3.1h","Requirement","ECSS-Q-ST-60_0480347",1,"Unchanged","For programmable devices, the representativeness shall include the programming hardware tools and the compatibility of the software."]
["ECSS-Q-ST-60-13C Rev.1","ECSS - Superseded v1.0","6.3.2h","Requirement","ECSS-Q-ST-60-13_0460545",1,"Unchanged"]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","6.3.9i","Requirement","ECSS-Q-ST-60_0480401",2,"Normative Change","The results of DPA shall be documented by a report sent to the customer, on request, for information."]
["ECSS-Q-ST-60C Rev. 3","ECSS - Superseded v1.0","6.6.2a","Requirement","ECSS-Q-ST-60_0480425",2,"Unchanged","ECSS-Q-60-02 shall apply. "]
["ECSS-Q-ST-60-13C Rev.1","ECSS - Superseded v1.0","8.2a","Requirement","ECSS-Q-ST-60-13_0460698",1,"Created"]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","5.2.1.1a","Requirement","ECSS-Q-ST-80_0720013",1,"Unchanged","The supplier shall develop a software product assurance plan in response to the software product assurance requirements in conformance with DRD in annex B."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","5.4.1.1a","Requirement","ECSS-Q-ST-80_0720037",1,"Unchanged","For supplier selection ECSS-Q-ST-20 clause 5.4.1 shall apply.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Results of pre-award audits and assessments [PAF, -; -];\n          b.Records of procurement sources [PAF, -; -]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","5.5.1a","Requirement","ECSS-Q-ST-80_0720046",1,"Unchanged","For procurement documents, ECSS-Q-ST-20 clause 5.4.2 shall apply."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.1.4a","Requirement","ECSS-Q-ST-80_0720071",1,"Unchanged","The software life cycle shall be reviewed for suitability and for the availability of resources to implement it by all functions involved in its application."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.2.4.3a","Requirement","ECSS-Q-ST-80_0720103",1,"Unchanged","The software configuration file and the software release document shall be provided with each software delivery.\n","EXPECTED OUTPUT: The following outputs are expected:\n          a.Software configuration file [DDF, SCF; -];\n          b.Software release document [DDF, SRelD; -]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.2.6.5a","Requirement","ECSS-Q-ST-80_0720123",1,"Unchanged","Software containing deactivated code shall be verified specifically to ensure that the deactivated code cannot be activated or that its accidental activation cannot harm the operation of the system.\n","EXPECTED OUTPUT: Software verification report [DJF, SVR; CDR, QR, AR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.3.3.2a","Requirement","ECSS-Q-ST-80_0720160",1,"Unchanged","Mandatory and advisory design standards shall be defined and applied.\n","EXPECTED OUTPUT: Design standards [PAF, -; SRR, PDR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.3.4.3a","Requirement","ECSS-Q-ST-80_0720169",1,"Unchanged","The tools to be used in implementing and checking conformance with coding standards shall be identified in the product assurance plan before coding activities start.\n","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.3.5.18a","Requirement","ECSS-Q-ST-80_0720194",1,"Unchanged","The need for regression testing and additional verification of the software shall be analysed after a change or update of any tool used to generate it.","NOTE For example: source code or object code.\nEXPECTED OUTPUT: Updated test documentation [DJF, -; CDR, QR, AR, ORR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","6.3.8.7a","Requirement","ECSS-Q-ST-80_0720227",1,"Unchanged","Maintenance records shall be established for each software product, including, as a minimum, the following information,:\n    1. list of requests for assistance or problem reports that have been received and the current status of each;\n    2. organization responsible for responding to requests for assistance or implementing the appropriate corrective actions;\n    3. priorities assigned to the corrective actions;\n    4. results of the corrective actions;\n    5. statistical data on failure occurrences and maintenance activities.","NOTE The record of the maintenance activities can be utilized for evaluation and enhancement of the software product and for improvement of the quality system itself.\nEXPECTED OUTPUT: Maintenance records [MF, -; -]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","7.2.1.1a","Requirement","ECSS-Q-ST-80_0720236",1,"Unchanged","The software quality requirements shall be documented in the requirements baseline and technical specification.","EXPECTED OUTPUT: The following outputs are expected:\n          a.Requirement baseline [RB, SSS; SRR];\n          b.Technical specification [TS, SRS; PDR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","7.5.2a","Requirement","ECSS-Q-ST-80_0720261",1,"Unchanged","The firmware device shall be indelibly marked to allow the identification (by reference) of the hardware component and of the software component.","EXPECTED OUTPUT: Software product assurance plan [PAF, SPAP; PDR]."]
["ECSS-Q-ST-80C Rev.1","ECSS - Superseded v1.0","B.2.1<7>b","Requirement","ECSS-Q-ST-80_0720296",1,"Unchanged","The description of the approach specified in B.2.1<7>a shall include the:\n    1. specification of the product metrics, their target values and the means to collect them;\n    2. definition of a timely metrication programme;\n    3. analyses to be performed on the collected metrics;\n    4. way the results are fed back to the development team;\n    5. documentation quality requirements;\n    6. assurance activities meant to ensure that the product meets the quality requirements."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","5.5a","Requirement","ECSS-Q-ST-70-60_1390014",1,"Created","The PCB manufacturer shall send a formal request for qualification to the qualification authority."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","5.9b","Requirement","ECSS-Q-ST-70-60_1390037",1,"Created","The audit shall occur when PCB production is in progress."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","5.9k","Requirement","ECSS-Q-ST-70-60_1390046",1,"Created","The audit report and any findings shall be approved and signed by the PCB manufacturer and qualification authority."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","5.14b","Requirement","ECSS-Q-ST-70-60_1390066",1,"Created","The QA report shall be issued quarterly."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","6.3i","Requirement","ECSS-Q-ST-70-60_1390093",1,"Created","The PCB manufacturer shall specify in its PID the range of etchback."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","6.5j","Requirement","ECSS-Q-ST-70-60_1390106",1,"Created","The PCB manufacturer shall control the storage conditions and duration of materials and chemistry with limited shelf­life and verify the validity of the relevant material for use. "]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","6.7.2a","Requirement","ECSS-Q-ST-70-60_1390122",1,"Created","The PCB manufacturer shall treat all processes from innerlayer etching until lay-up as critical processes with respect to cleanliness."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","6.10.2j","Requirement","ECSS-Q-ST-70-60_1390146",1,"Created","The total number of repairs in conformance with the requirements 6.10.2g, 6.10.2h and 6.10.2i shall not exceed 6 per 50 cm2 and 6 per PCB.","NOTE \tThis is based on ECSS-Q-ST-70-28 considering a maximum per PCB and per surface area, whichever is more restrictive.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","6.14e","Requirement","ECSS-Q-ST-70-60_1390171",1,"Created","The procurement authority shall list each PCB technology, in conformance with the requirement 5.11b, in the DML as a separate item."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","7.3b","Requirement","ECSS-Q-ST-70-60_1390194",1,"Created","The test selection for initial qualification of PCB manufacturer shall be in conformance with requirement 7.2b."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","7.6d","Requirement","ECSS-Q-ST-70-60_1390202",1,"Created","Upon approval of the delta qualification test report in conformance with requirements 5.10c and 5.10d, the PCB manufacturer shall document the qualified changes in the PID."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","8.2.2b","Requirement","ECSS-Q-ST-70-60_1390224",1,"Created","Coupons shall be designed in conformance with clause 15 of ECSS-Q-ST-70-12."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","8.2.4j","Permission","ECSS-Q-ST-70-60_1390771",1,"Created","Solderability test need not to be performed for procurement in case all the following conditions are met:\n1.\tThe surface finish is hot oil reflowed SnPb;\n2.\tThe thickness of the SnPb as specified on the CoC of the panel is in conformance with the requirements of Table 10-12;\n3.\tThe PID does not specify that solderability testing is mandatory for procurement.","NOTE \tIn case the thickness of SnPb is not in conformance with the requirements of Table 10-12 as determined during qualification (renewal), the PID can specify that solderability test is performed for all procurement. This is usually the case upon request by the qualification authority.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","8.4a","Requirement","ECSS-Q-ST-70-60_1390260",1,"Created","The procurement authority shall perform incoming inspection as follows:\n1.\tVisual inspection on all PCBs, in conformance with the clause 9.3,\n2.\tMicroscopic inspection on microsections, in conformance with the clause 10, by one of the following institutes:\n(a)\tprocurement authority;\n(b)\texternal third-party lab;\n(c)\tassembly house;\n(d)\tPCB manufacturer using another inspector than the one for outgoing inspection.\n3.\tVerification of the CoC and its lab reports, in conformance with the Annex B,\n4.\tVerification of quantity,\n5.\tVerification of integrity of packaging.","NOTE\t1\tThe PCB manufacturer provides microsections used for the CoC and customer coupons. Both can be used for the incoming inspection. To avoid deterioration of the surface quality of microsections, it is preferred to perform incoming inspection as soon as possible after delivery. \nNOTE\t2\tMicrosection inspection for qualitative aspects is important and detection can be operator dependent. Therefore this requirement specifies to perform an additional verification.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.2.4d","Requirement","ECSS-Q-ST-70-60_1390279",1,"Created","The temperature inside machine shall be (100 ± 2) °C and stabilized for (5 ± 1) minutes."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.3.3.3e","Requirement","ECSS-Q-ST-70-60_1390310",1,"Created","The length of the diagonal of the PCB shall be measured."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.3.7.2n","Permission","ECSS-Q-ST-70-60_1390787",1,"Created","In case the test fails because the set voltage is not achieved due to high capacitance caused by presence of plane layers, one further re-test may be performed with adjusted parameters.","NOTE \tSuch adjustment can include longer sustain time or longer ramp-up time.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.4.3j","Requirement","ECSS-Q-ST-70-60_1390361",1,"Created","The test vehicle shall be microsectioned at the zone that was bend during the test."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.4.5e","Requirement","ECSS-Q-ST-70-60_1390373",1,"Created","The tape shall have an adhesion of at least 4,4 N/cm.","NOTE \tExample of tape that can be used is 3M Brand 600 with a width of 13 mm.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.4.11.2a","Requirement","ECSS-Q-ST-70-60_1390385",1,"Created","The test pattern for solderability test shall be one of the following:\n1.\tCoupon A/B with PTH as specified in requirement 8.2.2d, or\n2.\tPCB sample with PTH."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.5.2.5b","Requirement","ECSS-Q-ST-70-60_1390413",1,"Created","Quality of laminate shall be inspected in dark field or an equivalent lighting method.","NOTE\t1\tDark field uses a high illumination intensity showing features underneath the surface of the microsection by transparency of the resin. A similar high illumination intensity can be obtained using polarisation filters.\nNOTE\t2\tSubsurface cracks in laminate can be visible as an area showing “iridescence” in dark field. To conclude on the nature of the iridescence it is good practice to perform progressive polishing to have the surface of the microsection at the same level of the feature. In this case a crack shows up in bright field since it is in the surface of the microsection.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.5.3g","Requirement","ECSS-Q-ST-70-60_1390421",1,"Created","The samples shall be inspected to evaluate the visual aspects of the substrate in conformance with clause 10.4."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.5.5.2.2a","Requirement","ECSS-Q-ST-70-60_1390442",1,"Created","IST shall be performed for procurement in case the PCB definition dossier includes one or more of the following:\n1.\tAny PCB with ≥ 0,3 mm in Z-direction as-designed insulation distance of no-flow prepreg or 85NT;\n2.\tEpoxy PCB with ≥ 12 copper layers;\n3.\tRigid-flex PCB with one or more of the following aspects:\n(a)\t≥ 12 copper layers, or\n(b)\t≥ 2 flex laminates, or\n(c)\tasymmetric build-up or asymmetric lamination;\n4.\tHDI PCB with microvias or with aspect ratio > 7.","NOTE\t1\tNo-flow prepreg and 85NT have high thermal expansion in Z-direction. The thermal expansion is the driver for barrel crack and therefore necessitates IST testing.\nNOTE\t2\tSee Table B-6 for an example of a build-up report with as-designed insulation distance.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.5.5.4.4a","Recommendation","ECSS-Q-ST-70-60_1390821",1,"Created","After IST testing, the coupon should be submitted to microsectioning."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.6.3g","Requirement","ECSS-Q-ST-70-60_1390477",1,"Created","The test pattern for intralayer insulation resistance shall have at least 25 mm parallel conductors.","NOTE \tInsulation distance between tracks or between layers is representative of the PCB, as specified in clause 15.2a of ECSS-Q-ST-70-12.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.7.2.4b","Requirement","ECSS-Q-ST-70-60_1390504",1,"Created","Breach of insulation that is demonstrated by microsectioning to be caused by lack of cleanliness shall be evaluated during the audit in conformance with clause 6.7.","NOTE \tThe test can only be treated as nonconform in case contamination is demonstrated to be the cause of breach of insulation. The electrical response only, is not sufficient. Hence, it is not necessary that the environmental parameters are fully representative of operational use. The test only serves to find contamination, if any. Test results of contamination causing breach of insulation are evaluated together with the cleanliness of processes during the audit. \n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.7.3.3f","Recommendation","ECSS-Q-ST-70-60_1390835",1,"Created","After the CAF test method, the location of breach of insulation should be determined on each pattern by electrical insulation of sections of the pattern.","NOTE \tLocalisation in A and B pattern comprises of determining the x, y location, which can be achieved by insulation of sections of the surface pattern. Localisation in C pattern comprises of determining the layer, which can be achieved by insulation of the interconnections to the planes that are designed on the surface.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","9.8.4h","Requirement","ECSS-Q-ST-70-60_1390537",1,"Created","The maximum temperature shall be between +130 °C and +145 °C.","NOTE \tThe Tg of laminates is typically higher than this temperature.\n"]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","10.3o","Requirement","ECSS-Q-ST-70-60_1390586",1,"Created","For the technological feature nail heading, the acceptance criteria, the inspection samples and the measurement method shall be in conformance with Table 10-31."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","10.4c","Requirement","ECSS-Q-ST-70-60_1390616",1,"Created","For the technological feature surface metallisation the acceptance criteria, the inspection samples and the measurement method shall be in conformance with Table 10-40."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","10.5n","Requirement","ECSS-Q-ST-70-60_1390655",1,"Created","For the technological feature marking adhesion strength for sculptured flex PCB, the acceptance criteria, the inspection samples and the measurement method shall be in conformance with Table 10-65."]
["ECSS-Q-ST-70-60C Corr.1","ECSS - Superseded v1.0","B.2.1.3b","Requirement","ECSS-Q-ST-70-60_1390698",1,"Created","The visual inspection of qualitative aspects shall include the review items from the MRR."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","5.2g","Permission","ECSS-Q-ST-70-12_1200376",1,"Created","As a result of the design review, the PCB manufacturer may identify to the supplier additional Review Items in the PCB definition dossier.\nNOTE \tReview Items can exist for PCB designs even within the capability of the PID. These Review Items and methods to mitigate them are specified in this standard as best practices and recommendations."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","7.1.2e","Recommendation","ECSS-Q-ST-70-12_1200380",1,"Created","Balancing of copper should be performed by including dummy non-functional copper.\nNOTE \tThis is more important for partial planes on thick copper layers such as 70 µm."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","7.1.3d","Recommendation","ECSS-Q-ST-70-12_1200385",1,"Created","The insulation distance as-designed between two layers in rigid laminate or prepreg in Z direction should be in conformance with the values from Table 13-7.\nNOTE \tThis table specifies a minimum distance of 100 µm."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","7.4.3c","Requirement","ECSS-Q-ST-70-12_1200047",1,"Created","In case the as-designed track width and spacing for external layers of rigid PCB is less than the values specified in the requirement 7.4.3b, the following conditions shall be met:\n1.\tthe manufacturing tolerances as specified in the PID are smaller than as specified in Table 7-3,\n2.\tthe as-manufactured dimensions specified in Table 7-4 and Table 13-7 are met, and\n3.\tit is recorded as a Review Item in the PCB definition dossier."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","7.5.2h","Recommendation","ECSS-Q-ST-70-12_1200405",1,"Created","The diameter of internal pads should be the diameter of drilled hole plus ≥ 0,3 mm.\nNOTE \t1\tThe drilled diameter is typically 0,2 mm larger than the as-manufactured minimum hole diameter.\nNOTE \t2\tIt is important to consider the number of drilling and lamination sequences and the PCB manufacturing tolerances for the design of the diameter of the pads."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","8.3.3a","Requirement","ECSS-Q-ST-70-12_1200086",1,"Created","The thickness of copper cladding shall be 17 µm, 35 µm or 70 µm."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","8.5.1a","Requirement","ECSS-Q-ST-70-12_1200100",1,"Created","Annular ring on a flex PCB shall be the distance of the surface copper from the hole wall to the clearance opening in the cover layer."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","8.7.3a","Requirement","ECSS-Q-ST-70-12_1200117",1,"Created","A single foil of copper shall be used in the build-up. \nNOTE \tCopper clad laminate is not used."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","9.3g","Requirement","ECSS-Q-ST-70-12_1200138",1,"Created","Except the cases specified in the requirement 9.3h the rigid-flex PCB shall be designed and delivered with a support frame."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","10.4.2b","Requirement","ECSS-Q-ST-70-12_1200166",1,"Created","The number of copper heat sink layers shall be ≤ 2."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","10.4.3e","Permission","ECSS-Q-ST-70-12_1200438",1,"Created","Molybdenum may be used to reduce in plane CTE and improve heat transfer.\nNOTE \tStandard specification for molybdenum is according to ASTM-B386-03."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","11.4.2a","Requirement","ECSS-Q-ST-70-12_1200194",1,"Created","The aspect ratio of a microvia on a HDI PCB shall be ≤ 1."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","12.3b","Requirement","ECSS-Q-ST-70-12_1200217",1,"Created","The tolerance on the as-manufactured resistance value shall be ≤ ±20%.\nNOTE \tDue to the relatively high tolerance, the application of embedded film resistors is limited to line termination."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","12.3i","Requirement","ECSS-Q-ST-70-12_1200220",1,"Created","The orientation of embedded film resistors shall be recorded as a Review Item in the PCB definition dossier.\nNOTE \tThe best etching accuracy is obtained when embedded film resistors are oriented in the direction of the conveyor of the etching process."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","13.4f","Permission","ECSS-Q-ST-70-12_1200466",1,"Created","In case sequential lamination increases the copper thickness, the current limits may be interpolated or extrapolated."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","13.8.2k","Requirement","ECSS-Q-ST-70-12_1200263",1,"Created","The insulation distance between the heat sink and a hole wall shall be in conformance with values from Table 13-3."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","13.9.3.3b","Requirement","ECSS-Q-ST-70-12_1200288",1,"Created","In case critical tracks are routed on external layers, they shall not be routed under components.\nNOTE \tThis is done to allow inspection of critical tracks."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","13.12.3.1c","Recommendation","ECSS-Q-ST-70-12_1200496",1,"Created","Direct coupling between bundles of non-critical signals specified in the requirement 13.12.3.1a should be avoided."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","14.2c","Requirement","ECSS-Q-ST-70-12_1200318",1,"Created","Pad geometry and outer layers shall be approved by the assembly house in compliance with requirements from clause 5 to clause 15 of ECSS-Q-ST-70-08 and in compliance with requirements from clause 5 to clause 16 of ECSS-Q-ST-70-38."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","14.3.4c","Recommendation","ECSS-Q-ST-70-12_1200513",1,"Created","The fan out should be symmetric.\nNOTE \tThis is done to avoid unwanted movement of components during reflow soldering. An example of a symmetric fan out is given in Figure 14-4."]
["ECSS-Q-ST-70-12C","ECSS - Superseded v1.0","15.2a","Recommendation","ECSS-Q-ST-70-12_1200521",1,"Created","The test coupon design should be representative of the PCB."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.1.1b","Requirement","ECSS-Q-ST-70-01_0500002",1,"Created","The supplier shall establish measures for the coordination and resolution of cleanliness and contamination control issues among the parties involved in the project."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.1.4b","Requirement","ECSS-Q-ST-70-01_0500011",1,"Created","These predictions shall be updated to evaluate the molecular and particulate contamination levels generated during all on ground activities and during launch and in-orbit phases.\n    NOTE Ground activities can be MAIT, storage, transportation, launch preparation."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.2.2.2d","Requirement","ECSS-Q-ST-70-01_0500044",1,"Created","A set of assembly tools and equipment for assembly and integration shall be used and maintained in clean conditions."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.3.1.1e","Requirement","ECSS-Q-ST-70-01_0500069",1,"Created","Entrances shall provide an air lock to allow a maintained pressurisation of the area."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.3.1.7f","Requirement","ECSS-Q-ST-70-01_0500102",1,"Created","Molecular contamination in controlled environments shall not exceed 0,5 ´ 10-7 g/cm2 during a continuous period of one week.\n    NOTE 1 In case of contamination sensitive equipment, a lower level can be required, based on the contamination budget (including exposure time).\n    NOTE 2 In a normal cleanroom (without charcoal filters) levels can be achieved that are 10 to 100 times better."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.3.1.8b","Requirement","ECSS-Q-ST-70-01_0500105",1,"Created","The temperature distribution inside a cleanroom shall be controlled at representative locations for the hardware items.\n    NOTE 1 In order to ensure that a nominal temperature is achieved throughout the room. Automatic devices can be used for temperature monitoring.\n    NOTE 2 If items being worked on are extremely sensitive to temperature changes, automatic devices with a warning system that comes into operation when a temperature change occurs can be used."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.3.1.13l","Requirement","ECSS-Q-ST-70-01_0500135",1,"Created","Exhaust systems for grinding, welding or soldering, machining or related operations shall be installed."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.4.2.1a","Requirement","ECSS-Q-ST-70-01_0500168",1,"Created","Particulate and molecular contamination shall be monitored during all the on ground phases.\n    NOTE For specific missions, particulate and molecular contamination can be monitored during launch and in space."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.4.3.2i","Requirement","ECSS-Q-ST-70-01_0500193",1,"Created","Independently of any stopping and verification criteria, the minimum bakeout duration shall be 72 hours."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","5.4.4d","Requirement","ECSS-Q-ST-70-01_0500202",1,"Created","Storage areas shall provide adequate protection to the package and the product for the intended storage period."]
["ECSS-Q-ST-70-01C","ECSS - Superseded v1.0","B.2.1<5.2>a","Requirement","ECSS-Q-ST-70-01_0500235",1,"Created","The C&CCP shall l contain the allocation of contamination levels through the splitting of cleanliness requirements during the major integration and testing phases.\n    NOTE In case the outgassing contribution to the performance loss is large with respect to other contributions (mainly for sensitive instruments with tight requirements), more detailed modelling are performed."]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","4.4a","Recommendation","ECSS-Q-ST-60-02_0450200",1,"Created","At the end of the ASIC and FPGA development cycle, the supplier should establish an experience summary report in conformance with the DRD in Annex I.\n    NOTE The experience summary report can be written in the frame of the supplier’s continued quality improvement activities in order to establish economic and efficient development and test requirements for expected future projects. "]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","5.4.3a","Requirement","ECSS-Q-ST-60-02_0450039",1,"Created","The supplier shall establish a verification plan in conformance with the DRD in Annex E."]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","5.5.4d","Requirement","ECSS-Q-ST-60-02_0450064",1,"Created","As a minimum the following tasks shall be performed and documented in a netlist generation report:\n    1. Consider the required derating factors;\n    2. Ensure that the appropriate library cells are used as to fulfil all the requirements collected in the ASIC and FPGA requirements specification;\n    3. Select or generate appropriate models for parasitism (e.g. wire load models);\n        NOTE This is not applicable for FPGA designs.\n    4. Perform a design parameter centring; \n        NOTE This is only applicable for analog ASIC designs.\n    5. Ensure that the intended operating (process, voltage, temperature) and environment (radiation) conditions are used during the translation and verification exercise;\n    6. If synthesis tools are used, generate scripts which allow performing the fully automatic pre-layout netlist generation in a repeatable way; \n    7. Ensure that these scripts, being part of the inputs to the design, are compliant to the general requirements for e.g. documentation, commenting and version control;\n    8. Specify timing constraints, and supplier or manufacturer-specific design rules;\n    9. Consider over-constraining to anticipate parasitic effects."]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","5.5.7g","Requirement","ECSS-Q-ST-60-02_0450073",1,"Created","In particular, when the layout is performed by another company (foundry), the reviewers shall assess the specific foundry requirements (netlist sign-off criteria).\n    ","EXPECTED OUTPUTS:\ta. Design entry report;\n    \t\t\tb. Netlist generation report;\n    \t\t\tc. Netlist verification report;\n    \t\t\td. Updated data sheet with pin-out;\n    \t\t\te. Updated design database, containing:\n        \t\t\t\t1. Pre-layout netlist;\n        \t\t\t\t2. Constraints for layout (i.e. floorplan and constraints for timing driven layout) as defined in the ADP;\n        \t\t\t\t3. Test vectors for production test;\n    \t\t\tf. MoM of DDR."]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","5.8.3c","Requirement","ECSS-Q-ST-60-02_0450106",1,"Created","The supplier shall ensure technical support of the device during the lifetime of the product. "]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","6.2a","Requirement","ECSS-Q-ST-60-02_0450131",1,"Created","The supplier shall schedule and conduct design reviews in conformance with ECSS-M-ST-10-01. "]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","6.2j","Requirement","ECSS-Q-ST-60-02_0450140",1,"Created","The MoMs of the review meetings shall be added to the management documentation. "]
["ECSS-Q-ST-60-02C","ECSS - Superseded v1.0","7.3.6a","Requirement","ECSS-Q-ST-60-02_0450163",1,"Created","The design validation documentation shall consist of the following contributions to the layout documentation:\n    1. The validation report presenting the scope, sequences, set-up and results of the validation tests performed as detailed in clause 5.8.1.\n    2. The radiation test report (if applicable) providing the test board circuitry and bias conditions, the test sequence and investigated irradiation levels, the performed measurements and the resulting degradations.\n    3. The release report summarizing all activities performed to assure that all necessary prerequisites are fulfilled to start a FM production (see clause 5.8.3).\n"]
["ECSS-Q-ST-60-15C","ECSS - Superseded v1.0","5.1a","Requirement","ECSS-Q-ST-60-15_1150001",1,"Created","Mission TID radiation environment shall be defined according to ECSS-E-ST-10-04 and documented in a Mission Radiation Environment Specification in conformance with the DRD in Annex A."]
["ECSS-Q-ST-60-15C","ECSS - Superseded v1.0","5.2j","Requirement","ECSS-Q-ST-60-15_1150035",1,"Created","Acceptable TNID test data shall be available latest at CDR."]
["ECSS-Q-ST-60-15C","ECSS - Superseded v1.0","5.3g","Requirement","ECSS-Q-ST-60-15_1150061",1,"Created","If acceptable component test data does not exist, heavy ion ground testing shall be performed."]
["ECSS-Q-ST-60-15C","ECSS - Superseded v1.0","5.3p","Requirement","ECSS-Q-ST-60-15_1150072",1,"Created","If acceptable proton SEE data is not available, proton ground testing shall be performed."]
["ECSS-Q-ST-60-15C","ECSS - Superseded v1.0","B.2.1<3>c","Requirement","ECSS-Q-ST-60-15_1150105",1,"Created","The radiation analysis report shall include the description of mechanical model, assumption, method and tools used for ray trace or Monte Carlo analysis, and results obtained."]
["ECSS-Q-ST-70-05C Rev.1","ECSS - Superseded v1.0","5.2.3.1a","Requirement","ECSS-Q-ST-70-05_0540022",1,"Informative Change","Surfaces shall be washed and wiped with solvents and tissues that are compatible with and do not damage the surface to be analysed. ","NOTE \t1\tFor example, solvation and swelling of any material that is not regarded as a contaminant.\nNOTE \t2\tScratching of the surface.\nNOTE \t3\tIPA and chloroform (CHCl3) are the most widely used solvents.\n"]
["ECSS-Q-ST-70-05C Rev.1","ECSS - Superseded v1.0","5.2.3.3b","Requirement","ECSS-Q-ST-70-05_0540028",1,"Informative Change","A blank analysis shall be performed in conformance with 5.2.3.3f and 5.2.3.3g until a background level of less than 5 ´ 10-7 g for any tissue size is obtained.","NOTE \tCleaning can be performed by Soxhlet extraction or immersion in chloroform.\n"]
["ECSS-Q-ST-70-05C Rev.1","ECSS - Superseded v1.0","5.4.3.1k","Requirement","ECSS-Q-ST-70-05_0540053",1,"Unchanged","The absorbance level of the NVR shall be lower than 0,000 1 AU in order to minimize disturbances."]
["ECSS-Q-ST-70-05C Rev.1","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-Q-ST-70-05_0540086",1,"Informative Change","The customer’s product assurance department shall audit the system after it has been built or purchased.","NOTE \tThe audit is necessary before the system can be accepted for running qualification or quality control tests on materials for use in customer projects.\n"]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","4.2.11.1a","Requirement","ECSS-E-ST-20-07_0080022",1,"Created","Bonding requirements are a mean for fulfilling grounding requirements.\n    NOTE Bonding for charging control is specified in ECSS-E-ST-20-06 “Electrical continuity”, including surfaces and structural and mechanical parts."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.2.2c","Requirement","ECSS-E-ST-20-07_0080047",1,"Created","The RF absorber shall be placed above, behind, and on both sides of the EUT, and behind the radiating or receiving antenna as shown in Figure 5-1."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.3.1d","Requirement","ECSS-E-ST-20-07_0080056",1,"Created","When a ground plane is not present in the actual EUT installation, the EUT shall be placed on a non-conductive table.\n    NOTE In such a case, test methods are specific and are likely to differ from the ones in the present standard."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.5.3a","Requirement","ECSS-E-ST-20-07_0080075",1,"Created","Checks shall be performed to assure that an overload condition does not exist.\n    NOTE Measurement receivers and transducers are subject to overload, especially receivers without preselectors and active transducers."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.8.2a","Requirement","ECSS-E-ST-20-07_0080113",1,"Created","A peak detector shall be used for all frequency domain emission and susceptibility measurements.\n    NOTE This device detects the peak value of the modulation envelope in the receiver pass band. Measurement receivers are calibrated in terms of an equivalent root mean square value of a sine wave that produces the same peak value."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.9.3b","Requirement","ECSS-E-ST-20-07_0080122",1,"Created","Minimum measurement time for analogue measurement receivers during emission testing shall be as specified in Table 5-2."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.2.11.1a","Requirement","ECSS-E-ST-20-07_0080147",1,"Created","Measurement antennas, current probes, field sensors, and other devices used in the measurement loop shall be calibrated at least every two years or when damaged."]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.4.5.2b","Requirement","ECSS-E-ST-20-07_0080180",1,"Created","A right-handed orthogonal coordinate system XYZ shall be assigned to the EUT geometric centre. "]
["ECSS-E-ST-20-07C","ECSS - Superseded v1.0","5.4.10.4a","Requirement","ECSS-E-ST-20-07_0080213",1,"Created","The measurement equipment shall be turned on and waited until it is stabilized."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","4.3.2b","Requirement","ECSS-E-ST-20-08_0090007",1,"Created","All instrumentation used for qualification and acceptance tests shall:\n    1. be calibrated, and \n    2. be within the specified calibration period at the time of test."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.3.2.4b","Permission","ECSS-E-ST-20-08_0091064",1,"Created","Standard atmospheric conditions may be assumed for general applications in the spacecraft, over a period of time that is agreed between the supplier and customer."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.3.3.2c","Requirement","ECSS-E-ST-20-08_0090040",1,"Created","Potential parallel connections shall not prevent performance measurement specified in requirement 5.3.3.2b."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.4.3.5b","Requirement","ECSS-E-ST-20-08_0090073",1,"Created","The visual inspection procedure and criteria shall be agreed with the customer and be described in the SCD-PVA."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.1.2c","Requirement","ECSS-E-ST-20-08_0090082",1,"Created","Qualification margins shall not exceed component and material specifications unless agreed between supplier and customer."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.1.3.4d","Requirement","ECSS-E-ST-20-08_0090107",1,"Created","For a LEO mission, the following cycling profiles shall be used:\n    1. A temperature profile which envelopes the variation of temperature extremes during the mission. \n    2. The total profile, divided into a number of equally shaped sub-profiles, where the number of sub-profiles are:\n        (a) equal to the number of years of the mission, and \n        (b) with extreme cycle temperatures derived from the slicing of the temperature profile of the whole mission."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.3.2.4b","Requirement","ECSS-E-ST-20-08_0090140",1,"Created","Cells and components shall not enter the stay-out zones indicated on the qualification coupon assembly drawing. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.3.2.12b","Requirement","ECSS-E-ST-20-08_0090166",1,"Created","Any defects listed in requirements 5.5.3.2.12a.1 to 5.5.3.2.12a.5, raised after acceptance shall be reported and traced throughout the qualification sequence."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.3.3.8a","Requirement","ECSS-E-ST-20-08_0090197",1,"Created","The thermal sensor resistance shall be measured at room temperature."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.3.4.2f","Requirement","ECSS-E-ST-20-08_0090206",1,"Created","Pre-test and post-test measurements shall be made with the same test set-up. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","5.5.3.10.1c","Requirement","ECSS-E-ST-20-08_0090231",1,"Created","If requirement 5.5.3.10.1b cannot be satisfied, a destructive test shall be applied."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.3.2a","Requirement","ECSS-E-ST-20-08_0090264",1,"Created","The test methods and conditions specified in clause 6.4.3 shall be applied."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.4.1c","Requirement","ECSS-E-ST-20-08_0090273",1,"Created","The qualification plan shall consist of the tests specified in Table 6-1."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.4.3.1.5d","Requirement","ECSS-E-ST-20-08_0090298",1,"Created","The total area of ARC and conductive coating voids, including evaporation jig marks, shall not exceed 3 % of the area of the coverglass."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.4.3.8.2c","Requirement","ECSS-E-ST-20-08_0090339",1,"Created","Relative humidity shall be higher than 90 %. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.4.3.11.2d","Requirement","ECSS-E-ST-20-08_0090355",1,"Created","The nominal rate shall be lower than or equal to 5 × 1011 e- cm-2 s-1."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","6.5.2a","Requirement","ECSS-E-ST-20-08_0090388",1,"Created","An SCA shall be considered as failed if it exhibits one or more of the failure modes detailed in clause 6.5.1."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.1.1.2a","Requirement","ECSS-E-ST-20-08_0090397",1,"Created","The conditions and methods of testing shall conform to the bare solar cell source control drawing (SCD-BSC).\n    NOTE The bare solar cell specification consists of two parts, the generic specification (this Standard) and the SCD-BSC. The SCD-BSC contains the technical specification for a cell type relevant to acceptance testing, as well as for the qualification testing. For the preparation of the SCD-BSC for bare solar cells, refer to Annex C."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.3.2.2.2e","Requirement","ECSS-E-ST-20-08_0090422",1,"Created","During measurement, the BSCs shall be kept at a constant temperature +/- 0,5 °C."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.5.1.5.2a","Requirement","ECSS-E-ST-20-08_0090455",1,"Created","The maximum dimension of voids or bubbles shall be 0,25 mm in diameter."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.5.4c","Requirement","ECSS-E-ST-20-08_0090477",1,"Created","Data for all electrical performance parameters at the different solar cell temperatures shall be provided."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.5.6.3c","Requirement","ECSS-E-ST-20-08_0090488",1,"Created","The coverglass as stated in the SCD-BSC shall be used."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.5.13.2a","Requirement","ECSS-E-ST-20-08_0090521",1,"Created","The solar cells shall be subjected to 1 MeV electron irradiation.\n    NOTE ISO 23038 outlines a methodology to perform this test."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","7.6.2b","Requirement","ECSS-E-ST-20-08_0090546",1,"Created","Failed components shall be identified as such and included in the delivery. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","8.6.2.1a","Requirement","ECSS-E-ST-20-08_0090579",1,"Created","Before starting production of the qualification lot, the manufacturer shall compile a production test schedule, showing by date and duration, production and test activities, including all major processing operations and key stages in the production and testing. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","8.7.1.3.1b","Requirement","ECSS-E-ST-20-08_0090588",1,"Created","For a coated coverglass, the uncoated area due to coating tools shall not exceed 1 % of the total coverglass area or 8 mm^2, whichever is greater."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","8.7.5.2.3a","Requirement","ECSS-E-ST-20-08_0090613",1,"Created","The reflectance cut-on shall be as stated in the SCD-CVG."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","8.7.13.2f","Requirement","ECSS-E-ST-20-08_0090650",1,"Created","The irradiation shall be performed at doses representative of LEO and GEO mission environments and at least 2 × Fp, as stated in the SCD-CVG."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","8.7.14.2d","Requirement","ECSS-E-ST-20-08_0090654",1,"Created","Tests shall be performed in a vacuum (pressure below 10-3 Pa)."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.2.1.3b","Requirement","ECSS-E-ST-20-08_0090679",1,"Created","The tests and inspections specified in clauses 9.4 and 9.5 shall be performed at the manufacturer’s plant or at a facility approved by the customer.\n    NOTE For test house requirements, see ECSS-Q-ST-20-07."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.5.3a","Requirement","ECSS-E-ST-20-08_0090712",1,"Created","The qualification plan shall consist of the tests specified in Table 9-4."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.6.4.2a","Requirement","ECSS-E-ST-20-08_0090737",1,"Created","All external protection diode qualification samples shall be submitted to thermal cycling consisting of TBSc cycles from -TBS1 °C to + TBS2°C under nitrogen gas environment, where the values TBSc, TBS1 and TBS2 are values to be specified in the SCD-EPD."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.6.12.2g","Requirement","ECSS-E-ST-20-08_0090770",1,"Created","After electron irradiation and temperature annealing, the requirements as stated in the SCD-EPD for the diode characteristics shall be satisfied."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.6.16.3b","Requirement","ECSS-E-ST-20-08_0090788",1,"Created","The diode electrical characteristics test shall satisfy the pass-fail criteria stated in the SCD-BSC or SCD-EPD."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","9.7.2a","Requirement","ECSS-E-ST-20-08_0090803",1,"Created","A component shall be considered to have failed if it exhibits one or more of the failure modes specified in clause 9.7.1. "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","10.2.2.3.1a","Requirement","ECSS-E-ST-20-08_0090836",1,"Created","SWS shall meet visual inspection requirements on defects (clauses 7.5.1.4 and 7.5.1.5 for bare solar cells, or clause 6.4.3.1 for SCA’s). "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","11.1.3.2c","Recommendation","ECSS-E-ST-20-08_0091087",1,"Created","The ohmic value of the shunt associated with the cabling and the network analyser should be measured at room temperature using one of the following two methods:\n    1. Calculation: to be used if the certified calibrated value of the shunt, of the cable and of the 50 W input are known. \nIn this case:\nRshunt measured =  \n\n    2. Direct measurement: measure Rshunt measured with the cell short-circuited, the channel A plugged on the network analyser, all the other cables unplugged (Figure 11-3), and a 4-wire setting, as follows:\n        (a) unplug the injection cable (RF channel);\n        (b) unplug the Vcell measuring cable and keep it insulated;\n        (c) unplug the cable on channel B of the network analyser and plug it into the input “input” of the ohmmeter with a BNC adaptor, paying attention to the polarities;\n        (d) unplug the measuring cable Vshunt and plug it in the input “sense” of the ohmmeter, paying attention to the polarities;\n        (e) monitor the calculated or measured value.                                 "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","11.2.2.1b","Recommendation","ECSS-E-ST-20-08_0091094",1,"Created","The voltage should be measured at the test specimen terminals."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","A.2.1<8.5>a","Requirement","ECSS-E-ST-20-08_0090903",1,"Created","In conformance with clause 5.5.3.5, the SCD-PVA shall state a procedure to measure the capacitance, including the test temperature (average operational temperature). "]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","B.2.1<6.13>a","Requirement","ECSS-E-ST-20-08_0090928",1,"Created","In conformance with clause 6.4.3.15, the SCD-SCA shall include the following:\n    1. The operational test temperature, in °C.\n    2. The EOL UV loss factor."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","C.2.1<6.3>a","Requirement","ECSS-E-ST-20-08_0090938",1,"Created","In conformance with clause 7.5.10, the SCD-BSC shall include:\n    1. The equipment to measure the contact thickness;\n    2. The maximum and minimum values of the contact thickness in mm."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","D.2.1<5>a","Requirement","ECSS-E-ST-20-08_0090969",1,"Created","The SCD-CVG shall include the following coverglass materials characteristics:\n    1. Coverglass base material, including doping elements and percentage (%).\n    2. Front surface coatings (including conductive coatings).\n    3. Rear surface coatings."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","E.2.1<2>a","Requirement","ECSS-E-ST-20-08_0090994",1,"Created","The SCD-EPD shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-20-08C","ECSS - Superseded v1.0","G.3.1g","Requirement","ECSS-E-ST-20-08_0091027",1,"Created","The DDP for SCA, BSC, CVG and protection diode shall consist of qualification test plan."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","4.3.1e","Requirement","ECSS-E-ST-50-05_0900024",1,"Created","The entire procedure of selection of frequencies shall be carried out under the management of the frequency coordinator.\n    NOTE The frequency coordinator has the exclusive authority for assigning frequencies."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-E-ST-50-05_0900033",1,"Created","In addition to clause 5.2.1a for Category B missions the short term frequency stability shall be such that the resulting phase error when tracking the carrier with a second-order PLL with loop bandwidth 2BL as specified for the mission, does not exceed 10 degrees peak in high signal-to-noise conditions and in non-coherent mode.\n    NOTE 1 The “short term frequency stability” includes phase noise contribution and any “instantaneous” phase or frequency variations (“discontinuities”) due to technological aspects and related to oscillator implementation.\n    NOTE 2 Depending on the link budget and on the ground station 2BL value, this requirement may have strong impact on the onboard subsystem architecture and the selection of the proper oscillator technology."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","6.1.4.1.3a","Requirement","ECSS-E-ST-50-05_0900071",1,"Created","For NRZ telemetry symbol rates above 60 ksps, subcarriers shall not be used and one of the following modulation schemes shall be used:\n    • SP-L encoded symbols and direct modulation on the carrier for symbol rates as high as 1 Msps in the 2 200 MHz - 2 300 MHz and 8 400 MHz - 8 500 MHz bands.\n    • Modulation in conformance to clause 6.2 of this Standard."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","6.1.5b","Requirement","ECSS-E-ST-50-05_0900090",1,"Created","To ensure recovery of the symbol clock by the ground demodulators, the maximum string of either ones or zeros shall be limited to 64 symbols."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","6.2.3.2a","Requirement","ECSS-E-ST-50-05_0900123",1,"Created","The modulation shall be phase reversal keying of two phase quadrature carriers of equal amplitude by data channels with equal symbol rates with the constellation bit mapping of Figure 6-3."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","6.2.3.2b","Requirement","ECSS-E-ST-50-05_0900124",1,"Created","The phase angle between the two quadrature carriers shall be (90 ±5)°."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","6.2.5a","Requirement","ECSS-E-ST-50-05_0900157",1,"Created","The telemetry symbol rate shall be within ±1 × 10-4 of its nominal value at all times."]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","7.2.2c","Requirement","ECSS-E-ST-50-05_0900194",1,"Created","To provide a means of estimating the best lock frequency, the transponder PLL error voltage (loop stress) shall be transmitted to the ground via the spacecraft telemetry. "]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","8.4a","Requirement","ECSS-E-ST-50-05_0900219",1,"Created","The compatibility of the space element and the ground stations shall be tested in conformance with requirements on “Communication compatibility test” of clauses on “ Overall system qualification test” and “Overall system acceptance test” of ECSS-E-ST-10-03.\n    NOTE Specific ranging and Doppler tracking tests are given in clause 5 of ECSS-E-ST-50-02. "]
["ECSS-E-ST-50-05C Rev. 1","ECSS - Superseded v1.0","9.2.2a","Requirement","ECSS-E-ST-50-05_0900225",1,"Created","The 4 dimensional-8PSK trellis coded modulator shall combine a serial to parallel converter, a differential encoder, a trellis encoder, i.e. a convolutional coder, a constellation mapper and an 8PSK modulator \n    NOTE See Figure 9-1. "]
["ECSS-E-ST-32-08C","ECSS - Superseded v1.0","4.2.7d","Requirement","ECSS-E-ST-32-08_0220013",1,"Created","For hygroscopic materials used in high stability structural applications, the CME shall be determined by test."]
["ECSS-E-ST-32-08C","ECSS - Superseded v1.0","4.4.4a","Requirement","ECSS-E-ST-32-08_0220038",1,"Created","All inserts shall have their surfaces protected against corrosion.\n    NOTE An insert system consists of a removable threaded fastener and a fixture embedded into the honeycomb structure using a potting mass."]
["ECSS-E-ST-32-08C","ECSS - Superseded v1.0","4.6.5e","Requirement","ECSS-E-ST-32-08_0220071",1,"Created","The NDI plan shall be available for review by the customer upon request."]
["ECSS-E-ST-32-08C","ECSS - Superseded v1.0","4.7a","Requirement","ECSS-E-ST-32-08_0220072",1,"Created","The supplier shall establish that all known factors influencing the deterioration of the candidate materials have been evaluated in the design."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","5.3.1d","Requirement","ECSS-E-ST-10_0790032",1,"Created","The system engineering organisation shall justify the functional architecture in the DJF in conformance with Annex K."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","5.4.1.3b","Requirement","ECSS-E-ST-10_0790065",1,"Created","The system engineering organisation shall ensure that design tools are validated and maintained."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","5.4.2.3b","Requirement","ECSS-E-ST-10_0790078",1,"Created","The system engineering organisation shall document the hierarchy and assembly sequence of the system elements with the physical architecture."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","5.6.4c","Requirement","ECSS-E-ST-10_0790098",1,"Created","All interface requirements shall be accompanied by their verification requirements. "]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","6.7c","Requirement","ECSS-E-ST-10_0790131",1,"Created","The system engineering organization shall support QR and AR and ensure implementation of the QR and AR actions."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","D.2.1<3.4>a","Requirement","ECSS-E-ST-10_0790156",1,"Created","The SEP shall describe the strategy for acquisition of the items of the system or products defined in the product tree (e.g. make or buy, product line, incremental development)."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","D.2.1<5.4>a","Requirement","ECSS-E-ST-10_0790189",1,"Created","The SEP shall describe any specific issues, problems requiring dedicated attention, investigations or actions during the current phase and identify risks, and risk mitigation measures."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","D.2.1<6>a","Requirement","ECSS-E-ST-10_0790190",1,"Created","The SEP shall introduce the system engineering activities, to be conducted during subsequent phase(s) of the project, and as a minimum, list any identified critical issue and risk to be mitigated during the subsequent phase(s)."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","G.2.1<3>a","Requirement","ECSS-E-ST-10_0790216",1,"Created","The DDF shall contain a brief description of the product and of the main technical requirements throughout its life cycle phases (e.g. launch, deployed, operations, end-of-life)."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","K.2.1<2>a","Requirement","ECSS-E-ST-10_0790255",1,"Created","The DJF shall list the applicable and reference documents in support to its generation."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","K.2.1<8.3>b","Requirement","ECSS-E-ST-10_0790280",1,"Created","The DJF shall cover the system and all disciplines relevant to the product, addressing all acceptance verification activities in line with the system verification Plan (VP)."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","L.2.1<2>a","Requirement","ECSS-E-ST-10_0790289",1,"Created","The trade-off report shall list the applicable and reference documents in support to the generation of the document and include the reference to the following applicable documents:\n    1. Mission description document, if relevant\n    2. Technical requirements specification\n    3. System engineering plan\n    4. Project phasing and planning requirement document."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","N.2.1<2>b","Requirement","ECSS-E-ST-10_0790314",1,"Created","The RTM shall include the following:\n    1. Technical requirements specification (as defined in ECSS-E-ST-10-06 Annex A) of the product and its lower level elements\n    2. Product tree (as defined in ECSS-M-ST-10 Annex B)\n    3. Specification tree (as defined in ECSS-E-ST-10 Annex J)."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","P.2.1<4.8>a","Requirement","ECSS-E-ST-10_0790347",1,"Created","The PUM shall describe the conditions and procedures for the installation of the product, be it integrated or stand-alone."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","P.2.1<5.8>g","Requirement","ECSS-E-ST-10_0790380",1,"Created","Where the recovery method for a failure or group of failures is mode, mission, or phase dependent, separate procedures shall be described for each mode/mission phase."]
["ECSS-E-ST-10C","ECSS - Superseded v1.0","Q.2.1<5>a","Requirement","ECSS-E-ST-10_0790389",1,"Created","The analysis report shall describe the basic assumptions, the boundary conditions, validity of the analysis, life profile aspects, and all other related limitations."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.1.3i","Recommendation","ECSS-E-ST-31-02_1190269",1,"Created","Technical requirements should be expressed in a positive way, as a complete sentence (with a verb and a noun)."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.5.3.3.1e","Requirement","ECSS-E-ST-31-02_1190055",1,"Created","Mechanical and thermal performance analysis and test prediction shall be documented in a dedicated report in conformance with ECSS-E-ST-31, Annex C.\n    ","NOTE Analysis and test prediction can be split in two documents."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.6.3.2.2a","Requirement","ECSS-E-ST-31-02_1190083",1,"Created","The accuracy of test instrumentation shall be verified in accordance with approved calibration procedures."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.6.5c","Requirement","ECSS-E-ST-31-02_1190092",1,"Created","In cases where proof pressure test is not feasible, margins against mechanical failure shall be verified by analysis in accordance with ECSS-E-ST-32-02."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.6.9.2.2a","Requirement","ECSS-E-ST-31-02_1190117",1,"Created","The maximum heat transport capability shall be measured for tilt heights from zero to a value at which the heat transport capability falls to a value <5 % of the maximum heat transport capability (at the test temperature)."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","5.6.12c","Requirement","ECSS-E-ST-31-02_1190142",1,"Created","Aging tests shall be performed in the functional test sequence as given in Figure 5-2 with a duration of 300 hours."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","B.2.1<7>a","Requirement","ECSS-E-ST-31-02_1190184",1,"Created","The VP shall describe the selected combination of the different verification methods at the applicable verification levels and stages, in general and for each requirement type/group (including software). "]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","B.2.1<7>b","Requirement","ECSS-E-ST-31-02_1190185",1,"Created","The allocation of the requirements to the specific verification tasks shall be given."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","E.2.1<8>b","Requirement","ECSS-E-ST-31-02_1190216",1,"Created","When constraints are identified on activities sequence, the TSPE shall specify them including necessary timely information between test steps."]
["ECSS-E-ST-31-02C","ECSS - Superseded v1.0","G.2.1<1>a","Requirement","ECSS-E-ST-31-02_1190240",1,"Created","The TRPT shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.2.5.1b","Requirement","ECSS-E-ST-33-01_0820014",1,"Created","For non-critical mechanisms, conformance to the reliability figure shall be demonstrated by simplified methods (e.g. parts count or other methods accepted by the customer).\n    NOTE The methods to achieve by design, derive by analysis, and demonstrate by test the specified reliability figures are presented in ECSS-Q-ST-30."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.2.5.2f","Requirement","ECSS-E-ST-33-01_0820023",1,"Created","Unless redundancy is achieved by the provision of a complete redundant mechanism, active elements of mechanisms, such as sensors, motor windings, brushes, actuators, switches and electronics, shall be redundant."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.5.3c","Requirement","ECSS-E-ST-33-01_0820052",1,"Created","All operational constraints shall be documented in the mechanism user manual.\n    NOTE For the contents of the user manual, see Annex D."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.3.4.2a","Requirement","ECSS-E-ST-33-01_0820080",1,"Created","Ball bearings shall be pre-loaded with a load calculated in order to withstand the mechanical environment during launch and throughout the mission. "]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.5.2.6a","Requirement","ECSS-E-ST-33-01_0820113",1,"Created","For the structural factors of safety, requirements of ECSS-E-ST-32-10 shall apply."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.5.2.6b","Requirement","ECSS-E-ST-33-01_0820114",1,"Created","In the computation of safety margins the following minimum factors of safety shall be used for standard metallic materials:\n    1. yield stress factor of safety:  1,25\n    2. ultimate stress factor of safety:  1,5\n    3. buckling factor of safety:  2\n    4. minimum fatigue factor (cycles):  4 "]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.5.4.4b","Requirement","ECSS-E-ST-33-01_0820147",1,"Created","End stops shall be provided to prevent interference with interfacing equipment.\n    NOTE Regular end stops are provided for proper functioning of the actuated item."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.5.4.10c","Requirement","ECSS-E-ST-33-01_0820172",1,"Created","Threaded fasteners shall be designed to be fail-safe."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.7.1.1g","Requirement","ECSS-E-ST-33-01_0820190",1,"Created","If brush motors are used, it shall be verified under representative environment and over specified lifetime that debris generation does not result in electrical failure.\n    NOTE For example, short circuit of commutators."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.7.7.7e","Requirement","ECSS-E-ST-33-01_0820213",1,"Created","Connections shall be protected from harness induced loads."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.8.2.3a","Requirement","ECSS-E-ST-33-01_0820238",1,"Created","For the derivation of margins of safety clause 4.7.4.1 shall apply.\n    NOTE See ECSS-E-ST-31 for thermal analysis of mechanisms."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.8.2.15b","Requirement","ECSS-E-ST-33-01_0820271",1,"Created","Conformance of limited-life components to the lifetime requirements specified in the specific mechanism specification shall be verified by analysis, using as a minimum the lifetime factors specified in clause 4.8.3.3.14 in addition to the fatigue factor specified in clause 4.7.5.2."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.8.3.3.9b","Requirement","ECSS-E-ST-33-01_0820304",1,"Created","Electrical wires shall be tested to withstand a voltage of 500 V AC (50 Hz) applied between each other or between wires and the structure for a duration of 1 min without causing disruptive discharges. \n    NOTE For example, flash-over, spark-over and breakdown."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","4.8.3.3.9c","Requirement","ECSS-E-ST-33-01_0820305",1,"Created","Motor windings shall be tested to verify their insulation from the structure and from each other by not less than 100 MW with a DC voltage of at least five times the worst-case flight operating voltage applied for a duration of 2 min or until a steady state resistance value is measured."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","A.2.1<1>b","Requirement","ECSS-E-ST-33-01_0820338",1,"Created","The SMS shall list any applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-33-01C","ECSS - Superseded v1.0","B.2.1<1>c","Requirement","ECSS-E-ST-33-01_0820363",1,"Created","The MDD shall include any additional definition, abbreviation or symbol used."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.2.1a","Requirement","ECSS-E-ST-10-02_0740002",1,"Created","The customer shall define the project requirements, verification objectives and constraints affecting the supplier verification process.\n    NOTE For example, ground segment characteristics, launch service, envisaged end to end tests involving several suppliers. The usual general objectives are listed in clause 4.1.1 “Verification objectives”."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.2.2.1e","Requirement","ECSS-E-ST-10-02_0740011",1,"Created","If the impact of the requirement is major, a risk mitigation plan (part of the VP) shall be defined which includes a cross check based on two independent analyses (in terms of model used and suppliers)."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.2.4.1d","Requirement","ECSS-E-ST-10-02_0740036",1,"Created","When the verification programme includes a post landing stage, the verification shall not rely only on in-orbit activities or post landing activities."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.2.7b","Requirement","ECSS-E-ST-10-02_0740069",1,"Created","Verification planning to assess feasibility and support programmatics shall start in the early phases.\n    NOTE For example, during phase A."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.3.2.3b","Requirement","ECSS-E-ST-10-02_0740094",1,"Created","The Review-of-design report (RRPT) shall be in conformance with the DRD in Annex D."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","5.3.2.5c","Requirement","ECSS-E-ST-10-02_0740103",1,"Created","The Verification report (VRPT) shall be submitted to the Verification Control Board (VCB) after the completion of the last contributing verification activities, within the time frame agreed with the customer."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","A.2.1<4>a","Requirement","ECSS-E-ST-10-02_0740131",1,"Created","The VP shall briefly describe the subject of the verification process."]
["ECSS-E-ST-10-02C","ECSS - Superseded v1.0","C.2.1<4>b","Requirement","ECSS-E-ST-10-02_0740160",1,"Created","The TRPT shall contain the analysis of test data and the relevant assessment."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.2.1a","Requirement","ECSS-E-ST-33-11_0280005",1,"Created","In case of redundancy, no component shall adversely affect its substitute."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.2.2f","Requirement","ECSS-E-ST-33-11_0280014",1,"Created","It shall be agreed with the customer which performance characteristics shall be declared as mean values with associated standard deviation (see 4.2.2g). "]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.4a","Requirement","ECSS-E-ST-33-11_0280039",1,"Created","The timing of each function of the explosive system shall be specified."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.5.2.5a","Requirement","ECSS-E-ST-33-11_0280072",1,"Created","The fire function shall be the last action in the sequence."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.8.1.3b","Requirement","ECSS-E-ST-33-11_0280093",1,"Created","The capability shall be provided to test the components separately."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.8.2.2b","Requirement","ECSS-E-ST-33-11_0280105",1,"Created","A separate command shall activate each component for launch vehicles."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.8.3.1b","Requirement","ECSS-E-ST-33-11_0280138",1,"Created","Protective features shall \n    1. be provided to prevent unintended initiation, \n    2. be provided to prevent loss of performance,\n    3. be tested to verify effectiveness."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.9j","Requirement","ECSS-E-ST-33-11_0280163",1,"Created","Degradation of the explosives shall not exceed agreed limits."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.10.7f","Requirement","ECSS-E-ST-33-11_0280196",1,"Created","The receptacle shall meet the requirements of clause 4.10.1.\n    NOTE Sub-D connector, self-locking bayonet or triple start thread type can be used."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.10.11.1c","Requirement","ECSS-E-ST-33-11_0280205",1,"Created","It shall not be possible to arm the safe and arm device in case an initiator has been activated with the safe and arm device in safe position."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.11.1.1b","Requirement","ECSS-E-ST-33-11_0280230",1,"Created","For other elements of the system, which can be fully tested before flight, the equipment environmental test conditions of the end-user shall apply.\n    NOTE The requirements for explosive components are given below as measurements to be made after specific preconditioning and under survival and operational conditions identified in 4.6."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.11.3.1a","Requirement","ECSS-E-ST-33-11_0280254",1,"Created","The configuration of the connector shall be used only for initiators.\n    NOTE This is the integral (upper) part of the initiator."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.12.2a","Requirement","ECSS-E-ST-33-11_0280287",1,"Created","The properties of the separation nut and bolt given in Table 4-18 shall be quantified and conform to the figures where shown."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.12.4a","Requirement","ECSS-E-ST-33-11_0280296",1,"Created","The properties of the pusher given in Table 4-20 shall be quantified and conform to the figures where shown."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.14.3.2a","Requirement","ECSS-E-ST-33-11_0280329",1,"Created","Test operation shall be performed in conformance with ECSS-E-ST-10-03."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.15.2c","Requirement","ECSS-E-ST-33-11_0280354",1,"Created","The containers shall protect the component from the mission."]
["ECSS-E-ST-33-11C","ECSS - Superseded v1.0","4.17.2b","Requirement","ECSS-E-ST-33-11_0280387",1,"Created","Age-sensitive parts and materials shall be identified."]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","6.3.2a","Permission","ECSS-E-ST-20-06_0070166",1,"Created","Except in the case specified in 6.3.2c, floating conductive parts may be used if they have an area less than 1 cm2 and have a total capacitance less than 10 pF with respect to the structure. \n    NOTE This is to limit the energy available to discharge. "]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","6.4a","Requirement","ECSS-E-ST-20-06_0070030",1,"Created","A surface charging analysis shall be performed, including:\n    1. A systematic inventory of all surface materials, their resistivity, area and thickness.\n    2. A systematic inventory of triple-points, floating conductors and multiple-conductor element components."]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","6.8.2a","Requirement","ECSS-E-ST-20-06_0070063",1,"Created","Material parameters shall be ascertained through testing, either by the manufacturer or as part of the selection procedure. \n    NOTE Examples are bulk conductivity and surface conductivity."]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","7.2.3.2j","Requirement","ECSS-E-ST-20-06_0070088",1,"Created","The cells need not be illuminated, but available current and capacitance shall be simulated by power sources and external capacitors CSAT and CSA representing the satellite and solar array capacitances as shown in Figure 7-1. \n    NOTE When occurring spontaneously in space, a primary discharge arises from the discharge of the various capacitances on the solar array. A typical order of magnitude of the total capacitance is 200 pF to 500 pF on a GEO spacecraft under 3 kV (around 1 µC or 1 mJ)."]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","7.3c","Requirement","ECSS-E-ST-20-06_0070097",1,"Created","Requirements on high voltage systems in clause 8 shall apply all exposed parts of a power system."]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","10.2.7a","Requirement","ECSS-E-ST-20-06_0070130",1,"Created","Mechanical hazards to the spacecraft and the debris hazards to other spacecraft associated with a tether that breaks due to electrical burn-out or other cause shall be analysed. "]
["ECSS-E-ST-20-06C","ECSS - Superseded v1.0","11.3.2a","Requirement","ECSS-E-ST-20-06_0070155",1,"Created","Computer models shall include the geometry of the spacecraft and its operative environment including thruster, power supply, grounding scheme and surfaces surrounding the thrusters and its plume. "]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","4.1.4.2a","Requirement","ECSS-E-ST-60-20_0920012",1,"Created","A sensor with the autonomous star tracking capability shall have the minimum outputs:\n    1. the position of each star image with respect to a sensor-defined reference frame;\n    2. the Measurement date.\n        NOTE This capability does not imply the stars to be explicitly identified by the unit. However, it does include the ability to maintain the identification of each star image once selected, to correctly update the co-ordinates of each image as it moves across the detector, and autonomously manage the set of star images being tracked."]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","5.4b","Requirement","ECSS-E-ST-60-20_0920049",1,"Created","The maximum magnitude of body rate shall be used.\n    NOTE The maximum body rate is the worst case condition for most missions. For specific cases, the worst case can be adapted, e.g. to include jitter."]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","5.4k","Requirement","ECSS-E-ST-60-20_0920058",1,"Created","EOL simulations used to predict EOL performance shall be verified by test cases verifiable against measurable BOL data."]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","5.5.7.1b","Requirement","ECSS-E-ST-60-20_0920091",1,"Created","The supplier shall document the maximum error and minimum frequency of the spacecraft velocity provided to the sensor."]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","5.10.1a","Requirement","ECSS-E-ST-60-20_0920116",1,"Created","For both BOL and EOL, the performance metrics shall be specified either:\n    • From the whole celestial sphere including the vault in the statistics,or\n    NOTE The statistical ensemble is then composed of measurements randomly performed on the entire celestial vault.\n    • From a set of fixed directions in the celestial sphere."]
["ECSS-E-ST-60-20C Rev. 1","ECSS - Superseded v1.0","5.10.3b","Requirement","ECSS-E-ST-60-20_0920125",1,"Created","For lunar and planetary effects on performance the following conditions shall be met:\n    1. If a statement of operation with the Moon in the FOV is specified, quote the Sensor Settling Time for the ‘Moon in FOV’ scenario.\n    2. If a statement of operation with planetary objects in the FOV is specified, quote the Sensor Settling Time for the ‘Planet in FOV’ scenario."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.2.4.4b","Requirement","ECSS-E-ST-33-01_0820011",1,"Unchanged","If the design is not maintenance free, the maintenance requirements shall be documented in the SMS, justified, agreed by the customer."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.4.2c","Requirement","ECSS-E-ST-33-01_0820031",1,"Unchanged","The envelope of movement for each moving part shall be defined."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.3.1g","Requirement","ECSS-E-ST-33-01_0820064",1,"Unchanged","Metal to metal tribological sliding contacts shall be composed of dissimilar materials in conformance with 4.5.2.3."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.3.4.3a","Requirement","ECSS-E-ST-33-01_0820089",1,"Unchanged","Mechanical cables under friction used on moving parts or assemblies shall be lubricated in conformance with 4.7.3.1, 4.7.3.2 and 4.7.3.3."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.4.3c","Requirement","ECSS-E-ST-33-01_0820098",1,"Unchanged","The MLI clearance assessment shall take into account the dynamic envelopes of the MLI during vibration exposure and venting or purging or in orbit environment.","NOTE \tFor example, spin.\n"]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.5.3.2c","Requirement","ECSS-E-ST-33-01_0820126",2,"Normative Change","When the actuation torque or force is supplied by an electrically controlled device, the actuation torque or force supplied by this device shall be derived considering worst-case conditions.","NOTE \t1\tExamples of such electrical devices are electromagnetic motor, piezo actuator, pneumatic, or smart materials.\nNOTE \t2\tExample of such worst case conditions are supplied voltage, current, and frequency.\n"]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.5.4.4a","Requirement","ECSS-E-ST-33-01_0820146",1,"Unchanged","Mechanisms with restricted travel or rotation shall be provided with regular or emergency mechanical end stops to limit their motion and travel extremes to the maximum position specified in the SMS."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.5.4.5i","Requirement","ECSS-E-ST-33-01_0820408",1,"Created","In case recommendation 4.7.5.4.5h is not met, justification shall be provided and approved by the customer."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.5.4.11c","Requirement","ECSS-E-ST-33-01_0820175",1,"Unchanged","If venting to the outside of a lubricated enclosure is implemented, compatibility of the lubricant with the other spacecraft materials used and with contamination requirements specified in the specific mechanism specification shall be verified."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.7.7.5d","Requirement","ECSS-E-ST-33-01_0820206",1,"Unchanged","Electrical connectors shall be redundant."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.8.2.4a","Requirement","ECSS-E-ST-33-01_0820239",1,"Informative Change","For the derivation of margins of safety clause 4.7.5.2 shall apply.","NOTE \t 1\tStructural analysis includes stiffness, stress or strength, thermo-mechanical effects, fatigue and fracture control. See ECSS-E-ST-32 for structural analysis of mechanisms.\nNOTE \t 2\tThe objective is to demonstrate adequate sizing of the part and the overall assembly for all sizing cases.\n"]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.8.2.13e","Requirement","ECSS-E-ST-33-01_0820264",1,"Unchanged","Characterization of non­linearities shall take place over the full range of displacements and over the full specified qualification temperature range. "]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.8.2.17a","Requirement","ECSS-E-ST-33-01_0820273",1,"Unchanged","The sizing of magnetic or electromagnetic components shall be verified by analysis."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.8.3.3.5a","Requirement","ECSS-E-ST-33-01_0820294",1,"Unchanged","Mechanisms shall be verified by test to withstand release and end shocks caused by the motion of the mechanism. "]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.8.3.4.2c","Requirement","ECSS-E-ST-33-01_0820327",1,"Unchanged","The acceptance level testing shall be carried out at levels, which are higher than expected in flight but less than the qualification levels."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","4.9.3a","Requirement","ECSS-E-ST-33-01_0820333",1,"Unchanged","The assembly of mechanisms shall be performed in a clean environment specified by the customer."]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","A.2.1<6>g","Requirement","ECSS-E-ST-33-01_0820357",1,"Unchanged","The SMS shall specify the reliability requirements, to verify the conformity of the design, material and manufacture of elements to be cut used in release and locking.","NOTE \tSee 4.7.5.4.12c.\n"]
["ECSS-E-ST-33-01C Rev.1","ECSS - Superseded v1.0","D.2.1<9>a","Requirement","ECSS-E-ST-33-01_0820390",1,"Unchanged","The user manual shall describe all activities to operate the mechanism on ground, including:\n1.\tPreparation for start up:\n(a)\toperational configuration;\n(b)\tGSE and special tools to be used;\n(c)\titems to be removed;\n(d)\tspecific precautions and safety instructions including limitations in terms of operation and performances;\n(e)\tcleaning instructions;\n(f)\tenvironmental conditions for operation.\n2.\tStep by step Start up operation instructions.\n3.\tFor each operational mode \n(a)\toperational configuration;\n(b)\tGSE and special tools to be used;\n(c)\tspecific precautions and safety instructions including limitations in terms of operation and performances;\n(d)\tenvironmental conditions for operation;\n(e)\tstep by step operation instructions;\n(f)\ttelemetry requirements and health monitoring;\n(g)\trecovery contingencies.","NOTE \tExample of such operational modes are release, calibration, deployment, and pointing, scanning.\n"]
["ECSS-E-ST-32-10C Rev. 1","ECSS - Superseded v1.0","4.1.4.1a","Requirement","ECSS-E-ST-32-10_0110004",1,"Created","For determination of the Design Limit Load (DLL) the Design Factor shall be used, this is defined as the product of the factors defined hereafter.\n    ","NOTE Robustness of the sizing process is considered through the Design Limit Loads (DLL)."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","5.2.2.1a","Requirement","ECSS-E-ST-50-12_0910005",1,"Created","Each signal wire shall be 28 AWG, constructed from seven strands of 36 AWG silver-coated, high-strength copper alloy."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","5.2.3.5b","Requirement","ECSS-E-ST-50-12_0910017",1,"Created","The braided shield type shall be of push-back type and provide not less than 90 % coverage."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","5.2.4.10b","Requirement","ECSS-E-ST-50-12_0910038",1,"Created","The thickness of silver shall be 2,5 mm minimum."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","5.3.7c","Requirement","ECSS-E-ST-50-12_0910071",1,"Created","If a PCB mounting right-angled connector is used, signals connected to the top row shall be given correspondingly shorter PCB track lengths than tracks going to the bottom row. \n    ","NOTE The reason is that the topmost row of pins on the right-angled connect have longer leads than the bottom row."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","5.5.2.1a","Requirement","ECSS-E-ST-50-12_0910080",1,"Created","Differential pair signals shall run on a pair of close, parallel PCB tracks with a differential impedance of (100 ± 6) W.\n    ","NOTE This differential impedance can be achieved by adjusting the track thickness, width, separation and height above the ground plane."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","7.2b","Requirement","ECSS-E-ST-50-12_0910105",1,"Created","The data-control flag shall be set to zero to indicate that the current character is a data character. "]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","8.3i","Requirement","ECSS-E-ST-50-12_0910138",1,"Created","If an FCT is received when the credit count is at or close to its maximum value (i.e. within eight of the maximum value) then the credit count shall not be incremented and a credit error shall be flagged (see clause 8.5.3.6 and 8.9.2.4)."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","8.5.2.6a","Requirement","ECSS-E-ST-50-12_0910171",1,"Created","The Connecting state shall be entered from the Started state after a NULL is received (gotNULL condition set). "]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","8.5.3.7.3a","Requirement","ECSS-E-ST-50-12_0910190",1,"Created","The parity error shall be detected by the receiver in the link interface.\n    ","NOTE The parity error event occurs if a parity error is detected (see clause 7.4). "]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","8.9.1c","Requirement","ECSS-E-ST-50-12_0910204",1,"Created","Empty packets, which can be received in addition to these errors, shall be discarded."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","8.11.1a","Requirement","ECSS-E-ST-50-12_0910229",1,"Created","The delay between the reset of the Strobe signal and the Data signal shall be between 555 ns (i.e. the period of slowest permitted transmit clock, 2 MHz – 10 %) and the shortest clock cycle time for the transmitter (i.e. the period of maximum clock, dependent upon implementation)."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","10.2.2b","Requirement","ECSS-E-ST-50-12_0910262",1,"Created","A SpaceWire routing switch shall transfer packets from the input port of the switch where the packet arrives, to a particular output port determined by the packet destination address. \n    ","NOTE The destination address can comprise several data characters (see clause 9.2.2). "]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","10.2.3i","Requirement","ECSS-E-ST-50-12_0910271",1,"Created","Regional addressing shall be used for larger networks with each cluster limited to a maximum of 224 logical addresses.\n    ","NOTE Regions using logical addressing can be connected to regions using path addressing."]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","10.4a","Requirement","ECSS-E-ST-50-12_0910296",1,"Created","A SpaceWire network shall comprise two or more SpaceWire nodes and zero or more SpaceWire routing switches. "]
["ECSS-E-ST-50-12C","ECSS - Superseded v1.0","12.2.8a","Requirement","ECSS-E-ST-50-12_0910328",1,"Created","An implementation of a SpaceWire routing switch which includes the LVDS drivers and receivers shall conform to all of the requirements given in all clauses listed in Table 12-8. \n    ","NOTE A routing switch meeting this specification may use the following conformance statement:\n“This product conforms to the SpaceWire LVDS routing switch specification ECSS-E-ST-50-12.”"]
["ECSS-E-ST-32-10C Rev.2","ECSS - Superseded v1.0","4.3.2.3a","Requirement","ECSS-E-ST-32-10_0110025",1,"Unchanged","The factor of safety for global and local buckling shall be selected from Table 4-5.","NOTE \tThe factor of safety does not cover the knock down factors commonly used in buckling analyses - see Buckling handbook (ECSS-E-HB-32-24).\n"]
["ECSS-E-ST-10-04C","ECSS - Superseded v1.0","6.2.3d","Requirement","ECSS-E-ST-10-04_0760024",1,"Created","The solar cycle activity in Table A-1 of the normative annex shall be extended by repetition of the 11­year cycle.\nNOTE \tAugust 2008 can be assumed as start of cycle 24 unless another estimate with a higher confidence level is released from the Solar Cycle 24 Prediction Panel (at NOAA Space Environment Center (SEC) [RD.4])."]
["ECSS-E-ST-10-04C","ECSS - Superseded v1.0","7.2.2a","Requirement","ECSS-E-ST-10-04_0760033",1,"Created","The HWM-93 model [RN.6] shall be used."]
["ECSS-E-ST-10-04C","ECSS - Superseded v1.0","9.2.1.2.1b","Requirement","ECSS-E-ST-10-04_0760058",1,"Created","For conservative analysis, the upper case model shall be used."]
["ECSS-E-ST-10-04C","ECSS - Superseded v1.0","10.2.2.2a","Requirement","ECSS-E-ST-10-04_0760091",1,"Created","The meteoroid model shall be selected according to the mission altitude as follows: \n1.\tFor the analysis of meteoroid fluxes in Earth altitudes below 36 786,0 km, use either the meteoroid part of the MASTER-2005 model specified in clause 10.2.3 or the model specified in clause 10.2.4.\nNOTE \tThe meteoroid model in 10.2.3 is defined for particle masses from 10-12g to 100g. The meteoroid model defined in 10.2.4 is defined for particle masses from 10-18g to 100g. \n2.\tFor the analysis of meteoroid fluxes in orbits not covered by 10.2.2.2a.1 and between the mean Venus and Mars heliocentric orbits, use the model specified in clause 10.2.4. \nNOTE \t1\tThis includes the moon distance and the Lagrange points of the Sun-Earth system. \nNOTE \t2\tContributions from the meteoroid stream model specified in clause 10.2.4.5 can be neglected for orbits between Venus and Mars and not covered by 10.2.2.2a.1.\nNOTE \t3\tFor interplanetary orbits outside of the range defined in 10.2.2.2a.1 and 10.2.2.2a.2 no reference model is specified. Available interplanetary meteoroid flux models are given in Annex J.2.1.5."]
["ECSS-E-ST-10-04C","ECSS - Superseded v1.0","10.2.4.4b","Requirement","ECSS-E-ST-10-04_0760101",1,"Created","If applied near the Moon, Venus or Mars the corresponding attraction and shielding factors of Annex C.1.2 and C.1.3 shall be modified by exchanging the parameters for Earth by the corresponding ones for Moon, Venus and Mars."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","4.2.1h","Requirement","ECSS-E-ST-20_0020028",1,"Created","In case a cold redundant function is simultaneously activated together with the nominal one, by a deliberate or wrong command or due to a fault, this shall not induce permanent degradation of either of the two functions or loss of the mission before FDIR action.\n    NOTE E.g. thermal and EMC functions."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","4.2.2.2c","Recommendation","ECSS-E-ST-20_0020389",1,"Created","The margin on the throughput of on-board communication networks should be\n    1. for new developments, 50 % as a minimum at PDR on the average throughput;\n    2. such that real time overflow is avoided."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","4.2.4h","Requirement","ECSS-E-ST-20_0020071",1,"Created","Stimuli points on equipment and payload shall not provoke unwanted operation."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.4e","Requirement","ECSS-E-ST-20_0020104",1,"Created","The solar array interface voltage shall include voltage losses within the electrical circuitry of the solar array, including at least blocking diodes, wiring resistance and losses associated with harness interconnections in operational conditions."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.5.2i","Requirement","ECSS-E-ST-20_0020113",1,"Created","In the flight configuration, bleeding resistors shall be implemented.\n    NOTE Bleeding resistors are used to control both electrostatic charging and power loss from the solar array section and dissipation in the resistor itself in case of a cell string to panel short (including de-rating)."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.6.2c","Requirement","ECSS-E-ST-20_0020138",1,"Created","Specific measures shall be taken in the battery design to keep under control the series inductance and the magnetic moment."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.6.5.2c","Requirement","ECSS-E-ST-20_0020166",1,"Created","Where 5.6.5.2b is not met, the design shall mitigate the damaging effects of any such failure mode \n    NOTE E.g. by containment of cell leakage at battery level."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.7.2j","Recommendation","ECSS-E-ST-20_0020402",1,"Created","Fuses should be avoided to maintain the quality of the bus.\n    NOTE The rationale for requirement 5.7.2h to 5.7.2j is the following:\nIn order to be advantageous over an unregulated scheme, a regulated bus ensures a good regulation quality at the regulation point, including when the various loads on the bus are changing. The regulated bus is designed to ensure that normal transients including interdomain are within 5% all included. Abnormal transients are more than twice the normal transients; the load is then designed to operate nominally in normal transients and sustain without damage abnormal transients."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.7.5a","Requirement","ECSS-E-ST-20_0020204",1,"Created","For converters and regulators of the power system (solar array regulators, battery chargers and dischargers) the phase margin shall be at least 60° and the gain margin 10 dB for worst case end-of-life conditions with representative loading."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","5.8.2f","Requirement","ECSS-E-ST-20_0020237",1,"Created","Harness shall be tested up to connector brackets under 500 V DC between conductors, conductors and structure, conductors and shielding. \n    NOTE 500 V DC is selected in order to detect insulation defects potentially induced by air voltage breakdown."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","6.3.1.3b","Requirement","ECSS-E-ST-20_0020262",1,"Created","The minimum margins shall be 20 dB for safety critical circuits, and 6 dB for mission critical circuits."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","7.2.2.1a","Requirement","ECSS-E-ST-20_0020296",1,"Created","The antenna category (7.2.2.2), composing elements (7.2.2.2.4), used technologies (7.2.2.4) and the performance parameters (7.2.2.5) shall be established at the beginning of the project phase B."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","7.2.2.2.4a","Requirement","ECSS-E-ST-20_0020305",1,"Created","For array-fed reflector antennas clauses 7.2.2.2.2 (Reflector/Lens antennas) and 7.2.2.2.3 (Array antennas) shall apply."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","7.2.2.5a","Requirement","ECSS-E-ST-20_0020340",1,"Created","The characterisation of antenna performances shall cover the following parameters.\n    1. Coverage or Beam shape;\n    2. Directivity;\n    3. Electrical boresight or Beam pointing;\n    4. Gain or Beam efficiency;\n    5. Input impedance mismatch factor;\n    6. Radiation pattern;\n    7. Sense of polarization;\n    8. Side lobe level;\n    9. Polarisation purity or Axial ratio;\n    10. Group delay;\n    11. Noise temperature, for receive antennas;\n    12. Phase centre position;\n    13. Variations with frequency, angle (where applicable) and aging of all above parameters."]
["ECSS-E-ST-20C","ECSS - Superseded v1.0","7.4.4d","Requirement","ECSS-E-ST-20_0020362",1,"Created","Qualification testing shall be carried out \n    1. on RF non radiative passive components, or equipments, or systems, over the full qualification temperature range,\n    2. on RF radiative components, equipments or systems over a temperature range to be agreed with the customer, range which can be limited to ambient temperature."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.1h","Requirement","ECSS-E-ST-35-06_0200008",1,"Created","During the design phase the necessity of cleanliness verification shall be assessed.\n    ","NOTE 1 This applies from components to the design of systems, and to operations as not to generate contamination and to enable cleaning.\nNOTE 2 Figure B-1 of ECSS-Q-ST-70-01 gives an overview of space system cleanliness requirements organized in a cleanliness control flow chart."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.2.2.1b","Requirement","ECSS-E-ST-35-06_0200017",1,"Created","Tank internal structures shall allow for draining and cleaning.","NOTE Examples of such structures are diaphragms, bladders, baffles, and surface tension screens."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.3.2a","Requirement","ECSS-E-ST-35-06_0200050",1,"Created","ECSS-Q-ST-70-01 requirements for ‘Manufacturing’ and ‘Assembly and integration’ shall apply."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.3.5f","Requirement","ECSS-E-ST-35-06_0200075",1,"Created","It shall be determined which environmental classes apply to 4.3.5c and 4.3.5e.\n    ","NOTE See Annex A."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.4.1h","Requirement","ECSS-E-ST-35-06_0200099",1,"Created","In cases where a component or subsystem was originally dimensioned for a smaller size system, but incorporated into a larger one, the smaller size system shall determine the class selection."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","4.4.4i","Recommendation","ECSS-E-ST-35-06_0200390",1,"Created","Cleaning and test liquids should be selected from Annex D."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","5.2.2a","Requirement","ECSS-E-ST-35-06_0200141",1,"Created","Hardware that has been exposed to propellant shall be decontaminated before precision cleaning.","NOTE Example of such a hardware is propellant loading equipment."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","5.4.1f","Requirement","ECSS-E-ST-35-06_0200174",1,"Created","Precision cleaned articles shall be packaged immediately after verification and drying operations, or suitably protected prior to leaving the controlled environment.\n    ","NOTE See also clause 4.6d."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","5.5.3.4a","Requirement","ECSS-E-ST-35-06_0200199",1,"Created","Pre-filtered drying gas shall be flowed through or over the affected surfaces of the item being tested."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","5.5.5.2a","Requirement","ECSS-E-ST-35-06_0200208",1,"Created","The following items shall accomplish the vacuum drying processes:\n    1. Clean vacuum oven, with temperature control. \n        NOTE Typically, temperature ranging from 45 °C to 130 °C.\n    2. (Vent) gas, in conformance with clauses 5.5.2a, 5.5.2b and 5.5.2c or HEPA filtered air.\n    3. Thermocouple, for independent temperature monitoring of parts during procedure qualification."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","6.2.3b","Requirement","ECSS-E-ST-35-06_0200241",1,"Created","The standard test sample shall be 1 l of test liquid per m2 of critical surface area. \n    ","NOTE This is to ensure that all critical surfaces are being flushed. "]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","6.4.1b","Requirement","ECSS-E-ST-35-06_0200272",1,"Created","After testing for particle population and NVR, all hardware shall be dried in conformance with clauses 4.4.3 and 5.5 to remove residual cleaning, rinsing, or other verification media."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","7.5.3d","Requirement","ECSS-E-ST-35-06_0200298",1,"Created","The cutting, purging and sealing techniques shall be as follows.\n    1. The cutting does not generate particles.\n    2. Prior to final sealing of the plastic film bag containing the clean component, the plastic film bag is purged with filtered gaseous nitrogen, filtered to remove particulates greater than 2 mm (in conformance with ISO 14951-3, Grade A).\n    3. Sealing under the following conditions:\n        (a) An all-purpose impulse sealer is used to produce effective seals with plastic films. \n        (b) All items are handled in a manner that avoids exposure of the interior critical surfaces to airborne particles. \n        (c) One corner of the completely sealed test bag is cut off so that an opening of a maximum of 20 mm in length is created."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","8.1g","Requirement","ECSS-E-ST-35-06_0200307",1,"Created","The item shall be double-bagged and packed to prevent damage during storage and handling."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","11.1.2f","Requirement","ECSS-E-ST-35-06_0200332",1,"Created","For individual components having a critical surface area larger than 0,5 m2, e.g. tanks, the test fluid shall be collected in or transferred to a single container, agitated, then sampled from the top, centre and bottom to obtain in total 500 ml of the original test fluid sample for analysis."]
["ECSS-E-ST-35-06C Rev.1","ECSS - Superseded v1.0","B.2.1<4>c","Requirement","ECSS-E-ST-35-06_0200365",1,"Created","The selected cleaning materials, equipment and process conditions shall be listed."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","6.1g","Requirement","ECSS-E-ST-32-01_0810017",1,"Created","Potential fracture-critical items (PFCI) identified in conformance with 6.1a, 6.1c, 6.1d, 6.1e shall be included in the potential fracture-critical item list (PFCIL), specified in clause 6.4."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","6.3.3f","Requirement","ECSS-E-ST-32-01_0810037",1,"Created","For composite, bonded and sandwich parts the fatigue assessment shall be performed using the mean fatigue life material characteristics, a design life factor of 1 and a load enhancement factor of 1,15."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","6.4.3b","Requirement","ECSS-E-ST-32-01_0810056",1,"Created","When testing is used in addition to analysis of PFCIs, FCIs, contained and restrained items, the test method and test results shall be documented in test plans, specifications, procedures and reports in conformance with:\n    1. ECSS-E-ST-10-02 ‘Verification plan - DRD’,\n    2. ECSS-E-ST-10-03 ‘Test specification (TSPE) - DRD’,\n    3. ECSS-E-ST-10-03 ‘Test procedure (TPRO) - DRD’,\n    4. ECSS-E-ST-10-02 ‘Test report (TRPT) - DRD’.\n        NOTE The “Verification plan” can be limited to a “Test plan”."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","7.2.5g","Requirement","ECSS-E-ST-32-01_0810081",1,"Created","For the derivation of the proof loading to be applied for identification of initial crack sizes, in the case of through cracks, and in case the elastic-plastic approach is applicable, a factor of 1,3 shall be applied to the complete K-R curve, or an equivalent factor 1,69 if the J-R curve is used."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","8.2.3.1e","Requirement","ECSS-E-ST-32-01_0810114",1,"Created","The verification of 8.2.3.1d, shall demonstrate safe life against hazardous leakage and burst."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","8.4.2.2a","Requirement","ECSS-E-ST-32-01_0810141",1,"Created","Mechanical damage shall be considered in conformance with the damage threat assessment as specified in clause 8.4.3\n    NOTE For example, the following mechanical damage due to events which can occur during the service life, can be considered:\n        · Impact\n        · Scratch\n        · Abrasion."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","8.4.3.4a","Requirement","ECSS-E-ST-32-01_0810150",1,"Created","Close visual inspection shall be performed for each PFCI and FCI, just before each launch or just before closeout of surrounding structure after which mechanical damage is no longer credible, as determined in 8.4.3.2."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","8.7g","Requirement","ECSS-E-ST-32-01_0810183",1,"Created","Proof testing or NDI, consistent with the loading expected during service life, shall be conducted to screen for manufacturing flaws in each potential fracture-critical glass item based on the result of the fracture mechanics analysis, with the following conditions:\n    1. Proof testing is performed for acceptance of pressurized glass components (such as windows and viewports) to screen the flaws larger than the initial crack depth, with minimum proof pressure of two (2) times the MDP.\n    2. Proof testing is performed in an environment suitable to limit flaw growth during test.\n    3. Humidity and encapsulated water is removed from the surface of the glass before proof testing.\n        NOTE Encapsulated water can be accumulated during e.g. storage before proof testing"]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","10.3.1l","Requirement","ECSS-E-ST-32-01_0810210",1,"Created","The applied NDI procedures and the justification of their crack detection capability shall be approved by the customer.\n    NOTE This applies to all NDI procedures applied for implementation of fracture control, including standard NDI procedures. See also 10.4.2.1c."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","10.3.2e","Requirement","ECSS-E-ST-32-01_0810216",1,"Created","Glass items shall be inspected and proof tested in conformance with clause 8.7."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","10.4.3.2b","Requirement","ECSS-E-ST-32-01_0810249",1,"Created","For metals other than titanium, inspected with fluorescent penetrant to less than level 3 sensitivity as defined in 10.4.3.2a, the standard crack sizes of Table 10-1, defined for titanium alloys shall be applied."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","10.5.2.2.1c","Requirement","ECSS-E-ST-32-01_0810274",1,"Created","Specimens with induced defects shall be used in the inspection procedure as standard for calibration."]
["ECSS-E-ST-32-01C Rev. 1","ECSS - Superseded v1.0","11.2.2.3a","Recommendation","ECSS-E-ST-32-01_0810332",1,"Created","The requirements of clauses 8.5 and 8.7 may be replaced by the following requirement: structural glass and other non-metallic items (other than composites, bonded and sandwich items) shall be proof-tested at 1,2 times the limit load.\n    NOTE It is well-known that glass and other brittle items subjected to static load can be sensitive to growth of inherent flaws (i.e. static fatigue). This effect is normally considered in the structural verification, taking into account empirical data (e.g. statistical methods, taking into account the surface roughness of the item). "]
["ECSS-E-ST-50-01C","ECSS - Superseded v1.0","7.2a","Requirement","ECSS-E-ST-50-01_0240024",1,"Created","For turbo coding, the frame synchronization defined in clause 8 shall be used."]
["ECSS-E-ST-50-01C","ECSS - Superseded v1.0","8.2.3b","Requirement","ECSS-E-ST-50-01_0240033",1,"Created","For a turbo coding system, the ASM shall be acquired in the channel symbol domain (i.e. the code symbol domain of the turbo code)."]
["ECSS-E-ST-50-03C","ECSS - Superseded v1.0","5.2.1b","Requirement","ECSS-E-ST-50-03_0880013",1,"Created","The Transfer Frame Primary Header shall consist of six fields, positioned contiguously, in the following sequence:\n    1. Master Channel Identifier\t\t12 bits\n    2. Virtual Channel Identifier\t\t3 bits\n    3. Operational Control Field Flag\t1 bit\n    4. Master Channel Frame Count\t8 bits\n    5. Virtual Channel Frame Count\t8 bits\n    6. Transfer Frame Data Field Status\t16 bits","NOTE 1 All six fields are always present in a Transfer Frame Primary Header.\nNOTE 2 Figure 5-2 shows the format of the Transfer Frame Primary Header.\nNOTE 3 The Transfer Frame Primary Header covers the following main functions:\n            · to identify the data unit as a TM Transfer Frame;\n            · to identify the master channel and virtual channel to which the frame belongs;\n            · to provide a counting mechanism for the virtual channels and the master channel;\n            · to provide status fields related to the data in the Transfer Frame Data Field.                               "]
["ECSS-E-ST-50-03C","ECSS - Superseded v1.0","5.2.7.1b","Requirement","ECSS-E-ST-50-03_0880040",1,"Created","The Transfer Frame Data Field Status shall be contained within bits 32-47 of the Transfer Frame Primary Header."]
["ECSS-E-ST-50-03C","ECSS - Superseded v1.0","5.2.7.3c","Requirement","ECSS-E-ST-50-03_0880049",1,"Created","The Synchronization Flag shall signal the formatting of the Transfer Frame Data Field, as follows:\n    1. ‘0’ if octet-synchronized and forward-ordered packets or idle data are inserted;\n    2. ‘1’ otherwise.\n        ","NOTE 1 The values of the Packet Order Flag, the Segment Length Identifier and the First Header Pointer are also affected by the value of the Synchronization Flag. See clauses 5.2.7.4, 5.2.7.5 and 5.2.7.6\nNOTE 2 When the Synchronization Flag is set to ‘0’, the value of the First Header Pointer is used to distinguish between packets and idle data as defined in clause 5.2.7.6"]
["ECSS-E-ST-50-03C","ECSS - Superseded v1.0","5.3.2.1c","Requirement","ECSS-E-ST-50-03_0880074",1,"Created","The Transfer Frame Secondary Header Identification shall comprise two fields, positioned contiguously, in the following sequence:\n    1. Transfer Frame Secondary Header Version Number\t2 bits\n    2. Transfer Frame Secondary Header Length\t\t6 bits\n        ","NOTE Both fields are always present in a Transfer Frame Secondary Header Identification."]
["ECSS-E-ST-50-03C","ECSS - Superseded v1.0","5.4.3.5d","Requirement","ECSS-E-ST-50-03_0880107",1,"Created","Any idle packets extracted from Transfer Frame Data Fields shall be discarded."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","5.2.1e","Requirement","ECSS-E-ST-50-04_0890005",1,"Created","If the next lower sublayer below the segmentation sublayer is the transfer sublayer, then each TC Segment shall be placed in the Transfer Frame Data Field of a TC Transfer Frame such that the Transfer Frame Data Field contains exactly one complete TC Segment.\n    ","NOTE In this case, the length of the Transfer Frame Data Field is equal to the length of the TC Segment."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","5.4.2d","Requirement","ECSS-E-ST-50-04_0890028",1,"Created","If the blocking of packets is enabled for a MAP, then all data units for that MAP, that are passed to the segmentation sublayer from the next higher layer or sublayer at the sending end, shall be packets with the properties defined in clause 5.4.4."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","5.4.5d","Requirement","ECSS-E-ST-50-04_0890038",1,"Created","If the blocking function processes packets for the sequence-controlled service and packets for the expedited service, then all packets that are blocked into the same data unit shall be for the same service.\n    ","NOTE The transfer sublayer supports the sequence-controlled service and the expedited service."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","6.2.2.2c","Requirement","ECSS-E-ST-50-04_0890071",1,"Created","The Transfer Frame Version Number shall be set to the binary value ‘00’.\n    ","NOTE The value '00' defines version 1 of the TC Transfer Frame. Other values of this field are reserved."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","6.2.3a","Requirement","ECSS-E-ST-50-04_0890096",1,"Created","The Transfer Frame Data Field shall always be present in a TC Transfer Frame."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","6.2.4.2a","Requirement","ECSS-E-ST-50-04_0890105",1,"Created","The encoding procedure shall be as follows:\n    1. The encoding procedure accepts an (n-16)-bit TC Transfer Frame, excluding the Frame Error Control Field, and generates a systematic binary (n,n-16) block code by appending a 16-bit Frame Error Control Field as the final 16 bits of the codeblock.\n    2. The equation for the contents of the Frame Error Control Field is:\n\tFECF = [(X16 × M(X)) + (X(n-16) × L(X))] modulo G(X)\nwhere\n        • all arithmetic is modulo 2;\n        • FECF is the 16-bit Frame Error Control Field and the first bit transferred is the most significant bit, taken as the coefficient of the highest power of X;\n        • n is the number of bits in the encoded message;\n        • M(X) is the (n-16)-bit information message to be encoded expressed as a polynomial with binary coefficients, and the first bit transferred is the most significant bit M0 taken as the coefficient of the highest power of X;\n        • L(X) is the presetting polynomial given by:\n        • L(X) =  \t\t\t\t\n        • G(X) is the generating polynomial given by:\n        • G(X) = X16 + X12 + X5 + 1","NOTE 1 The X(n-16) × L(X) term has the effect of presetting the shift register to all ‘1’ state prior to encoding.\nNOTE 2 The encoding has the characteristics of a cyclic redundancy code.\nNOTE 3 A sample implementation of an encoder is described in Annex A."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","6.6.2a","Requirement","ECSS-E-ST-50-04_0890130",1,"Created","If the length of the candidate frame is less than the minimum length of a TC Transfer Frame, then the candidate frame shall be discarded."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","7.4.3.3d","Requirement","ECSS-E-ST-50-04_0890163",1,"Created","After each Accept Response to Request to Transfer FDU (AD service), but asynchronously from that response, FOP-1 shall send a transfer notification signal with the notification type set to one of the following confirm responses:\n    1. Positive Confirm Response to Request to Transfer FDU (AD Service)\n    2. Negative Confirm Response to Request to Transfer FDU (AD Service).\n        ","NOTE 1 The Positive Confirm Response to Request to Transfer FDU (AD Service) confirms that the FDU arrived at the receiving end and was acknowledged by a CLCW.\nNOTE 2 FOP-1 signals a Negative Confirm Response to Request to Transfer FDU (AD Service) when it is unable to guarantee that an FDU arrived at the receiving end, despite retry attempts. The negative confirm response does not carry a parameter giving the reason for the failure to confirm the requested data transfer service. However, whenever a condition is detected which can give rise to a negative confirm response, FOP-1 issues an Alert notification."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","7.8.2b","Requirement","ECSS-E-ST-50-04_0890189",1,"Created","The COP-1 control command contained in the Transfer Frame Data Field of a type-BC frame shall be one of the following:\n    1. Unlock, or\n    2. Set V(R).\n        ","NOTE All other uses of the Transfer Frame Data Field of a type-BC frame are reserved for future application."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","8.2.2a","Requirement","ECSS-E-ST-50-04_0890220",1,"Created","The Information field shall always be present in a BCH codeblock."]
["ECSS-E-ST-50-04C","ECSS - Superseded v1.0","8.2.3.3a","Requirement","ECSS-E-ST-50-04_0890229",1,"Created","The Filler bit, F0, shall always be present in a BCH codeblock."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","5.2.1.3a","Requirement","ECSS-E-ST-50_0970002",1,"Created","As an output from the requirements engineering activity, the customer shall produce the space communication system requirements specification (CSRD) in conformance with the DRD of Annex A."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","5.3.1b","Requirement","ECSS-E-ST-50_0970027",1,"Created","During emergency operations, bandwidth allocation priority shall be given to essential commands and telemetry.\n    ","NOTE For essential telecommand see 5.4.4b. For essential telemetry, see 5.5.2b"]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","5.4.4d","Requirement","ECSS-E-ST-50_0970036",1,"Created","For critical operations, execution of the essential commands shall not depend on software functions.\n    ","NOTE Example of critical operations is switching the transmitters on and off."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","5.6.12.3a","Requirement","ECSS-E-ST-50_0970079",1,"Created","Unwanted RF emissions shall be kept at a level such that they do not interfere with users of other bands.\n    ","NOTE Requirements on spurious emissions address both:\n        · a global limitation on the level of the spurious signals over the whole frequency spectrum, and\n        · special protection applicable to the band of the particularly interference-sensitive services: radio astronomy and deep space."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","5.6.14.5a","Requirement","ECSS-E-ST-50_0970093",1,"Created","The isochronous services shall be specified as a nominal data rate, a maximum nominal latency and a maximum deviation characteristic from that latency."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","A.2.1<5>c","Requirement","ECSS-E-ST-50_0970126",1,"Created","The CSRD shall summarize major project milestones relating to the communication system."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","B.2.1<6>b","Recommendation","ECSS-E-ST-50_0970229",1,"Created","The CSBD should: \n    1. list all communication system issues to be resolved by modelling or simulation, and\n    2. describe the modelling or simulation technique to be applied."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","B.2.1<10>a","Requirement","ECSS-E-ST-50_0970160",1,"Created","The CSBD shall describe any special project facilities for the development and implementation of the communication system (e.g. the modification of existing ground facilities, or the adaptation of reused flight software)."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","D.2.1<4>c","Requirement","ECSS-E-ST-50_0970185",1,"Created","The CSVP shall list any special tools or facilities to be used."]
["ECSS-E-ST-50C","ECSS - Superseded v1.0","H.2.1<4>d","Recommendation","ECSS-E-ST-50_0970234",1,"Created","The CSOM should include any procedure for the communication system reconfiguration that can be expected during the mission, such as the switch-over to a redundant communication chain, or the update of onboard routing tables;"]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","4.3.2.3a","Requirement","ECSS-E-ST-10-03_0750019",1,"Created","A PTR shall be held in order to formally declare the test completed and allow the release of the item under test and test facility for further activity.\n    ","NOTE The release of the test facility includes the breaking of the test configuration."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","4.3.3.3c","Requirement","ECSS-E-ST-10-03_0750030",1,"Created","The way the requirement 4.3.3.3b is achieved shall be agreed between the customer and the supplier."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","4.5.2b","Requirement","ECSS-E-ST-10-03_0750063",1,"Created","Qualification testing shall be conducted on dedicated qualification models except when using protoflight approach."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.1i","Requirement","ECSS-E-ST-10-03_0750096",1,"Created","Any space segment equipment pressurized during ascent shall be tested as specified in ECSS-E-ST-32-02 clause 5.4.4, and verified for internal pressure decay."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.5.1.3d","Requirement","ECSS-E-ST-10-03_0750121",1,"Created","The space segment equipment shall be either selected at random from production lot or be the qualification space segment equipment."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.5.2.3a","Requirement","ECSS-E-ST-10-03_0750130",1,"Created","Random vibration tests shall be conducted in launch configuration for all axes."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.5.3.2c","Requirement","ECSS-E-ST-10-03_0750169",1,"Created","The influence of temperature on test validity shall be in conformance with ECSS-E-ST-32-02 requirements 5.4.1c and 5.5.1b."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.5.4.1m","Requirement","ECSS-E-ST-10-03_0750187",1,"Created","In case of internal redundancy, thermal tests shall be performed on both chains taking into account the type of redundancy (e.g. hot or cold)."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","5.5.4.2d","Recommendation","ECSS-E-ST-10-03_0750456",1,"Created","In line with requirement 5.5.4.2c the test profile should start with a maximum non-operating temperature."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.1d","Requirement","ECSS-E-ST-10-03_0750221",1,"Created","The sequence of test shall be agreed by the customer depending on the nature of the space segment element and how performances are tested.","NOTE 1 For Infrared instrument or satellite including IR instrument the TV test is the one that allows performance verification, in this case it is often the last test performed.\nNOTE 2 For RF radiometer the performance are verified in anechoic chamber, in this case the auto compatibility / Radiated EMC is often one of the last tests performed."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.5.1.3b","Requirement","ECSS-E-ST-10-03_0750254",1,"Created","For cross-strapped configuration, requirements for performance tests shall be agreed with the customer."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.5.2.6a","Requirement","ECSS-E-ST-10-03_0750287",1,"Created","Acoustic tests shall be conducted with the element in launch configuration mounted on a test fixture."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.5.2.8g","Requirement","ECSS-E-ST-10-03_0750312",1,"Created","A resonance search shall be performed before and after the sinusoidal vibration tests to determine resonance frequencies to evaluate the product integrity and to compare the resonance frequency distribution with that of the mathematical model or modal survey.","NOTE 1 Any significant shift in resonance frequencies from those analytically determined is an indication of improper assembly or materials defects.\nNOTE 2 This resonance search can be used to update the Finite Element Model in case of design modification w.r.t. the previously tested model."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.5.3.3c","Requirement","ECSS-E-ST-10-03_0750330",1,"Created","Requirements of ECSS-E-ST-32-02 clauses 5.4.1 and 5.4.6 shall be applied for design burst pressure tests."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","6.5.4.1l","Requirement","ECSS-E-ST-10-03_0750345",1,"Created","The temperatures of all the space segment equipment shall be monitored to ensure that the space segment equipment are not damaged during test."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","7a","Requirement","ECSS-E-ST-10-03_0750378",1,"Created","Pre-launch tests shall confirm that all elements needed for the launch, including their interfaces are verified, and that their parameters are within the specified limits.\n    ","NOTE 1 Elements needed for the launch are: Launch segment element, space segment element and associated GSE.\nNOTE 2 For space segment element, the set of parameters checked as part of pre-launch testing is a sub set of those used during AIT. The definition of this sub set is subject to agreement with the customer."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","7j","Requirement","ECSS-E-ST-10-03_0750387",1,"Created","For crewed mission, final crew interface verification in all operational configurations shall be performed."]
["ECSS-E-ST-10-03C","ECSS - Superseded v1.0","B.2.1<7>a","Requirement","ECSS-E-ST-10-03_0750412",1,"Created","The TSPE shall describe the applicable test facility requirements together with the instrumentation and measurement accuracy, data acquisition and test space segment equipment to be used."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","4.2.4.2b","Requirement","ECSS-E-ST-20-07_0080007",1,"Unchanged","EMI control from residual ESD shall be performed by a combination of shielding and passive or active filtering techniques, implemented on the main structure, at subsystem level or inside equipment."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","4.2.13.2e","Requirement","ECSS-E-ST-20-07_0080042",1,"Unchanged","Overshields shall be bonded to chassis ground:\n    1. at both ends,\n    2. using a 360° direct contact or a bond strap of less than 30 nH\n        NOTE See NOTE of clause 4.2.11.2e."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.2.4a","Requirement","ECSS-E-ST-20-07_0080064",1,"Unchanged","The impedance of power sources providing input power to the EUT shall be controlled by Line Impedance Stabilization Networks (LISNs) for all measurement."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.2.5.1a","Requirement","ECSS-E-ST-20-07_0080073",1,"Unchanged","Clause 4.2.7 shall apply for tests involving high electromagnetic power or high voltage test equipment."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.2.6.6.3e","Requirement","ECSS-E-ST-20-07_0080098",1,"Unchanged","All power leads shall be supported 5 cm above the ground plane."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.2.9.4g","Requirement","ECSS-E-ST-20-07_0080131",1,"Unchanged","For frequency domain plots, emission data shall be reported in graphic form with frequency resolution of 1 %, or twice the measurement receiver bandwidth, whichever is less stringent."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.2.10.4a","Requirement","ECSS-E-ST-20-07_0080140",1,"Unchanged","The susceptibility criteria defined in the EMI test procedure shall be repeated in the test report, or the “as run” EMI test procedure shall be an annex to the EMI test report."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.3.8b","Requirement","ECSS-E-ST-20-07_0080163",1,"Unchanged","Absence of passive intermodulation products shall be verified in accordance with the requirements for “Passive intermodulation” specified in ECSS-E-ST-20."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.4.7.4c","Requirement","ECSS-E-ST-20-07_0080201",1,"Unchanged","The EUT shall be tested as follows:\n    1. Turn on the EUT and wait until it is stabilized.\n    2. Set the signal generator to the lowest test frequency, and increase the signal level until the testing voltage or current limit specified by application of clause 4.2.8, is reached on the power lead.\n    3. Repeat 5.4.7.4c.2 at all frequency steps through the testing frequency range.\n    4. Evaluate the susceptibility as follows.\n        (a) Monitor the EUT for degradation of performance.\n        (b) If susceptibility is noted, determine the threshold level in accordance with 5.2.10.3.\n    5. Repeat 5.4.7.4c.2 to 5.4.7.4c.4 for each power lead."]
["ECSS-E-ST-20-07C Rev. 1","ECSS - Superseded v1.0","5.4.11.3c","Requirement","ECSS-E-ST-20-07_0080220",1,"Unchanged","Test equipment shall be configured as specified in Figure 5-26."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","4.2.1b","Recommendation","ECSS-E-ST-20_0020022",2,"Normative Change","Redundant signal or power lines should be segregated via physically separated connectors and harnesses."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","4.2.1k","Requirement","ECSS-E-ST-20_0020031",1,"Unchanged","In case of signal cross-strapping, no single failure of either interface circuit shall propagate to the other one."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","4.2.3g","Recommendation","ECSS-E-ST-20_0020393",2,"Normative Change","For supplies and signals of pyrotechnics and non-explosive single shot device drivers, different connectors should be used for different classes of electrical functions."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","4.3.2c","Requirement","ECSS-E-ST-20_0020087",1,"Unchanged","FMECA shall be performed and based on the failure modes previously defined at component level."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.5.2g","Requirement","ECSS-E-ST-20_0020111",2,"Normative Change","In the flight configuration, solar array conductive panels and spacecraft structure shall be insulated from each other, disregarding the bleed resistor.","NOTE\t1\tExamples of such structural parts of the SA panel are hold-down mechanisms, yokes, hinges and CCL (Closed Cable Loop).\nNOTE\t2\tTypical value of insulation is in the order of 100 MΩ, and typical bleed resistor is in between 2 kΩ to 20 kΩ.\n"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.6.2e","Requirement","ECSS-E-ST-20_0020140",1,"Unchanged","Batteries having to tolerate a single fault shall be designed such that they can operate with one cell either failed shorted or open circuit."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.6.3b","Requirement","ECSS-E-ST-20_0020151",1,"Unchanged","The ability of a cell to meet mission lifetime requirements, where not covered by qualification life testing or previous in flight experience, shall be justified by the ground test data or by dedicated tests under representative conditions."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.7.2g","Recommendation","ECSS-E-ST-20_0020401",2,"Normative Change","For fully regulated buses, the nominal bus voltage value should be standardized according to the following:\n1.\t28 V for power up to 1,5 kW; \n2.\t50 V for power up to 8 kW;\n3.\t100 V and 120 V for higher power.","NOTE\t1\tBus voltage types are standardized in order to maximize the reuse of equipment.\nNOTE\t2\tThe rationale for this requirement is the following:\n\tIt is in practice difficult to design output impedance below 10 milliohm without an unwanted effect of the intrinsic connections and components resistance. For the design of a bus with 10 milliohm output impedance such that a 50 % load modulation induces a 1 % voltage change maximum as per 5.7.2i.1 requirement:\n\t0,5 P/U ´ 0,01 < 0,01U which means P < U2/0,5\n\tThus for\tU = 28 V, P < 1,57 kW\t\n\t\t\tU = 50 V, P < 5 kW\t\n\t\t\tU = 100 V, P < 20 kW\n\tIn practice, at 50 V for example, higher power has been used on telecom spacecraft buses, because the 1 % voltage change referred to a lower load change of 20 % to 30 % instead of 50 %.\n"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.7.5e","Requirement","ECSS-E-ST-20_0020208",2,"Normative Change","If a switching converter is externally synchronized, it shall deliver output voltages within specification for any increase or decrease of synchronizing frequency, intermediate amplitude of synchronizing signal, phase jumps, or loss and recovery of the signal."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.8.1b","Requirement","ECSS-E-ST-20_0020217",2,"Deleted","<<deleted, replaced by requirements 5.8.1q to 5.8.1v>>"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","5.8.2c","Requirement","ECSS-E-ST-20_0020234",2,"Normative Change","With the exception of the solar array and electrical bus bars, harness power lines shall be such that each line is twisted with its return, when the structure is not used as a return.","NOTE \tThe purpose of the requirements b and c is to minimize current loop area and harness inductance.\n"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","6.3.4.1a","Requirement","ECSS-E-ST-20_0020267",2,"Normative Change","A spacecraft charging protection programme shall be produced by the supplier for the PDR, and submitted to the customer for approval, in conformance with ECSS-E-ST-20-06 clause 5 and Annex A. "]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","6.4.2a","Requirement","ECSS-E-ST-20_0020290",1,"Unchanged","Safety margins for critical or EED circuit shall be demonstrated at system-level."]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","7.2.2.2.2a","Requirement","ECSS-E-ST-20_0020299",1,"Informative Change","The reflection and transmission properties (losses, depolarisation and diffusivity) of the reflecting or transmitting elements shall be quantified and their impact on antenna performances assessed.","NOTE \tReflector/Lens antennas are constituted by one or more radiating elements (7.2.2.3.1), possibly including an antenna RF chain (7.2.2.3.5), one or more (partially) reflecting or transmitting elements (reflectors - 7.2.2.3.2, lenses - 7.2.2.3.3) and an antenna support structure (in one or more portions- 7.2.2.3.6). If several radiating elements are present, also a Beam Forming Network can be present to distribute the RF signal (7.2.2.3.4). \n"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","7.2.2.4.1b","Requirement","ECSS-E-ST-20_0020332",1,"Informative Change","The impact of thermally-induced effects on the generation of passive intermodulation products shall be quantified and the impact on antenna performances assessed.","NOTE \tA typical example of thermally induced effects triggering the generation of PIM is the sudden releases of stresses in metal-to-metal joints due to temperature variations.\n"]
["ECSS-E-ST-20C Rev.1","ECSS - Superseded v1.0","7.4.3b","Requirement","ECSS-E-ST-20_0020357",1,"Unchanged","For each of the conditions identified in 7.4.3a, the frequencies, number of carriers and power levels of these carriers shall be determined. "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","4.3.2e","Requirement","ECSS-E-ST-20-08_0090010",1,"Unchanged","The accuracy of mass measurements shall be better than ±1 % or 0,01 g, whichever is higher."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.2b","Requirement","ECSS-E-ST-20-08_0090019",1,"Unchanged","The SCD-PVA shall be prepared by the supplier, in conformance with Annex A, and provided to the customer for reviewing and agreement."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.3.3.1c","Requirement","ECSS-E-ST-20-08_0090037",1,"Unchanged","Repair method shall be feasible in horizontal and vertical panel positions."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.4.3.6c","Requirement","ECSS-E-ST-20-08_0090076",1,"Unchanged","The maximum values of resistance shall be given in the SCD-PVA."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.1.3.3i","Requirement","ECSS-E-ST-20-08_0090101",1,"Unchanged","At least 3 thermocouples on the front side and 3 on the rearside of each qualification coupon shall be placed for temperature monitoring."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.1.3.4g","Requirement","ECSS-E-ST-20-08_0090110",1,"Unchanged","Monitoring of the continuity of the solar cell circuits shall:\n1.\tbe performed in conformance with clause 5.5.3.3.2,\n2.\ttake place during cycles for the complete activity,\n3.\tbe performed on a regular, at least daily basis for a number of cycles, such that:\n(a)\tduring 10 % of these cycles of the cell circuit, and\n(b)\tduring 90 % of these cycles on the protection diode network shall be monitored.\n4.\tbe performed by measuring both cell circuit continuity, at the beginning and at the end of the cycles in conformance to the relevant percentage specified in requirement 5.5.1.3.4g.3."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.3.2.5b","Requirement","ECSS-E-ST-20-08_0090143",1,"Unchanged","The insulator material shall show no evidence of delamination.","NOTE \tThe insulator material is usually kapton.\n"]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.3.2.14a","Requirement","ECSS-E-ST-20-08_0090168",1,"Unchanged","Welding of wires at string terminations and terminals shall be in conformance with the SCD-PVA."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.3.3.8b","Requirement","ECSS-E-ST-20-08_0090198",1,"Unchanged","The thermal sensor resistance shall be the value stated in the SCD PVA."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.3.8b","Requirement","ECSS-E-ST-20-08_0090225",1,"Unchanged","The reflectance shall be measured over a range from 280 nm to 2  500 nm."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","5.5.3.11.2a","Requirement","ECSS-E-ST-20-08_0090234",1,"Unchanged","The components to be checked for electrical continuity shall be identified in the SCD-PVA."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.3.3.2c","Requirement","ECSS-E-ST-20-08_0090267",1,"Unchanged","The accuracy of Iop and Vop shall be provided to the customer."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.4.3.1.4c","Requirement","ECSS-E-ST-20-08_0090292",1,"Unchanged","Defects of the types specified in requirement 6.4.3.1.4a occurring in the contact weld area shall be prevented."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.4.3.1.6a","Requirement","ECSS-E-ST-20-08_0090301",1,"Unchanged","There shall be no delamination or discolouration in the adhesive, except in the area opposite rear welds, where discolouration may be present."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.4.3.6.2c","Recommendation","ECSS-E-ST-20-08_0091076",1,"Unchanged","For subgroup B step 18 and for subgroup C, the portable absorptance and the normal emittance should be measured according to ECSS-Q-ST-70-09, provided that the same measurements have been performed in all samples of subgroup B step 15."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.4.3.9.2d","Requirement","ECSS-E-ST-20-08_0090348",1,"Unchanged","Any visible delamination of parts of the coverglass coating shall not exceed the limits specified in requirement 6.4.3.1.4e."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","6.6a","Requirement","ECSS-E-ST-20-08_0090391",1,"Unchanged","The supplier shall provide a data documentation package in conformance with Annex G for the qualification approval records and for each SCA delivery lot."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.3.1f","Requirement","ECSS-E-ST-20-08_0090416",1,"Unchanged","For cells with integral diode the acceptance tests described in Table 9‑1 shall be performed."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.3.2.2.4a","Requirement","ECSS-E-ST-20-08_0090425",1,"Unchanged","The BSCs tested in conformance with clause 7.3.2.2.2 and accepted shall be graded for Itest. performance "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.5.1.5.2d","Requirement","ECSS-E-ST-20-08_0090458",1,"Unchanged","Digs or depressions deeper than 0,025 mm shall not be present."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.5.5.2d","Requirement","ECSS-E-ST-20-08_0090483",1,"Unchanged","For multi-junction solar cells, it shall be ensured that the measurements are performed on the current limiting subcell, and that it is working close to short-circuit conditions."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.5.8.2c","Requirement","ECSS-E-ST-20-08_0090509",1,"Unchanged","The adhesive tape used for this test shall be clear in colour with an adhesive strength on steel of at least 0,28 N/mm.","NOTE \tFor measuring the adhesive strength on steel, EN 1939 can be used.\n"]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.5.13.2d","Requirement","ECSS-E-ST-20-08_0090524",1,"Unchanged","The nominal rate shall be lower than 5 × 1011 e- cm-2 s-1."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","7.8a","Requirement","ECSS-E-ST-20-08_0090549",1,"Unchanged","All deliverable hardware specified in the order shall be delivered together with documentation in conformance with the requirements specified in clause 7.7."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","8.6.2.2b","Requirement","ECSS-E-ST-20-08_0090582",1,"Unchanged","The coverglass qualification set shall be chosen statistically and at random from the first coating lots, as stated in the SCD-CVG.","NOTE \tFor sampling see ISO 2859.\n"]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","8.7.4.4a","Requirement","ECSS-E-ST-20-08_0090607",1,"Unchanged","The edge parallelism shall be as stated in the SCD-CVG. "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","8.7.6a","Requirement","ECSS-E-ST-20-08_0090616",1,"Unchanged","The normal emittance shall be measured according to ECSS-Q-ST-70-09."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","8.7.13.2e","Requirement","ECSS-E-ST-20-08_0090649",1,"Unchanged","Tests shall be performed in vacuum (pressure below 10-3 Pa) or in inert gas atmosphere."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","8.7.16c","Requirement","ECSS-E-ST-20-08_0090659",1,"Unchanged","The coverglasses shall show no degradation in the measured optical performance."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","9.2.2.2a","Requirement","ECSS-E-ST-20-08_0090682",1,"Unchanged","Delivered external protection diodes shall be processed and inspected in conformance with the requirements of the process identification document (PID) defined in clause 9.3, and "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","9.5.2d","Requirement","ECSS-E-ST-20-08_0090707",1,"Unchanged","The subgroup A tests applicable for bare solar cells shall be done on the integral protection diodes also. "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","9.6.5.2a","Requirement","ECSS-E-ST-20-08_0090739",1,"Unchanged","Each qualification sample shall be submitted to a burn-in process under ambient pressure conditions. "]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","9.6.13.2b","Requirement","ECSS-E-ST-20-08_0090772",1,"Unchanged","After the test, the samples shall be kept at temperatures below 50 °C until the diode characterization test is performed."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","9.6.18.2b","Requirement","ECSS-E-ST-20-08_0090797",1,"Unchanged","The life test shall always be preceded by a burn-in test as described in clause 9.6.6."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","10.1.2c","Requirement","ECSS-E-ST-20-08_0090819",1,"Unchanged","For bare solar cells and SCAs, testing, the largest dimension of the detector shall be less than half of the smallest dimensions of the cell, with a minimum dimension of 1 cm for rectangular detector, or a minimum area of 1cm² for circular detector."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","10.2.2.3.2a","Requirement","ECSS-E-ST-20-08_0090838",1,"Unchanged","The stability of the sensitivity of the SWS under operating conditions shall be verified by comparing the short-circuit current of five of the SWS before and after a photon-irradiation test with the short-circuit current of the remaining five SWS which are kept in the dark."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","11.1.3.3a","Recommendation","ECSS-E-ST-20-08_0091088",1,"Unchanged","The cell should be measured with the network analyser as follows:\n1.\tIf the measurement is performed at several temperatures in a thermostatic chamber:\n(a)\tWait for thermal equilibrium.\n(b)\tDetermine the resistance value of the shunt at each temperature (requirement 11.1.3.2c).\n2.\tDetermine and record the voltage of the power supply to obtain the bias voltages defined in clause 11.1.1.2 and set the power supply to 0 V at the end.\n3.\tMeasure the B/A ratios for the chosen bias voltages, as follows. For each bias voltage:\n(a)\tAdjust the power supply voltage to the determined value.\n(b)\tNote the cell and the shunt voltages.\n(c)\tMeasure the B/A ratios in the complex form X+j ´ Y; or in the amplitude |B/A| and phase j (B/A) from 10 Hz to 10 MHz, and store the data file in the network analyser.\n(d)\tNote or record the cell voltage change (to detect a temperature increase of the cell).\n(e)\tSet the power supply voltage to 0 V.\n(f)\tRecord the stored data file."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","11.2.2.1d","Recommendation","ECSS-E-ST-20-08_0091096",1,"Unchanged","External parallel capacitors to derive the capacitance of the qualification coupon or SCA should not be used because this parameter depends on the rate of change of the transient."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","A.2.1<8.3>d","Requirement","ECSS-E-ST-20-08_0090897",1,"Unchanged","For bleed resistor test, in conformance with clause 5.5.3.3.5, the SCD-PVA shall state the range of values, in kW, of the bleed resistor."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","B.2.1<6.15>a","Requirement","ECSS-E-ST-20-08_0090930",1,"Unchanged","In conformance with clause 6.4.3.17, the SCD-SCA shall include the minimum flatness, as a maximum deviation given in mm."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","C.2.1<7.15>a","Requirement","ECSS-E-ST-20-08_0090963",1,"Unchanged","In conformance with clause 7.5.18, the SCD-BSC shall include:\n1.\tThe deviation of total energy in the spectral region of 0,8 mm to 1,1 mm as a percentage, using a non-infrared rich solar simulator.\n2.\tThe maximum delta in Voc of the cell under both solar simulator conditions (1 S.C. (AM0) and non-infrared rich)."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","D.2.1<5>a","Requirement","ECSS-E-ST-20-08_0090969",1,"Unchanged","The SCD-CVG shall include the following coverglass materials characteristics:\n1.\tCoverglass base material, including doping elements and percentage (%).\n2.\tFront surface coatings (including conductive coatings).\n3.\tRear surface coatings."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","E.2.1<4>a","Requirement","ECSS-E-ST-20-08_0090996",1,"Unchanged","In conformance with requirement 9.2.1.2.2d, the SCD-EPD shall include the justification for any deviation in the in-process, acceptance and qualification tests."]
["ECSS-E-ST-20-08C Rev.1","ECSS - Superseded v1.0","G.2.1a","Requirement","ECSS-E-ST-20-08_0091020",1,"Unchanged","The PVA-DDP of coupons for the delivery review board (DRB) shall include, as a minimum, the following items:\n1.\ttable of contents;\n2.\tcertificate of conformance;\n3.\tshipping documents;\n4.\tconfiguration item data list (CIDL);\n5.\tproduct manufacturing and control file (PMCF);\n6.\tparts, materials and processes (PMP) list;\n7.\tlist of requests for deviations;\n8.\tlist of requests for waivers;\n9.\tlist of nonconformances, including copies of nonconformance reports (NCRs) NRB documentation including failure analysis and failed coupon list;\n10.\thistory record;\n11.\tconnector mate and de-mate record;\n12.\tserialized components list;\n13.\tin-process inspection test results, including positioning in the manufacturing flow chart;\n14.\topen work or open test;\n15.\treplacement or temporary installation record;\n16.\tacceptance and qualification test procedures and test reports;\n17.\tassembly drawings and circuit diagram;\n18.\tnotes and comments;\n19.\toperation and maintenance manuals and user restrictions;\n20.\tminutes of delivery review board (DRB) meetings;\n21.\tlower level data documentation packages (DDPs)."]
["ECSS-E-ST-10-24C","ECSS - Superseded v1.0","5.5d","Requirement","ECSS-E-ST-10-24_1290023",1,"Created","The CR shall be agreed and signed by each of the actors and by the interface responsible before it becomes applicable for implementation."]
["ECSS-E-ST-10-24C","ECSS - Superseded v1.0","5.6f","Requirement","ECSS-E-ST-10-24_1290032",1,"Created","If validation is included, the customer and suppliers shall agree on the interface validation approach."]
["ECSS-E-ST-10-24C","ECSS - Superseded v1.0","B.2.1<3>c","Requirement","ECSS-E-ST-10-24_1290056",1,"Created","The ICD shall include the following references:\n1.\tProduct tree (as defined in ECSS-M-ST-10 Annex B),\n2.\tSpecification tree (as defined in ECSS-E-ST-10)."]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","5.2.4.3a","Requirement","ECSS-E-ST-50_0970014",1,"Unchanged","During the space communication system implementation activity the supplier shall deliver the complete communication system to the customer. \n"]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","5.5.2a","Requirement","ECSS-E-ST-50_0970043",2,"Normative Change","The design of the space communication system shall enable essential telemetry to be acquired from critical monitoring points and transmitted to the ground, even when only one of the redundant parts of the other systems, including the CDMU, is operational.\n"]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","5.6.11.3b","Requirement","ECSS-E-ST-50_0970067",1,"Unchanged","The ability to operate under the worst case run length and transition densities shall be demonstrated by simulation during the analysis, implementation, and verification phases.\n"]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","5.6.12.1a","Requirement","ECSS-E-ST-50_0970076",1,"Unchanged","The space link media shall be used to communicate between spacecraft and ground segment and between one spacecraft and another spacecraft.\n"]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","5.7.1.4a","Requirement","ECSS-E-ST-50_0970101",2,"Normative Change","The on-board network shall provide the capability of performing asynchronous data transfers between connected nodes.\n"]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","A.2.1<5>c","Requirement","ECSS-E-ST-50_0970126",1,"Unchanged","The CSRD shall summarize major project milestones relating to the communication system."]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","A.2.1<7.2>a","Requirement","ECSS-E-ST-50_0970135",1,"Unchanged","The CSRD shall list the overall system requirements on the communication system including requirements related to: \n1.\toverall system availability and reliability, \n2.\tend­to­end performance,\n3.\tcommunication system lifetime, \n4.\tdesign and implementation, \n5.\tinterfaces to existing external entities, and \n6.\tcompatibility with specific communications protocols."]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","B.2.1<11>a","Requirement","ECSS-E-ST-50_0970161",1,"Unchanged","The CSBD shall describe the support to be provided to other spacecraft disciplines by the communication system supplier. \n    ","NOTE \tThis can include the provision of simulation models of communication system components, and test harnesses."]
["ECSS-E-ST-50C Rev. 1","ECSS - Superseded v1.0","D.2.1<7>a","Requirement","ECSS-E-ST-50_0970192",1,"Unchanged","The CSVP shall describe each verification test to be performed, including the following information for each one:\n1.\ta statement of the purpose of the verification test;\n2.\ta detailed description of the test;\n3.\ta list of the tools, equipment, or facilities to perform the test;\n4.\ta definition of the configuration of the test environment and the unit under test at the start of the test (i.e. pre­conditions);\n5.\ta description of the expected result (i.e. post­conditions);\n6.\tpass and fail criteria for the test.\n        ","NOTE \tThe purpose of these test description is to ensure that the verification tests can be repeated."]
["ECSS-E-AS-50-24C","ECSS - Superseded v1.0","4a","Requirement","ECSS-E-AS-50-24_1550001",1,"Created","CCSDS 231.0-B-3, TC Synchronization and Channel Coding, Issue 2, September 2010 shall apply with the following modifications listed in Table 4‑1."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.3.2.4a","Requirement","ECSS-E-ST-40_0860024",1,"Created","The autocode input models shall be reviewed together with the rest of the software specification, architecture and design.\n    NOTE The autocode input models are integral part of the software specification, architecture and design.\n","EXPECTED OUTPUT: Autocode input model review [MGT, SDP; SRR, PDR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.3.3.3a","Requirement","ECSS-E-ST-40_0860033",1,"Created","In addition to the software project reviews, software technical reviews (i.e. joint reviews organized under the responsibility of the customer or the supplier aiming at defining a technical baseline) shall be defined.\n","EXPECTED OUTPUT: Software technical reviews included in the software life cycle definition [MGT, SDP; SRR, PDR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.4.2.4a","Requirement","ECSS-E-ST-40_0860058",1,"Created","The supplier shall conduct a software requirement review (SWRR) as anticipation of the PDR, in conformance with 5.3.4.2b."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.5.4.2a","Requirement","ECSS-E-ST-40_0860091",1,"Created","The supplier shall integrate the software units and software components, and test them, as the aggregates are developed, in accordance with the integration plan, ensuring that each aggregate satisfies the requirements of the software item and that the software item is integrated at the conclusion of the integration activity. \n","EXPECTED OUTPUT: Software integration test report [DJF, - ; CDR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.7.3.3a","Requirement","ECSS-E-ST-40_0860119",1,"Created","The acceptance shall include generation of the executable code from configuration managed source code components and its installation on the target environment.\n","EXPECTED OUTPUT: Software product [DDF, - ; AR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.8.2.1a","Requirement","ECSS-E-ST-40_0860124",1,"Created","The verification process shall be established by the supplier to verify the software products.\n","EXPECTED OUTPUT: Software verification plan - verification process identification [DJF, SVerP; PDR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.9.2.3a","Requirement","ECSS-E-ST-40_0860159",1,"Created","The SOS entity shall establish procedures for receiving, recording, resolving, tracking problems, and providing feedback. \n    NOTE ECSS-Q-ST-80 clause 5.2.6 (nonconformances) and clause 5.2.5 (software problems) contain further requirements relevant for this clause.\n","EXPECTED OUTPUT: Software operation support plan - procedures for problem handling [OP, - ; ORR]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","5.10.4.2a","Requirement","ECSS-E-ST-40_0860184",1,"Created","All changes to the software product shall be documented in accordance with the procedures for document control and configuration management.\n","EXPECTED OUTPUT: Modification documentation [MF, - ;-]."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","B.2.1<4.4>f","Requirement","ECSS-E-ST-40_0860217",1,"Created","The computer infrastructure to be used shall be also described."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","B.2.1<5.2>e","Requirement","ECSS-E-ST-40_0860226",1,"Created","The SSS shall state the capabilities to be implemented by on-board control procedures (OBCP) (5.2.4.6)"]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","B.2.1<7>a","Permission","ECSS-E-ST-40_0860670",1,"Created","The system models may be placed as appendix to the SSS if a specification language is used to support the system and software co-engineering processes in order to enable the generation of the software specification and architecture from the (formal) system specification\n    NOTE The system specification language intends to produce in particular the computational model, the data model, the functional model, the event model and the failure model. The models include at least the definition of the logical properties, the liveliness properties and the timeless properties. The models are exercised to verify the properties by schedulability analysis or model checking. "]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","D.2.1<5.2>d","Recommendation","ECSS-E-ST-40_0860678",1,"Created","Each requirement definition should be organized according to the following:\n    1. General\n    2. Inputs\n    3. Outputs\n    4. Processing"]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","D.2.1<5.5>c","Permission","ECSS-E-ST-40_0860680",1,"Created","Diagrams may be used to show the intended operations and related modes–transitions."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","E.2.1<2>a","Requirement","ECSS-E-ST-40_0860316",1,"Created","The ICD shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","F.2.1<5.2>a","Requirement","ECSS-E-ST-40_0860350",1,"Created","The SDD shall describe the software architectural design, from a static point of view and also, when the software to be developed has real time constraints, from a dynamic point of view, and from a behaviour point of view."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","F.2.1<5.4.8>d","Permission","ECSS-E-ST-40_0860703",1,"Created","If the information in <5.4.8>c. is implicit in the definition of the type of component, a description need not be done. "]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","H.2.1<7.3>a","Requirement","ECSS-E-ST-40_0860408",1,"Created","The SUM shall describe through a block diagram the principal software parts of the system, including other software, such as operating systems, utilities, other supporting systems, and other facilities, equipment, or resources."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","I.2.1<4.2>a","Requirement","ECSS-E-ST-40_0860432",1,"Created","The SVerP shall describe the organization of the documentation review, proofs, and tracing activities. "]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","I.2.1<6.1>a","Requirement","ECSS-E-ST-40_0860441",1,"Created","The SVerP shall address the verification activities of each software item."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","J.2.1<6>b","Requirement","ECSS-E-ST-40_0860474",1,"Created","The SValP shall describe the selected approach to accomplish validation of those software specification requirements to be validated by inspection and analysis or review of design."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","K.2.1<7.3>a","Requirement","ECSS-E-ST-40_0860499",1,"Created","The SUITP shall describe all the features to be tested, making references to the applicable documentation."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","K.2.1<8.2.2>b","Requirement","ECSS-E-ST-40_0860508",1,"Created","Reference to appropriate documentation shall be made and traceability information shall be provided."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","L.2.1<5.4>a","Requirement","ECSS-E-ST-40_0860541",1,"Created","The SVS w.r.t. TS or RB shall describe the general criteria to be used to determine whether or not tests are passed."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","L.2.1<7.2.2>a","Requirement","ECSS-E-ST-40_0860559",1,"Created","The SVS w.r.t. TS or RB shall describe, for each test case, the inputs to execute the test case."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","N.2.1<4>a","Requirement","ECSS-E-ST-40_0860598",1,"Created","The SRF shall describe the technical and management information available on the software intended for reuse."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","N.2.1<8>b","Requirement","ECSS-E-ST-40_0860607",1,"Created","The SRF shall document the detailed results of the implementation of the identified corrective actions."]
["ECSS-E-ST-40C","ECSS - Superseded v1.0","O.2.1<5.3>d","Requirement","ECSS-E-ST-40_0860632",1,"Created","The selected design (architectural design and detailed design) methods shall be stated and referenced.\n    NOTE Reference to applied literature or other standards can be described here."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.1.1a","Requirement","ECSS-E-ST-40-07_1440002",1,"Created","All SMP fields, parameters, constants and properties shall be of either a Primitive Type as per PrimitiveTypes.h in [SMP_FILES], or a User Defined Type published to the Type Library.","NOTE\tThis specification is compliant with the types specified in Table 5-1.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.2b","Requirement","ECSS-E-ST-40-07_1440028",1,"Created","The ICollection at method shall return the element with the given position or name, with the following behaviour:\n1.\tIf no element exists with the given position or name, it returns nullptr."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.3.1h","Requirement","ECSS-E-ST-40-07_1440038",1,"Created","The IComponent GetFields method shall return a collection of the component fields as per FieldCollection in IField.h in [SMP_FILES]."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.5.2a","Requirement","ECSS-E-ST-40-07_1440059",1,"Created","All SMP Objects which represent a composition of child Components shall implement the IContainer interface as per IContainer.h in [SMP_FILES].","NOTE\t1\tThe container components life-cycle coincides with its parent one.\nNOTE\t2\tThe container is a named Object as per 5.2.1.\nNOTE\t3\tThe container allows adding children to a parent object.\nNOTE\t4\tEach container holds objects of only one type.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.8.2c","Requirement","ECSS-E-ST-40-07_1440095",1,"Created","The IRequest GetParameterCount method shall return the number of parameters of the request object.","NOTE\tThis operation only considers parameters of direction in, out or in/out, but not of type return.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.11.4f","Requirement","ECSS-E-ST-40-07_1440128",1,"Created","The ISimpleArrayField SetValues method shall allow setting all values of an array with the following arguments and behaviour:\n1.\tArguments:\n(a)\t“length” giving the length of the array with values to be set;\n(b)\t“values” giving an array of values to be set in the array.\n2.\tBehaviour:\n(a)\tIf the given length does not match the ArrayField length, it throws a InvalidArraySize as per InvalidArraySize.h in [SMP_FILES];\n(b)\tIf any of the given values simple type kind does not match the array item simple type kind, then it throws an InvalidFieldValue as per InvalidFieldValue.h in [SMP_FILES].\n(c)\tIf any of the given values simple type kind does match the array item simple type kind, then it stores the given values into the corresponding array item values."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.2.11.6c","Requirement","ECSS-E-ST-40-07_1440137",1,"Created","The IForcibleField Unforce method shall remove the forcing or freezing condition on the field so that GetValue called on the field returns the current field value.","NOTE\tThe handling of the forced field value within a model is undefined. \n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.2g","Requirement","ECSS-E-ST-40-07_1440164",1,"Created","The ITimeKeeper GetSimulationTime method shall return the Simulation time."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.4f","Requirement","ECSS-E-ST-40-07_1440197",1,"Created","The IEventManager Unsubscribe method shall remove a pair from the list, with the following arguments and behaviour: \n1.\tArguments:\n(a)\t“event” giving the ID of the event to be unsubscribed;\n(b)\t“entryPoint” giving a pointer to the entry point to be unsubscribed. \n2.\tBehaviour:\n(a)\tIf called with a pair of event identifier and entry point that is currently in the internal list, it removes this pair to the internal list;\n(b)\tIf called with a pair of event identifier and entry point that is not in the internal list, it throws an EntryPointNotSubscribed exception as per Services/EntryPointNotSubscribed.h in [SMP_FILES];\n(c)\tIf called with an invalid event id, it throws an InvalidEventId exception as per Services/InvalidEventId.h in [SMP_FILES]. "]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.7a","Requirement","ECSS-E-ST-40-07_1440212",1,"Created","The simulation environment shall provide a Simulator Object implementing the ISimulator interface as ISimulator.h in [SMP_FILES].","NOTE\t1\tThe ISimulator gives access to the simulation environment state and state transitions.\nNOTE\t2\tThe ISimulator interface provides methods to add models and to add and retrieve simulation services.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.7t","Requirement","ECSS-E-ST-40-07_1440231",1,"Created","The ISimulator GetLogger method shall return the interface of the mandatory logger service.","NOTE\tThis is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.9.1j","Requirement","ECSS-E-ST-40-07_1440264",1,"Created","The IPublication PublishProperty method shall allow publishing a property, with the following arguments and behaviour:\n1.\tArguments:\n(a)\t“name“ giving the property name;\n(b)\t“description“ giving the property description.\n(c)\t“uuid“ giving the property type.\n(d)\t“accessKind“ giving the property access restrictions as per AccessKind.h in [SMP_FILES] allowing the following values:\n(1)\tRead and write;\n(2)\tRead only;\n(3)\tWrite only.\n(e)\t“view“ giving its view kind attribute as per ViewKind.h in [SMP_FILES].\n2.\tBehaviour:\n(a)\tIf a Property with the same Name is already published, it updates the “description”, “uuid”, “accessKind” and “view” of the previous Property;\n(b)\tIf the given Uuid is not a valid Uuid of a registered type, it throws a TypeNotRegistered exception as per TypeNotRegistered.h in [SMP_FILES]."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.3.10.3a","Requirement","ECSS-E-ST-40-07_1440289",1,"Created","The simulation environment shall provide a class implementing the IStructureType interface as per Publication/IStructureType.h in [SMP_FILES]."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.4.1.2.3b","Requirement","ECSS-E-ST-40-07_1440322",1,"Created","A Named Element Id shall be unique in its Document."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.4.1.2.8c","Requirement","ECSS-E-ST-40-07_1440347",1,"Created","Reference upper bound shall be ‐1, larger or equal to Reference lower bound."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.4.1.2.10d","Requirement","ECSS-E-ST-40-07_1440356",1,"Created","A Parameter shall only have a default value if its type is Value Type."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","5.4.1.3h","Requirement","ECSS-E-ST-40-07_1440373",1,"Created","Each public Property of an interface, model or service shall be defined in a catalogue."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","6.1.4.6b","Requirement","ECSS-E-ST-40-07_1440418",1,"Created","The access specifier of the Property member methods shall be defined as follows:\n1.\tIf the Operation belongs in an Interface, the member is public;\n2.\tIf the Operation does not belong in an Interface, the mapping of the Visibility attribute is used.","NOTE\tSee clause 6.1.3 for details on the mapping of Visibility attributes.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","6.1.4.7a","Requirement","ECSS-E-ST-40-07_1440428",1,"Created","Operation elements shall be mapped to ISO/ANSI C++ member methods as follows:\n1.\tIf neither the Operator nor the Constructor attribute is set, syntax is as per “Operation” template in Table 6-1.\n2.\tIf the Operator attribute is set, syntax is as per “Operator” template in Table 6-1.\n3.\tIf the Constructor attribute is set, syntax is as per “Constructor” template in Table 6-1.","NOTE\t1\tOperator and Constructor attributes cannot be both set at the same time for a given Operation element as they are mutually exclusive.\nNOTE\t2\tConstructor methods inherit the name from the element the Operation is member of, therefore their own Name attribute is ignored.\n"]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","6.1.5.2b","Requirement","ECSS-E-ST-40-07_1440462",1,"Created","Literal elements shall be mapped to ISO/ANSI C++ enumeration literals with value assignment as per “Literal” template in Table 6-1."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","6.1.6.4f","Requirement","ECSS-E-ST-40-07_1440487",1,"Created","If the Exception type has the Abstract attribute set to “true”, the destructor shall be declared as pure virtual."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","6.2.3f","Requirement","ECSS-E-ST-40-07_1440521",1,"Created","The Initialise function shall call the Initialise$Package.Name$ ( ) function."]
["ECSS-E-ST-40-07C","ECSS - Superseded v1.0","D.2.1e","Requirement","ECSS-E-ST-40-07_1440546",1,"Created","In the SMP Manifest file the, the Value shall start at the first non-whitespace character after the colon (“:”), and is terminated by the end of line."]
["ECSS-S-ST-00C","ECSS - Superseded v1.0","9.3b","Requirement","ECSS-S-ST-00_1000006",1,"Created","The documentation identifying the compliance to ECSS requirements applicable to the project (e.g. the ECM) shall include following data:\n    1. The complete list of ECSS requirements applicable to the project (e.g. in the EARM).\n    2. For each requirement, the actual indication of compliance. When deviation is identified the justification is provided."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","5.2.3b","Requirement","ECSS-E-ST-10-02_0740031",1,"Unchanged","When a requirement is fully verified at lower level, the traceability to lower level verification evidence shall be identified."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","5.2.6.1b","Requirement","ECSS-E-ST-10-02_0740055",2,"Normative Change","All verification tools shall be validated and maintained for their intended use."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","5.2.6.4a","Requirement","ECSS-E-ST-10-02_0740064",1,"Unchanged","Simulators shall be verified to demonstrate that the simulator characteristics are representative of the simulated product to the extent required for the verification to be supported."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","5.3.2.4a","Requirement","ECSS-E-ST-10-02_0740097",2,"Normative Change","The Inspection report shall be submitted for each Inspection verification task identified in the Verification Plan to the Verification Control Board (VCB) after the inspection completion, within the time frame agreed with the customer."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","5.4.3b","Requirement","ECSS-E-ST-10-02_0740120",1,"Unchanged","The Verification Control Document (VCD) shall be updated by the supplier to record as open, those requirements subject to re-verification until this is performed and closeout agreed by the customer."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","A.2.1<6>a","Requirement","ECSS-E-ST-10-02_0740133",1,"Unchanged","The VP shall describe the selected models and the associated model philosophy, product matrix."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","E.2.1<3>a","Requirement","ECSS-E-ST-10-02_0740176",2,"Normative Change","The Inspection Report shall list the applicable dictionary or glossary and the meaning of specific terms or abbreviations utilized in the document with the relevant meaning."]
["ECSS-E-ST-10-02C Rev.1","ECSS - Current v1.0","F.2.1<4>b","Requirement","ECSS-E-ST-10-02_0740185",2,"Normative Change","The Verification Report shall identify the deviations from the verification plan."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","5.2.3.9a","Requirement","ECSS-E-ST-10_0790028",2,"Normative Change","The system engineering function shall establish the list of documents constituting the system requirements baselines in contribution to the configuration baselines.","NOTE\tDetails on configuration baselines are provided in ECSS-M-ST-40.\n"]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","5.3.4g","Requirement","ECSS-E-ST-10_0790053",2,"Normative Change","The system engineering function shall ensure that modelling and test accuracy as well as limitations are considered (as part of Annex K) when establishing the performances and specifying environmental conditions for product verification."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","5.4.1.2b","Requirement","ECSS-E-ST-10_0790062",2,"Normative Change","The system engineering function shall apportion and control budget requirements to all levels of system decomposition."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","5.6.1b","Requirement","ECSS-E-ST-10_0790087",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","5.6.9b","Requirement","ECSS-E-ST-10_0790110",2,"Normative Change","The system engineering function shall provide a technical assessment on any nonconformance to the status of the product ","NOTE \tNonconformance treatment is described by ECSS-Q-ST-10-09.\n"]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","C.2.1b","Requirement","ECSS-E-ST-10_0790147",1,"Unchanged","This report shall address all technical (e.g. engineering disciplines), programmatic and related aspects relevant to the system."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","D.2.1<5.1.2>b","Requirement","ECSS-E-ST-10_0790172",1,"Unchanged","The SEP shall define the process and control to be put in place to meet requirements for the thermal, structures, mechanisms, environmental control and life support, propulsion, pyrotechnics, mechanical parts, and materials functions and interfaces.","NOTE\tThese requirements refer to Mechanical engineering as defined in ECSS-E-ST-3x series of standards.\n"]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","D.2.1<5.1.2>k","Requirement","ECSS-E-ST-10_0790181",1,"Unchanged","The SEP shall define the process and control to be put in place to meet requirements for human activities and environments associated with space systems. ","NOTE\tThese requirements refer to Human factors engineering as defined in ECSS-E-ST-10-11.\n"]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","G.2.1<2>a","Requirement","ECSS-E-ST-10_0790213",1,"Unchanged","The DDF shall contain the list of applicable and reference documents, used in support to the generation of the document. "]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","H.2.1<2>a","Requirement","ECSS-E-ST-10_0790238",1,"Unchanged","The function tree document shall contain the list of applicable and reference documents, used in support to the generation of the document."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","I.2.1<5>a","Requirement","ECSS-E-ST-10_0790247",1,"Unchanged","The technical budget shall contain a conclusion that identifies the key engineering parameters having a negative margin, and identify for each of those:\n1.\tthe impact on the technical requirements and the associated risk for the project, and\n2.\tthe specific program to conform to the specified value and for project risk mitigation."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","K.2.1<7>e","Requirement","ECSS-E-ST-10_0790271",1,"Unchanged","The DJF shall reference the requirements traceability matrix, e.g. w.r.t. building up the justification of a considered system top level requirements in terms of the various elements contributing to it, including where relevant contribution from other disciplines (e.g. pointing as a function of thermal, structures, and AOCS)."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","L.2.1<10>b","Requirement","ECSS-E-ST-10_0790304",1,"Unchanged","The trade-off report shall present the identified technical and programmatic risks induced by the choice of the recommended solution, and any additional activity necessary to be performed for risk mitigation."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","P.2.1<4.1>a","Requirement","ECSS-E-ST-10_0790338",1,"Unchanged","The PUM shall include the following:\n1.\tsummary of the product design, showing the definition of the product, its constituents, the distribution of functions and the major interfaces;\n2.\tblock diagram of the product;\n3.\ttop-level description of the product software architecture;\n4.\tdescription of nominal product operations scenarios and constraints e.g. mutually exclusive modes of operation, power or resource sharing."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","P.2.1<5.3>a","Requirement","ECSS-E-ST-10_0790363",2,"Normative Change","The following shall be provided for each product constituent:\n1.\ta detailed design description, including block diagrams, functional diagrams, logic and circuit diagrams;\n2.\tphysical characteristics including location and connections to the support structure, axes definition and alignment where relevant, dimensions and mass properties;\n3.\tprinciple of operation and operational constraints of the product constituent;\n4.\tlower level of breakdown for products composed of many complex elements."]
["ECSS-E-ST-10C Rev.1","ECSS - Current v1.0","P.2.1<5.6>c","Requirement","ECSS-E-ST-10_0790372",1,"Unchanged","Each telecommand shall have a functional description with utilization conditions (e.g. pre-transmission validity, criticality level), command parameters (syntax and semantics) and execution verification in telemetry."]
["ECSS-E-ST-10-06C","ECSS - Current v1.0","7.2.2b","Requirement","ECSS-E-ST-10-06_0770004",1,"Created","The responsible entity of the specification shall define the content and format of the attributes listed in clause 8."]
["ECSS-E-ST-10-06C","ECSS - Current v1.0","8.2.6a","Requirement","ECSS-E-ST-10-06_0770028",1,"Created","A technical requirement shall be identified in relation to the relevant function, product or system."]
["ECSS-E-ST-10-06C","ECSS - Current v1.0","A.2.1<2>a","Requirement","ECSS-E-ST-10-06_0770045",1,"Created","The TS shall list the applicable and reference documents in support of the generation of the document."]
["ECSS-E-ST-10-09C","ECSS - Current v1.0","5.3.2b","Recommendation","ECSS-E-ST-10-09_0230093",1,"Created","Recognised international names should not be used if the exact definition is not followed.\n    ","NOTE E.g. the name “Pseudo True of Date” can be used if the conventional definition of ToD is not strictly followed."]
["ECSS-E-ST-10-09C","ECSS - Current v1.0","5.4.6a","Requirement","ECSS-E-ST-10-09_0230049",1,"Created","The specification of geodetic/planetocentric coordinates shall include the parameters of the ellipsoid used, direction and origin of longitude, and definition of the North Pole."]
["ECSS-E-ST-10-09C","ECSS - Current v1.0","A.2.1<7>b","Requirement","ECSS-E-ST-10-09_0230082",1,"Created","The CSD shall describe all parameterisations used within a transformation (e.g. quaternions, Euler angles), including the applicable type of coordinate systems where this parameterisation is allowed."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.3.2a","Requirement","ECSS-E-ST-10-11_0780015",1,"Created","Throughout the project the HFE shall:\n    1. be responsible for establishing and updating of the users’ roles,\n    2. be responsible for the definition, maintenance and verification of system human related requirements,\n    3. support and approve establishing and updating of users manuals, operations nomenclature and procedures,\n    4. support and approve definition, design, development and assessment of the required Crew Systems,\n    5. support and approve definition, design, development and assessment of the required Human Computer Interface software,\n    6. support and approve definition, design, development and assessment of the required Training Materials."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.3.4c","Requirement","ECSS-E-ST-10-11_0780020",1,"Created","The user manual shall follow project review cycles, and be kept under configuration control."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.4.3.6d","Requirement","ECSS-E-ST-10-11_0780048",1,"Created","Design evaluations shall be organised into Evaluation Events"]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.7.4a","Requirement","ECSS-E-ST-10-11_0780081",1,"Created","Architecture complements specified in 4.7.4c shall be provided for all elements being part of a mission infrastructure that foresee the presence of human crew either in the pressurised or un-pressurised parts.\n    NOTE Architecture complements functions are provided according to the mission and functions of the human infrastructure."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.7.6b","Requirement","ECSS-E-ST-10-11_0780090",1,"Created","Work station shall be either outfitted with equipment (including lights) and tools (including restrains) to support the foreseen crew activities or shall be provided with the necessary restraints and hook points to enable their outfitting."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.9.3c","Requirement","ECSS-E-ST-10-11_0780115",1,"Created","All resources and boundary conditions shall be compatible with the work/rest cycles of the crew as defined according to clause 4.5.4."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","4.10.2.4a","Requirement","ECSS-E-ST-10-11_0780148",1,"Created","Whole System Simulations shall be included in the System Engineering Plan.\n    NOTE 1 In order to avoid so called “human errors” and regardless if Phase C/D and Phase E are in two separated contracts several Whole System Simulations must be held when the flight segment is operatively tested/verified with the ground segment and with the users that are operating them.\n    NOTE 2 The purpose of Whole System Simulations is also to verify achievement of high level human in the loop requirements together with timeline and other ops products feasibility considerations and communication verification"]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","B.2.1<2>a","Requirement","ECSS-E-ST-10-11_0780181",1,"Created","The HFE analysis and simulation report shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-10-11C","ECSS - Current v1.0","D.2.1<2>a","Requirement","ECSS-E-ST-10-11_0780193",1,"Created","The HFE test report shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","5.5.3.1a","Requirement","ECSS-E-ST-10-12_0980017",1,"Created","It shall be demonstrated that the equipment reliability requirements include the potential for large uncertainties in predicting SEE.\n    NOTE 1 For a rationale, see clause 5.1.3\n    NOTE 2 It is common practice in SEE evaluation to use worst-case environmental assumptions and perform worst-case analysis of system impacts. As indicated in clause 5.2, when such worst-case analysis is performed, additional margins are not applied.\n    NOTE 3 Prediction errors of a factor 10 are possible in some circumstances."]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","6.3.2.1a","Requirement","ECSS-E-ST-10-12_0980042",1,"Created","The effect of the parts packaging in the radiation shielding model shall be assessed as follows:\n    1. Place the target point inside the package, located on top or inside the active region of the volume \n        NOTE The objective is to get the best possible estimate of the deposited dose at die level, the target point. The active region is typically a silicon chip.\n    2. For hybrid devices containing several sensitive dies, use one target point per die.\n        NOTE The reason is that the calculated dose level can vary significantly depending on the die location.\n    3. For situations where the total ionising dose from X-ray or g-ray fields is the largest contribution, assess the influence of local high-Z materials and include it in the calculations.\n        NOTE Example of high-Z materials are gold contacts or tungsten silicide layers and vias."]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","9.4.1.1a","Requirement","ECSS-E-ST-10-12_0980075",1,"Created","When predicting component SEE rates, the following shall be assessed:\n    1. The probability of SEE occurrence for the environments as specified in clause 9.2, using the methods specified in clause 9.4.1.2 to 9.4.1.8.\n        NOTE 1 More information on this method is available in ECSS-E-HB-10-12 Section 8.2.\n        NOTE 2 Total ionising dose induced in semiconductors can increase sensitivity to single event effects. Therefore, potential SEE/TID synergy can be important in special cases, both in estimating single event rate for the operating environment, as well as assessing the suitability of data collected from proton and ion beam irradiations. \n        NOTE 3 In some special cases, single event effect rates have been shown to vary significantly depending upon the angle of incidence of the incident particle, even for protons and neutrons.\n    2. The influence of shielding in attenuating the primary particle environment and modification to its spectrum, as specified in Clause 6.\n        NOTE The effects of the component packaging (as described in Clause 6.3) can be considered. "]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","9.4.1.5a","Requirement","ECSS-E-ST-10-12_0980084",1,"Created","For SEL and SESB experimental data shall be used to determine the LET threshold for susceptibility to SEL or SESB."]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","10.4.1b","Requirement","ECSS-E-ST-10-12_0980109",1,"Created","Background effects in instruments shall be analysed using:\n    1. calculations or simulations of the energy-deposition processes in sensitive volumes, or\n    2. results from particle accelerator irradiations of the instrument or its sensitive components, or\n    3. a combination of both of the requirements 10.4.1b.1 and 10.4.1b.2."]
["ECSS-E-ST-10-12C","ECSS - Current v1.0","11.3a","Requirement","ECSS-E-ST-10-12_0980134",1,"Created","Radiobiological effects resulting from the following environments shall be analysed for all manned missions:\n    1. trapped proton and electron belts (terrestrial and other planetary belts);\n    2. solar protons and ions;\n    3. cosmic ray protons and heavier nuclei;\n    4. bremsstrahlung produced as secondaries from electrons;\n    5. secondary protons, neutrons and other nuclear fragments which can be generated in atmospheric showers in the planetary environment or within the spacecraft or planetary-habitat structure, including the body itself. \n        NOTE This contribution is particularly important for cosmic-ray induced secondaries.\n    6. emmisions from radioactive or nuclear-energy sources on the spacecraft.\n        NOTE For example, RTGs generating g-ray and neutron radiation."]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.2.1b","Requirement","ECSS-E-ST-31_0800017",1,"Created","The mission phases shall be represented by a coherent set of thermal design cases covering the extreme range of conditions experienced by an item during its lifetime. "]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.3.7a","Requirement","ECSS-E-ST-31_0800050",1,"Created","TCS shall derive and agree with the system authority requirements related to the launcher interface based on the launcher ICD.\n    NOTE This is particularly important for:\n        · launcher envelope both for static and dynamic conditions, including ventilation effects;\n        · accessibility requirements;\n        · launch-pad air - conditioning requirements;\n        · launcher depressurization profile;\n        · heat fluxes from the fairing and to the launcher interface;\n        · heat flux from the spacecraft to the launcher."]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.4.1e","Requirement","ECSS-E-ST-31_0800059",1,"Created","If suitable data are not available, then a material test programme shall be implemented."]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.5.2.1g","Requirement","ECSS-E-ST-31_0800084",1,"Created","Conformance to specified performance shall be demonstrated by performing thermal balance, thermal vacuum and climatic tests."]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.6.2d","Requirement","ECSS-E-ST-31_0800117",1,"Created","Quality assurance requirements for manufacturing as specified in ECSS-ST-Q-20 clause 5.5 shall apply;"]
["ECSS-E-ST-31C","ECSS - Current v1.0","4.6.7b","Requirement","ECSS-E-ST-31_0800126",1,"Created","Items containing hazardous material or those subjected to special packaging, handling and transportation shall be identified."]
["ECSS-E-ST-31C","ECSS - Current v1.0","B.2.1<3>a","Requirement","ECSS-E-ST-31_0800161",1,"Created","The thermal and geometrical model description shall list the applicable directory or glossary and the meaning of specific terms or abbreviations utilized in this document."]
["ECSS-E-ST-31C","ECSS - Current v1.0","C.2.1<6>b","Requirement","ECSS-E-ST-31_0800186",1,"Created","The TCS analysis report shall describe the different analysis techniques used."]
["ECSS-E-ST-31C","ECSS - Current v1.0","D.2.1<10>a","Requirement","ECSS-E-ST-31_0800211",1,"Created","The TCS interface control document shall identify the following thermal hardware constraints with respect to operation, handling and maintenance:\n    1. Operational constraints of thermal control components.\n        NOTE For example: Heat pipe unit and heat pipe system operation at different temperatures and tilt, minimum start-up power of two-phase loops, dry-run capabilities of mechanical pumps.\n    2. Accommodation constraints of thermal control hardware.\n        NOTE For example: MLI maximum mounting / de-mounting cycles.\n    3. Requirements to prevent contamination of sensitive thermal surfaces.\n        NOTE For example: Cover on thermal radiators during ground handling and storage.\n    4. Environmental requirements during transportation and at the launch site.\n    5. Precautions and safety requirements for thermal pressurized components."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.2.3.1e","Requirement","ECSS-E-ST-32-02_0260009",1,"Created","Procedures to ensure compatibility of the pressurizing system with the structural capability of the pressurized hardware shall be established."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.2.3.3a","Requirement","ECSS-E-ST-32-02_0260018",1,"Created","The results of stress and safe-life analyses shall be used in conjunction with the results from the structural development and the qualification tests to define quantitative acceptance criteria for inspection and repair."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.3.2.1g","Requirement","ECSS-E-ST-32-02_0260043",1,"Created","For corrosion effects (control and prevention), the requirements in ECSS-E-ST-32 shall apply."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.3.3.2e","Permission","ECSS-E-ST-32-02_0260445",1,"Created","When the vibration loads are enveloped by the other qualification tests, the vibration tests specified in 4.3.3.2c may be deleted with customer approval."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.3.4.2a","Requirement","ECSS-E-ST-32-02_0260099",1,"Created","A first qualification test article shall be submitted to the following chronology of operations:\n    1. non-destructive inspection (NDI);\n    2. proof pressure test;\n    3. leak test;\n    4. design burst pressure test;\n    5. burst test."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.3.4.3a","Requirement","ECSS-E-ST-32-02_0260109",1,"Created","All hardware shall be submitted to the following chronology of operations:\n    1. initial NDI, in order to establish the initial condition of the hardware;\n    2. proof pressure test;\n    3. leak test;\n    4. final NDI. ","NOTE For example:\n            · The NDI prior to proof test can be substituted for that of the manufacturing process.\n            · Proof test monitoring by acoustic emission is acceptable for composite items instead of post testing NDI, with customer approval."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.4.3.1d","Requirement","ECSS-E-ST-32-02_0260142",1,"Created","The failure mode shall be demonstrated by analysis or test or both according to clause 5.3."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.4.4.1f","Requirement","ECSS-E-ST-32-02_0260167",1,"Created","The CPS shall exhibit a LBB failure mode."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.5.1.3c","Requirement","ECSS-E-ST-32-02_0260200",1,"Created","For pressure components other than lines and fittings at unit level, clauses 5.4.1 and 5.4.6 shall be applied to the qualification tests."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.5.2.2c","Requirement","ECSS-E-ST-32-02_0260209",1,"Created","A strength and stability demonstration shall be performed by analysis and test."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.5.3.2c","Requirement","ECSS-E-ST-32-02_0260237",1,"Created","A strength and stability demonstration shall be performed by analysis and test."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.6.1.2d","Requirement","ECSS-E-ST-32-02_0260266",1,"Created","The development approach for batteries with pressurized cells that meet the definition of a pressure vessel shall conform to clause 4.3.2.1. "]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.6.2.2d","Requirement","ECSS-E-ST-32-02_0260291",1,"Created","The failure mode shall be demonstrated by analysis or test or both according to clause 5.3."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.6.2.2m","Requirement","ECSS-E-ST-32-02_0260300",1,"Created","Inspections shall be applied according to clause 5.7.","NOTE The development approach is illustrated in Figure 4-4. "]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","4.6.3.3e","Permission","ECSS-E-ST-32-02_0260467",1,"Created","When the vibration loads are enveloped by the other qualification tests, the vibration tests specified in 4.6.3.3c may be deleted with customer approval."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","5.3.2b","Requirement","ECSS-E-ST-32-02_0260358",1,"Created","When LBB demonstration is based on a through crack with a length less than 10 times the wall thickness in accordance with 5.3.2a.2, the considered initial crack size shall be justified.\n    ","NOTE Justification of initial surface crack size can be based on NDI capability or on a crack whose depth is as close as possible to the wall thickness, within the range of a/c specified in clause 5.3.2a."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","5.4.5a","Requirement","ECSS-E-ST-32-02_0260426",1,"Created","Pressure cycles shall range from zero differential pressure to MDP and back to zero differential pressure for at least 50 cycles or four times the number of planned pressure cycles expected in one service life, whichever is greater."]
["ECSS-E-ST-32-02C Rev. 1","ECSS - Current v1.0","5.5.1b","Requirement","ECSS-E-ST-32-02_0260396",1,"Created","When an acceptance test is conducted at temperature other than temperature expected for the design loads, the change of material properties at this temperature shall be verified:\n    - by adjustment of the pressure and load level, or\n    - by analysis, supported by tests on samples or sub-scale articles and providing material strength design allowable versus temperature."]
["ECSS-E-ST-32-03C","ECSS - Current v1.0","4.4c","Requirement","ECSS-E-ST-32-03_0100006",1,"Created","The reduced model shall be supplied with related instructions for model integration."]
["ECSS-E-ST-32-03C","ECSS - Current v1.0","5.7a","Requirement","ECSS-E-ST-32-03_0100039",1,"Created","The modal analysis of the free model shall show the expected number of “rigid body” with frequencies equal or less than δ Hz, to be agreed with the customer.\n    ","NOTE 1 Six rigid body motions are expected for a three dimensional model without internal mechanisms.\nNOTE 2 A typical value is δ Hz = 0,005 Hz."]
["ECSS-E-ST-32-08C Rev. 1","ECSS - Current v1.0","4.2.10a","Requirement","ECSS-E-ST-32-08_0220018",2,"Normative Change","For mechanical contact surface effects the requirements of clause 5.1.16 of ECSS-Q-ST-70 shall apply.\n    ","NOTE For very clean surfaces strong adhesion occurs at the regions of real contact, a part of which can result from to cold-welding."]
["ECSS-E-ST-32-08C Rev. 1","ECSS - Current v1.0","4.3.6b","Requirement","ECSS-E-ST-32-08_0220026",1,"Unchanged","Spalling of the thermal barrier coating shall be verified by inspection.\n    ","NOTE Thermal coatings are applied to selected regions only."]
["ECSS-E-ST-32-08C Rev. 1","ECSS - Current v1.0","4.6.3c","Requirement","ECSS-E-ST-32-08_0220077",1,"Created","Stress-corrosion tests shall be performed in conformance with requirements from clause 5 of ECSS-Q-ST-70-37."]
["ECSS-E-ST-32-11C","ECSS - Current v1.0","4.1.6a","Requirement","ECSS-E-ST-32-11_0250008",1,"Created","After modifications have been made to the test item and modal testing is repeated in order to demonstrate the improvements in performance, it shall be verified that all other conditions applying to the predecessor are unchanged. \n    NOTE 1 This is particularly relevant for the boundary conditions.\n    NOTE 2 Poor repeatability can cause difficulties in interpreting the changes that are revealed. Otherwise, the improvements due to the structural modifications cannot be clearly identified. "]
["ECSS-E-ST-32-11C","ECSS - Current v1.0","5.3.2.1a","Requirement","ECSS-E-ST-32-11_0250041",1,"Created","The boundary conditions for the test set-up (in a laboratory environment) shall represent the boundary conditions for the launch, or any other configuration for which the modal characteristics are being determined.\n    NOTE Table 5-1 summarizes the most common modal survey test objectives and the associated requirements for the test boundary conditions."]
["ECSS-E-ST-32-11C","ECSS - Current v1.0","5.3.2.1b","Recommendation","ECSS-E-ST-32-11_0250132",1,"Created","When selecting the test boundary conditions, it should be taken into account that testing with “free-free” conditions results, in general, in the loading of other test article areas, stiffness and masses than when testing with “fixed-free” boundary conditions."]
["ECSS-E-ST-32-11C","ECSS - Current v1.0","5.4.3a","Requirement","ECSS-E-ST-32-11_0250075",1,"Created","The type of the excitation signal shall be defined. \n    NOTE The most commonly applied excitation signals are given in Annex A. "]
["ECSS-E-ST-32-11C","ECSS - Current v1.0","5.8.2.2b","Requirement","ECSS-E-ST-32-11_0250108",1,"Created","Conformance shall be demonstrated by comparing the dynamic behaviour of the reduced mathematical model with the dynamic analysis results obtained from the detailed FEM."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.2.1e","Requirement","ECSS-E-ST-32_0050005",1,"Created","Service-life evaluations shall determine: \n    1. the inspection and maintenance requirements,\n    2. the item replacement procedure (preventive maintenance), and\n    3. the inspection and repair procedures and intervals (corrective maintenance)."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.2.5b","Requirement","ECSS-E-ST-32_0050014",1,"Created","Loads shall be defined according to their nature, (i.e. static or dynamic) and their level, occurrence time and duration."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.3.12a","Requirement","ECSS-E-ST-32_0050041",1,"Created","Structural requirements derived from electromagnetic compatibility requirements shall be identified."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.5.10.1a","Requirement","ECSS-E-ST-32_0050071",1,"Created","Design allowables for glass and ceramics shall be derived through a probabilistic approach, covering all size effects.\n    NOTE For brittle materials such as glass and ceramics the lack of ductility results in very low failure strains. The large scatter observed in component testing is primarily caused by the variable severity of flaws distributed within the material (volume flaws) or flaws extrinsic to the material volume (surface flaws). The different physical nature of the flaws result in dissimilar failure response to identical external loading conditions. Due to the random distribution of flaws the failure of a complex structural part can be initiated not only at the point of highest stress."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.6.2.3c","Requirement","ECSS-E-ST-32_0050104",1,"Created","Provisions shall be made to include the effects of residual stresses due to the manufacturing process (e.g. welding)."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.6.2.3d","Requirement","ECSS-E-ST-32_0050105",1,"Created","Static analysis shall take into account stress concentrations.\n    NOTE Stress concentrations essentially take place in areas with steeply varying shape or section and with notches (macro and micro stress raisers). For metals stress concentrations are known to have a detrimental effect on fatigue lifetime. For fibre reinforced plastics stress concentrations have a detrimental effect on static strength. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.6.2.21a","Requirement","ECSS-E-ST-32_0050138",1,"Created","The structural responses at the locations of sensitive receivers due to disturbance sources shall be analysed. \n    NOTE Disturbance sources are e.g. reaction wheels, human induced vibrations, microcracking.”"]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.6.3.17a","Requirement","ECSS-E-ST-32_0050171",1,"Created","Contamination tests shall determine the particle fall-out (PFO) on specified spacecraft systems."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.7.3a","Requirement","ECSS-E-ST-32_0050191",1,"Created","Manufacturing drawings shall be established in conformity to the functional requirements and design drawings."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.8.1b","Requirement","ECSS-E-ST-32_0050204",1,"Created","Ground inspection shall be performed after the return of a recoverable structure.\n    NOTE Ground inspection techniques can generally be those which are applied during system integration or during assembly manufacturing stages."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","4.9.8a","Requirement","ECSS-E-ST-32_0050237",1,"Created","Traceability of design data and relationship between each other shall be provided including CAD, CAE, CAM models, structural analysis and test documentation."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","A.2.1<4.2>a","Requirement","ECSS-E-ST-32_0050262",1,"Created","The CADMDD shall summarize and include a justification of the modelling assumptions and methodology. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","A.2.1<6.5>a","Requirement","ECSS-E-ST-32_0050295",1,"Created","The CADMDD shall collect any other topic of interest. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","A.2.1<7.1>a","Requirement","ECSS-E-ST-32_0050296",1,"Created","The CADMDD shall report the results of dedicated checks performed to assess the model geometry correctness and completeness. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","C.2.1<3>a","Requirement","ECSS-E-ST-32_0050329",1,"Created","The DSA shall include the terms and definitions, abbreviated terms, and symbols used."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","D.2.1<1>a","Requirement","ECSS-E-ST-32_0050352",1,"Created","The DL shall contain a description of the purpose, objective, applicability, content and the reason prompting its preparation"]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","E.2.1<8.4>a","Requirement","ECSS-E-ST-32_0050386",1,"Created","The containment analysis of relevant item shall be reported and the significant results summarized, including the derivation of the velocity and energy of the projectile as it strikes the container and all maximum forces and stresses in attachments, brackets and other relevant items occurring during impact."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","F.2.1<3>a","Requirement","ECSS-E-ST-32_0050395",1,"Created","The FCP shall include the terms and definitions, abbreviated terms, and symbols used."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","G.2.1<5>d","Recommendation","ECSS-E-ST-32_0050772",1,"Created","The PFCIL, FCIL and FLLIL should include a clear identification system for the PFCI which ensures traceability throughout the FCIL, FLLIL and fracture control analysis report."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","I.2.1<6.3>a","Requirement","ECSS-E-ST-32_0050453",1,"Created","The MMDD shall include a mathematical model summary as a table that summarizes model data, showing the total number of each type of data."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","I.2.1<9.1>a","Requirement","ECSS-E-ST-32_0050486",1,"Created","The MMDD shall describe the model load sets. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","I.2.1<9.1>b","Requirement","ECSS-E-ST-32_0050487",1,"Created","Each load set shall be independently described, including the following information:\n    1. Types of load included in each load set k shall be listed (e.g. forces, line distributed loads, pressure, gravity) and related values shall be indicated.\n    2. Total resultant forces and moment (w.r.t. a specified point) shall be given, in code output format."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","J.2.1<6>a","Requirement","ECSS-E-ST-32_0050525",1,"Created","The MDRA shall include the results of the modal analysis and the detailed description of the performed calculations, by including:\n    1. list of eigenvalues and natural frequencies;\n    2. list of modal effective masses including percentage w.r.t. rigid mass;\n    3. plots and descriptions of the significant mode shapes."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","K.2.1<7.2>b","Requirement","ECSS-E-ST-32_0050552",1,"Created","Reasons for the choice and limitations of the models shall be summarized here."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","K.2.1<10.1>b","Recommendation","ECSS-E-ST-32_0050776",1,"Created","Details of correspondence between analysis and lower level part numbers should be provided inside the analyses presentation."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","K.2.1<10.3>f","Requirement","ECSS-E-ST-32_0050586",1,"Created","The SSA shall report the stress analysis performed for each structural part. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","L.2.1<4.5>a","Requirement","ECSS-E-ST-32_0050611",1,"Created","The SAB shall describe all the coordinate systems used in the SAB by giving, for each coordinate system, the following information:\n    1. the coordinate system identifier;\n    2. the type (e.g. rectangular);\n    3. the coordinate system definition (origin and orientation of the axes);\n    4. a brief description to explain its use."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","N.2.1<2>a","Requirement","ECSS-E-ST-32_0050644",1,"Created","The SMS shall list the applicable and reference documents in support to the generation of the document."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","O.2.1<2>a","Requirement","ECSS-E-ST-32_0050663",1,"Created","The TAC shall list the applicable and reference documents in support to the generation of the document."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","O.2.1<7>a","Requirement","ECSS-E-ST-32_0050677",1,"Created","The TAC shall summarize the main aspects of the test predictions and reference documentation shall be indicated. "]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","P.2.1<6.6>c","Requirement","ECSS-E-ST-32_0050710",1,"Created","The TE shall include a reviewing of the interface requirements for strength, stiffness, and interface degrees of freedom for the test article’s support fixture."]
["ECSS-E-ST-32C Rev. 1","ECSS - Current v1.0","Q.2.1<4.5>a","Requirement","ECSS-E-ST-32_0050735",1,"Created","Nonconformances potentially affecting the test results shall be reported in the TP, and a justification included."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.2.2.2a","Requirement","ECSS-E-ST-34_0830018",1,"Created","The range and the accuracy to monitor the atmosphere total pressure in the pressurized volume shall be specified."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.2.2.7a","Requirement","ECSS-E-ST-34_0830027",1,"Created","Addition of gaseous oxygen into the atmosphere shall be provided at a rate capable of maintaining the oxygen partial pressure in the accessible volume within the specified range."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.2.6.3a","Requirement","ECSS-E-ST-34_0830052",1,"Created","The range and accuracy for monitoring the atmosphere’s carbon monoxide partial pressure shall be specified."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.3.5.4a","Requirement","ECSS-E-ST-34_0830086",1,"Created","The functionality to recover from a hazardous atmosphere shall be provided.\n    ","NOTE Recovery options can include venting of the habitable volume atmosphere and subsequent atmosphere restoration. Additional recovery options can include throttling up of the existing contaminant removal system, and activation of a secondary contaminant removal system coupled with an emergency source of breathable air."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.4.4.3a","Requirement","ECSS-E-ST-34_0830117",1,"Created","Water shall be supplied to points of use in conformance with the interface specifications for water temperature, pressure, flow rate and quality."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.4.4.4a","Requirement","ECSS-E-ST-34_0830118",1,"Created","The water peak usage and contingency needs shall be specified."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.5.1.5a","Requirement","ECSS-E-ST-34_0830140",1,"Created","The capability to dispose excess carbon dioxide shall be provided."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.4.6.1.4a","Requirement","ECSS-E-ST-34_0830165",1,"Created","Re-compression procedure of the airlock for a crew member from the external ambient pressure to the habitable volume pressure shall be supported at a specified nominal rate."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.6.3.6a","Requirement","ECSS-E-ST-34_0830198",1,"Created","The requirements for electric power supply to ECLSS shall be specified.\n    ","NOTE For example, peak and average electric power, duty cycles, and backup electric power."]
["ECSS-E-ST-34C","ECSS - Current v1.0","4.8a","Requirement","ECSS-E-ST-34_0830213",1,"Created","Product assurance and safety provisions shall apply to design, production manufacturing testing and utilization of ECLSS.\n    ","NOTE For product assurance and safety, refer to the Q-branch of the ECSS Standards."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.4a","Requirement","ECSS-E-ST-35-01_0840013",1,"Created","The liquid propulsion system shall conform to its specified spacecraft interfaces, including:\n    1. Structure\n        NOTE For example: inserts, tank support structure and vibration levels.\n    2. Thermal\n        NOTE For example: conduction, radiation levels, tank, thruster and line thermal control.\n    3. Power\n        NOTE For example: valve drivers, pressure transducers, thermistors, heaters and thermocouples.\n    4. Electromagnetic compatibility\n    5. Pyrotechnics\n        NOTE For example: pyrotechnic valves.\n    6. Mechanisms\n        NOTE For example: valves, regulators, actuators and actuation system.\n    7. AOCS, OBDH and TM/TC.\n        NOTE For example: commanding, handling of data for status and health monitoring and failure detection."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.5.5.2b","Requirement","ECSS-E-ST-35-01_0840046",1,"Created","The expected maximum level of contaminants inside the propulsion system shall be specified."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.5.14.4a","Requirement","ECSS-E-ST-35-01_0840079",1,"Created","The thruster design shall allow nominal operation during possible heat soak-back conditions inherent to the specified thruster operation modes (i.e. duty cycles)."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.5.14.4b","Requirement","ECSS-E-ST-35-01_0840080",1,"Created","The thruster integrity shall not be impaired by heat soak-back."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.6.2.2.6b","Requirement","ECSS-E-ST-35-01_0840113",1,"Created","It shall be established whether protection devices are required at spacecraft level."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.6.3.2e","Requirement","ECSS-E-ST-35-01_0840138",1,"Created","Component proof pressure tests shall conducted at a pressure higher than the particular MEOP of this component.\n    NOTE For details on ‘proof pressure test’ see ECSS-E-ST-10-03."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.6.3.14a","Requirement","ECSS-E-ST-35-01_0840168",1,"Created","All components or subsystems that provide data shall be calibrated."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","4.8.1e","Requirement","ECSS-E-ST-35-01_0840179",1,"Created","At the end of any operation, the propulsion system shall be configured by isolating, draining or venting the system, to minimize risks.\n    NOTE Minimize the risks of, e.g. explosion, toxicity and corrosion."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.3.1a","Requirement","ECSS-E-ST-35-01_0840204",1,"Created","The constraints induced by thruster initialisation, start up and restart sequences shall be identified and reported in the DJF."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.5.2.2c","Requirement","ECSS-E-ST-35-01_0840237",1,"Created","Compatibility of the selected materials, propellants and test fluids shall be demonstrated for all components."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.5.8.2a","Requirement","ECSS-E-ST-35-01_0840262",1,"Created","In case the mass flow rate is not-self-adjusted, the design shall address the specific issues related to the very small, well regulated mass flow rates used in electric propulsion.\n    NOTE Example of self-adjusted mass flow rate is by capillary-fed thrusters."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.5.11a","Requirement","ECSS-E-ST-35-01_0840271",1,"Created","For EP systems working in blow-down mode clause 4.5.12 shall be applied."]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.5.15.5b","Requirement","ECSS-E-ST-35-01_0840306",1,"Created","The design of the EP system shall prevent the presence of gases during the operation of the thruster.\n    NOTE Parasitic discharge can be enhanced by the presence of gas. Gas can appear due to venting, trapped gas or outgassing. "]
["ECSS-E-ST-35-01C","ECSS - Current v1.0","5.6.3.1b","Requirement","ECSS-E-ST-35-01_0840328",1,"Created","The verification tests of each block shall be defined to represent the conditions that are expected to be encountered during the operation of the complete system. "]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","4.3.1c","Requirement","ECSS-E-ST-35-02_1100012",1,"Created","The maximum allowable dynamic mechanical loads induced by the solid rocket motor during transient phases shall be specified vs frequency. \n    ","NOTE For example shock during ignition and pressure wave."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","4.3.6a","Requirement","ECSS-E-ST-35-02_1100021",1,"Created","Constraints on parts foreseen to be ejected during the missions by the solid rocket motor shall be specified.\n    ","NOTE For example nozzle plugs and igniters."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","4.5.2.4a","Requirement","ECSS-E-ST-35-02_1100045",1,"Created","The motor shall be protected against external contaminants (including moisture) which can enter the motor."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","4.5.5.4.2b","Permission","ECSS-E-ST-35-02_1100163",1,"Created","If requirements 4.5.5.2.1b and 4.5.5.2.1c are not applied an alternative methodology may be used under customer approval."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","4.10.1a","Requirement","ECSS-E-ST-35-02_1100102",1,"Created","ECSS-E-ST-35 clause 4.10 shall apply."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","A.2.1<6.2>e","Requirement","ECSS-E-ST-35-02_1100125",1,"Created","An estimate of the accuracy of the methodology shall be included in the AR-DY."]
["ECSS-E-ST-35-02C","ECSS - Current v1.0","B.2.1<2>f","Requirement","ECSS-E-ST-35-02_1100140",1,"Created","The AR-MSDS shall provide the Risk/compatibility category."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","6.2a","Requirement","ECSS-E-ST-35-03_1110004",1,"Created","The dimensioning of the liquid propulsion system and its components shall conform to the overall launch vehicle dimensions, interfaces between stages, ground infrastructure and requirements for transportation."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.3.4a","Requirement","ECSS-E-ST-35-03_1110037",1,"Created","For the selection of the engine, a trade-off analysis shall be performed using the following parameters:\n    1. global stage performance (e.g. Isp, mass budget);\n    2. development costs;\n    3. recurring cost;\n    4. industrial infra structure;\n    5. test infra structure;\n    6. reliability;\n    7. strength;\n    8. architecture and overall dimensions;\n    9. the technical readiness level of the technologies;\n    10. any additional parameters specified by the customer."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.4.3.2a","Requirement","ECSS-E-ST-35-03_1110046",1,"Created","In-flight draining shall not create conditions that can lead to loss of performance of the launch vehicle."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.4.4.3b","Requirement","ECSS-E-ST-35-03_1110071",1,"Created","For all tanks, the location of fill-and-drain valves and the piping layout shall be such that liquids are not trapped in the system by on-ground draining and dissimilar fluids do not come into contact with each other."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.3.1b","Requirement","ECSS-E-ST-35-03_1110102",1,"Created","Engine performance losses shall be analysed and reported in the design justification file in as defined in ECSS-E-ST-10 Annex K DRD."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.3.4.3g","Requirement","ECSS-E-ST-35-03_1110128",1,"Created","If a liquid propulsion system is expected to be activated after a ballistic flight, a propellant settling analysis shall be carried out."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.3.4.6b","Requirement","ECSS-E-ST-35-03_1110137",1,"Created","The tail-off characteristics shall be reproducible within the specified range."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.4.7h","Requirement","ECSS-E-ST-35-03_1110170",1,"Created","The pressure oscillation history shall be reported in the design definition file, as defined in the ECSS-E-ST-10 Annex G DRD.\n    ","NOTE The pressure oscillation history is the level of pressure oscillation with respect to frequency and time."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.4.8.4a","Requirement","ECSS-E-ST-35-03_1110195",1,"Created","For radiative nozzle, the self induced heat loads shall be assessed during operation and after shut-down of the engine."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.6.2v","Requirement","ECSS-E-ST-35-03_1110228",1,"Created","Barriers shall prevent contact between non-compatible fluids."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.5.8.3c","Requirement","ECSS-E-ST-35-03_1110253",1,"Created","Accounting for the elements identified in accordance with 9.5.8.3a. and 9.5.8.3b., the amount of gas and the type of gas to be used during the autonomous operation of the stage shall be identified according to the extreme envelope."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.6b","Requirement","ECSS-E-ST-35-03_1110275",1,"Created","ECSS-E-ST-32-02 (Structural design and verification of pressurized hardware) and ECSS-E-ST-32-01 (Fracture control) shall not be applicable to the following liquid propulsion system components:\n    1. combustion chamber\n    2. gas generator\n    3. pre burner\n    4. turbopump\n    5. nozzle extension\n    6. igniter\n    7. mechanisms"]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","9.6u","Requirement","ECSS-E-ST-35-03_1110294",1,"Created","Both internal and external load cases shall be used when establishing dimensioning load cases."]
["ECSS-E-ST-35-03C","ECSS - Current v1.0","14.2c","Requirement","ECSS-E-ST-35-03_1110319",1,"Created","The number of launch aborts the propulsion system can undergo shall be specified."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","4.2.1a","Requirement","ECSS-E-ST-35-10_1050007",1,"Created","Compatibility testing of material combinations in propulsion systems shall be done in case there is no experimental or historical evidence that the combination meets the compatibility requirements.\n    NOTE This includes simulation and cleaning fluids, purging gases and cleaning and drying processes."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","6.1.4.3a","Requirement","ECSS-E-ST-35-10_1050040",1,"Created","Exposure of the material to the fluid for two hours at ambient temperature and pressure shall not generate any visible effects or changes in either the material or the fluid."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","6.4.3a","Requirement","ECSS-E-ST-35-10_1050065",1,"Created","Materials, which do not meet the selection requirements in ECSS-Q-ST-70-36, shall be tested and classified in conformance with ECSS-Q-ST-70-37."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","6.7.2.3b","Permission","ECSS-E-ST-35-10_1050189",1,"Created","Ageing behaviour may be accelerated by testing at temperatures higher than the upper temperature of the qualification temperature range."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","6.7.2.3h","Requirement","ECSS-E-ST-35-10_1050104",1,"Created","The compatibility test plan shall include the: \n    1. test objectives,\n    2. compatibility test procedures,\n    3. duration of the test runs, including accelerated aging,\n    4. loads, conditions and environment in conformance with 6.7.2.2a,\n    5. instants to take the samples."]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","6.9.1b","Requirement","ECSS-E-ST-35-10_1050131",1,"Created","Exposure to the test environment of samples shall be representative of the specific application in terms of hydrogen concentration, pressure and temperature. "]
["ECSS-E-ST-35-10C","ECSS - Current v1.0","A.2.1<7>c","Requirement","ECSS-E-ST-35-10_1050165",1,"Created","In case the incompatibility issue for the propulsion system has been addressed by test, the CAAR shall state the type and number of tests to be performed."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.3i","Requirement","ECSS-E-ST-35_0850010",1,"Created","The level of testing shall be justified and submitted for customer approval.\n    NOTE The level of testing include:\n        · The level of configuration: at equipment, subsystem or system level\n        · The representativeness of the mission and environment constraints\n        · The represetativeness of the propellants"]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.5.1c","Requirement","ECSS-E-ST-35_0850019",1,"Created","The propulsion system lay-out shall allow the replacement of subsystems"]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.5.4.1b","Requirement","ECSS-E-ST-35_0850044",1,"Created","The supplier shall provide a report on the result of the propulsion transient analysis in conformance with Annex G.\n    NOTE Transients cover the parameter variation that occurs during a voluntary change (including start-up and shut down) of operating conditions."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.5.11.4a","Requirement","ECSS-E-ST-35_0850086",1,"Created","The amount of leakage that can be expected for each of the fluids in the propulsion system (leakage budget) shall be determined by analysis."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.5.14.2a","Requirement","ECSS-E-ST-35_0850109",1,"Created","It shall be ensured that lines in the harness do not introduce spurious signals in adjacent or other lines.\n    NOTE For example by strictly separating lines for different functions. "]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.8.2.1b","Requirement","ECSS-E-ST-35_0850134",1,"Created","Any differences between the ground test conditions and the expected flight conditions shall be identified and documented."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","4.8.2.2e","Requirement","ECSS-E-ST-35_0850143",1,"Created","Sub-system or component tests shall be performed to demonstrate margins concerning failure modes identified in the FMECA."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","A.2.1<6.2>g","Requirement","ECSS-E-ST-35_0850176",1,"Created","If modelling is used, the models shall be referenced and summarized."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","B.2.1<6.2>f","Requirement","ECSS-E-ST-35_0850201",1,"Created","If data from modelling, not within the project is used, the models from which this data results, shall be referenced. "]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","B.2.1<8>a","Requirement","ECSS-E-ST-35_0850210",1,"Created","The AR-G, based on the information provided in section B.2.1<7>, shall list the following recommendations:\n    1. Suggestions for future work and additional investigations or improvements\n        NOTE For example, lessons learned, state-of-the-art.\n    2. Feedback to improve the gauging and gauging analysis."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","D.2.1<5>b","Requirement","ECSS-E-ST-35_0850236",1,"Created","The AR-Pl shall also include a discussion on the understanding and clarification of the requirements."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","E.2.1<6.2>a","Requirement","ECSS-E-ST-35_0850267",1,"Created","The AR-N shall include a description and a discussion of the analysis methodology, describing what is done and why."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","F.2.1<6.2>e","Requirement","ECSS-E-ST-35_0850300",1,"Created","If data from modelling, not within the project is used, the data shall be referenced or reproduced;"]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","G.2.1<6.2>f","Requirement","ECSS-E-ST-35_0850325",1,"Created","If data from modelling, not within the project is used, the models from which this data results shall be referenced and a discussion of these models included."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","G.2.1<8>d","Requirement","ECSS-E-ST-35_0850334",1,"Created","In case previous propulsion transients’ analyses are available, the AR-Tr shall include a comparison of the result of the present transient analysis with the previous ones and a report on the discussion of the differences."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","H.2.1<5.12>b","Requirement","ECSS-E-ST-35_0850367",1,"Created","The UM shall describe:\n    1. All the activities that verify that the propulsion system is in a proper condition to be activated and operated.\n    2. The measures to control the status of the propulsion system and to bring it in a proper condition to be activated and operated.\n    3. The means to identify the status of redundant propulsion system branches and to close-off failed branches.\n    4. The procedures to start, operate and shut-off the propulsion system in orbit or trajectory.\n    5. The off-design use and the off-design procedures in case of propulsion system anomalies.\n        NOTE For example, the use of AOCS thrusters for orbit raising in case of failure of the apogee boost motor."]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","I.2.1<8>a","Requirement","ECSS-E-ST-35_0850397",1,"Created","In the MM-PA a summary of the results shall be given also describing the limitations of the performed work. "]
["ECSS-E-ST-35C Rev. 1","ECSS - Current v1.0","K.2.1<1>a","Requirement","ECSS-E-ST-35_0850400",1,"Created","In a MMDD of a propulsion system, subsystem or component, the information as specified in the MMDD DRD in ECSS-E-ST-32 shall be provided."]
["ECSS-E-ST-50-02C","ECSS - Current v1.0","4.2.2.4a","Requirement","ECSS-E-ST-50-02_0870022",1,"Created","When an optimum choice of tone frequency is established, on the basis of the criteria set out in clause 4.2.3.2, modulation indexes shall be selected for both signals taking the following into account:\n    1. power sharing;\n    2. mutual interference;\n    3. reduction of the downlink ranging-signal power due to the uplink noise."]
["ECSS-E-ST-50-02C","ECSS - Current v1.0","4.5.6d","Requirement","ECSS-E-ST-50-02_0870055",1,"Created","In the case of standard off-the-self transponders designed for multiple versions, the ranging tone selection shall be carried out taking into account available transponder noise bandwidths to minimize the loss in the effective Space-to-Earth link ranging modulation index."]
["ECSS-E-ST-50-02C","ECSS - Current v1.0","5.1a","Permission","ECSS-E-ST-50-02_0870102",1,"Created","The tests to demonstrate compatibility of ranging transponder and Earth equipment as specified in clause 5.2 may be combined with similar telecommand and telemetry compatibility tests;"]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","5.1.1.14b","Recommendation","ECSS-E-ST-60-30_1160142",1,"Created","For diagonal terms, the following convention should be used:\n ,   ,   "]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","5.1.3.1a","Requirement","ECSS-E-ST-60-30_1160031",1,"Created","The AOCS shall contribute to the definition of a propulsion thruster configuration for:\n    1. force and torque directions, according to mission needs,\n    2. pure torque or pure force generation, if needed by the mission.\n        ","NOTE Some missions can require several kinds of propulsion and thrusters, resulting in identification of multiple configurations."]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","5.2.2.3c","Requirement","ECSS-E-ST-60-30_1160053",1,"Created","AOCS shall provide the capability to switch on a redundant unit for health diagnostic without impacting the current mode functionality.\n    ","NOTE 1 This requirement might not be applicable to all cases of actuators, such as magnetorquers or thrusters. \nNOTE 2 This cannot be applied to low cost satellites without redundancy."]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","5.4.3c","Requirement","ECSS-E-ST-60-30_1160088",1,"Created","The simulation models of the AOCS sensors and actuators shall be based on data requested to the equipment suppliers in their statements of work. \n    ","NOTE The level of representativeness needed for the simulation models is usually evaluated by the AOCS responsible, and used to specify the input data to be delivered by the equipment supplier. "]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","5.4.4c","Requirement","ECSS-E-ST-60-30_1160097",1,"Created","The selected approach for the analyses and simulations shall be defined and justified.\n    ","NOTE The approach can use for instance Monte Carlo method, worst case analysis or sensitivity analysis providing the knowledge of the key parameters and their impacts."]
["ECSS-E-ST-60-30C","ECSS - Current v1.0","A.2.1b","Requirement","ECSS-E-ST-60-30_1160122",1,"Created","The AOCS design definition file shall provide the interfaces between AOCS and ground system, payload, satellite level FDIR and other functional chains"]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","5.5.2a","Requirement","ECSS-E-ST-50-13_1010014",1,"Created","For Table 5-1 and Table 5-2, the RT address shall be obtained by connecting straps between an RT address or RT Address Parity signal and a GND signal such that:\n    1. A logical “1” level is defined by an unconnected RT address signal.\n    2. A logical “0” level is defined by a strap between the RT address signal and a GND signal.\n        NOTE For the case of a 9-pole connector no specific address connector is specified."]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","7.3.2a","Requirement","ECSS-E-ST-50-13_1010047",1,"Created","For ReadStatus primitive Table 7-6 shall apply."]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.3.1.1a","Requirement","ECSS-E-ST-50-13_1010073",1,"Created","The BC shall split the time between the start of two Time Synchronization Messages into N intervals, each interval housing a series of 1553 messages making up a Communication Frame. "]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.3.1.1h","Requirement","ECSS-E-ST-50-13_1010080",1,"Created","The BC shall send the Communication Frame Synchronization Messages in broadcast mode."]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.5.1b","Requirement","ECSS-E-ST-50-13_1010105",1,"Created","The transfers resulting from an invocation of the Get Data service shall take place at the earliest after the start of the next Communication Frame.\n    NOTE Synchronization for data access within RT is insured by predefined Bus Profile and RT data refresh time."]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.6.2.1f","Requirement","ECSS-E-ST-50-13_1010138",1,"Created","The poll of the RT for a need of transfer shall be done by reading the RT Acquisition Transfer Request message from SA 28T."]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.6.2.2d","Requirement","ECSS-E-ST-50-13_1010147",1,"Created","The Acquisition Transfer Request shall be in conformance with Table 8-6 with the following meaning:\n    1. Reserved bits: all to be set to zero. \n        NOTE These bits are reserved for future use.\n    2. Number of bytes for next Acquisition Data Block: \n        (a) This data field to indicate the number of bytes in the Acquisition Data Block.\n        (b) A field value of zero to be interpreted as 4096. \n        (c) An odd number to indicate that the least significant byte of the last word of the last message contains a Filler Octet. \n            NOTE 1 This Filler Octet is generated by the sender, when splitting a user data block into 1553-messages. \n            NOTE 2 The Filler-octet can contain any data. \n        (d) If the Reset flag is ‘1’ this field to be set to zero.\n    3. QoS - Quality of Service: \n        (a) A ‘0’ in this field to indicate that the Distribution Data Block is transferred with Best Effort. \n        (b) A ‘1’ in this field to indicate that the Distribution Data Block is transferred with Verified Data Length. \n        (c) If the Reset flag is ‘1’ this field to be set to ‘0’.\n    4. Reset: \n        (a) A ‘0’ in this data field to indicate that the protocol carries on. \n        (b) A ‘1’ in this data field to indicate that a protocol reset is requested or that the RT has been reset.\n    5. Mode: \n        (a) A ‘0’ in this data field to indicate that multiple subaddresses are used to transfer the data. \n        (b) A ‘1’ in this data field to indicate that a single subaddress is used. \n        (c) If the Reset flag is ‘1’ this field to be set to ‘0’.\n    6. SA:\n        (a) In case the Mode flag is ‘1’ this data field to indicate to which subaddress data are written. \n        (b) In case the Mode flag is ‘0’ this field to be ‘01011’, showing SA 11.\n    7. Acquisition Block Count: \n        NOTE This field is a circular 8-bit-counter, identifying the current data block.\n        (a) If the Reset flag is ‘1’ the Acquisition Block Count to be set to zero.\n        (b) At the first transfer after a protocol reset, the Acquisition Block Count to be set to 1.\n        (c) For each new transfer to be carried out the ABC to be incremented by one and when the ABC reaches 255 the next count number to be 1.\n            NOTE 1 In case the service user performs a retry of the same data block the count is still incremented as the service does not differentiate retries from new transfers \n            NOTE 2 By using a counter, which is incremented with every new request, and which is returned to the RT after a successful transfer, the RT is able to detect the completion of a specific Acquisition Transfer, even if successive acquisition data blocks are identical (in size or contents).\n            NOTE 3 To avoid that after an RT initialization or reset an identical value to the previous one is used for the Acquisition Block Count, there is one fixed value foreseen for that case. This value does never appear in any other transfer, it is skipped in the normal sequence of acquisitions, when this counter wraps around.                                                                                                    "]
["ECSS-E-ST-50-13C","ECSS - Current v1.0","8.7.3g","Requirement","ECSS-E-ST-50-13_1010172",1,"Created","The value ‘1’ in a bit of the RT_Health command word shall result in the reset of the corresponding bit of the RT_Health data; a value ‘0’ shall have no effect.\n    NOTE A value of ‘1111 1111 1111 1111’ in the RT_Health command word results in the complete reset of the RT_Health data while a value ‘0000 0000 0000 0000’ has no effect."]
["ECSS-E-ST-50-14C","ECSS - Current v1.0","5.2.2.3.1b","Requirement","ECSS-E-ST-50-14_0940025",1,"Created","If 5.2.2.3.1a is not met, n-tuples shall be used."]
["ECSS-E-ST-50-14C","ECSS - Current v1.0","6.1.2.2.1a","Requirement","ECSS-E-ST-50-14_0940043",1,"Created","The source circuit shall meet the characteristics specified in Table 6-1."]
["ECSS-E-ST-50-14C","ECSS - Current v1.0","8.2.2b","Recommendation","ECSS-E-ST-50-14_0940167",1,"Created","The peripheral element should be designed to be compatible with any tb specified in 8.3.4.8 and 8.4.4.9."]
["ECSS-E-ST-50-14C","ECSS - Current v1.0","8.3.4.5b","Requirement","ECSS-E-ST-50-14_0940091",1,"Created","The peripheral element shall ensure that the data on this signal is valid and stable on every DATA_CLK_OUT falling edge when GATE_READ is asserted."]
["ECSS-E-ST-50-14C","ECSS - Current v1.0","8.4.4.8b","Requirement","ECSS-E-ST-50-14_0940116",1,"Created","Shortly after the GATE_WRITEDOWN the core element shall set the DATA_OUT signal to the value of the most significant bit, bit 0, of the data word to be transferred."]
["ECSS-E-ST-50-51C","ECSS - Current v1.0","5.2.4a","Requirement","ECSS-E-ST-50-51_1070012",1,"Created","If a packet arrives with a Protocol Identifier or Extended Protocol Identifier that is not supported (unknown) by that target then the packet shall be discarded.\n    ","NOTE The target can count the number of packets that arrive at a target with unknown Protocol Identifier or Extended Protocol Identifier can be kept and made available by the target."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.1.4.1a","Requirement","ECSS-E-ST-50-52_1080007",1,"Created","The Instruction field shall be an 8-bit composite field that comprises the packet type, command and Reply Address length fields."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.3.1.5.3c","Requirement","ECSS-E-ST-50-52_1080053",1,"Created","The Reply bit shall be:\n    1. Set (1) if a reply to the write command is required, and \n    2. Clear (0) otherwise. "]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.3.1.12a","Requirement","ECSS-E-ST-50-52_1080064",1,"Created","The Data Length field format shall be as defined in clause 5.1.11.\n    ","NOTE This gives a maximum Data Length of 16 Megabytes -1 in a single write command. If a single byte is being written this field is set to one. If set to zero then no bytes are written to memory which can be used as a test transaction depending upon the implementation."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.3.3.4.2b","Recommendation","ECSS-E-ST-50-52_1080402",1,"Created","If an EEP or EOP is received before the complete header including header CRC has been received the target should update the error information to reflect the “EEP” or “Early EOP” error if the target supports error information gathering."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.3.3.6.10a","Requirement","ECSS-E-ST-50-52_1080122",1,"Created","If the Verify-Data-Before-Write bit is clear (0) in the command field of the header and if there is a Data CRC error the target shall:\n    1. Update the error information to reflect the “invalid Data CRC” error if the target supports error information gathering,\n    2. Return an “invalid Data CRC” error as specified in clause 5.6 to the node specified in the Reply Address and Initiator Logical Address fields if a reply has been requested, Reply bit set (1).\n        ","NOTE 1 If verify before write bit is clear (0) then the Data CRC error is reported after the data has been transferred to target memory.\nNOTE 2 The sequence of events that occurs when the Data CRC detects an error in the data field is illustrated in Figure 5-6."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.3.3.7a","Recommendation","ECSS-E-ST-50-52_1080419",1,"Created","Once data has been written to memory the target user application should be informed that a write operation has taken place (Write Data Indication)."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.4.1.7a","Requirement","ECSS-E-ST-50-52_1080156",1,"Created","The Reply Address field shall be as defined in clause 5.1.6."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.4.3.3a","Requirement","ECSS-E-ST-50-52_1080189",1,"Created","In response to the read request the initiator shall construct the read command including the Header CRC and send it across the SpaceWire network to the target (Read Command).\n    ","NOTE The Target SpaceWire Address and Target Logical Address are used to route the command packet to the target."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.4.3.6b","Requirement","ECSS-E-ST-50-52_1080214",1,"Created","If the Increment bit is clear (0) in the command field of the header, the memory address read from in the target shall remain constant i.e. all data is read from the same memory location."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.4.3.10a","Recommendation","ECSS-E-ST-50-52_1080437",1,"Created","If the read memory operation memory fails, the target should stop reading from memory as soon as the memory error is detected."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.5.1.14a","Requirement","ECSS-E-ST-50-52_1080255",1,"Created","The Data field shall contain the data that is combined with the mask and the data read from memory before the result is written into the memory of the target as defined in clause 5.1.13."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.5.2.13a","Requirement","ECSS-E-ST-50-52_1080280",1,"Created","The Data CRC shall contain an 8-bit CRC as defined in clauses 5.1.15 and 5.2."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.5.3.5.2a","Requirement","ECSS-E-ST-50-52_1080374",1,"Created","If the value of the Key is not the value expected by the target user application, the target shall:\n    1. Discard the command packet,\n    2. Return an “invalid key” error as specified in clause 5.6 to the node specified in the Reply Address and Initiator Logical Address fields."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.5.3.7b","Requirement","ECSS-E-ST-50-52_1080379",1,"Created","The new data shall be written to the memory location(s) that was previously read."]
["ECSS-E-ST-50-52C","ECSS - Current v1.0","5.7.1.3a","Requirement","ECSS-E-ST-50-52_1080347",1,"Created","A target shall be able to receive RMAP commands and send replies."]
["ECSS-E-ST-50-53C","ECSS - Current v1.0","5.3.3b","Requirement","ECSS-E-ST-50-53_1090027",1,"Created","The Protocol Identifier field shall be set to the value 2 (0x02) which is the Protocol Identifier for the CCSDS Packet Encapsulation Protocol."]
["ECSS-E-ST-50-53C","ECSS - Current v1.0","5.5.3a","Requirement","ECSS-E-ST-50-53_1090044",1,"Created","In response to the send request the initiator shall encapsulate the CCSSDS Space Packet into a SpaceWire packet as described in clause 5.4 and send it across the SpaceWire network to the target (Transfer Packet).\n    ","NOTE The Target SpaceWire Address and Target Logical Address are used to route the command packet to the target."]
["ECSS-E-ST-60-10C","ECSS - Current v1.0","4.1.3a","Requirement","ECSS-E-ST-60-10_1020002",1,"Created","When specifying a requirement on the knowledge of the performance, the following elements shall be specified:\n    1. The quantities to be constrained.\n        NOTE 1 This is usually done specifying the appropriate indices (AKE, MKE, RKE) as defined in 3.2                                                     \n        NOTE 2 All the elements needed to fully describe the constrained quantities are listed there; for example, the associated timescales for MKE or RKE.\n    2. The allowed range for each of these quantities.\n    3. The probability that each quantity lies within the specified range.\n        NOTE This is often called the confidence level. See 4.1.4;\n    4. The interpretation of this probability.\n        NOTE 1 This is often referred to as the “statistical interpretation”. See annex A.1.2                                                     \n        NOTE 2 The way to specify the statistical interpretation is described in 4.1.4.2                                                     \n    5. The conditions under which the requirement applies.\n        NOTE These conditions can be that the requirement refers to the state of knowledge on-board, on ground before post processing, or after post processing. This is explained further in annex A.1.3."]
["ECSS-E-ST-60-10C","ECSS - Current v1.0","5.2.5a","Requirement","ECSS-E-ST-60-10_1020035",1,"Created","Nominal stability margins are given by specifying values  ,  ,  , and   such that the following relations shall be met:\n1.\tThe gain margin is greater than  \n2.\tThe phase margin is greater than  \n3.\tThe modulus margin is greater than  \n4.\tThe peak sensitivity and complementary sensitivity functions is lower than  ."]
["ECSS-E-ST-70-01C","ECSS - Current v1.0","5.2.6a","Requirement","ECSS-E-ST-70-01_1060021",1,"Created","Mathematical, time, string and bitwise operations and functions shall be supported."]
["ECSS-E-ST-70-01C","ECSS - Current v1.0","5.3.1a","Requirement","ECSS-E-ST-70-01_1060054",1,"Created","An editor (read and write) shall be provided for preparing OBCPs."]
["ECSS-E-ST-70-01C","ECSS - Current v1.0","5.4.2.3b","Requirement","ECSS-E-ST-70-01_1060075",1,"Created","If the OBCP engine receives a request that is not consistent with the current state of an OBCP, it shall fail the request and generate a telecommand verification failure.\n    NOTE For example, an Activate request for an already active OBCP."]
["ECSS-E-ST-70-01C","ECSS - Current v1.0","5.4.4.1a","Requirement","ECSS-E-ST-70-01_1060087",1,"Created","A given on-board application process shall implement at most one OBCP engine whose function is the execution and associated handling of OBCPs."]
["ECSS-E-ST-70-01C","ECSS - Current v1.0","6.2.1b","Requirement","ECSS-E-ST-70-01_1060120",1,"Created","The OBCP system management process shall include the following activities:\n    1. collection of needs from the various stakeholders (see clause 4.2);\n    2. trade-off analysis between implementing the needs as OBSW or as OBAP (see clause 6.2.2);\n    3. analysis of the use case inputs for future OBOP needs (see clause 6.2.3) and expected benefits in terms of engineering effort (see clause 6.2.4) and assignment of requirements to the on-board system and to the ground system."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","4.5a","Requirement","ECSS-E-ST-70-11_0290005",1,"Created","No single command function executed at the wrong time or in the wrong configuration shall lead to the loss of the mission.\n    ","NOTE For a mission-critical command function, this can be ensured by the provision of two independent commands, both to be executed (e.g. ARM and FIRE)."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","4.6d","Requirement","ECSS-E-ST-70-11_0290014",1,"Created","For each on-board function, there shall be at least one alternative configuration that can achieve the same function using different on-board units."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.3.1k","Requirement","ECSS-E-ST-70-11_0290047",1,"Created","Vital space segment health functions shall be monitored with redundant telemetry parameters (e.g. primary bus current and voltage, and propellant tank pressure)."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.4e","Requirement","ECSS-E-ST-70-11_0290072",1,"Created","After initialization of an application process using time synchronization, telemetry shall be provided to notify the ground segment when time synchronization has been achieved."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.5.1d","Requirement","ECSS-E-ST-70-11_0290085",1,"Created","Where a given function is invoked by a sequence of two or more telecommands, the capability shall be provided to “pack” such telecommands within a single telecommand packet."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.5.4i","Requirement","ECSS-E-ST-70-11_0290113",1,"Created","If a telecommand is invalid, it shall fail verification at the acceptance stage and shall not be distributed further.\n    ","NOTE For example, the length or CRC are wrong or the APID is invalid."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.7.2b","Requirement","ECSS-E-ST-70-11_0290138",1,"Created","The on-board autonomy management functions shall be capable of performing all operations to continue mission operations for an autonomy duration of <AUT_DUR_EXEC>."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.7.5.5c","Requirement","ECSS-E-ST-70-11_0290171",1,"Created","A failure in the performance of an autonomous recovery action shall be followed by an action to ensure the safety of the spacecraft, subsystem or payload.\n    ","NOTE In some cases, pre-defined retries are implemented in the system (e.g. for protocol handling)."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.8.2c","Requirement","ECSS-E-ST-70-11_0290196",1,"Created","The capability shall be provided to add and delete parameters from the set being evaluated."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.8.3f","Requirement","ECSS-E-ST-70-11_0290205",1,"Created","The capability shall be provided for the ground segment to dump any memory area, on request."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.8.6j","Requirement","ECSS-E-ST-70-11_0290246",1,"Created","All changes of monitoring status shall be reported to the ground segment by means of a “check transition” telemetry packet.\n    ","NOTE For example, a check transition telemetry packet produced when a parameter goes out-of-limits and when it subsequently returns back into limits."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.8.9d","Requirement","ECSS-E-ST-70-11_0290262",1,"Created","The content of the anomaly log specified in requirement 5.8.9c shall be persistent even after a reconfiguration or a cold restart of the application process managing the store."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.9.1c","Recommendation","ECSS-E-ST-70-11_0290360",1,"Created","A processor switchover should not invalidate telecommands not yet released from any ground schedule.\n    ","NOTE This implies that telecommands defined for the prime unit are also valid for the redundant unit, except for any command routing data which the ground system can automatically change when addressing the redundant processor."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.9.2f","Requirement","ECSS-E-ST-70-11_0290320",1,"Created","Vital power control functions shall have a switch-over function to the redundant path, but never a switch-off function."]
["ECSS-E-ST-70-11C","ECSS - Current v1.0","5.9.4c","Requirement","ECSS-E-ST-70-11_0290329",1,"Created","The telemetry of stimulated detectors shall be designed to handle all flight-phase conditions either in normal mode telemetry or by mode-switching to extended range."]
["ECSS-E-ST-70C","ECSS - Current v1.0","5.2.2.3g","Requirement","ECSS-E-ST-70_0060014",1,"Created","The contents of the CFISRD shall be in conformance with Annex J."]
["ECSS-E-ST-70C","ECSS - Current v1.0","5.4.1a","Requirement","ECSS-E-ST-70_0060039",1,"Created","The inputs to the mission operations data validation process shall be the ones specified in Table 5-5:"]
["ECSS-E-ST-70C","ECSS - Current v1.0","5.5.2c","Requirement","ECSS-E-ST-70_0060048",1,"Created","The operations teams shall be assigned and trained such that they are familiar with the mission and the supporting facilities before the start of operational validation."]
["ECSS-E-ST-70C","ECSS - Current v1.0","5.8.2.3e","Requirement","ECSS-E-ST-70_0060080",1,"Created","Health monitoring of the space and ground segments shall be performed."]
["ECSS-E-ST-70C","ECSS - Current v1.0","6.2.1a","Requirement","ECSS-E-ST-70_0060105",1,"Created","The inputs to the ground segment definition process shall be the ones identified in Table 6-1."]
["ECSS-E-ST-70C","ECSS - Current v1.0","6.3.2g","Requirement","ECSS-E-ST-70_0060138",1,"Created","Acceptance test reports shall be produced for each ground system."]
["ECSS-E-ST-70C","ECSS - Current v1.0","6.5.2.2e","Requirement","ECSS-E-ST-70_0060163",1,"Created","The incident management process shall log incidents and restore normal service operation in line with availability requirements."]
["ECSS-E-ST-70C","ECSS - Current v1.0","6.6.2c","Requirement","ECSS-E-ST-70_0060172",1,"Created","The disposal analysis shall cover cost and organization of the disposal."]
["ECSS-E-ST-70C","ECSS - Current v1.0","A.2.1<2>a","Requirement","ECSS-E-ST-70_0060209",1,"Created","The CRD shall list the applicable and reference documents in support of the generation of the document."]
["ECSS-E-ST-70C","ECSS - Current v1.0","B.2.1<9>a","Requirement","ECSS-E-ST-70_0060229",1,"Created","The MAR shall document the propellant budget for orbit control including routine orbit change manoeuvres (and delta-V manoeuvres in the case of interplanetary missions)."]
["ECSS-E-ST-70C","ECSS - Current v1.0","C.2.1<4>a","Requirement","ECSS-E-ST-70_0060238",1,"Created","The MOCD shall describe the capabilities and characteristics of the space segment platform, payload(s) and the space link subnet, including:\n    1. on-board autonomous functions;\n    2. the mechanisms for on-board generation, storage and downlink of mission data products;\n    3. the end-user services to be provided.\n        NOTE The objective is to capture all the salient operational characteristics that are needed for the analysis of the operations processes."]
["ECSS-E-ST-70C","ECSS - Current v1.0","E.2.1<4.4>a","Requirement","ECSS-E-ST-70_0060263",1,"Created","The system-level budgets shall provide the distribution (or allocation) of the following budgets, per platform subsystem or payload, or per mission phase:\n    1. satellite mass evolution;\n    2. satellite mass properties evolution;\n    3. power consumption for all operational modes;\n    4. power available in different mission phases;\n    5. thermal budget and constraints and predictions;\n    6. RF links (down and up);\n    7. telemetry and telecommand date rates;\n    8. memory;\n    9. timing (including allocation between space and ground segments);\n    10. propulsion system data;\n    11. attitude measurement sensor data;\n    12. pointing accuracy in routine phase;\n    13. pointing accuracy in manoeuvre phase;\n    14. alignment;\n    15. outages resulting from satellite operations.\n        NOTE For example, pointing accuracy degradation during a manoeuvre or degraded performance during an eclipse."]
["ECSS-E-ST-70C","ECSS - Current v1.0","F.2.1<3.1>a","Requirement","ECSS-E-ST-70_0060296",1,"Created","The OVP shall include:\n    1. a statement of the operational validation objectives;\n    2. a presentation of the overall structure and schedule for the operational validation, including major milestones;\n    3. identification of any constraints or mission-specific considerations;\n    4. identification of the mechanisms and criteria to be used for measuring and evaluating the success of the operational validation."]
["ECSS-E-ST-70C","ECSS - Current v1.0","H.2.2<6>a","Requirement","ECSS-E-ST-70_0060329",1,"Created","The OAR shall propose a course of action for further investigation and resolution of the anomaly:\n    1. Either internally by the ground segment and operations supplier, or\n    2. By external parties."]
["ECSS-E-ST-70C","ECSS - Current v1.0","J.2.1<5>a","Requirement","ECSS-E-ST-70_0060354",1,"Created","The CFISRD shall define the requirements for the delivery of space segment models (hardware or software) for integration into an operational simulator, covering:\n    1. Scope and fidelity of models;\n    2. Specification of the ICD between the models and the operational simulator kernel;\n    3. Pre-delivery validation requirements;\n    4. Content of the delivery\n        NOTE For example, code, documentation, delivery note, and software problems reports/lists/database.\n    5. Delivery schedule for different versions."]
["ECSS-E-ST-70C","ECSS - Current v1.0","J.2.1<10>a","Requirement","ECSS-E-ST-70_0060359",1,"Created","The CFISRD shall identify the requirements for post-launch technical support from the OC, covering:\n    1. On-site participation of project support teams during LEOP and commissioning phase operations, including responsibilities, required skills, schedule for support;\n    2. On-call engineering support to mission operations at the mission control centre: response time as a function of mission phase;\n    3. Call-out engineering support for satellite anomaly recovery operations at the mission control centre, including response time as a function of mission phase;\n    4. Off-site support for analysis of satellite anomalies, including inputs to be provided to the OC (in particular anomaly reports, in accordance with Annex H), definition of close-out report, and response times."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","5.3b","Requirement","ECSS-E-ST-50-05_0900037",1,"Unchanged","Earth stations shall be capable of transmitting right-hand or left-hand circular polarization upon discretion of the user. \n    NOTE 1 For practical reasons, spacecraft generally use the same sense of polarization for the Earth-space link and the space-Earth link.\n    NOTE 2 Most Earth stations have the capability of combining two orthogonal circular polarizations on the space-Earth link."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","6.1.2a","Permission","ECSS-E-ST-50-05_0900275",1,"Created","The following modulating waveforms may be used:\n    1. Telemetry, a subcarrier modulated by PCM data.\n    2. Telemetry, PCM data, SP-L encoded.\n    3. Telecommand, a subcarrier modulated by PCM data.\n    4. Telecommand, PCM data, SP-L encoded.\n    5. Ranging, the appropriate ranging baseband signal.\n        NOTE 1 In the case of simultaneous telecommand, ranging and telemetry, when selecting telecommand and telemetry modulation schemes it is important to take into account their mutual interference. \n        NOTE 2 See also ECSS-E-ST-50-02."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","6.1.4.1.3a","Requirement","ECSS-E-ST-50-05_0900071",1,"Unchanged","For NRZ telemetry symbol rates above 60 ksps, subcarriers shall not be used and one of the following modulation schemes shall be used:\n    • SP-L encoded symbols and direct modulation on the carrier for symbol rates as high as 1 Msps in the 2 200 MHz - 2 300 MHz and 8 400 MHz - 8 500 MHz bands.\n    • Modulation in conformance to clause 6.2 of this Standard."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","6.1.7a","Requirement","ECSS-E-ST-50-05_0900096",1,"Unchanged","A positive-going video signal shall result in an advance of the phase of the radio frequency carrier."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","6.2.3.3a","Requirement","ECSS-E-ST-50-05_0900129",1,"Unchanged","The data shall consist of two channels with different symbol rates and the modulation shall be phase-reversal keying of two-phase quadrature RF carriers with different amplitude."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","6.2.6c","Requirement","ECSS-E-ST-50-05_0900162",1,"Unchanged","Phase noise of the unmodulated carrier, integrated between 100 Hz and 1 MHz shall be less than 6° r.m.s. at SHF for the 8 025 MHz - 8 500 MHz band."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","7.2.1l","Requirement","ECSS-E-ST-50-05_0900190",1,"Unchanged","Onboard demodulators shall not use frequency sweep for subcarrier (when present) or bit clock acquisition. "]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","7.2.4b","Recommendation","ECSS-E-ST-50-05_0900285",1,"Created","The Earth station design should be such that it can enable the support of transponders with other PLL bandwidths.\n    NOTE This can be achieved by including flexibility on the parameters given in 7.2.4a."]
["ECSS-E-ST-50-05C Rev. 2","ECSS - Current v1.0","9.2.3a","Recommendation","ECSS-E-ST-50-05_0900298",1,"Created","To eliminate 22,5° phase ambiguity on carrier synchronization, the codes represented in Figure 9-2 should be used."]
["ECSS-E-ST-70-32C","ECSS - Current v1.0","5.1j","Permission","ECSS-E-ST-70-32_0950049",1,"Created","Preconditions and confirmation conditions may also be defined for steps."]
["ECSS-E-ST-70-32C","ECSS - Current v1.0","5.2a","Requirement","ECSS-E-ST-70-32_0950019",1,"Created","The capability shall be provided to request the execution of any space system activity."]
["ECSS-E-ST-70-32C","ECSS - Current v1.0","5.3b","Recommendation","ECSS-E-ST-70-32_0950059",1,"Created","The PLUTO procedure language, engineering units and functions, as specified in Annex A should be used for the automation of procedures in the development and exploitation phases of space systems.\n    ","NOTE Use of the PLUTO language ensures conformance with all requirements of this Standard. It also facilitates the transfer of procedure knowledge, acquired in the development phase during functional testing, to the mission operations phase (for a given mission) and encourages the use of a common procedure language across missions."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.2.3e","Requirement","ECSS-E-ST-70-31_0270019",1,"Created","The capability to assign engineering units to constants shall be supported."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.3.2.7b","Requirement","ECSS-E-ST-70-31_0270059",1,"Created","When one (or more) property of an activity has changed between successive product deliveries, a new version shall be defined for this activity."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.5.3.2a","Requirement","ECSS-E-ST-70-31_0270084",1,"Created","For system elements of type “system” that utilise ECSS-E-ST-70-41, the additional data specified in Table 6-12 shall be provided."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.5.5.3.2a","Requirement","ECSS-E-ST-70-31_0270093",1,"Created","For the data types of the packet fields of the device command distribution service, the additional data shown in Table 6-21 shall be provided.\n    ","NOTE See clauses 6.5.12, 6.5.13 and 6.5.14 for the related CPDU, On/Off and register load device data."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.5.5.11.1a","Requirement","ECSS-E-ST-70-31_0270118",1,"Created","For the definition of the tailoring of the on-board monitoring service, the additional data shown in Table 6-46 shall be provided."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.6.3.3.2a","Requirement","ECSS-E-ST-70-31_0270151",1,"Created","When an interpretation function is used to translate the raw value into an engineering value, the additional data specified in Table 6-77 shall be provided."]
["ECSS-E-ST-70-31C","ECSS - Current v1.0","6.6.6.1a","Requirement","ECSS-E-ST-70-31_0270160",1,"Created","For reporting data that is limit-checked, the additional data specified in Table 6-85 shall be provided."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","5.1.1.2a","Requirement","ECSS-E-ST-50-15_1270007",1,"Created","Bus terminators shall be implemented according to ISO 11898-2:2003 clause 7.5.2."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","5.2.2.4a","Requirement","ECSS-E-ST-50-15_1270030",1,"Created","Pins designated as ‘Reserved’ in clause 10 of this standard shall not be used.","NOTE\tReserved Pins are reserved for functions in future updates to this standard."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","5.4.2b","Permission","ECSS-E-ST-50-15_1270253",1,"Created","A device may implement additional bit rates only after complying to all the rates stated in 5.4.2a. "]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","6.7c","Requirement","ECSS-E-ST-50-15_1270078",1,"Created","The result of the test shall be accessible in a dedicated object."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","6.10c","Requirement","ECSS-E-ST-50-15_1270087",1,"Created","The capability shall be provided to change any non-restricted COB-ID of a device at any time up to the completion of system level testing without need for a re-qualification of the device.","NOTE\tThis implies that COB-ID reassignment capability can be implemented by using SDOs but also by other means such as PROM boxes, straps in connectors, S/W updates or similar can be considered if acceptable for the particular application."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","7.1.3b","Requirement","ECSS-E-ST-50-15_1270112",1,"Created","The Local UTC Set object shall provide the capability of setting the local time of the node via the CAN Network."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","7.2.3h","Requirement","ECSS-E-ST-50-15_1270134",1,"Created","Each Time consumer shall map the Local SCET Get object (7.1.2) or the Local UTC Get object (7.1.3) to a dedicated Local Time PDO transmit PDO."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","8.3.3f","Requirement","ECSS-E-ST-50-15_1270156",1,"Created","The Redundancy Master shall command slave nodes that have performed a bus switch as defined in 8.3.3e into operational mode.","NOTE\t1\tFigure 8-2 shows the bus monitoring logic.\nNOTE\t2\tOptionally, in case a node misses the Master Heartbeat the node can send an EMCY message on the active bus before switching bus."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","9.4.4c","Requirement","ECSS-E-ST-50-15_1270187",1,"Created","The PDO communication parameter object relative to a Data Transmission triggered by a Telemetry Request shall correspond to the structure and entries defined in Table 9-5 and Table 9-6."]
["ECSS-E-ST-50-15C","ECSS - Current v1.0","10.3.2e","Requirement","ECSS-E-ST-50-15_1270228",1,"Created","The key orientation for the secondary bus shall be A."]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.2.4.1.1a","Requirement","ECSS-E-ST-20-20_1320017",1,"Created","In case the load current exceeds the relevant limit, the LCL/RLCL/HLCL shall switch-off within its trip-off time min to max range defined in Table 3-1, Table 3-2 and Table 3-3"]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.2.13.2.1a","Requirement","ECSS-E-ST-20-20_1320045",1,"Created","For LCL/HLCL, the load power consumption considered as negligible in terms of power budget shall be specified by the system integrator.","NOTE \tThe \"negligible\" power consumption is intended as the one that can be drawn from the power bus without the system integrator or system responsible being forced to disconnect it.\nSuch power level is indeed added to the power budget.\n"]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.2.16.1.1a","Requirement","ECSS-E-ST-20-20_1320051",1,"Created","The LCL/RLCL/HLCL state shall not change from the commanded one due to spurious perturbations, including:\n1.\tEM emissions, both conducted and radiated,\n2.\tSEE,\n3.\tESD,\n4.\tON/OFF commands to other LCL/RLCL lines, and\n5.\tOvercurrent events to other LCL/RLCL lines."]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.4.2.2.1a","Requirement","ECSS-E-ST-20-20_1320078",1,"Created","Maximum LCL/RLCL/HLCL switch-off current rate dI/dt shall be 1A/µs."]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.4.12.1a","Requirement","ECSS-E-ST-20-20_1320107",1,"Created","The LCL/RLCL/HLCL ON/OFF status shall confirm that the LCL/RLCL/HLCL output voltage is within its nominal range with an accuracy of ±10 %."]
["ECSS-E-ST-20-20C","ECSS - Current v1.0","5.5.3.2.1a","Requirement","ECSS-E-ST-20-20_1320115",1,"Created","For LCL/RLCL, at those frequencies in which the difference between the load impedance phase and the source impedance phase is equal to \n-180°±n*360°, the difference between the load impedance gain and the LCL impedance gain shall be greater than 5 dB. ","NOTE \tn is a positive integer including 0.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","5.3.3.2e","Requirement","ECSS-E-ST-70-41_1330022",1,"Created","For each request type that contains several instruction types, the allowed combinations of instruction types that can be used in a request of that request type shall be declared when specifying that request type.","NOTE\tAn allowed combination of instruction types means that the realizations of two or more of those instruction types can be merged in a single request of the corresponding request type, see for example the add report types to the application process storage-control configuration specified in clause 6.15.4.4.1.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","5.4.2.1b","Requirement","ECSS-E-ST-70-41_1330055",1,"Created","Each application process that hosts at least one subservice provider shall be identified by an application process identifier that is unique across the system that hosts that subservice provider.","NOTE 1\tThis Standard acknowledges that the same application process identifier can be used to identify several application processes. This is for example the case during the space system development where different representations of a given application process are used, e.g. a simulated version of an application process used for testing the ground segment but also during operations, e.g. in case of cold redundancy.\nNOTE 2\tThe system introduced in this requirement can be, for example, the spacecraft that hosts the on-board application process. The concept of system identifier is also used in this Standard to uniquely identify that system across the overall space system. This Standard does not further elaborate on this system concept and its identifier.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","5.4.4a","Requirement","ECSS-E-ST-70-41_1330080",1,"Created","For each checksum algorithm used on-board, the list of subservice providers that use that checksum algorithm shall be declared when specifying the spacecraft architecture.","NOTE 1\tThis requirement is justified by the system need to ensure that all subservice providers that provide means to checksum a specific data object use the same checksum algorithm. For example, if a file contains an OBCP that can be checksummed by the OBCP service and that file is also managed by a memory service, the same checksum algorithm is used by both services.\nNOTE 2\tThe checksum algorithm implies the type of checksum i.e. ISO or CRC, and the size of the checksum.\nNOTE 3\tThe checksum algorithm to use to checksum all telemetry packets and the checksum algorithm to use for all telecommand packets are specified in requirements 7.4.3.2e and 7.4.4.2d.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","5.4.7.2.2a","Requirement","ECSS-E-ST-70-41_1330097",1,"Created","Each subservice shall provide exactly one subservice provider.","NOTE\tA subservice provider is an operational element of a subservice that is in charge of execution of the subservice requests and generation of the subservice reports. The subservice providers are usually hosted by the on-board application processes.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","5.4.11.3.3a","Requirement","ECSS-E-ST-70-41_1330121",1,"Created","For each data report that can be generated in an autonomous data reporting transaction, the destination of the data report in that case shall be declared when specifying the related subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.1.4.3c","Requirement","ECSS-E-ST-70-41_1330145",1,"Created","Each failed acceptance notification shall contain:\n1.\tthe identifier of the request that failed the acceptance verification;\n2.\tthe failure notice made of:\n(a)\ta failure code;\n(b)\tauxiliary data, if any, used to explain the reason for the failed acceptance.","NOTE\tFor item 2, see requirements 6.1.4.3d and 6.1.4.3e.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.2.5.2a","Requirement","ECSS-E-ST-70-41_1330178",1,"Created","The device access subservice capability to distribute register load commands shall be declared when specifying that subservice.","NOTE 1\tThe corresponding requests are of message type \"TC[2,2] distribute register load commands\".\nNOTE 2\tFor that declaration, refer to requirement 6.2.3a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.2.5.3c","Requirement","ECSS-E-ST-70-41_1330187",1,"Created","Each instruction to distribute a register dump command shall contain:\n1.\tthe register address.","NOTE\tFor item 1, refer to requirement 6.2.5.1b.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.2.7.1.3b","Requirement","ECSS-E-ST-70-41_1330212",1,"Created","Each request to acquire data from physical devices shall contain an ordered list of one or more instructions to acquire data from a physical device."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.3.2a","Requirement","ECSS-E-ST-70-41_1330245",1,"Created","The on-board resources allocated to the housekeeping reporting subservice to host the housekeeping parameter report structures shall be declared when specifying that subservice.","NOTE\tThe allocated resources constrain the number of housekeeping parameter report structures and their content, in number of parameters.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.3.5.1b","Requirement","ECSS-E-ST-70-41_1330269",1,"Created","Each request to create a housekeeping parameter report structure shall contain exactly one instruction to create a housekeeping parameter report structure."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.3.9b","Requirement","ECSS-E-ST-70-41_1330302",1,"Created","Each request to modify the collection interval of housekeeping parameter report structures shall contain one or more instructions to modify the collection interval of a housekeeping parameter report structure."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.3.10d","Requirement","ECSS-E-ST-70-41_1330311",1,"Created","The housekeeping reporting subservice shall reject any instruction to report the periodic generation properties of a housekeeping parameter report structure if:\n1.\tthat instruction refers to a housekeeping parameter report structure that is unknown."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.4.5d","Requirement","ECSS-E-ST-70-41_1330336",1,"Created","The diagnostic reporting subservice shall reject any instruction to disable the periodic generation of a diagnostic parameter report if:\n1.\tthat instruction refers to a diagnostic parameter report structure that is unknown."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.4.10c","Requirement","ECSS-E-ST-70-41_1330369",1,"Created","Each instruction to append parameters to a diagnostic parameter report structure shall contain:\n1.\tthe diagnostic parameter report structure identifier to modify;\n2.\tif the diagnostic parameter report structure only includes simply commutated parameters, at least one of:\n(a)\tthe ordered list of simply commutated parameters to add;\n(b)\tthe ordered list of super commutated parameter sets to add;\n3.\tif the diagnostic parameter report structure includes super commutated parameters:\n(a)\tthe ordered list of super commutated parameter sets to add."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.5.3c","Requirement","ECSS-E-ST-70-41_1330394",1,"Created","The parameter functional reporting configuration subservice shall reject any request to apply parameter functional reporting configurations if:\n1.\tthat request refers to an invalid configuration execution flag."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.5.4.1e","Requirement","ECSS-E-ST-70-41_1330407",1,"Created","For each request to create a parameter functional reporting definition that is rejected, the parameter functional reporting configuration subservice shall generate a failed start of execution notification."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.3.5.6.2d","Requirement","ECSS-E-ST-70-41_1330435",1,"Created","For each request to remove parameter report definitions from a parameter functional reporting definition that is rejected, the parameter functional reporting configuration subservice shall generate a failed start of execution notification."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.4.4b","Requirement","ECSS-E-ST-70-41_1330460",1,"Created","Each request to reset the parameter statistics shall contain exactly one instruction to reset the parameter statistics.","NOTE\tThe instructions to reset the parameter statistics contain no argument.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.4.7.1e","Requirement","ECSS-E-ST-70-41_1330493",1,"Created","The parameter statistics reporting subservice shall reject any instruction to add or update a parameter statistics definition if any of the following conditions occurs:\n1.\tthat instruction refers to a parameter that is unknown;\n2.\tthe sampling interval is greater than the reporting interval;\n3.\tthat instruction implies adding a parameter statistics definition but the maximum number of definitions that the subservice supports is already reached.","NOTE\tFor item 3, refer to requirement 6.4.3.1a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.4.7.2f","Requirement","ECSS-E-ST-70-41_1330502",1,"Created","The parameter statistics reporting subservice shall process any valid instruction that is contained within a request to delete parameter statistics definitions regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.5.5.2e","Requirement","ECSS-E-ST-70-41_1330527",1,"Created","For each instruction to enable the report generation of an event definition that it rejects, the event reporting subservice shall generate the failed start of execution notification for that instruction."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.3.3.1g","Requirement","ECSS-E-ST-70-41_1330560",1,"Created","For each request to load raw memory data areas that contains only valid instructions, the raw data memory management subservice shall execute those instructions in the order of their appearance in that request."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.3.4g","Requirement","ECSS-E-ST-70-41_1330580",1,"Created","For each instruction to dump a raw memory data that it rejects, the raw data memory management subservice shall generate the failed start of execution notification for that instruction."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.3.5j","Requirement","ECSS-E-ST-70-41_1330593",1,"Created","For each valid request to check raw memory data, the raw data memory management subservice shall generate a single checked raw memory data report that contains:\n1.\tif the raw data memory management subservice manages more than one memory, the identifier of the memory;\n2.\tall related checked raw memory data notifications.","NOTE\tFor item 1, refer to requirement 6.6.3.2a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.4.4d","Requirement","ECSS-E-ST-70-41_1330626",1,"Created","Each instruction to load an object memory data shall contain:\n1.\tthe byte offset within the memory object identified by the base identifier;\n2.\tthe data to load;\n3.\tif the structured data memory management subservice provides checksumming, the checksum value for the verification of the data after it has been loaded to the memory.","NOTE\tFor item 3, refer to requirement 6.6.4.1a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.4.6h","Requirement","ECSS-E-ST-70-41_1330651",1,"Created","The structured data memory management subservice shall process any valid instruction that is contained within a request to check object memory data regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.5.1c","Requirement","ECSS-E-ST-70-41_1330684",1,"Created","For each valid instruction to abort all memory dumps, the common memory management subservice shall:\n1.\tif the service includes a raw data memory management subservice, abort the execution of all dump requests that are under execution by that subservice;\n2.\tif the service includes a structured data memory management subservice, abort the execution of all dump requests that are under execution by that subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.6.6.1.4d","Requirement","ECSS-E-ST-70-41_1330693",1,"Created","The memory configuration subservice shall reject any request to enable the scrubbing of a memory if:\n1.\tthat request contains an instruction that refers to a memory that cannot be scrubbed.","NOTE\tFor item 1, refer to requirement 6.6.6.1.2a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.8.2.1.1a","Requirement","ECSS-E-ST-70-41_1330718",1,"Created","Each function management service shall contain at least one function management subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.9.4.3a","Requirement","ECSS-E-ST-70-41_1330750",1,"Created","The time reporting subservice capability to generate time reports in CDS time format shall be declared when specifying that subservice.","NOTE 1\tThe corresponding reports are data reports of message type \"TM[9,3] CDS time report\".\nNOTE 1\tFor that declaration, refer to requirement 6.9.4.1a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.4.2d","Requirement","ECSS-E-ST-70-41_1330775",1,"Created","The time margin that the time-based scheduling subservice uses when inserting activities in the time-based schedule or time-shifting activities shall be declared when specifying that subservice.","NOTE 1\tThe time margin is present in order to ensure the consistency and operability of the schedule at any time. Inserting activities or time-shifting them can only be performed if the release time of these activities is greater than or equal to the current time plus a time margin.\nNOTE 1\tThe time margin parameter is called the \"time-based schedule time margin\".\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.4.3.3c","Requirement","ECSS-E-ST-70-41_1330784",1,"Created","For each valid instruction to disable the time-based schedule execution function, the time-based scheduling subservice shall:\n1.\tset the time-based schedule execution function status to \"disabled\".","NOTE\tDisabling the time-based schedule execution function does not depend on the presence of scheduled activities in the schedule.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.5.2.2f","Requirement","ECSS-E-ST-70-41_1330817",1,"Created","The time-based scheduling subservice shall process any valid instruction that is contained within a request to disable time-based sub-schedules regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.6.3.1b","Requirement","ECSS-E-ST-70-41_1330842",1,"Created","Each request to enable time-based scheduling groups shall contain:\n1.\tone or more instructions to enable a time-based scheduling group, or\n2.\texactly one instruction to enable all time-based scheduling groups.","NOTE\tThe instructions to enable all time-based scheduling groups contain no argument.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.8.2c","Requirement","ECSS-E-ST-70-41_1330875",1,"Created","For each valid instruction to summary-report all time-based scheduled activities, the time-based scheduling subservice shall generate, for each scheduled activity contained within the time-based schedule, a single time-based schedule summary notification.","NOTE\t The time-based schedule summary notification content is specified in clause 6.11.7.1.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.9.3c","Requirement","ECSS-E-ST-70-41_1330891",1,"Created","The time-based scheduling subservice shall reject any request to time-shift scheduled activities identified by request identifier if:\n1.\tthe time obtained by adding the time offset to the release time of the earliest activity identified by an instruction in the request is earlier than the time obtained by adding the time-based schedule time margin to the current time.","NOTE\tIf the time offset is sufficient to result in a scheduled activity with a release time in the past or with a release time that is too close to the current time, that request is rejected and no activities are time-shifted.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.9.5c","Requirement","ECSS-E-ST-70-41_1330908",1,"Created","Each instruction to detail-report a time-based scheduled activity identified by request identifier shall contain:\n1.\tthe identifier of the scheduled activity to report.","NOTE\tThe activity identifier is specified in requirement 6.11.4.2b.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.11.10.6a","Requirement","ECSS-E-ST-70-41_1330941",1,"Created","The time-based scheduling subservice capability to detail-report the time-based scheduled activities identified by a filter shall be declared when specifying that subservice.","NOTE 1\tThe corresponding requests are of message type \"TC[11,11] detail-report the time-based scheduled activities identified by a filter\". The responses are data reports of message type \"TM[11,10] time-based schedule detail report\"(refer to clause 6.11.7.2).\nNOTE 2\tThat capability implies that the subservice provides the capability of the time-window filtering function (refer to requirement 6.11.10.1a).\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.3.3f","Requirement","ECSS-E-ST-70-41_1330965",1,"Created","Monitoring intervals shall be expressed in \"on-board parameter minimum sampling interval\" units.","NOTE\tThe on-board parameter minimum sampling interval is driven by requirement 5.4.3.2c.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.3.5.1a","Requirement","ECSS-E-ST-70-41_1330974",1,"Created","The parameter monitoring subservice shall provide the capability to enable the parameter monitoring function.","NOTE 1\tThe corresponding requests are of message type \"TC[12,15] enable the parameter monitoring function\".\nNOTE 2\tFor the capability to disable the parameter monitoring function, refer to clause 6.12.3.5.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.3.7e","Requirement","ECSS-E-ST-70-41_1331007",1,"Created","The maximum transition reporting delay shall be expressed in \"on-board parameter minimum sampling interval\" units.","NOTE\tThe on-board parameter minimum sampling interval is driven by requirement 5.4.3.2c.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.3.9.3g","Requirement","ECSS-E-ST-70-41_1331032",1,"Created","For each valid instruction to delete a parameter monitoring definition, the parameter monitoring subservice shall:\n1.\tremove the parameter monitoring definition that is referred to by that instruction from the PMON list."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.3.11c","Requirement","ECSS-E-ST-70-41_1331051",1,"Created","For each valid instruction to report the status of each parameter monitoring definition, the parameter monitoring subservice shall:\n1.\tgenerate, for each parameter monitoring definition in the PMON list, a single parameter monitoring definition status notification that includes:\n(a)\tthe identifier of the parameter monitoring definition;\n(b)\tits PMON status."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.4.5.3b","Requirement","ECSS-E-ST-70-41_1331089",1,"Created","Each request to disable functional monitoring definitions shall contain one or more instructions to disable a functional monitoring definition."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.4.6.1d","Requirement","ECSS-E-ST-70-41_1331098",1,"Created","The functional monitoring subservice shall reject any instruction to protect a functional monitoring definition if:\n1.\tthat instruction refers to a functional monitoring definition identifier that is not in the FMON list."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.12.4.8g","Requirement","ECSS-E-ST-70-41_1331131",1,"Created","For each valid instruction to report a functional monitoring definition, the functional monitoring subservice shall\n1.\tgenerate a single functional monitoring definition notification that includes:\n(a)\tthe content of the functional monitoring definition that is referred to by that instruction;\n(b)\tif the functional monitoring subservice supports the capability for protecting functional monitoring definitions, the FMON protection status of that functional monitoring definition;\n(c)\tthe FMON status of that functional monitoring definition.","NOTE 1\tFor item 1(a), the content of a functional monitoring definition is specified in requirement 6.12.4.2.1f.\nNOTE 2\tFor item 1(b), refer to requirement 6.12.4.6.1a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.13.3.3.2d","Requirement","ECSS-E-ST-70-41_1331156",1,"Created","For each part report that is received, the receiving entity of the large packet downlink subservice shall include that part in the reconstruction process of the related large packet."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.13.4.2a","Requirement","ECSS-E-ST-70-41_1331165",1,"Created","The resources allocated to the uplink receiving entity of the large packet uplink subservice to process large packets shall be declared when specifying the spacecraft architecture and its operations."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.2.5a","Requirement","ECSS-E-ST-70-41_1331201",1,"Created","The maximum number of event report blocking forward-control definitions that the real-time forwarding control subservice can contemporaneously control shall, at any time, correspond to the number of application processes that are controlled by that subservice and that provide the capability for generating event reports.","NOTE 1\tFor the number of application processes, see requirement 6.14.3.1.1a.\nNOTE 1\tThe event report blocking forward-control configuration contains the event report blocking forward-control definitions of the real-time forwarding control subservice.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.4.1j","Requirement","ECSS-E-ST-70-41_1331222",1,"Created","The real-time forwarding control subservice shall process any valid instruction that is contained within a request to add report types to the application process forward-control configuration regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.5.1j","Requirement","ECSS-E-ST-70-41_1331255",1,"Created","For each valid instruction to add all structure identifiers to the housekeeping parameter report forward-control configuration, the real-time forwarding control subservice shall:\n1.\tadd, for the specified application process identifier, a housekeeping parameter report forward-control definition if not already existing;\n2.\tdelete, if any, all housekeeping parameter report structure identifiers of the related housekeeping parameter report forward-control definition. ","NOTE\tFor item 2, deleting a housekeeping parameter report structure identifier implies deleting the corresponding subsampling rate if any (see also requirement 6.14.3.2.1d).\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.6.1i","Requirement","ECSS-E-ST-70-41_1331280",1,"Created","For each valid instruction to add a structure identifier to the diagnostic parameter report forward-control configuration, the real-time forwarding control subservice shall:\n1.\tadd, for the specified application process identifier, a diagnostic parameter report forward-control definition if not already existing;\n2.\tadd, to the related diagnostic parameter report forward-control definition, the specified diagnostic parameter report structure identifier, if not already existing;\n3.\tif subsampling is supported, set, to the related diagnostic parameter report forward-control definition and the specified diagnostic parameter report structure identifier, the specified subsampling rate. ","NOTE\tFor item 3, refer to requirement 6.14.3.2.1d.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.6.2h","Requirement","ECSS-E-ST-70-41_1331289",1,"Created","For each instruction to delete an application process from the diagnostic parameter report forward-control configuration that it rejects, the real-time forwarding control subservice shall generate the failed start of execution notification for that instruction. "]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.14.3.7.3c","Requirement","ECSS-E-ST-70-41_1331322",1,"Created","For each valid instruction to report the content of the event report blocking forward-control configuration, the real-time forwarding control subservice shall generate, for each existing event report blocking forward-control definition, a single event report blocking forward-control definition notification that includes:\n1.\tthe related application process identifier;\n2.\tfor each event definition identifier entry:\n(a)\tthe event definition identifier."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.3.2c","Requirement","ECSS-E-ST-70-41_1331347",1,"Created","Each instruction to enable the storage function of a packet store shall contain:\n1.\tthe packet store identifier of the packet store to enable for storage."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.4.1b","Requirement","ECSS-E-ST-70-41_1331362",1,"Created","For each packet store whose packet store open retrieval status is \"in-progress\", the storage and retrieval subservice shall:\n1.\tretrieve the stored packets chronologically according to their storage time tags starting from the open retrieval start time tag of that packet store;\n2.\troute these packets to the virtual channel associated with that packet store.","NOTE\tFor item 2, if the subservice supports prioritizing the packet retrievals from packet stores, the routing is done according to the retrieval policy, refer to requirements 6.15.3.1m and 6.15.3.1n.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.4.3g","Requirement","ECSS-E-ST-70-41_1331380",1,"Created","For each valid instruction to resume the open retrieval of a packet store, the storage and retrieval subservice shall:\n1.\tset the packet store open retrieval status of that packet store to \"in progress\";\n2.\tif that subservice supports prioritizing the packet retrievals from packet stores,  set the retrieval priority accordingly."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.7.1b","Requirement","ECSS-E-ST-70-41_1331413",1,"Created","Each request to delete the content of packet stores up to the specified time shall contain:\n1.\tthe storage time that is the limit of the deletion;\n2.\tone or more instructions to delete the content of a packet store up to the specified time, or\n3.\texactly one instruction to delete the content of all packet stores up to the specified time.","NOTE\tThe instructions to delete the content of all packet stores up to the specified time contain no argument.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.8.4f","Requirement","ECSS-E-ST-70-41_1331446",1,"Created","The set of packets identified by the \"select all packets stored after time tag\" filtering mechanism shall be all packets that are stored at and after that specified \"from time tag\"."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.9.4b","Requirement","ECSS-E-ST-70-41_1331471",1,"Created","Each request to change the virtual channel used by a packet store shall contain exactly one instruction to change the virtual channel used by a packet store."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.3.10.1e","Requirement","ECSS-E-ST-70-41_1331480",1,"Created","For each instruction to summary-report the content of a packet store that it rejects, the storage and retrieval subservice shall generate the failed start of execution notification for that instruction."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.2.4a","Requirement","ECSS-E-ST-70-41_1331500",1,"Created","For each packet store, the maximum number of diagnostic parameter report storage-control definitions that the packet selection subservice can contemporaneously control shall, at any time, correspond to the number of application processes that are controlled by that subservice and that provide the capability for generating diagnostic parameter reports.","NOTE 1\tFor the number of application processes, see requirement 6.15.4.1.1a.\nNOTE 1\tThe diagnostic parameter report storage configuration for a packet store contains the diagnostic parameter report storage definitions that the packet selection subservice maintains for that packet store.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.4.2h","Requirement","ECSS-E-ST-70-41_1331537",1,"Created","Each instruction to delete a service type from the application process storage-control configuration shall contain:\n1.\tif the packet selection subservice controls more than one application process, the application process identifier addressed by that instruction,\n2.\tthe service type identifier. "]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.4.2q","Requirement","ECSS-E-ST-70-41_1331546",1,"Created","For each valid instruction to delete an application process from the application process storage-control configuration, the packet selection subservice shall, for the related packet store:\n1.\tdelete the application process storage-control definition related to that specified application process identifier."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.5.2f","Requirement","ECSS-E-ST-70-41_1331571",1,"Created","Each instruction to delete an application process from the housekeeping parameter report storage-control configuration shall contain:\n1.\tthe application process identifier addressed by that instruction."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.6.2j","Requirement","ECSS-E-ST-70-41_1331604",1,"Created","For each valid instruction to delete a structure identifier from the diagnostic parameter report storage-control configuration , the packet selection subservice shall, for the related packet store:\n1.\tdelete the diagnostic parameter report structure identifier related to the specified application process identifier;\n2.\tif that diagnostic parameter report structure identifier deletion results in an emptied diagnostic parameter report storage-control definition, delete that diagnostic parameter report storage-control definition. ","NOTE\tDeleting a diagnostic parameter report structure identifier implies deleting the corresponding subsampling rate if any (see also requirement 6.15.4.2.1d).\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.15.4.7.3b","Requirement","ECSS-E-ST-70-41_1331637",1,"Created","Each request to report the content of the event report blocking storage-control configuration shall contain exactly one instruction to report the content of the event report blocking storage-control configuration."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.2.3a","Requirement","ECSS-E-ST-70-41_1331662",1,"Created","Each on-board control procedure service shall be associated to exactly one OBCP engine."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.4.2.1d","Requirement","ECSS-E-ST-70-41_1331673",1,"Created","If the at-step-level OBCP execution observability is selected, in addition to the \"at-procedure-level\" OBCP execution events, the OBCP management subservice shall raise an OBCP execution observability event:\n1.\tfor each step of the OBCP that has been reached.","NOTE\tRefer to clause 6.5.3 for additional requirements related to these events.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.4.4.4c","Requirement","ECSS-E-ST-70-41_1331695",1,"Created","Each instruction to unload an OBCP shall contain:\n1.\tthe identifier of the OBCP."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.4.4.9a","Requirement","ECSS-E-ST-70-41_1331728",1,"Created","The OBCP management subservice shall provide the capability to abort an OBCP.","NOTE\tThe corresponding requests are of message type \"TC[18,12] abort an OBCP\".\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.4.4.10d","Requirement","ECSS-E-ST-70-41_1331737",1,"Created","For each request to abort all OBCPs and report that is rejected, the OBCP management subservice shall generate a failed start of execution notification."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.4.6.3c","Requirement","ECSS-E-ST-70-41_1331762",1,"Created","Each instruction to activate and execute one OBCP step shall contain:\n1.\tthe identifier of the OBCP;\n2.\tif selecting the OBCP execution observability level is supported, the observability level to use during the execution of the OBCP;\n3.\tif the OBCP uses arguments, the argument values.","NOTE\tFor item 2, refer to requirement 6.18.4.2.1a.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.18.5.1.2b","Requirement","ECSS-E-ST-70-41_1331795",1,"Created","Each request to stop the OBCP engine shall contain exactly one instruction to stop an OBCP engine.","NOTE\tThe instructions to stop the OBCP engine contain no argument.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.19.6.1a","Requirement","ECSS-E-ST-70-41_1331811",1,"Created","The event-action subservice shall provide the capability to enable the event-action function.","NOTE 1\tThe corresponding requests are of message type \"TC[19,8] enable the event-action function\".\nNOTE 2\tFor the capability to disable the event-action function, refer to clause 6.19.6.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.19.8.5a","Requirement","ECSS-E-ST-70-41_1331852",1,"Created","The event-action subservice capability to report the status of each event-action definition shall be declared when specifying that subservice.","NOTE\tThe corresponding requests are of message type \"TC[19,6] report the status of each event-action definition\". The responses are data reports of message type \"TM[19,7] event-action status report\".\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.19.8.6f","Requirement","ECSS-E-ST-70-41_1331861",1,"Created","The event-action subservice shall process any valid instruction that is contained within a request to report event-action definitions regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.20.5.1b","Requirement","ECSS-E-ST-70-41_1331886",1,"Created","The list of memories that the parameter management subservice uses for managing parameter definitions shall be declared when specifying that subservice. ","NOTE\tThis allows restricting the memories on which new parameters can be mapped.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.21.5.1b","Requirement","ECSS-E-ST-70-41_1331919",1,"Created","If the capability to load a request sequence by reference is provided, whether the request sequencing subservice supports a loading policy shall be declared when specifying that subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.21.5.3c","Requirement","ECSS-E-ST-70-41_1331928",1,"Created","Each instruction to load a request sequence by reference shall contain:\n1.\tthe identifier of the request sequence;\n2.\tif the request sequence is not to be loaded according to the loading policy, the file path of the on-board file that contains the request sequence to load.","NOTE\tWhen the loading policy is used, the policy determines which on-board file contains the request sequence to load, refer to requirement 6.21.5.1b.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.21.5.7d","Requirement","ECSS-E-ST-70-41_1331953",1,"Created","The request sequencing subservice shall reject any request to abort a request sequence if any of the following conditions occurs:\n1.\tthat request contains an instruction with a request sequence identifier that refers to a request sequence that is not loaded;\n2.\tthat request contains an instruction that refers to a request sequence whose execution status is \"inactive\"."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.5a","Requirement","ECSS-E-ST-70-41_1331984",1,"Created","Whether the position-based scheduling subservice provides the capability for persistent scheduling shall be declared when specifying that subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.6.6k","Requirement","ECSS-E-ST-70-41_1332018",1,"Created","For each valid instruction to insert an activity into the position-based schedule, the position-based scheduling subservice shall:\n1.\tcreate a new scheduled activity in the schedule;\n2.\tplace the request specified in that instruction into the new scheduled activity;\n3.\tset the position tag of the new scheduled activity to the position tag specified in that instruction;\n4.\tif persistent scheduling is supported, set the activity persistency status of the new scheduled activity to \"persistent\" or \"non-persistent\" using the status specified in that instruction;\n5.\tif sub-schedules are supported, associate the new scheduled activity to the sub-schedule specified in the request to insert activities into the position-based schedule;\n6.\tif groups are supported, associate the new scheduled activity to the group specified in that instruction.\n7.\tif the activity is \"persistent\" and the release orbit position for that activity is earlier than the sum of the current position and the position-based schedule position margin, increment the orbit number of that activity by its persistent activity periodicity as many times as necessary for the release position-tag to be above that margin."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.8.1a","Requirement","ECSS-E-ST-70-41_1332043",1,"Created","The maximum number of groups that the position-based scheduling subservice can contemporaneously manage shall be declared when specifying that subservice."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.8.2.2a","Requirement","ECSS-E-ST-70-41_1332052",1,"Created","The position-based scheduling subservice shall provide the capability to delete position-based scheduling groups if the capability to create position-based scheduling groups is provided by that subservice.","NOTE 1\tThe corresponding requests are of message type \"TC[22,23] delete position-based scheduling groups\".\nNOTE 1\tFor the capability to create position-based scheduling groups, refer to clause 6.22.8.2.1.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.8.3.3b","Requirement","ECSS-E-ST-70-41_1332077",1,"Created","Each request to report the status of each position-based scheduling group shall contain exactly one instruction to report the status of each position-based scheduling group.","NOTE\tThe instructions to report the status of each position-based scheduling group contain no argument.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.11.3c","Requirement","ECSS-E-ST-70-41_1332110",1,"Created","Each instruction to position-shift a scheduled activity identified by request identifier shall contain:\n1.\tthe identifier of the scheduled activity to position-shift. ","NOTE\tSee requirement 6.22.6.2b.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.11.4f","Requirement","ECSS-E-ST-70-41_1332122",1,"Created","The position-based scheduling subservice shall process any valid instruction that is contained within a request to summary-report position-based scheduled activities identified by request identifier regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.22.12.3c","Requirement","ECSS-E-ST-70-41_1332143",1,"Created","Each instruction to delete the position-based scheduled activities identified by a filter shall contain:\n1.\ta position window, consisting of:\n(a)\tthe type of the position window that is one of \"select all\", \"from position tag\", \"to position tag\", \"from position tag to position tag\";\n(b)\tfor \"from position tag\" and \"from position tag to position tag\", the from position tag;\n(c)\tfor \"to position tag\" and \"from position tag to position tag\", the to position tag;\n2.\tif sub-schedules are supported, zero or more sub-schedules;\n3.\tif groups are supported, zero or more groups.","NOTE 1\tFor the filtering mechanism, including the interaction of the parts of the filter, refer to clause 6.22.12.2.\nNOTE 1\tFor sub-schedule support, refer to requirement 6.22.6.1a.\nNOTE 2\tFor group support, refer to requirement 6.22.6.1b.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.3.4.3a","Requirement","ECSS-E-ST-70-41_1332176",1,"Created","The file management service shall have access to the locking status of any file located in file systems that support locking.","NOTE\tRefer to requirement 5.4.5e.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.4.3.1f","Requirement","ECSS-E-ST-70-41_1332201",1,"Created","For each valid instruction to lock a file, the file handling subservice shall:\n1.\trequest the underlying file system to lock the file referred to by that instruction;\n2.\tif the underlying file system reports an error in locking the file, generate a failed \"completion of execution\" notification."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.4.5.3d","Requirement","ECSS-E-ST-70-41_1332234",1,"Created","Each instruction to rename a directory shall contain:\n1.\tthe repository path and current directory name of the directory;\n2.\tthe new directory name of the directory."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.4.6f","Requirement","ECSS-E-ST-70-41_1332243",1,"Created","For each request to summary-report the content of a repository that is rejected, the file handling subservice shall generate a failed start of execution notification."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.5.3.1a","Requirement","ECSS-E-ST-70-41_1332268",1,"Created","The file copy subservice capability to suspend file copy operations shall be declared when specifying that subservice.","NOTE 1\tThe corresponding requests are of message type \"TC[23,16] suspend file copy operations\".\nNOTE 2\tThis capability applies both to the file copy operations that have been initiated using a request to copy a file or to move a file.\nNOTE 3\tFor the capability to resume file copy operations, refer to clause 6.23.5.3.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.5.4.1f","Requirement","ECSS-E-ST-70-41_1332295",1,"Created","The file copy subservice shall process any valid instruction that is contained within a request to abort file copy operations regardless of the presence of faulty instructions."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","6.23.5.5.2f","Requirement","ECSS-E-ST-70-41_1332309",1,"Created","For each valid instruction to enable the periodic reporting of the file copy status, the file copy subservice shall:\n1.\tset the file copy status periodic reporting status to \"enabled\";\n2.\tset the file copy status periodic reporting interval to the specified interval."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","7.3.6b","Requirement","ECSS-E-ST-70-41_1332340",1,"Created","The PFCs specified in Table 7-6 shall be used for packet fields carrying real values."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","7.3.13b","Requirement","ECSS-E-ST-70-41_1332382",1,"Created","The PFCs specified in Table 7-12 shall be used for packet fields carrying packets."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","7.4.4.1f","Requirement","ECSS-E-ST-70-41_1332411",1,"Created","For each request that it issues, each application process shall set the source ID field to its source identifier.","NOTE\tFor the source identifier, see requirement 5.4.11.2.1c.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.2.2.4a","Requirement","ECSS-E-ST-70-41_1332457",1,"Created","Each telecommand packet transporting a request to distribute register dump commands shall be of message subtype 5. ","NOTE\tFor the corresponding system requirements, refer to clause 6.2.5.3.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.2.2.8b","Requirement","ECSS-E-ST-70-41_1332470",1,"Created","For each telemetry packet transporting a physical device data report, the source data field shall have the structure specified in Figure 8-17."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.3.2.14a","Requirement","ECSS-E-ST-70-41_1332521",1,"Created","Each telemetry packet transporting a diagnostic parameter report shall be of message subtype 26. ","NOTE\tFor the corresponding system requirements, refer to clause 6.3.4.3.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.3.2.25b","Requirement","ECSS-E-ST-70-41_1332555",1,"Created","For each telecommand packet transporting a request to apply parameter functional reporting configurations, the application data field shall have the structure specified in Figure 8-45."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.4.2.4b","Requirement","ECSS-E-ST-70-41_1332592",1,"Created","For each telecommand packet transporting a request to enable the periodic parameter statistics reporting, the application data field shall have the structure specified in Figure 8-55."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.4.2.8b","Requirement","ECSS-E-ST-70-41_1332604",1,"Created","For each telecommand packet transporting a request to report the parameter statistics definitions, the application data field shall be omitted."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.6.2.6a","Requirement","ECSS-E-ST-70-41_1332650",1,"Created","Each telemetry packet transporting a dumped raw memory data report shall be of message subtype 6. ","NOTE\tFor the corresponding system requirements, refer to clause 6.6.3.4.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.6.2.18b","Requirement","ECSS-E-ST-70-41_1332686",1,"Created","For each telemetry packet transporting a checked object memory object report, the source data field shall have the structure specified in Figure 8-82."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.11.2.1a","Requirement","ECSS-E-ST-70-41_1332718",1,"Created","Each telecommand packet transporting a request to enable the time-based schedule execution function shall be of message subtype 1. ","NOTE\tFor the corresponding system requirements, refer to clause 6.11.4.3.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.11.2.10a","Requirement","ECSS-E-ST-70-41_1332742",1,"Created","Each telemetry packet transporting a time-based schedule detail report shall be of message subtype 10. ","NOTE\tFor the corresponding system requirements, refer to clause 6.11.7.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.11.2.21c","Requirement","ECSS-E-ST-70-41_1332776",1,"Created","To disable all time-based sub-schedules, N shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.12.2.5f","Requirement","ECSS-E-ST-70-41_1332823",1,"Created","For delta-checking, the check type dependent criteria field of the add parameter monitoring definitions request shall have the structure specified in Figure 8-117."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.12.2.13a","Requirement","ECSS-E-ST-70-41_1332861",1,"Created","Each telecommand packet transporting a request to report the status of each parameter monitoring definition shall be of message subtype 13. ","NOTE\tFor the corresponding system requirements, refer to clause 6.12.3.11.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.12.2.17b","Requirement","ECSS-E-ST-70-41_1332871",1,"Created","For each telecommand packet transporting a request to enable the functional monitoring function, the application data field shall be omitted."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.13.2.2a","Requirement","ECSS-E-ST-70-41_1332920",1,"Created","Each telemetry packet transporting an intermediate downlink part report shall be of message subtype 2. ","NOTE\tFor the corresponding system requirements, refer to clause 6.13.3.3.1.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.14.2.5b","Requirement","ECSS-E-ST-70-41_1332955",1,"Created","For each telecommand packet transporting a request to add structure identifiers to the housekeeping parameter report forward-control configuration, the application data field shall have the structure specified in Figure 8-150."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.14.2.13c","Requirement","ECSS-E-ST-70-41_1332989",1,"Created","To delete an application process from the event report blocking forward-control configuration, N2 shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.14.2.16d","Requirement","ECSS-E-ST-70-41_1333000",1,"Created","To report that no event definition for the related application process is in the event report blocking forward-control configuration, N2 shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.15.2.8c","Requirement","ECSS-E-ST-70-41_1333033",1,"Created","To delete the content of all packet stores up to the specified time, N shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.15.2.22a","Requirement","ECSS-E-ST-70-41_1333077",1,"Created","Each telecommand packet transporting a request to resize packet stores shall be of message subtype 25. ","NOTE\tFor the corresponding system requirements, refer to clause 6.15.3.9.1.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.15.2.30d","Requirement","ECSS-E-ST-70-41_1333111",1,"Created","To delete an application process from the event report blocking storage-control configuration, N2 shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.17.1a","Requirement","ECSS-E-ST-70-41_1333140",1,"Created","Each packet transporting a test message shall be of service type 17."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.18.2.6a","Requirement","ECSS-E-ST-70-41_1333169",1,"Created","Each telecommand packet transporting a request to resume an OBCP shall be of message subtype 6. ","NOTE\tFor the corresponding system requirements, refer to clause 6.18.4.6.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.18.2.18b","Requirement","ECSS-E-ST-70-41_1333204",1,"Created","For each telecommand packet transporting a request to stop and unload an OBCP, the application data field shall have the structure specified in Figure 8-211."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.19.3b","Requirement","ECSS-E-ST-70-41_1333248",1,"Created","The values of the event-action status shall be as specified in Table 8-20."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.21.2.3b","Requirement","ECSS-E-ST-70-41_1333285",1,"Created","For each telecommand packet transporting a request to unload a request sequence, the application data field shall have the structure specified in Figure 8-230."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.21.2.8a","Requirement","ECSS-E-ST-70-41_1333298",1,"Created","Each telecommand packet transporting a request to load by reference and activate a request sequence shall be of message subtype 8. ","NOTE\tFor the corresponding system requirements, refer to clause 6.21.5.6.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.22.2.8b","Requirement","ECSS-E-ST-70-41_1333342",1,"Created","For each telecommand packet transporting a request to position-shift the scheduled activities identified by a filter, the application data field shall have the structure specified in Figure 8-244."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.22.2.21a","Requirement","ECSS-E-ST-70-41_1333378",1,"Created","Each telecommand packet transporting a request to disable position-based sub-schedules shall be of message subtype 21. ","NOTE\tFor the corresponding system requirements, refer to clause 6.22.7.2.2.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.22.2.23c","Requirement","ECSS-E-ST-70-41_1333388",1,"Created","To delete all position-based scheduling groups, N shall be set to 0."]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.23.2.8a","Requirement","ECSS-E-ST-70-41_1333436",1,"Created","Each telemetry packet transporting a found files report shall be of message subtype 8. ","NOTE\tFor the corresponding system requirements, refer to clause 6.23.4.4.\n"]
["ECSS-E-ST-70-41C","ECSS - Current v1.0","8.23.2.20b","Requirement","ECSS-E-ST-70-41_1333473",1,"Created","For each telecommand packet transporting a request to resume all file copy operations involving a repository path, the application data field shall have the structure specified in Figure 8-280."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","4.2.1e","Requirement","ECSS-E-ST-60-21_1350005",1,"Created","The gyro shall be capable to autonomously enter the measurement mode after power on."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","4.6.1c","Requirement","ECSS-E-ST-60-21_1350030",1,"Created","Scale factor of the gyro channels shall be positive when a positive rotation is applied around the sensing axis.","NOTE\t1\tPositive scale factor means that angular increment is positive or cumulated angular increments output increases.\nNOTE\t2\tThe positive rotation is intended in a trigonometric sense.\n"]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","4.9.1d","Requirement","ECSS-E-ST-60-21_1350045",1,"Created","The measurement bandwidth shall be specified for each of the following outputs:\n1.\tangular rate, unfiltered or filtered, or\n2.\tan angular increment, unfiltered or filtered, or\n3.\ta cumulated angular increment, unfiltered.","NOTE\tFor further details, see clause 5.4.9.\n"]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.2a","Requirement","ECSS-E-ST-60-21_1350071",1,"Created","The test method to verify performance specification shall be justified by the supplier."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.4.2.2.3d","Requirement","ECSS-E-ST-60-21_1350096",1,"Created","The bias repeatability between before and after irradiation shall be specified by the customer denoting the performance type in terms of maximum, 1 sigma, 68% confidence level or peak to peak.","NOTE\tDepending of the gyro use, the repeatability requirements can be combined into a single specification.\n"]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.4.2.3.2a","Requirement","ECSS-E-ST-60-21_1350105",1,"Created","The duration of the test shall be long enough to obtain the required confidence level in the bias estimate."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.4.4.2.2c","Requirement","ECSS-E-ST-60-21_1350130",1,"Created","In the range of low angular rate outside of the deadband range, the scale factor non-linearity error shall be specified by the customer denoting the performance type in terms of maximum, 1 sigma, 68% confidence level or peak to peak.","NOTE\tThe customer can define an input range smaller than the deadband range.\n"]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.4.5.2.3b","Requirement","ECSS-E-ST-60-21_1350163",1,"Created","The repeatability between before and after, or after versus before, thermal vacuum cycling of the absolute gyro axes alignment w.r.t. mechanical reference frame shall be specified by the customer, irrespective of the off time duration."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.4.8.2a","Requirement","ECSS-E-ST-60-21_1350194",1,"Created","The maximum integrated gyro drift over the warm-up phase shall be specified by the customer."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","5.5e","Requirement","ECSS-E-ST-60-21_1350213",1,"Created","The functional mathematical model shall model all the performance errors defined in the performance requirements."]
["ECSS-E-ST-60-21C","ECSS - Current v1.0","A.2.1<4>b","Requirement","ECSS-E-ST-60-21_1350223",1,"Created","The outputs of the FMM shall include as a minimum:\n1.\tthe measured angular rate and time delivered by the gyro;\n2.\tthe gyro health status."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.3.1a","Requirement","ECSS-E-ST-31-02_1190027",1,"Unchanged","The qualification stage shall be completed before launch."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.5.3.3.1d","Requirement","ECSS-E-ST-31-02_1190054",1,"Unchanged","Discrepancies between analytical prediction and test results shall be analysed in order to demonstrate that the objective of the qualification is not compromised."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.5.4.1a","Requirement","ECSS-E-ST-31-02_1190062",1,"Unchanged","Equipment for which a full qualification programme is required as per Table 5-1 shall be qualified by test according to clause 5.5.3.2 and 5.6 and by analysis according to clause 5.5.3.3."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.6.5a","Requirement","ECSS-E-ST-31-02_1190090",1,"Unchanged","Proof pressure test shall be performed applying 1,5 times MDP as specified in ECSS-E-ST-32-02 for duration of 15 minutes.","NOTE\tDuring manufacturing processes (e.g. curing of panels with embedded heat pipes) the pressure can be higher than MDP, as long as the unit material stays in the elastic domain.\n"]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.6.9.4a","Requirement","ECSS-E-ST-31-02_1190125",2,"Normative Change","For HP Diode, the following tests shall be performed:\n1.\tThe tests specified in clause 5.6.9.2.1 to 5.6.9.2.4.\n2.\tA test to determine the time-to-shutdown of the HP Diode, according to the following sequence:\n(a)\tapply pre-defined heat loads to the nominal condenser;\n(b)\tvary the vapour temperature in suitable increments within the specified operational temperature range in order to generate a smooth performance over temperature curve;\n(c)\tensure that the pre-defined heat loads are 10 %, 30 %, 50 % and 80 % of the derived Qmax in nominal mode for the specific heat pipe profile;\n(d)\tderive the energy needed for shutdown for each of the above tests.\n3.\tA test to determine the time to start-up the heat pipe diode, according to the following sequence:\n(a)\tapply pre-defined heat loads to the nominal evaporator;\n(b)\tensure that the pre-defined heat loads are 10 %, 30 %, 50 % and 80 % of the derived Qmax in nominal mode for the specific heat pipe profile."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","5.7b","Requirement","ECSS-E-ST-31-02_1190157",1,"Unchanged","The procedures specified in 5.7a shall be compatible with the safety requirements and personnel control requirements at the facility where the operations are conducted."]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","6.2.7b","Requirement","ECSS-E-ST-31-02_1190287",1,"Created","The confirmation can be performed during the similarity analysis of clause 4.5 and 6.1.Test procedures in conformance with ECSS-E-ST-10-03 Annex C shall be established for each test performed.","NOTE\tSeveral test procedures can be grouped in one document.\n"]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","A.2.1<4>a","Requirement","ECSS-E-ST-31-02_1190172",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","D.2.1<5>a","Requirement","ECSS-E-ST-31-02_1190205",2,"Deleted","<<deleted>> "]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","F.2.1<8>a","Requirement","ECSS-E-ST-31-02_1190230",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-31-02C Rev.1","ECSS - Current v1.0","F.2.1<14>c","Requirement","ECSS-E-ST-31-02_1190239",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.2.5.1a","Requirement","ECSS-E-ST-33-11_0280022",2,"Normative Change","The explosive subsystem shall sustain, before, during and after firing: \n1.\tthe internal loads due to operation and \n2.\tthe external loads defined by the end-user. ","NOTE\tThese loads represent the sum of preload, static, dynamic, thermal and any other load seen in service.\n"]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.3b","Requirement","ECSS-E-ST-33-11_0280037",1,"Informative Change","The environmental conditions, life cycle and the functions being activated shall be specified.","NOTE\tE.g. ground storage, transport, launcher ignition, staging and safety functions, spacecraft separation, motor ignition, solar array, antenna, boom or cover release, propulsion subsystem branch opening or closing, de-orbiting.\n"]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.5.2.4c","Requirement","ECSS-E-ST-33-11_0280070",1,"Unchanged","The arm function shall be used to control only one explosive function."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.8.1.4a","Requirement","ECSS-E-ST-33-11_0280095",2,"Normative Change","For launch segment, it shall be ensured that components intended for different applications cannot be confused."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.8.2.1e","Requirement","ECSS-E-ST-33-11_0280103",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.8.2.8f","Requirement","ECSS-E-ST-33-11_0280417",1,"Created","For launchers only, provision shall be made to isolate power lines and return lines of the explosive subsystem from electrical ground."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.9e","Requirement","ECSS-E-ST-33-11_0280158",2,"Normative Change","Age-sensitive materials shall only be used where degradation causes no loss of explosive subsystem performance beyond limits agreed with the end-user."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.10.3b","Requirement","ECSS-E-ST-33-11_0280178",1,"Unchanged","Isolators shall provide 20 dB attenuation at the specified electromagnetic frequencies."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.10.6c","Requirement","ECSS-E-ST-33-11_0280190",1,"Unchanged","The power provided at the power distribution points shall be such that the requirements of 4.8.2.6 allowing for losses are met."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.10.11.6c","Requirement","ECSS-E-ST-33-11_0280224",1,"Unchanged","Visibility of the status indicators when installed on the spacecraft or launcher shall be ensured."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.11.3.1b","Requirement","ECSS-E-ST-33-11_0280255",1,"Unchanged","The interface shall allow for sealing."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.11.10b","Requirement","ECSS-E-ST-33-11_0280278",2,"Normative Change","Under the conditions in column E of Table 4-16, the properties in column A, expressed in the units specified in column B, shall be between the values in column C (maximum) and column D (minimum)."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.12.2e","Requirement","ECSS-E-ST-33-11_0280291",1,"Unchanged","Under the conditions in column E of Table 4-18, the properties in column A, expressed in the units specified in column B, shall be between the values in column C (maximum) and column D (minimum)."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.14.3.2a","Requirement","ECSS-E-ST-33-11_0280329",2,"Normative Change","Test procedure (TPRO) shall be  in conformance with the DRD in Annex C of ECSS-E-ST-10-03."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.14.4.3a","Requirement","ECSS-E-ST-33-11_0280348",1,"Unchanged","Lot acceptance tests shall be performed."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.15.2f","Requirement","ECSS-E-ST-33-11_0280357",1,"Unchanged","Identification label shall be marked before delivery in a permanent way on each deliverable."]
["ECSS-E-ST-33-11C Rev.1","ECSS - Current v1.0","4.16.2a","Requirement","ECSS-E-ST-33-11_0280380",1,"Unchanged","Only planned and approved activities which follow approved procedures shall be undertaken."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.2.1a","Requirement","ECSS-E-ST-50-11_1410001",1,"Created","The SpaceFibre protocol stack shall have a Network layer, Data Link layer, Multi-Lane layer, Lane layer, Physical layer and Management Information Base.","NOTE\t1\tThe SpaceFibre protocol stack is illustrated in Figure 5-1 for a single lane and in Figure 5-2 for a multi-lane link. The service interfaces for each layer of the SpaceFibre protocol stack are specified in clause 6.\nNOTE\t2\tFrom the perspective of the layers of the OSI Model, the Lane layer and the Multi-Lane layer are sublayers of the Data Link layer. The Data Link, Multi-Lane and Lane layers form one layer from the implementation perspective. The separation into layers has been done to group related functionalities together for ease of understanding.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.3.2a","Requirement","ECSS-E-ST-50-11_1410037",1,"Created","The SKIP control word shall begin with a comma, K28.7, which is in the least significant symbol position of the control word and is sent first."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.3.7e","Requirement","ECSS-E-ST-50-11_1410062",1,"Created","The Inverse INIT2 control word shall not be generated by the SpaceFibre port.","NOTE\tThe Inverse INIT2 is formed when the PCB layout in a SpaceFibre transmitter or receiver crosses over the two signals, CML+ and CML-, making up the differential signal.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.3.10a","Requirement","ECSS-E-ST-50-11_1410079",1,"Created","The LOST_SIGNAL control word shall begin with a comma, K28.7, which is in the least significant symbol position of the control word and is sent first."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.4.3e","Requirement","ECSS-E-ST-50-11_1410095",1,"Created","The 4-bit Lane Number field of the ALIGN control word shall contain the lane number of the lane used to send the ALIGN control word."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.5.1.7a","Requirement","ECSS-E-ST-50-11_1410128",1,"Created","The SIF control word shall be used to indicate the start of an idle frame."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.5.2e","Requirement","ECSS-E-ST-50-11_1410137",1,"Created","The Multiplier field shall indicate the value of the FCT, the FCT being exchanged for M×64 data words, where M is the value of the FCT Multiplier field plus 1, so that M=1 to 8 corresponds to field values of 0 to 7 respectively."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.6b","Requirement","ECSS-E-ST-50-11_1410162",1,"Created","The RXERR control word, shall be used to indicate that the received data or control word contained an error or is likely to have contained an error."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.8.3f","Requirement","ECSS-E-ST-50-11_1410195",1,"Created","The PRBS shall be generated using the algorithm specified in clause 5.7.6.2.3."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.3.8.4e","Requirement","ECSS-E-ST-50-11_1410206",1,"Created","The B_TYPE field shall identify the type of broadcast message."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.2.1b","Requirement","ECSS-E-ST-50-11_1410254",1,"Created","A serialiser shall be used to convert each parallel 10-bit symbol for transmission into a serial bit stream with each bit of the symbol being sent one after the other.","NOTE\tOne, two or four symbols are provided to the serialiser in parallel.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.2.2c","Requirement","ECSS-E-ST-50-11_1410263",1,"Created","The far-end serial loopback shall connect the digital signal from the output of the line receiver directly to the input of the line driver."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.3.3c","Requirement","ECSS-E-ST-50-11_1410295",1,"Created","The serial input shall be AC coupled using 100 nF to 200 nF series capacitors on both the receive signals, RXp and RXn.","NOTE\tAC coupling protects the driver and receiver in the event of a failure that results in a high DC voltage on the signal lines. It helps to prevent fault propagation. It also prevents DC ground loops. The serial output is also AC coupled on the output side, see clause 5.4.3.2.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.4.4.1a","Requirement","ECSS-E-ST-50-11_1410330",1,"Created","Type-B flight electrical medium from and including the Type-B connector at one end of a lane to and including the Type-B connector at the other end of that lane, shall:\n1.\tMaintain a signal path of 50 ohm ±5 ohm single-ended impedance or 100 ohm ±10 ohm differential impedance.\n2.\tHave an insertion loss of less than 2,2 dB/m plus 2 dB per connector pair at a maximum operating bit rate specified for the SpaceFibre electrical medium.\n3.\tHave a return loss of more than 10 dB.\n4.\tHave a near-end crosstalk isolation of better than 35 dB.\n5.\tHave a far-end crosstalk isolation of better than 35 dB.\n6.\tHave a signal skew between TXp and TXn, measured at the receiving end of a lane, of less than the larger of:\n(a)\t±20 ps.\n(b)\t±10 % of the shortest bit interval that the medium is used for.","NOTE\t±20 ps corresponds to a difference in path length of around ±2 mm. 10 Gbit/s = 100 ps bit time, which is around 15 mm signal length. 10 % of this length is 1,5 mm which is difficult to manufacture.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.4.4.4b","Requirement","ECSS-E-ST-50-11_1410339",1,"Created","Type-B flight cable assemblies shall carry one or more lanes."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.4.6.3a","Requirement","ECSS-E-ST-50-11_1410368",1,"Created","Type-D EGSE cable shall be either:\n1.\t50 ohm ±5 ohm single-ended impedance.\n2.\t100 ohm ±10 ohm differential impedance.","NOTE\tCable with single-ended impedance is cable with a single signal conductor and shield, such as coaxial cable. Two of these cables make a differential pair. Cable with differential impedance is cable with signal arranged in pairs, such as twisted pair or twin-axial cable.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.6.1.2b","Requirement","ECSS-E-ST-50-11_1410410",1,"Created","The minimum quality level shall be IEC 60793-2-10 A1a.2:2015.","NOTE\tThese correspond to OM3 respectively. This is needed to achieve 10 Gbit/s over a link length of 300 meters (IEEE802.3:2012 Clause 52.5). Optical Multi-mode (OM) describes the modal bandwidth of the fibre by quantifying the modal dispersion characteristics of the optical fibre.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.4.6.2.4c","Requirement","ECSS-E-ST-50-11_1410431",1,"Created","The Type-B fibre optic cable assembly shall contain one or more pairs of fibre with each pair connected as specified in Table 5-31.","NOTE\tA Type-B fibre optic cable assembly containing two fibres is illustrated in Figure 5-23.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.5.1p","Requirement","ECSS-E-ST-50-11_1410467",1,"Created","The Lane layer shall provide the following status information to the Management Information Base:\n1.\tLane State(i).\n2.\tError Information(i).\n3.\tLoss of Signal Information(i).\n4.\tFar End Capabilities (i).\n5.\tReceive Polarity(i).","NOTE\tThe interfaces to and from the Lane layer are illustrated in Figure 5-27 for a single lane link and in Figure 5-28 for a multi-lane link.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.5.2.4c","Recommendation","ECSS-E-ST-50-11_1410476",1,"Created","When in the ClearLine state the Lane Initialisation state machine should disable the receiver and receive clock-data recovery circuitry.","NOTE\tThis is to save power and also resets the clock recovery logic in case there has been a problem causing the SerDes to fail and the lane to disconnect in consequence.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.5.2.9c","Recommendation","ECSS-E-ST-50-11_1410501",1,"Created","When in the Connecting state and RxOnly is asserted the Lane Initialisation state machine should disable the transmitter driver. "]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.5.5c","Requirement","ECSS-E-ST-50-11_1410534",1,"Created","When enabled, the near-end parallel loopback shall replace the words in the receive stream, after data rate adjustment, with the words from the transmit stream."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.5.6f","Requirement","ECSS-E-ST-50-11_1410541",1,"Created","The 10-bit wide input stream shall be aligned or realigned to form a stream of correctly aligned symbols so that each 10-bit group contains one complete symbol."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.6.1c","Requirement","ECSS-E-ST-50-11_1410567",1,"Created","The Multi-Lane layer shall receive data words and Data Link layer control words from the Data Link layer."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.6.4.2g","Requirement","ECSS-E-ST-50-11_1410600",1,"Created","At the end of a data frame, when the EDF control word is placed in each Active lane, the 16-bit CRC computed independently for each data-sending lane shall be placed in the CRC_LS and CRC_MS fields of the EDF control words."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.6.6.3g","Requirement","ECSS-E-ST-50-11_1410625",1,"Created","A correctly received ALIGN control word shall be valid when all of the following conditions are fulfilled:\n1.\tThe #Lanes field of the ALIGN control word is equal to the number of active lanes with receive enable (RxEn asserted) at the end of the link receiving the ALIGN control word.\n2.\tThe lane number contained in the Lane Number field of the ALIGN control word is the same as the lane number of the lane in which the ALIGN control word is received."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.6.9.3a","Requirement","ECSS-E-ST-50-11_1410658",1,"Created","TxOnly for lane L, TxOnly(L), shall be asserted when either of the following conditions occur:\n1.\tLaneState(L) is not ClearLine AND TxEn(L) = 1 AND RxEn(L) = 0.\n2.\tLaneState(L) = Started AND FarEndActive(L)."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.6.10d","Requirement","ECSS-E-ST-50-11_1410667",1,"Created","If the number of active transmitting lanes is less than or equal to the value of the “maximum number of data-sending lanes” configuration parameter, all active transmitting lanes shall be data-sending lanes."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.2.1f","Requirement","ECSS-E-ST-50-11_1410692",1,"Created","A particular virtual channel shall be identified by its virtual channel number."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.4.1c","Requirement","ECSS-E-ST-50-11_1410725",1,"Created","Only virtual channels whose FCT credit counter indicates that its input virtual channel buffer at the far-end of the SpaceFibre link has room to accept the data words to be sent in the next data segment shall be permitted to compete for sending the next data segment."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.4.5e","Requirement","ECSS-E-ST-50-11_1410749",1,"Created","A virtual channel shall be allocated a portion of the Link Bandwidth that it expects to use, its Normalised Expected Bandwidth, which includes the overhead due to the use of frame delimiters and other control words.","NOTE\t1\tThis information is provided, using management parameters, for all virtual channels regardless of the quality of service they are providing.\nNOTE\t2\tThe Normalised Expected Bandwidth assigned to each virtual channel has to account for any protocol overhead. When data is being sent in one direction only, the transmit side sends SDF-DATA-EDF, the receive side sends FCT-ACK, the transmit side replies with an ACK to the receive side FCT. This means that the best-case protocol overhead for unidirectional transmission is: 2+1/64+2+1 ~ 4% or 64/64+2+1 ~ 96% of effective bandwidth. For a link with a data signalling rate of 2,5 Gbit/s this results in a maximum user data throughput of 1,91 Gbit/s. When data is being sent in both directions at the same time, the transmit side sends the following control words in addition to those sent over a unidirectional link: an ACK for the receive-side data frame and its corresponding FCT to allocate more data space. This means that the best-case protocol overhead for bidirectional transmission is: 2+1+2/64+2+1+2 ~ 7% or 64/64+2+1+2 ~ 93% of effective bandwidth. For a link with a data signalling rate of 2,5 Gbit/s this results in a maximum user data throughput of 1,86 Gbit/s. When sending small data frames or many broadcast messages, the overhead can be higher.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.4.5n","Requirement","ECSS-E-ST-50-11_1410758",1,"Created","The Minimum Bandwidth Credit Threshold shall be set at approximately 90 % of the value of the Negative Bandwidth Credit Limit."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.6.2.1f","Requirement","ECSS-E-ST-50-11_1410791",1,"Created","The least-significant bit of the least-significant character in each word shall be scrambled first."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.6.3.2d","Requirement","ECSS-E-ST-50-11_1410816",1,"Created","The Receive Polarity Flag shall be determined by the Receive Error state machine."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.6.6a","Requirement","ECSS-E-ST-50-11_1410849",1,"Created","Idle frames shall be generated when there are no data frames, FCTs, broadcast frames or FULLs to send."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.7.1a","Requirement","ECSS-E-ST-50-11_1410858",1,"Created","Data segments, FCTs and broadcast messages shall be temporarily placed in an error recovery buffer prior to passing them to the Multi-Lane or Lane layer for sending over the SpaceFibre link, so that they can be resent if an error occurs."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.7.1r","Requirement","ECSS-E-ST-50-11_1410875",1,"Created","When a total of 127 frames or FCTs are pending to be acknowledged FULL words shall be sent.","NOTE\t127 is the maximum number of frames or FCTs that can be outstanding due to the size of the Sequence Number.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.8.3a","Requirement","ECSS-E-ST-50-11_1410915",1,"Created","The RxDataFrame state shall be entered on one of the following conditions:\n1.\tFrom the RxNothing state, when an SDF is received.\n2.\tFrom the RxIdleFrame state, when an SDF is received.\n3.\tFrom the RxBroadcast&DataFrame state, when an EBF is received."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.7.9.5b","Requirement","ECSS-E-ST-50-11_1410940",1,"Created","When in the Link Initialised state, the Link Reset state machine shall initiate the following actions:\n1.\tPass near-end Lane Capability information to the Lane layer or Multi-Lane layer with the INIT3LinkResetFlag field set to 0."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.1f","Requirement","ECSS-E-ST-50-11_1410949",1,"Created","The Network layer shall pass Broadcast Messages for sending over the SpaceFibre network to the Data Link layer."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.3q","Requirement","ECSS-E-ST-50-11_1410982",1,"Created","A virtual network shall comprise one virtual channel on each of the links it uses in a SpaceFibre network.","NOTE\tThe virtual channels on the links used by the virtual network are each a part of the virtual network.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.6b","Requirement","ECSS-E-ST-50-11_1411007",1,"Created","If the end-point on the virtual network becomes temporarily unable to accept more N-Chars, the network layer shall wait until the end-point is able to accept more N-Chars."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.8.2f","Requirement","ECSS-E-ST-50-11_1411037",1,"Created","An invalid routing table entry shall be one that is undefined or not yet configured."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.8.3c","Requirement","ECSS-E-ST-50-11_1411041",1,"Created","If the virtual channel in the output port is not currently transmitting a packet, it shall be allocated to transmit the newly arrived packet.","NOTE\tAllocating the packet to the output port effectively connects the input virtual channel to the output virtual channel.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.9.4a","Requirement","ECSS-E-ST-50-11_1411074",1,"Created","If a port with a specific number does not exist in the routing switch, a packet arriving with a leading data character that references that non-existent port shall be discarded."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","5.8.13i","Permission","ECSS-E-ST-50-11_1411107",1,"Created","When logic resources are extremely limited, a SpaceFibre node may support only one virtual network.","NOTE\tA node with only one virtual network is not recommended, as many of the benefits of SpaceFibre are lost when only one virtual network is supported.\n"]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","6.2.2.2.3a","Requirement","ECSS-E-ST-50-11_1411134",1,"Created","When the user has a packet to send over the SpaceFibre network, it shall generate a SEND_PACKET.request primitive to request to send a SpaceFibre packet over the network using a specific virtual network."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","6.2.3.2.3a","Requirement","ECSS-E-ST-50-11_1411143",1,"Created","When the SpaceFibre user has a broadcast message to send it shall generate a BROADCAST_MESSAGE.request primitive to request a SpaceFibre node to send the broadcast message of a particular type over a specific broadcast channel."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","6.4.2.2.2a","Requirement","ECSS-E-ST-50-11_1411176",1,"Created","The TX_SYMBOL.request primitive shall provide the following parameters:\n1.\tTX_SYMBOL.request (Symbol)."]
["ECSS-E-ST-50-11C","ECSS - Current v1.0","6.4.3.3.2a","Requirement","ECSS-E-ST-50-11_1411189",1,"Created","The PHYSICAL_STATUS.indication primitive shall have the following parameters: \n1.\tPHYSICAL_STATUS.indication (LossOfSignal)."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.2.2b","Requirement","ECSS-E-ST-50-12_1420032",1,"Created","The SpaceWire cable shall comprise four screened twisted-pairs with an overall shield constructed according to ESCC 3902/003 or ESCC 3902/004.","NOTE\tESCC 3902/003 describes variants of the SpaceWire cable to suit a range of spacecraft on-board applications. ESCC 3902/004 describes a low-mass variant of the SpaceWire cable.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.2.2c","Permission","ECSS-E-ST-50-12_1420033",1,"Created","For Type B cable assemblies, specified in clause 5.3.4.4, alternative forms of cable construction may be used provided that the cable characteristics fulfil the requirements in clauses 5.3.2.3 to 5.3.2.6.","NOTE\tThis is to permit special forms of cable construction for specific applications.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.3.5a","Recommendation","ECSS-E-ST-50-12_1420074",1,"Created","Flying lead connectors should be used for connection to a PCB."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.5.1a","Requirement","ECSS-E-ST-50-12_1420111",1,"Created","When using LVDS signals, the PCB tracks shall be differential tracks with a differential impedance of 100 Ohm ± 10 Ohm."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.6.2.3a","Requirement","ECSS-E-ST-50-12_1420139",1,"Created","The receive signals shall be terminated by a 100 Ohm ± 10 Ohm termination resistor."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.3.7.2d","Requirement","ECSS-E-ST-50-12_1420164",1,"Created","The system architect shall specify nominal and worst-case contributions of skew and jitter of Data and Strobe at component level: units and cable assembly.","NOTE\tThe worst-case values include allowance for radiation and ageing effect\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.4.2f","Requirement","ECSS-E-ST-50-12_1420180",1,"Created","The encoding layer shall inform the data link layer of changes in the encoding layer indicated by the following status flags:\n1.\tDisconnect, which indicates that the link has been disconnected.\n2.\tReceive error, which indicates that an error has been detected in a received symbol.\n3.\tgotNull, which indicates that the first Null control code has been received without any parity errors.","NOTE\tA parity error is an example of a receive error.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.4.6b","Requirement","ECSS-E-ST-50-12_1420210",1,"Created","The gotNull condition shall only be cleared when the RX Enable flag is de-asserted"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.5.4b","Requirement","ECSS-E-ST-50-12_1420243",1,"Created","Each flow control token shall be exchanged for eight N-Chars."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.5.4c","Requirement","ECSS-E-ST-50-12_1420244",1,"Created","An FCT shall be sent from the data link layer to the encoding layer when the data link layer is ready to receive a further eight N-Chars. "]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.5.7.5b","Requirement","ECSS-E-ST-50-12_1420277",1,"Created","The Link state machine shall leave the Started state on one of the following conditions:\n1.\tWhen LinkDisabled is asserted, move to the ErrorReset state.\n2.\tWhen a disconnect occurs, move to the ErrorReset state.\n3.\tWhen a parity error occurs, move to the ErrorReset state.\n4.\tWhen an ESC error, move to the ErrorReset state.\n5.\tWhen an FCT, N-Char or broadcast code is received from the Encoding Layer, move to the ErrorReset state.\n6.\tWhen enable is asserted, at least one Null has been sent and gotNull is asserted, move to the Connecting state.\n7.\t12,8 µs after entering the Started state, move to the ErrorReset state.","NOTE\tThe Null that is received causing the gotNull condition to be asserted, can occur in the ErrorWait, Ready or Started state.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.4.4a","Requirement","ECSS-E-ST-50-12_1420310",1,"Created","A network supporting time-code broadcast shall have a single time-code master application on a single node which is responsible for sending time-codes over the network."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.4.9a","Requirement","ECSS-E-ST-50-12_1420319",1,"Created","When an invalid time-code is received by an end-point with a time-code register, it shall update the time-code register associated with the end-point to the value of the received time-code.","NOTE\tThis is so that when a time-code is lost for any reason the time-code broadcast mechanism can recover and continue to broadcast time-codes across the network after a few more time-codes have been sent. The number of time-codes that are sent following a missing time-code to recover time-code distribution depends on the size of the network. If there is active redundancy in the network the missing time-code is likely to be recovered by that same time-code being received via another path through the network.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.5.5f","Requirement","ECSS-E-ST-50-12_1420343",1,"Created","On reset the interrupt relay register shall be cleared to zero."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.6b","Requirement","ECSS-E-ST-50-12_1420368",1,"Created","A SpaceWire node shall comprise:\n1.\tOne or more end-points each of which provides an interface between one port and the host system, and\n2.\tZero or more time-code registers.","NOTE\tThe UML diagram in Figure 5-26 illustrates the components and specialisations of a SpaceWire node.\n"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.8.5c","Requirement","ECSS-E-ST-50-12_1420401",1,"Created","If the entry in the routing table referenced by the leading data character of a packet has not been configured to contain a valid port number, the packet shall be discarded."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.9c","Requirement","ECSS-E-ST-50-12_1420434",1,"Created","The routing table in a routing switch shall be configurable via the routing switch configuration port."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","5.6.9d","Requirement","ECSS-E-ST-50-12_1420435",1,"Created","The port time-out timer for each port shall be configurable via the routing switch configuration port."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","6.1.3.4.2a","Requirement","ECSS-E-ST-50-12_1420480",1,"Created","The DISTRIBUTED_INTERRUPT_ACK.request primitive shall have the following parameters: \n1.\tDISTRIBUTED_INTERRUPT_ACK.request (End-point, Interrupt Identifier)"]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","6.2.2.2.4a","Requirement","ECSS-E-ST-50-12_1420500",1,"Created","On receipt of the BROADCAST_CODE.request primitive the port shall send the broadcast code immediately after the character current has finished being sent."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","6.3.2.4.3a","Requirement","ECSS-E-ST-50-12_1420525",1,"Created","The DISCONNECT.indication primitive shall be passed to the data link layer, when the SpaceWire link becomes disconnected."]
["ECSS-E-ST-50-12C Rev.1","ECSS - Current v1.0","6.3.2.6.4a","Requirement","ECSS-E-ST-50-12_1420534",1,"Created","The effect on receipt of the gotNull.indication primitive by the data link layer shall be according to the state machine of clause 5.5.6."]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","6.2.1c","Permission","ECSS-E-ST-20-06_0070179",1,"Created","The test specified in requirement 6.2.1b may be replaced by an ESD analysis under the condition that the ESD responsible agrees that the result of this analysis demonstrate that the effect of such a worst-case ESD is acceptable."]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","6.6.1b","Requirement","ECSS-E-ST-20-06_0070035",1,"Unchanged","The rationale behind the test, the details of the procedure and the test results shall be submitted to the customer for approval."]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","6.8.3a","Requirement","ECSS-E-ST-20-06_0070065",1,"Unchanged","It shall be demonstrated that the continuity of current paths is not compromized by environmental effects, including \n1.\tmechanical effects (vibration, shocks and depressurization),\n2.\tthermal changes, and \n3.\tsurface erosion."]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","6.8.4e","Requirement","ECSS-E-ST-20-06_0070070",1,"Unchanged","If assessment of the electric fields and space charge density in a large volume is performed, the 3-D spacecraft charging codes to be used shall be defined.","NOTE \tThese 3-D spacecraft charging codes can consider the detailed geometry of the spacecraft. Various charging codes with different complexity are available for performing the assessment (see Annex C).\n"]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","7.3b","Requirement","ECSS-E-ST-20-06_0070096",2,"Normative Change","Testing requirements for solar arrays in 7.2.3 shall apply to all exposed parts of a power system with a test set-up including representative inductance and capacitance and taking into account dielectric aging due to dose.","NOTE \tThe objective is to demonstrate that secondary arcing due to any kind of primary phenomenon cannot lead to damage.\n"]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","9.3h","Requirement","ECSS-E-ST-20-06_0070120",1,"Unchanged","For materials other than those covered by 9.3e and 9.3f, a validation process shall be carried out to establish that the maximum electric field and internal absolute surface voltage remain below Emax (107V/m) and Vmax respectively, when irradiated with the worst-case environment, in the orbit and position on the spacecraft and at the lowest temperature, in which it is intended to be used. ","NOTE \t1\tThis involves either\n·\texperimental validation using a worst-case spectrum in a laboratory chamber, or \n·\tcomputer simulation.\nNOTE \t2\tFor simple structures a 1-d analytical charge deposition and conductivity code such as given in annex D.2 can be suitable. This calculation uses information on the environment and the density of the shield and dielectric and its electrical properties. For complicated structures, 3-d Monte Carlo simulations can be used to calculate current deposition. However, after this the field is calculated using the electrical properties of the structure. \n"]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","11.2.5a","Requirement","ECSS-E-ST-20-06_0070153",1,"Unchanged","It shall be verified that the level of plasma density is not high enough to produce discharges through the gas.","NOTE \tEP systems can emit substantial quantities of neutral gas. Examples are gas emitted by electro-thermal thrusters and gas emitted by gridded ion engines and electrodynamic thrusters at start-up before the internal discharges are initiated. These neutral gas emissions, after photo-ionization, can dramatically increase the plasma density around the spacecraft. This can result in the triggering of discharges on charged surfaces or between surfaces actively kept at different potentials.\n"]
["ECSS-E-ST-20-06C Rev.1","ECSS - Current v1.0","11.3.5b","Requirement","ECSS-E-ST-20-06_0070178",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-32-10C Rev.2 Corr.1","ECSS - Current v1.0","4.3.2.1e","Requirement","ECSS-E-ST-32-10_0110034",1,"Created","For glass and ceramic structural parts the value for the FOSU verification by analysis only shall be agreed between the customer and the developer for each specific application.","NOTE \tNASA SSP 52005 specifies a figure of 5,0 for unpressurized glass and ceramics parts (analysis only).\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.5.2.4a","Requirement","ECSS-E-ST-33-01_0820037",1,"Unchanged","Materials shall be selected as specified in ECSS-Q-ST-70-36."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.3.1d","Requirement","ECSS-E-ST-33-01_0820061",1,"Unchanged","The use of sliding surfaces shall be avoided. "]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.3.1e","Requirement","ECSS-E-ST-33-01_0820062",2,"Normative Change","If requirement 4.7.3.1d cannot be met, sliding surfaces are used one of the surfaces shall be hard and the other be lubricated or be composed of a self-lubricating material.","NOTE \tExample of self-lubricating material: polyimide resins.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.4.2e","Requirement","ECSS-E-ST-33-01_0820095",1,"Unchanged","The mechanism design shall take into account the worst-case combinations (including uncertainties) of:\n1.\textremes of operational and survival steady­state, \n2.\ttransient temperatures, \n3.\tmechanism heat dissipation, and\n4.\tthe temperature gradients across the mechanism.","NOTE \tFailure to consider the effects of differential expansion can lead to a catastrophic failure.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.5.2.6g","Requirement","ECSS-E-ST-33-01_0820399",1,"Unchanged","In case the verification of fatigue by test is needed, the factor 4 shall apply to the quantity of fatigue cycle on the mechanism part that is susceptible to fatigue.","NOTE \t1\tMechanism parts are considered susceptible to fatigue if it cannot be demonstrated infinite life by analysis.\nNOTE \t2\tNo fatigue test is needed if the analysis demonstrate the factor minimum of 8.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.5.4.3g","Requirement","ECSS-E-ST-33-01_0820143",1,"Unchanged","Latches shall be resettable for ground testing."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.5.4.4g","Requirement","ECSS-E-ST-33-01_0820152",1,"Unchanged","Electrical deployment indicators shall not be used as mechanical end stops.","NOTE \tExample of electrical deployment indicators are micro-switches.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.5.4.11a","Requirement","ECSS-E-ST-33-01_0820173",1,"Unchanged","Unless the mechanism is hermetically sealed or sized in all its functions and performances for internal pressure build­up, all closed cavities shall be provided with a venting hole sized according to the launch ascent depressurisation profile."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.7.7.5a","Requirement","ECSS-E-ST-33-01_0820203",1,"Unchanged","With the exception of the bonding strap for grounding, all electrical connections to the mechanism shall be made through electrical connectors of a type qualified for the intended application."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.8.2.1c","Requirement","ECSS-E-ST-33-01_0820236",1,"Unchanged","The analyses specified in requirement 4.8.2.1a shall cover \n1.\tthe combinations of range of extreme conditions for the flight system and which do not necessarily all occur during qualification testing \n2.\tthe effect of on-ground environmental conditions \n3.\tthe worst or extreme case conditions.","NOTE \t1\tto item 1: For example, worst-case friction levels.\nNOTE \t2\tto item 2: For example, air pressure, gravity effects, and test rigs perturbations.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.8.2.2a","Requirement","ECSS-E-ST-33-01_0820237",1,"Unchanged","The worst-case operational and non­operational sizing of a mechanism shall be identified according to the environmental, load and functional performance characteristics for the particular spacecraft and mechanism."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.8.2.15a","Requirement","ECSS-E-ST-33-01_0820270",2,"Unchanged","Limited­life items shall be identified."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.8.3.3.5b","Requirement","ECSS-E-ST-33-01_0820295",1,"Unchanged","Latching shock emissions shall be measured."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","4.8.3.4.2a","Requirement","ECSS-E-ST-33-01_0820325",1,"Unchanged","New builds of qualified designs shall be acceptance tested to verify that the actual manufactured hardware is free from manufacturing defects. "]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","A.2.1<4>b","Requirement","ECSS-E-ST-33-01_0820348",1,"Unchanged","The SMS shall include the sterilization requirements and the sterilization test procedure requirements."]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","A.2.1<6>d","Requirement","ECSS-E-ST-33-01_0820354",1,"Unchanged","The SMS shall include the qualification temperature range under all ground, test, launch and in­orbit conditions.","NOTE \tThis is used for the mechanism thermal design and sizing (see 4.7.4.2a).\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","D.2.1<6>a","Requirement","ECSS-E-ST-33-01_0820387",1,"Unchanged","The user manual shall describe the following topics:\n1.\tmechanism configuration for storage, transportation and handling;\n2.\tcontainer characteristics and operation instructions;\n3.\tpacking, and transportation instructions;\n4.\tunpacking and incoming inspections;\n5.\thandling and storage instructions;\n6.\tenvironmental conditions for the in  D.2.1<6>a.1.to  D.2.1<6>a.5. defined phases.","NOTE \tExamples of such environmental conditions are mechanical, thermal, hygrometry, and pressure, cleanliness.\n"]
["ECSS-E-ST-33-01C Rev.2","ECSS - Current v1.0","G.2.1<2>b","Requirement","ECSS-E-ST-33-01_0820443",1,"Unchanged","The MSVR shall include a comprehensive list of the test conditions."]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","4.1.2.2a","Requirement","ECSS-E-ST-60-20_0920002",1,"Unchanged","A sensor with cartography capability shall have the following minimum outputs:\n1.\tstar position,\n2.\tmeasurement date."]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","4.2.4a","Requirement","ECSS-E-ST-60-20_0920030",1,"Unchanged","An autonomous star tracker shall include the following minimum capabilities:\n1.\tautonomous attitude determination (‘lost in space’ solution);\n2.\tautonomous attitude tracking (with internal initialization)."]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","5.2.4d","Requirement","ECSS-E-ST-60-20_0920164",1,"Created","The test success criteria shall be derived from the customer requirements taking into account the test setup error budget."]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","5.5.4.1d","Requirement","ECSS-E-ST-60-20_0920173",1,"Created","The error classification of the FOV spatial error shall be discussed and agreed between supplier and customer.","NOTE \tThe temporal behaviour of the FOV spatial error is a function of the star velocity across the STR field of view. FOV errors lead to bias error in the case of inertial pointing, while they contribute to random noise for angular rate. \n"]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","5.5.5.2b","Requirement","ECSS-E-ST-60-20_0920081",1,"Unchanged","All other error sources with relevant spatial behaviour shall be identified by the supplier and used for the assessment of performances."]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","5.9.1a","Requirement","ECSS-E-ST-60-20_0920105",1,"Unchanged","When Autonomous Attitude Tracking is performed by using repetitive Autonomous Attitude Determination the metrics relative to autonomous attitude tracking specified in 5.10 shall be applied.","NOTE \tThis capability is often referred to as the ability to solve the ‘lost in space’ problem. The orientation, or attitude, measurement is nominally in the form of a quaternion that parameterizes the transformation between the Inertial reference frame and the sensor-defined reference frame. The determination is nominally performed by comparing star images measured on a detector to known star positions and characteristics stored in a star catalogue within the sensor.\n"]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","5.11.1b","Requirement","ECSS-E-ST-60-20_0920129",1,"Unchanged","Contributing error sources shall be established.","NOTE \tThey are a function of the precise technique used to determine the rate.\n"]
["ECSS-E-ST-60-20C Rev. 2","ECSS - Current v1.0","A.2.1<4>e","Requirement","ECSS-E-ST-60-20_0920146",2,"Normative Change","Modelling constraints and critical implementation issues shall be described and their relevance on performance be indicated."]
["ECSS-E-ST-20-21C","ECSS - Current v1.0","5.1.1d","Requirement","ECSS-E-ST-20-21_1400004",1,"Created","An end to end test shall be performed to ensure that the actuator pulses are effectively present at actuator interface when a system level verification is done.","NOTE\tThe end to end test is performed with the actual flight actuator if resettable and safe. Alternatively, it is performed with a flight representative actuator or - if not possible for safety or practical reasons - with a load of the same impedance as the flight actuator.\n"]
["ECSS-E-ST-20-21C","ECSS - Current v1.0","5.2.3c","Requirement","ECSS-E-ST-20-21_1400028",1,"Created","The commands for ARM and for SELECT/FIRE shall follow completely independent physical paths, such that no single failure in the complete command chain can result in a fire action.","NOTE\tFor example, ARM enable is driven by high power command while SELECT, FIRE and ARM disable are driven by serial command interface.\n"]
["ECSS-E-ST-20-21C","ECSS - Current v1.0","5.5.2b","Requirement","ECSS-E-ST-20-21_1400061",1,"Created","For current-driven actuators, the maximum fault current emission from the actuator electronics to the actuator shall not exceed two times the maximum nominal specified value according to requirement 5.3.1a.2."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.2.1a","Requirement","ECSS-E-ST-35-06_0200014",1,"Unchanged","Designs shall be such that the product\n    1. avoids contamination and \n    2. allows for cleaning and drying."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.2.3b","Requirement","ECSS-E-ST-35-06_0200039",1,"Unchanged","Systems requiring cleaning and cleanliness verification shall have no protective filters at fill and drain valves or test ports."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.2.4e","Requirement","ECSS-E-ST-35-06_0200048",1,"Unchanged","Filtration of simulation fluids or propellants shall be performed to a cleanliness class equal or better than the propulsion system requirements.\n    ","NOTE See Annex A."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.3.5l","Requirement","ECSS-E-ST-35-06_0200081",1,"Unchanged","For the purpose of cleaning, the non-single-use valve or regulator shall be operated during flushing or purging."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.4.1g","Requirement","ECSS-E-ST-35-06_0200098",1,"Unchanged","In cases where the flow systems, or sections thereof (propellant or pressurant), consist of more than one line size, the smallest flow system size shall specify the selection."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","4.4.4g","Requirement","ECSS-E-ST-35-06_0200114",1,"Unchanged","Argon shall be equivalent to MIL-PRF-27415B, Grade A."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","5.2.3b","Requirement","ECSS-E-ST-35-06_0200147",1,"Unchanged","Only qualified cleaning processes shall be used. "]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","5.4.1d","Requirement","ECSS-E-ST-35-06_0200172",1,"Unchanged","For precision cleaning, clause 4.6 shall apply."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","5.5.5.1a","Requirement","ECSS-E-ST-35-06_0200205",1,"Unchanged","The vacuum pressure shall be monitored."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","6.1.2b","Requirement","ECSS-E-ST-35-06_0200230",1,"Unchanged","Dry surfaces of completed items shall be wetted with a few drops of high purity water, with a pH range of 5,0 to 8,0, meeting the requirements of ISO 14951-10:2000, to permit testing as required. "]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","6.2.2g","Permission","ECSS-E-ST-35-06_0200397",1,"Unchanged","Alternatively to 6.2.2f, the polymer components may be vacuum dried as described in 6.2.6 and 6.2.7."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","6.3.1a","Requirement","ECSS-E-ST-35-06_0200259",1,"Unchanged","Fluid containing components (e.g. vessels, pipe and tubing systems, pipe, tubing and flex hose subsystems) shall be maintained under the pressurant gas purge overpressure until all ports, orifices and fittings are sealed. \n    ","NOTE Typical over-pressures range from 0,01 MPa to 0,05 MPa"]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","7.5.3a","Requirement","ECSS-E-ST-35-06_0200295",1,"Unchanged","Fabricated bags shall be sealed across the open end. "]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","8.1d","Requirement","ECSS-E-ST-35-06_0200304",1,"Unchanged","Clean bags shall have been cleaned internally and verified in conformance with clause 7.5. "]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","11.1.3d","Requirement","ECSS-E-ST-35-06_0200337",1,"Unchanged","The liquid shall be sampled to obtain a maximum of 500 ml of the original test fluid sample for analysis."]
["ECSS-E-ST-35-06C Rev.2","ECSS - Current v1.0","B.2.1<3>b","Requirement","ECSS-E-ST-35-06_0200362",1,"Unchanged","The CTS shall include any additional term, definitions, abbreviated terms and symbol used."]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","4.3.1.3c","Requirement","ECSS-E-ST-20-01_1450023",1,"Created","For multipactor design and verification, the failures modes shall be included only if the equipment recovery is possible."]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","4.6.2.2b","Permission","ECSS-E-ST-20-01_1450038",1,"Created","The reduced margins, as indicated in Table 4-3 and Table 4-4, may be used if justification is given by the supplier.","NOTE\tThe nominal and reduced margins as indicated in Table 4-3 and Table 4-4 include modelling error.\n"]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","5.3.2.1a","Requirement","ECSS-E-ST-20-01_1450064",1,"Created","Design analysis shall be applied to equipment or components P1 and P2, according to clause 4.6.2 for single carrier and clause 4.7.2 for multicarrier."]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","5.3.3.2b","Requirement","ECSS-E-ST-20-01_1450097",1,"Created","For the nominal dimension, the analysis shall be performed without including the manufacturing tolerances and the thermal effect."]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","6.3f","Requirement","ECSS-E-ST-20-01_1450123",1,"Created","A maximum acceptable temperature of the TRP shall be specified by the customer."]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","6.4.3.2b","Requirement","ECSS-E-ST-20-01_1450132",1,"Created","A single carrier equivalent power for a test as described under 6.4.3.2a above shall be defined as follows:\n1.\tperform a single carrier analysis at the average frequency of the multicarrier signal in accordance with clause 5.3.2.1 and 5.3.2.2.3 for L1 or 5.3.2.3.3 for L2 where the threshold power in Watts is denoted Pth,sc,\n2.\tperform a multicarrier analysis on the same analysis level, L1 or L2,as the single carrier analysis specified in 1 above,\n3.\tcalculate the average threshold power in Watts, sum of all carrier power values, found in the multicarrier analysis, denoted Pth,mc with m the number of carriers, using for both, the single carrier and the multi carrier analysis, identical design charts, identical electromagnetic computational model as well as identical material parameters and geometry definitions,\n4.\tcalculate the equivalent power for a single carrier test of a multicarrier device using following formula: \nPeq,sc = P0 · Pth,sc/Pth,mc, where P0 is the nominal multicarrier average power in Watts, sum of all carrier power values, of the input signal,\n5.\tverify that the computed equivalent power from step 4 for a single carrier test of a multicarrier device is always bounded by P0 ≤ Peq,sc ≤ NP0, where N is the number or of carriers,\n6.\tThe single carrier test frequency is the average frequency of the multi-carrier signal as for the single carrier analysis in step 1.","NOTE\t1\tIf the single carrier analysis was an L1 analysis performed according to clause 5.3.2.1 and 5.3.2.2.3, the multicarrier analysis is performed according to clauses 5.3.2.1 and 5.3.2.2.4.\nNOTE\t2\tIf the single carrier analysis was an L2 analysis performed according to clauses 5.3.2.1 and 5.3.2.3.3, the multicarrier analysis is performed according to clauses 5.3.2.1 and 5.3.2.3.4.\n"]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","7.3.2b","Requirement","ECSS-E-ST-20-01_1450157",1,"Created","When harmonic detection is used, the residual harmonic level in the test system shall be minimised, in order to improve detection sensitivity. ","NOTE\tIt is good practice to keep the residual harmonics system level at least 100 dBc with respect to the carrier power level.\n"]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","8.4h","Requirement","ECSS-E-ST-20-01_1450190",1,"Created","Any detected pressure rise above the value specified in clause 6.2 or temperature above the maximum allowed value at the TRP according to requirement 6.3f shall cause an interruption of the test until satisfactory conditions are restored. "]
["ECSS-E-ST-20-01C","ECSS - Current v1.0","9.2a","Requirement","ECSS-E-ST-20-01_1450206",1,"Created","If the manufacturing process or the material of any potential critical gap is changed, a representative SEY sample of the new equipment or component shall be used for SEY measurements.","NOTE\tAny change of manufacturing process and any change of materials can be traced by means of DPL and DML according to ECSS-Q-ST-70.\n"]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","6.2.2a","Requirement","ECSS-E-ST-10-04_0760017",1,"Informative Change","For daily and 81-day averaged values of F10.7, S10.7 and M10.7 the values given in Table A-1 shall be used.","NOTE\t1\tAp is only weakly correlated with the solar activity indices. It has a seasonal variation and is higher at the equinoxes.\nNOTE\t2\t81 days corresponds to 3 solar rotations and 81 day averaged values are used as input for atmosphere models.\nNOTE\t3\tAlternative daily and 81-day average values and forecast methods are available [ISO 27852:2016]. Their values can be more appropriate depending on the use-case.\n"]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","7.2.1.1b","Permission","ECSS-E-ST-10-04_0760026",2,"Normative Change","The JB-2006 model [RN.5] or JB-2008 model [RN.39] may be used for calculating the total atmospheric density above an altitude of 120 km."]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","9.2.1.1d","Requirement","ECSS-E-ST-10-04_0760055",2,"Normative Change","The dates of Minima and Maxima that shall be used for solar cycles 1 to 24 and the algorithm for forecasting future Minima and Maxima are presented in Annex B.1 and Table B-2.","NOTE\tAs it is difficult to define the % of solar MIN and MAX to apply for missions not scheduled in Max or Min periods, a more conservative analysis can be obtained for all periods using AE8MAX for electron fluxes and AP8MIN for proton fluxes.\n"]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","9.2.2.3b","Requirement","ECSS-E-ST-10-04_0760074",2,"Normative Change","In Table B-10, Table B-11, and Table B-12 all ions shall be treated as fully ionised for geomagnetic shielding calculations.","NOTE \tIn cases where the instantaneous solar proton flux is required or as a function of time during an event, there are several large events that have been measured, their spectral fits are provided in Annex I.2.4.\n"]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","9.3a","Requirement","ECSS-E-ST-10-04_0760079",1,"Unchanged","A specification of the expected radiation environment of a space system shall be established. "]
["ECSS-E-ST-10-04C Rev.1","ECSS - Current v1.0","10.2.4.4a","Requirement","ECSS-E-ST-10-04_0760100",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","5.2.1k","Requirement","ECSS-E-ST-50-16_1490011",1,"Created","If the SM is connected to the CM via a TT Switch, then this Switch shall be transparent with regards to PCF frames.","NOTE\tTransparent means, that the TT Switch needs to update its transparent clock in PCF frames passing this Switch as described in [SAE AS6802] §5.1.\n"]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","6.2.5.2a","Requirement","ECSS-E-ST-50-16_1490045",1,"Created","The MAC shall treat a valid MAC frame as Critical Traffic if the CT-Marker matches the CT-Marker entry of the Table 7-9."]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","6.2.7c","Requirement","ECSS-E-ST-50-16_1490070",1,"Created","When the Switch finishes executing the last entry of the Schedule Table, the Switch shall restart with the first entry of the Schedule Table."]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","7.2.3.2a","Requirement","ECSS-E-ST-50-16_1490082",1,"Created","A Switch shall associate each Time-Triggered frame it forwards with a SW_TT_TX_LENGTH, a SW_TT_TX_PERIOD, and a SW_TT_TX_PHASE. ","NOTE\tA scheduler for Time-Triggered frames typically takes the SW_TT_TX_LENGTH and SW_TT_TX_PERIOD values of all frames as an input and returns a value for SW_TT_TX_PHASE for each Time-Triggered frame as an output. \n\tSW_TT_TX_LENGTH is the allowed length of an Ethernet frame including IFG and preamble:\n·\tMinimum(SW_TT_TX_LENGTH) = IFG (12 bytes) + preamble (7 bytes) + start of frame delimiter (1 bytes) + frame (64 bytes)\n·\tMaximum(SW_TT_TX_LENGTH) = IFG (12 bytes) + preamble (7 bytes) + start of frame delimiter (1 bytes) + frame (1518 bytes)\n\tSW_TT_TX_PERIOD is the transmission period with which the Switch dispatches the respective Time-Triggered frame.\n\tSW_TT_TX_PHASE is a value given by: \n \n\twhere:\n\tSW_SCHEDULE_GRANULARITY is the granularity of the schedule\n\tK is a natural number such that SW_TT_TX_PHASE <= SW_TT_TX_PERIOD holds. \n"]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","7.2.4.3b","Requirement","ECSS-E-ST-50-16_1490115",1,"Created","In case redundancy management is enabled, the End-System shall accept the first received valid Time-Triggered frame and discard all following Time-Triggered frames which are inside the configured time skew and contain the same VL-ID."]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","7.5.7a","Recommendation","ECSS-E-ST-50-16_1490152",1,"Created","The minimum gap between two scheduled virtual links (VL1, VL2) sent by the same End-System should be defined according to the following formula: \n","NOTE\tThis value is the minimum bound to be used. Any larger value is possible well but the bandwidth usable for TT messages on the related links is decreased. Overlapping Tx windows causes frames to queue on egress if the distance between scheduled send events is less than the min_gap. \n"]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","8.2.2h","Requirement","ECSS-E-ST-50-16_1490165",1,"Created","In transmission, in the IPv4 packet structure, the Time to Live field shall be equal to 1.","NOTE\tTo avoid propagation through routers.\n"]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","8.3.2c","Recommendation","ECSS-E-ST-50-16_1490186",1,"Created","A TFTP server according to [RFC 1350] and [RFC 768] should be used to provide the configuration and application data to the network."]
["ECSS-E-ST-50-16C","ECSS - Current v1.0","8.4.3.2p","Recommendation","ECSS-E-ST-50-16_1490219",1,"Created","If an ICMP frame length of the Switch is smaller than 1 bytes, the frame should be discarded and the MIB counter ICMProtocolInError be incremented."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","5.1e","Permission","ECSS-E-ST-32-01_0810318",1,"Unchanged","For unmanned, single-mission, space vehicles and their payloads, and GSE the reduced fracture control programme, specified in clause 11, may be implemented."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","6.3.2d","Requirement","ECSS-E-ST-32-01_0810027",1,"Unchanged","For metallic materials the maximum sustained stress-intensity factor Kmax, shall not exceed the threshold stress-intensity factor for stress-corrosion cracking KISCC."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","6.3.3e","Requirement","ECSS-E-ST-32-01_0810036",1,"Unchanged","For metallic parts, mean fatigue life material characteristics and a design life factor of at least four (4) shall be used. "]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","7.1a","Requirement","ECSS-E-ST-32-01_0810059",1,"Unchanged","Fracture mechanics analysis shall be performed to determine the analytical life of a safe life metallic item."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","7.2.6c","Requirement","ECSS-E-ST-32-01_0810086",1,"Unchanged","Crack aspect ratios (a/c) of 0,2 and 1,0 shall be considered in the analysis."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","7.2.8j","Requirement","ECSS-E-ST-32-01_0810100",2,"Normative Change","For manufacturing steps, which can cause crack extension without the possibility of subsequent NDT the maximum possible crack growth shall be considered in the safe life calculation.","NOTE\tFor example, the autofrettage pressure cycle during manufacturing of a COPV which can lead to crack growth by linear or non-linear material behaviour. Especially the non-linear material behaviour can lead to stable crack growth (ductile tearing) which can be considerably underestimated. More information on autofrettage can be found in [R8].\n"]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","8.2.5a","Permission","ECSS-E-ST-32-01_0810341",1,"Created","Sealed containers meeting the following criteria may be used:\n1.\tThe container is not part of a system with a pressure source and is individually sealed.\n2.\tLeakage of the contained gas does not result in a catastrophic hazard and the pressure shell is verified leak before burst (LBB) at MDP.\n3.\tThe part is manufactured from metal alloys used for commercially available sealed containers procured to an aerospace standard or equivalent that are not susceptible to crack extension related to SCC.\n4.\tThe MDP does not exceed 0,15 MPa.\n5.\tThe stored energy potential does not exceed 19310 joules (14240 foot-pounds).\n6.\tThe container does not have an impervious barrier or coating that inhibits leakage on either the interior or exterior surfaces.\n7.\tThe container is subject to the following:\n(a)\tTested for leaks before repressurization.\n(b)\tRe–flight containers are tested for leaks before being re-flown."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","8.4.4.1a","Requirement","ECSS-E-ST-32-01_0810153",1,"Unchanged","A fail safe item shall meet all the requirements for the fail safe approach described in clauses 6.2, 6.3, and 10.7."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","8.8a","Requirement","ECSS-E-ST-32-01_0810186",1,"Unchanged","Fasteners smaller than diameter 5 mm (or 3/16”) shall not be used in safe life applications."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","10.3.1k","Requirement","ECSS-E-ST-32-01_0810209",2,"Deleted","<<deleted (moved to ECSS-Q-ST-70-15)>>"]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","10.3.2c","Requirement","ECSS-E-ST-32-01_0810214",2,"Deleted","<<deleted (moved to ECSS-Q-ST-70-15)>>"]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","10.4.2.2e","Requirement","ECSS-E-ST-32-01_0810240",2,"Deleted","<<deleted (moved to ECSS-Q-ST-70-15)>>"]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","10.5.2.2.1b","Requirement","ECSS-E-ST-32-01_0810273",2,"Deleted","<<deleted (moved to ECSS-Q-ST-70-15)>>"]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","10.6.2a","Requirement","ECSS-E-ST-32-01_0810282",1,"Unchanged","All associated drawings, manufacturing and quality control documentation shall identify that the item is a potential fracture-critical item (unless when it is a fail-safe or low-risk fracture metallic item) or a fracture critical item."]
["ECSS-E-ST-32-01C Rev. 2","ECSS - Current v1.0","11.2.2.3a","Permission","ECSS-E-ST-32-01_0810332",1,"Unchanged","The requirements of clauses 8.5 and 8.7 may be replaced by the following requirement: structural glass and other non-metallic items (other than composites, bonded and sandwich items) shall be proof-tested at 1,2 times the limit load.","NOTE\tIt is well-known that glass and other brittle items subjected to static load can be sensitive to growth of inherent flaws (i.e. static fatigue). This effect is normally considered in the structural verification, taking into account empirical data (e.g. statistical methods, taking into account the surface roughness of the item). \n"]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","4.2.11.2b","Requirement","ECSS-E-ST-20-07_0080024",1,"Unchanged","An equipment bonding stud connected to the unit housing shall be provided as a ground reference at equipment level."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.2.3a","Requirement","ECSS-E-ST-20-07_0080049",1,"Unchanged","The ambient electromagnetic level shall be measured with the EUT not operating and all auxiliary equipment turned on."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.4i","Requirement","ECSS-E-ST-20-07_0080072",1,"Unchanged","The LISN impedance shall be measured at least annually under the following conditions:\n1.\tthe impedance, measured between the power output lead on the EUT side of the LISN and the metal enclosure of the LISN,\n2.\tan unterminated power input terminal on the power source side of the LISN."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.6.6.1c","Requirement","ECSS-E-ST-20-07_0080274",1,"Created","Connector savers can affect the test results, in particular radiated emission test results, and therefore shall either not be used, or be chosen or modified in such a way as to ensure shield continuity."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.7.2a","Requirement","ECSS-E-ST-20-07_0080109",1,"Unchanged","Measurements shall be performed with the EUT tuned to not less than three frequencies within each tuning band, tuning unit, or range of fixed channels, consisting of one mid-band frequency and a frequency within ±5% from each end of each band or range of channels."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.10.1i","Requirement","ECSS-E-ST-20-07_0080282",1,"Created","Scan rates and step sizes shall be decreased if necessary to permit the observation of a response."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.2.10.4f","Requirement","ECSS-E-ST-20-07_0080145",1,"Unchanged","Data shall be provided with a minimum amplitude resolution of 1 dB for each plot."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.3.8b","Requirement","ECSS-E-ST-20-07_0080163",1,"Unchanged","Absence of passive intermodulation products shall be verified in accordance with the requirements for “Passive intermodulation” specified in ECSS-E-ST-20."]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.4.6.3c","Requirement","ECSS-E-ST-20-07_0080189",1,"Unchanged","To test the EUT antenna positioning, the test setup boundary of the EUT and associated cabling for use in positioning of antennas shall be determined. "]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.4.11.2a","Requirement","ECSS-E-ST-20-07_0080217",2,"Normative Change","The test equipment shall be as follows:\n1.\tRF signal generators,\n2.\tRF power amplifiers,\n3.\tLinearly polarized transmit antennas\n4.\tThree-axis isotropic electric field sensors (physically small - electrically short) with appropriate frequency response to cover the wanted test frequency range,\n5.\tMeasurement receiver,\n6.\tPower meter,\n7.\tDirectional coupler,\n8.\tAttenuator,\n9.\tData recording device,\n10.\tLISN defined in 5.2.4.","NOTE \t1\tto 5.4.11.2a.3: The following antennas are commonly used:\n·\t30 MHz to 200 MHz, biconical, 137 cm tip to tip,\n·\t200 MHz to 1 GHz, double ridge horn, 69,0 cm by 94,5 cm opening, or log-periodic,\n·\t1 GHz to 18 GHz, double ridge horn, 24,2 cm by 13,6 cm opening.\nNOTE \t2\tto 5.4.11.2a.10: The LISN is providing a defined common mode impedance.\n"]
["ECSS-E-ST-20-07C Rev. 2","ECSS - Current v1.0","5.4.14.5a","Requirement","ECSS-E-ST-20-07_0080320",1,"Created","Data presentation shall be as follows:\n1.\tESD generator settings,\n2.\tOscilloscope records taken during calibration,\n3.\tTable stating compliance to the requirements."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","4.1a","Requirement","ECSS-E-ST-10-03_0750001",1,"Informative Change","A coherent test programme shall be established, encompassing each verification stage and level to implement the verification by testing.","NOTE\t1\tThe testing programme is performed incrementally at different product decomposition levels.\nNOTE\t2\tRefer to clause 3.1 for determining the type of item for which the test programme is defined (i.e. space segment equipment or space segment element) and to ECSS-S-ST-00-01 Glossary of terms.\nNOTE\t3\tThe number and type of testing levels depends upon the complexity of the project and on its characteristics in accordance with the Verification programme (see ECSS-E-ST-10-02).\nNOTE\t4\tThe test programme documentation is defined in 4.3.3.\n"]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","4.3.3.2b","Requirement","ECSS-E-ST-10-03_0750026",2,"Normative Change","The agreed AIT Plan shall be available, at the latest, for the TRR of the test programme."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","4.4.3e","Requirement","ECSS-E-ST-10-03_0750059",2,"Deleted","<<deleted>>"]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","4.5.3a","Requirement","ECSS-E-ST-10-03_0750068",1,"Unchanged","Acceptance testing shall be performed to provide evidence that the space segment element or equipment performs in accordance with the specifications in the intended environments with the specified acceptance margins.","NOTE \tThis evidence is used, further to analysis as relevant, to provide via verification reports (defined in ECSS-E-ST-10-02 Annex F) the elements for the close-out of the VCD (defined in ECSS-E-ST-10-02 Annex B).\n"]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.4b","Requirement","ECSS-E-ST-10-03_0750101",1,"Unchanged","The following qualification tests shall be performed on a dedicated model and never on the Protoflight Model:\n1.\tlife test \n2.\tburst pressure test, \n3.\tESD. "]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.5.1.3f","Requirement","ECSS-E-ST-10-03_0750123",1,"Unchanged","Performances shall be monitored continuously or at regular intervals."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.5.2.6c","Requirement","ECSS-E-ST-10-03_0750148",1,"Unchanged","The equipment shall be mounted to a fixture using its normal mounting points."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.5.3.5a","Requirement","ECSS-E-ST-10-03_0750174",1,"Unchanged","Burst test shall be performed in conformance with ECSS-E-ST-32-02 clause 5.4.7."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.5.4.1i","Requirement","ECSS-E-ST-10-03_0750183",1,"Unchanged","The test profile shall include a non operating cycle."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","5.5.5.3a","Requirement","ECSS-E-ST-10-03_0750207",1,"Unchanged","The ESD test on space segment equipment shall be performed in conformance with ECSS-E-ST-20-07 clause 5.4.12."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.1.2.1b","Requirement","ECSS-E-ST-10-03_0750231",1,"Unchanged","The RFT content shall be agreed with the customer."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.1.5d","Requirement","ECSS-E-ST-10-03_0750264",1,"Unchanged","The polarity test shall be one of the last tests before shipment to the launch site."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.2.1e","Requirement","ECSS-E-ST-10-03_0750272",1,"Unchanged","Spin balance tests shall be used for spin stabilized systems."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.2.7k","Requirement","ECSS-E-ST-10-03_0750305",1,"Unchanged","For space segment element which is designed to be re-flown, the qualification test duration per axis shall be in conformance with Table 6‑2 plus 50 seconds per additional flight."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.2.11d","Requirement","ECSS-E-ST-10-03_0750486",1,"Unchanged","If necessary, for the purpose of the test, mitigation actions shall be taken to reduce the background noise.","NOTE \tBackground noise can be due to the external environment (e.g. road, sea, wind, people around, other ongoing activities/tests), facilities (e.g. air conditioning, lights), MGSE, EGSE, FGSE (e.g. pumps). Background noise can be different depending on the time (night/day, presence of other activities).\n"]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.4.3d","Requirement","ECSS-E-ST-10-03_0750356",2,"Normative Change","The space segment element shall be mounted in a temperature chamber if the atmospheric mission pressure is near the Earth atmospheric pressure and in a pressure chamber with temperature control capability or in a vacuum chamber with pressure and temperature control capabilities if the atmospheric mission pressure is different from the Earth atmospheric pressure."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","6.5.6.1a","Requirement","ECSS-E-ST-10-03_0750365",1,"Unchanged","The aero-thermodynamic tests shall be performed on dedicated scaled models in wind tunnels for different conditions.","NOTE\t1\tE.g. hot and cold hypersonic, low supersonic and subsonic.\nNOTE\t2\tThe aero-thermodynamic test verifies the aerodynamic and thermal loads on the space segment element performing atmospheric entry.\n"]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","A.2.1<5>a","Requirement","ECSS-E-ST-10-03_0750393",2,"Normative Change","The AIT Plan shall document the AIT activities and associated planning."]
["ECSS-E-ST-10-03C Rev.1","ECSS - Current v1.0","C.2.1<1>a","Requirement","ECSS-E-ST-10-03_0750419",1,"Unchanged","The TPRO shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","4.1.2f","Requirement","ECSS-E-ST-20_0020006",2,"Unchanged","Signal interfaces shall withstand without damage positive or negative nominal voltages that are accessible on the same connector, coming from the unit itself, from the interfaced units or from EGSE."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","4.1.3i","Requirement","ECSS-E-ST-20_0020015",1,"Unchanged","Any on–board processing which issues commands to reconfigure subsystems or payloads shall be overridable and potentially inhibited by ground command.","NOTE \tFor criticality categories, see ECSS‑Q‑ST‑30 or ECSS-Q-ST-40.\n"]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","4.2.1.2.3b","Requirement","ECSS-E-ST-20_0020429",1,"Created","The presence of foreign particles inside equipment, subsystem or system shall be treated as a credible event.","NOTE\t1\tExample of foreign particles are the materials used for manufacturing, piece of wire, nuts, washers, components and pins.\nNOTE\t2\tVisual inspection is normally done to avoid the presence of foreign conductive particles that can create loss of insulation. Such particles might be there before equipment/subsystem /system closure or integration, or being the result of vibration exposure due to poor fixation. Potential particles and the activities that leads to emerging of these particles are identified and control plan is created if needed.\nNOTE\t3\tVisual inspection is done on equipment, subsystem or system level before final assembly to avoid the presence of such particles that might create loss of insulation.\nNOTE\t4\tThe visual inspection method used is compatible with the minimum size of the particle to be detected.\n"]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","4.2.1.2.3aa","Permission","ECSS-E-ST-20_0020454",1,"Created","The electrical diagrams, layout and assembly drawings providing the information of the critical lines or nets may be part of the relevant analysis report."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","4.2.3m","Requirement","ECSS-E-ST-20_0020061",2,"Unchanged","The following shall be performed for any connector the loss of which can lead to the loss of the mission:\n1.\tDocument the connector in the single point failure list\n2.\tVerify and document its integrity up to the highest spacecraft integration level, to avoid accidental demating."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.3a","Requirement","ECSS-E-ST-20_0020096",2,"Unchanged","Any protection function of a power converter or regulator preventing failure propagation shall: \n1.\tnot be implemented in the same integrated circuit, and \n2.\tnot utilize common references."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.5.2a","Requirement","ECSS-E-ST-20_0020105",2,"Unchanged","The solar array shall be specified to provide the requested power and ensure the energy balance in each mission phase during operational life including any string loss tolerance defined by the customer, spacecraft charging effects and worst case conditions. ","NOTE\t1\tThe solar array is designed to be single-failure tolerant at string level.\nNOTE\t2\tIn order to meet the solar array reliability requirements, the impact of other loss factors can lead to the addition of other spare strings.\nNOTE\t3\tThe computation of the energy balance is a typical task for the large system integrator based on defined power points expressed as a specification to the SA manufacturer.\n"]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.5.4b","Requirement","ECSS-E-ST-20_0020134",2,"Unchanged","The design of the insulation barriers between adjacent wires, connector pins and slip rings shall be such that no discharge phenomena can occur."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.6.4b","Requirement","ECSS-E-ST-20_0020158",1,"Unchanged","For the procurement of cells and batteries the manufacturer shall supply a user manual in conformance with Annex D."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.6.5.2d","Recommendation","ECSS-E-ST-20_0020398",1,"Unchanged","The failure of one or more cells within a battery due to imbalance in the state of charge, temperature or other parameter between cells should be prevented by the battery control electronics."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.7.4b","Requirement","ECSS-E-ST-20_0020199",2,"Unchanged","All non-essential loads shall be switched-off autonomously in the event of reaching the battery energy level that is able to maintain all essential loads for a time guaranteeing safe recovery."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.8.1k","Requirement","ECSS-E-ST-20_0020226",2,"Unchanged","The stability of current limiters shall be ensured for the actual loads characteristics. "]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","5.11.1a","Recommendation","ECSS-E-ST-20_0020248",2,"Unchanged","The requirements of this Clause 5 should be verified by the verification methods and at the verification points listed in Table 8‑3.","NOTE\t1\tTable 8‑3 can be used as a starting point for the definition of the verification methods.\nNOTE\t2\tFor more details on verification, see also ECSS-E-ST-10-02, in particular requirements 5.2.1c, 5.2.1d and 5.2.1e.\n"]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","6.3.4.3b","Requirement","ECSS-E-ST-20_0020404",2,"Unchanged","<<deleted>>"]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","6.3.7.3a","Requirement","ECSS-E-ST-20_0020281",1,"Unchanged","On the basis of the attitude control requirements, the supplier shall derive magnetic requirements for the spacecraft so as to limit transient, diurnal and secular torques. "]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","7.2.2.3.2b","Requirement","ECSS-E-ST-20_0020314",1,"Unchanged","The reflective and transmissive properties (losses, depolarisation, diffusivity) of the materials and composites used for polarisation and frequency selective reflectors shall be quantified and their impact on antenna performances assessed."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","7.2.2.4.3c","Requirement","ECSS-E-ST-20_0020339",1,"Unchanged","Measures to drain accumulated electric charges from all plastic parts shall be implemented to avoid electrostatic discharge (ESD)."]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","7.3.2.1a","Requirement","ECSS-E-ST-20_0020348",1,"Unchanged","All the components and equipments of the RF chain shall be able to stand the maximum specified operating RF power during its application in space with:\n1.\tno degradation of the component, \n2.\tno degradation of the RF signal including radiative losses, and \n3.\twith their thermal levels not exceeding those corresponding to the maximum available RF power at the maximum qualification temperature. "]
["ECSS-E-ST-20C Rev.2","ECSS - Current v1.0","C.2.1c","Requirement","ECSS-E-ST-20_0020377",1,"Unchanged","The EMEVR shall include any additional definition, abbreviation or symbol used."]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.2.3c","Requirement","ECSS-E-ST-20-40_1580024",1,"Created","Design and verification responsibilities shall be assigned to different people in order to guarantee independent verification. [ALL]","NOTE\tFor example, the FPGA Responsible Engineer can take over the role of the FPGA Designer or of the FPGA Verification Engineer, but not both.\n"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.4.4d","Requirement","ECSS-E-ST-20-40_1580057",1,"Created","The DEVICE Database shall include the description of what the DEVICE Database contains, including the files’ structure, naming conventions and version control labels. [ALL]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.5.2t","Requirement","ECSS-E-ST-20-40_1580082",1,"Created","Influences from layout such as cross talk and matching shall be accounted for during the detail design work. [D-ASIC, A-ASIC, --, IP]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.5.5d","Requirement","ECSS-E-ST-20-40_1580091",1,"Created","The DEVICE Database shall include the preliminary test vectors for Production Tests. [D-ASIC, A-ASIC, --, --]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.6.8c","Requirement","ECSS-E-ST-20-40_1580124",1,"Created","The following expected outputs shall be reviewed during DEVICE Layout Phase Review: [ALL]\n1.\tLayout Generation Report\n2.\tLayout Verification Report\n3.\tDEVICE Validation Plan (update) (DVaP) as in DRD in Annex D\n4.\tDEVICE Radiation Test Plan\n5.\tDEVICE Data Sheet (update) as in DRD in Annex H\n6.\tESCC Detail Specification (preliminary)\n7.\tDEVICE database (update)\n8.\tDEVICE VCD (update)\n9.\tDEVICE Feasibility and Risk Assessment Report (update) (DFRAR) as in DRD in Annex F"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","5.8.6b","Requirement","ECSS-E-ST-20-40_1580147",1,"Created","The reviewers shall review expected outputs of DEVICE Implementation Phase, in addition to all the expected outputs of this DEVICE Validation, Qualification and Acceptance Phase. [ALL]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","A.2.1<2>c","Requirement","ECSS-E-ST-20-40_1580157",1,"Created","The DRS shall specify the requirements concerning intellectual property rights of the DEVICE. [ALL]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","B.2.1<1>b","Requirement","ECSS-E-ST-20-40_1580182",1,"Created","The DDP shall include the references to all the applicable and reference documents used during the DEVICE development, including best design practices and coding rules. [ALL]","NOTE\tFor example, internal and external standards.\n"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","C.2.1<2>c","Requirement","ECSS-E-ST-20-40_1580215",1,"Created","If the planned coverage cannot be achieved, justification for the impossibility to reach that coverage and what is the maximum coverage achieved, shall be provided and approved by the customer. [ALL]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","F.2.1<2>c","Requirement","ECSS-E-ST-20-40_1580248",1,"Created","The DFRAR shall include conclusions regarding the remaining lifetime of the baseline DEVICE technology, including the package choices, for both the final DEVICE and any preliminary prototype versions. [ALL]"]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","G.2.1a","Requirement","ECSS-E-ST-20-40_1580273",1,"Created","The DADR shall include a subdivision of the DEVICE into its fundamental functions or blocks, identifying and documenting their main interfaces, functionalities, performances, hierarchical dependencies and flowing down all the requirements for each block. [ALL] "]
["ECSS-E-ST-20-40C","ECSS - Current v1.0","G.2.1j","Requirement","ECSS-E-ST-20-40_1580282",1,"Created","The DADR shall identify any functional blocks which are reused at different locations of the DEVICE or with potential to become an IP Core or Building Block for reuse in other DEVICEs. [ALL]"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","4.3.1d","Requirement","ECSS-E-ST-20-08_0091104",1,"Created","For long term storage longer than 6 months qualification coupons shall be kept in the dark in a dry nitrogen environment.","NOTE \tIt is good practice to use light tight coverage to keep the DVT coupons in darkness during periods shorter than 6 months.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.3.3.1b","Requirement","ECSS-E-ST-20-08_0090036",1,"Unchanged","The capability for replacement of cracked, broken or damaged SCAs shall be included in the design. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.3.3.4b","Permission","ECSS-E-ST-20-08_0091066",1,"Unchanged","To test the technique of interconnecting strings, the negative ends of individual strings may be connected in a way that is representative for flight panels. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.4.3.4a","Requirement","ECSS-E-ST-20-08_0090070",1,"Unchanged","The adherence of the SCAs to the substrate, shall be performed in parallel to panel laydown."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.1.3.3k","Requirement","ECSS-E-ST-20-08_0090103",1,"Unchanged","Dedicated electrical test points shall be included in the electrical design of the qualification coupon such that the capacitance of single strings can be measured."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.2.2a","Requirement","ECSS-E-ST-20-08_0091113",1,"Created","Qualification coupons shall follow the acceptance test program as shown in Table 5‑2, if not covered by qualification tests as specified in Table 5‑1.","NOTE \t1\tThe thermal cycling acceptance testing, specified in 5.5.3.7, is typically covered by the vacuum thermal cycling, specified in 5.5.3.11, of the qualification test program.\nNOTE \t2\tFlight hardware is subject to acceptance testing after qualification has been successfully completed, ref ECSS-E-ST-10-03.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.3.2.6c","Requirement","ECSS-E-ST-20-08_0090147",1,"Unchanged","Any defect in conformance with requirement 5.5.3.2.6b, raised after acceptance shall be reported and traced throughout the qualification sequence."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.3.2.10c","Requirement","ECSS-E-ST-20-08_0090160",1,"Unchanged","None of the interconnectors shall exhibit lifting tears, breaks or cracks."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.3.3.6d","Requirement","ECSS-E-ST-20-08_0090193",1,"Unchanged","Test conditions and requirements shall be stated in the SCD-PVA."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.3.7.3b","Requirement","ECSS-E-ST-20-08_0090218",2,"Normative Change","The number of cycles specified in requirement 5.5.3.7.3a shall be between 3 and 10."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.5.3.9a","Requirement","ECSS-E-ST-20-08_0090227",1,"Unchanged","X-ray photographs shall be taken of all busbars, wire collection strips and diode boards on the qualification coupons. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","5.8b","Requirement","ECSS-E-ST-20-08_0090249",1,"Unchanged","One set of documents shall be sent to the customer."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.4.2.2c","Requirement","ECSS-E-ST-20-08_0090282",1,"Unchanged","The test samples shall be chosen statistically and at random from the first manufacturing lots of the procurement lot.","NOTE \tFor sampling, see ISO 2859.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.4.3.1.6b","Requirement","ECSS-E-ST-20-08_0090302",1,"Unchanged","Adhesive voids along the cover edge shall not exceed 0,6 mm in depth."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.4.3.7.2a","Requirement","ECSS-E-ST-20-08_0090336",1,"Unchanged","The number of cycles and the extreme temperatures shall be as stated in the SCD-SCA."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.4.3.8.2h","Requirement","ECSS-E-ST-20-08_0090344",2,"Normative Change","If there are requirements on specific environmental conditions, they shall be stated in the SCD-SCA.","NOTE \tFor example, chemical vapour requirements and/or voltage loading to simulate ambient illumination.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.4.3.14.3a","Requirement","ECSS-E-ST-20-08_0090368",1,"Unchanged","The parameters of reverse I/V characteristics measurement shall be as stated in the SCD-SCA concerning temperature, hold time, current limitation, maximum reverse bias (voltage)."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","6.5.2c","Requirement","ECSS-E-ST-20-08_0090390",1,"Unchanged","Failure analysis of these SCAs shall be performed by the supplier and the results provided to the customer, as part of an NRB documentation.","NOTE \tFor NRB, see ECSS-Q-ST-10-09.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.1.1.2c","Requirement","ECSS-E-ST-20-08_0090399",1,"Unchanged","Any deviation from in-process, acceptance and qualification test procedures shall be justified in the SCD-BSC."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.4.2.2c","Requirement","ECSS-E-ST-20-08_0090438",1,"Unchanged","The qualification lot shall be a production lot of at least 400 cells or the number of cells to be integrated on the solar array, whichever is lower."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.5.1.5.2b","Requirement","ECSS-E-ST-20-08_0090456",1,"Unchanged","The maximum dimension of drops and spatter shall be 0,1 mm in diameter and 0,03 mm in height."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.5.6.3c","Requirement","ECSS-E-ST-20-08_0090488",1,"Unchanged","The coverglass as stated in the SCD-BSC shall be used."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.5.10.2a","Requirement","ECSS-E-ST-20-08_0090513",1,"Unchanged","The thickness of the solar cell metal contact in the interconnector weld area or on dedicated in-process test samples shall be checked with a step-height profiler, as stated in the SCD-BSC.","NOTE \tFor example, with a betascope or a similar instrument.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.5.13.2b","Requirement","ECSS-E-ST-20-08_0090522",1,"Unchanged","The flux density and energy shall be uniform over the cell area within ±10 %. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","7.5.19.2a","Requirement","ECSS-E-ST-20-08_0090542",1,"Unchanged","The flatness shall be determined by measuring the maximum deflection, d, of the bare solar cell measured on an optically flat surface with an orientation and method as stated in the SCD-BSC."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","8.6.1b","Requirement","ECSS-E-ST-20-08_0090575",1,"Unchanged","All coverglass procurement lots shall be qualified."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","8.7.1.3.4c","Permission","ECSS-E-ST-20-08_0091079",1,"Unchanged","Edge chips with a dimension of the projection into the coverglass face of b < 0,1 mm and a length of the chip a < 0,2 mm (in conformance with Figure 8‑2) may be ignored."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","8.7.4.4b","Requirement","ECSS-E-ST-20-08_0090608",1,"Unchanged","The edge parallelism shall be measured using a calibrated micrometer."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","8.7.12.2b","Requirement","ECSS-E-ST-20-08_0090641",1,"Informative Change","For photons with a wavelength between 200 nm to 400 nm, the integrated intensity at the end of test shall be as follows: \n1.\tequal to (1000 - 1500) Sun-hours or 1 % of the mission life, whichever is the longer period;\n2.\thave an UV irradiation acceleration factor of less than 10 S.C. (AM0).","NOTE \tFor photons with a wavelength between 200 nm to 400 nm, spectral irradiance requirements for UV light sources are specified in ECSS-Q-ST-70-06.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","8.8.2b","Requirement","ECSS-E-ST-20-08_0090666",1,"Unchanged","Failed components shall be identified as such and included in the delivery. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.4.5.2.2c","Requirement","ECSS-E-ST-20-08_0090699",2,"Normative Change","In case of an integral protection diode the electrical isolation of cell and diode shall be tested by measuring the current when a voltage (as stated in the SCD-BSC) is applied between the front contacts of the protection diode and of the cell at the temperature as stated in the SCD-BSC"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.5.2e","Requirement","ECSS-E-ST-20-08_0090708",1,"Unchanged","The integral protection diodes shall be equipped with front interconnectors as step 7 in Table 7‑2."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.6.5.2c","Requirement","ECSS-E-ST-20-08_0090741",1,"Unchanged","During the process the samples shall be under load. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.6.10.2a","Requirement","ECSS-E-ST-20-08_0090756",2,"Normative Change","All diodes shall be subjected to a coating adherence test on both full sample faces."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.6.12.2a","Requirement","ECSS-E-ST-20-08_0090764",1,"Unchanged","The external protection diodes shall be subjected to 1 MeV electron irradiation.","NOTE \tISO 23038 outlines a methodology to perform this test.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","9.6.17.2a","Requirement","ECSS-E-ST-20-08_0090789",1,"Unchanged","The protection diodes shall be equipped with interconnects."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","10.1.2f","Requirement","ECSS-E-ST-20-08_0090822",2,"Normative Change","The irradiance uniformity of the solar simulator in the test plane shall not introduce errors due to the positioning accuracy of the relevant cells higher than 1 % or other value proposed by the supplier and accepted by the customer."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","10.2.4a","Requirement","ECSS-E-ST-20-08_0090847",1,"Unchanged","All standard solar cells (primary and SWS) shall be kept at temperatures below 50 °C during operation and storage. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.2.1.2a","Requirement","ECSS-E-ST-20-08_0091151",1,"Created","The conditions and methods of planar blocking diode testing shall conform to the source control drawing (SCD-PBD) detailed in Annex H.","NOTE \tThe planar blocking diode specification consists of two parts, the generic specification (this Standard) and the SCD-PBD. The SCD-PBD contains the technical specification for a diode type relevant to acceptance testing, as well as for the qualification testing. For the preparation of the SCD-PBD for planar blocking diodes, refer to Annex H, checklist for SCD-PBD.\n"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.4.2d","Requirement","ECSS-E-ST-20-08_0091165",1,"Created","The test documentation of the acceptance tests shall be delivered together with the delivered diodes and the qualification test lot."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.6.1.3e","Requirement","ECSS-E-ST-20-08_0091187",1,"Created","There shall be no evidence of corrosion, peeling of finish or plating or of holes and cracks."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.6.7.3.1c","Requirement","ECSS-E-ST-20-08_0091220",1,"Created","The reverse bias shall be a DC bias."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.6.8.2e","Requirement","ECSS-E-ST-20-08_0091229",1,"Created","The activation energy shall be:\n1.\tdetermined in accordance with ESCC 2265000, or\n2.\tfor silicon PN junction blocking diodes be 0,7 eV."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","12.6.14.3a","Requirement","ECSS-E-ST-20-08_0091255",1,"Created","The surface finish of the metal layers of the diode contact shall conform to the requirements of the interconnection process, as specified in the SCD-PBD, and the certified procurement specification of the supplier."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","A.2.1<6.5>a","Requirement","ECSS-E-ST-20-08_0090887",1,"Unchanged","In conformance with clause 5.4.3.6, the SCD-PVA shall state the maximum value of the resistance, in W."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","B.2.1<2>a","Requirement","ECSS-E-ST-20-08_0090912",1,"Unchanged","The SCD-SCA shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","C.2.1<6.5>b","Requirement","ECSS-E-ST-20-08_0090941",1,"Unchanged","In conformance with clause 7.3.2.2.3 for the pass-fail criteria, the following requirements shall be included:\n1.\tthe minimum value for Itest, in mA;\n2.\tthe average value for Itest, in mA;"]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","C.2.1<7.5>b","Requirement","ECSS-E-ST-20-08_0090953",1,"Unchanged","Coverglass gain-loss\n1.\tThe SCD-BSC shall include the same provisions as in the coverglass gain-loss for acceptance tests (in conformance with clause C.2.1<6.10>)."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","D.2.1<8.2>a","Requirement","ECSS-E-ST-20-08_0090978",1,"Unchanged","In conformance with clause 8.7.1.2, the SCD-CVG shall include:\n1.\tThe maximum dimensions, in mm, of scratches and digs.\n2.\tThe maximum number of corner chips per coverglass."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","E.2.1<7.7>a","Requirement","ECSS-E-ST-20-08_0091011",1,"Unchanged","In conformance with clause 9.6.7.3, the SCD-EPD shall include the maximum and minimum values of the contact thickness in mm."]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","H.2.1<6>a","Requirement","ECSS-E-ST-20-08_0091284",1,"Created","The level of the traceability of the manufactured planar blocking diodes in their marking shall be specified. "]
["ECSS-E-ST-20-08C Rev.2","ECSS - Current v1.0","H.2.1<8.2>a","Requirement","ECSS-E-ST-20-08_0091293",1,"Created","In conformance with clause 12.6.2, the SCD-PBD shall include: \n1.\tthe lateral dimensions and thickness, including tolerances. \n2.\tthe contact dimensions, including tolerances. \n3.\tthe maximum weight, in mg. "]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.1.2e","Requirement","ECSS-E-ST-80_0600011",1,"Created","A Security Management Plan shall describe resources under the same management control."]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.1.5c","Requirement","ECSS-E-ST-80_0600034",1,"Created","Processes and tools shall be in place to detect and address unauthorized equipment, personnel use or access."]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.3.2d","Requirement","ECSS-E-ST-80_0600067",1,"Created","In order to select appropriate security controls, organizations shall categorize the information to be handled by the system according to the criteria of Confidentiality, Availability, and Integrity.\nEXPECTED OUTPUT:\tSystem Security Engineering Plan [TS; SRR, PDR, CDR, QR]","NOTE\tNational security regulations as well as other laws (e.g., export, personal sensitive data and copyright restrictions) controlling the handling of specific information types override organizational discretion in categorizing information.\n"]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.3.2m","Requirement","ECSS-E-ST-80_0600076",1,"Created","The security obsolescence plan shall be agreed with the security risk owner and maintained during the system lifetime."]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.4.1e","Requirement","ECSS-E-ST-80_0600101",1,"Created","The preliminary security risk assessment shall consider at least the following:\n1.\tThe type of the mission and the information security threats to that mission. \n2.\tAll parts of the mission and system architecture during all phases of the mission/project, as the relevant threats can change during their lifecycle."]
["ECSS-E-ST-80C","ECSS - Current v1.0","5.4.5a","Requirement","ECSS-E-ST-80_0600134",1,"Created","Independent penetration tests shall be performed during development, as part of the qualification, before acceptance and during operation.","NOTE\tIndependent means that the penetration testers have not been involved in the design, development or implementation of the system(s).\n"]
["ECSS-E-ST-10-24C Rev.1","ECSS - Current v1.0","5.4e","Requirement","ECSS-E-ST-10-24_1290018",1,"Unchanged","The ICD shall be put under configuration control prior to interface end suppliers PDR."]
["ECSS-E-ST-10-24C Rev.1","ECSS - Current v1.0","5.8.1f","Requirement","ECSS-E-ST-10-24_1290087",1,"Created","The equipment EICD shall include the lists of all electrical Interfaces of the equipment classified per signal type, electrical connector list and types (including supplier) and the equipment electrical connectors pin-to pin table.","NOTE \tIt is necessary to produce such lists and tables respecting a specific format for supporting the harness design (electrical interconnections with other equipment) at a higher level.\n"]
["ECSS-E-ST-10-24C Rev.1","ECSS - Current v1.0","5.8.2i","Requirement","ECSS-E-ST-10-24_1290103",1,"Created","The instrument/sub-system EICD shall include the allocation tables per electrical interface types. ","NOTE \tFor example, LCL allocation table with LCL classes, heaters allocation table, thermistors allocation table per thermistor type, etc.\n"]
["ECSS-E-ST-10-24C Rev.1","ECSS - Current v1.0","A.2.1<4>d","Requirement","ECSS-E-ST-10-24_1290042",1,"Unchanged","For each verification requirement as defined in A.2.1<4>c., the verification responsibility shall be defined.","NOTE \tThis can be joint responsibility, stand-alone responsibility or any combination of them.\n"]
["ECSS-E-ST-10-24C Rev.1","ECSS - Current v1.0","C.2.2<1>a","Permission","ECSS-E-ST-10-24_1290075",1,"Unchanged","The IDD may take different forms depending on the kind of interface end it documents.","NOTE \tExamples of different forms are: a mechanical drawing, interface 3D CAD model, electrical circuit schematic, software API, software architectural or detailed design document.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.2.3.1a","Requirement","ECSS-E-ST-40_0860004",1,"Informative Change","The customer shall specify the requirements needed for planning and setting up the system verification and validation process related to software.\nEXPECTED OUTPUT:\tVerification and validation process requirements [RB, SSS; SRR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.3.2.1d","Requirement","ECSS-E-ST-40_0860021",1,"Informative Change","The output of each phase and their status of completion, submitted as input to joint reviews, shall be specified in the software life cycle definition, including documents in complete or outline versions, and the results of verification of the outputs of the phase. \nEXPECTED OUTPUT:\tSoftware life cycle definition [MGT, SDP; SRR, PDR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.3.7.1a","Requirement","ECSS-E-ST-40_0860048",2,"Normative Change","Interface management procedures shall be defined in accordance with ECSS-M-ST-40 requirements.\nAIM:\tDefine procedures that guarantee the consistency of the system interfaces.\nEXPECTED OUTPUT:\tInterface management procedures [MGT, - ; SRR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.5.2.2a","Requirement","ECSS-E-ST-40_0860073",1,"Informative Change","The supplier shall develop and document a detailed design for the interfaces external to the software item, between the software components, and between the software units, in order to allow coding without requiring further information.\nEXPECTED OUTPUT:\tThe following outputs are expected:\na.\tExternal interfaces design (update) [TS, ICD; CDR];\nb.\tInternal interfaces design (update) [DDF, SDD; CDR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.5.2.7a","Requirement","ECSS-E-ST-40_0860082",1,"Informative Change","It shall be ensured that all the methods utilized for different item of the same software are, from a dynamic stand–point, consistent among themselves and consistent with the selected computational model.\nEXPECTED OUTPUT:\tCompatibility of real-time design methods with the computational model [DDF, SDD; CDR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.7.2.3a","Requirement","ECSS-E-ST-40_0860112",1,"Informative Change","The supplier shall develop procedures to install the software product in the target environment.\nEXPECTED OUTPUT:\tInstallation procedures [DDF, SCF ; AR]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.8.3.5b","Requirement","ECSS-E-ST-40_0860135",2,"Normative Change","The supplier shall verify that the following code coverage is achieved\n \nEXPECTED OUTPUT:\tCode coverage verification report [DJF, SVR; CDR, QR, AR].","NOTE \tThis requirement is met by running unit, integration and validation tests, measuring the code coverage, and achieving the code coverage by additional (requirement based) tests, inspection or analysis. \n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.9.5.2a","Requirement","ECSS-E-ST-40_0860167",1,"Informative Change","The SOS entity shall forward user requests to the maintenance process for resolution.\nEXPECTED OUTPUT:\tUser’s request record - actions [OP, - ; - ]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.10.5.2a","Requirement","ECSS-E-ST-40_0860191",1,"Informative Change","Upon successful completion of the reviews, a baseline for the change shall be established.\nEXPECTED OUTPUT:\tBaseline for changes [MF, - ; - ]."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.11.3d","Requirement","ECSS-E-ST-40_0860750",1,"Created","Where the software is part of a system, the security analysis shall be based on the security analysis from the next higher product architectural level, if there is one.\nEXPECTED OUTPUT:\tSoftware security analysis report [SF, SSAR; SRR].","NOTE \tSoftware that is not part of a system will already be at the top architectural level.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","5.11.5.2b","Requirement","ECSS-E-ST-40_0860770",1,"Created","The software security analysis shall be extended and revised iteratively during the definition of the software architecture to ensure that identified security risks are addressed by the chosen architecture, and to identify security vulnerabilities in the architectural design.\nEXPECTED OUTPUT:\tSoftware security analysis report [SF, SSAR; PDR].","NOTE \tIdentified security vulnerabilities are an input to the architectural design process and may drive it in order to reduce or remove them.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","B.2.1<3>a","Requirement","ECSS-E-ST-40_0860207",2,"Normative Change","The SSS shall include any additional terms, definition or abbreviated terms used not already defined in any applicable or reference documentation."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","B.2.1<4.4>e","Requirement","ECSS-E-ST-40_0860216",1,"Unchanged","References to the interface requirements documents that define the external interfaces with the other systems shall be provided"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","B.2.1<6.3>c","Recommendation","ECSS-E-ST-40_0860669",2,"Normative Change","If a given requirement need not to be taken into account for the software validation against the requirements baseline, then it should be clearly identified.","NOTE \tA matrix (requirements to validation method correlation table) can be used to state the validation methods applicable to each requirement. This information can be further split into an information for validation requirements and an information for acceptance requirements, depending upon the project needs.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","D.2.1<4.3>a","Requirement","ECSS-E-ST-40_0860271",1,"Unchanged","The SRS shall describe in detail the product’s relationship to other systems."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","D.2.1<5.9>a","Requirement","ECSS-E-ST-40_0860297",1,"Unchanged","The SRS shall list any portability requirement applicable to the software item."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","E.2.1<5.3>e","Permission","ECSS-E-ST-40_0860796",1,"Created","Each interface external to the software may be organized as follows:\n¾\tData item (Name, description, unique identifier, description, source, destination, unit of measure, limit/range, accuracy, precision, frequency, rate, legality checks, data type, data representation);\n¾\tMessage item;\n¾\tCommunication protocol (by reference to the applicable documents)."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","F.2.1<4.1>b","Requirement","ECSS-E-ST-40_0860337",1,"Unchanged","The SDD shall also describe any system state or mode in which the software operates."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","F.2.1<5.4.6>a","Recommendation","ECSS-E-ST-40_0860699",1,"Unchanged","The subordinates of a component should be described by listing the immediate children. ","NOTE 1\tThe subordinates of a unit are the units that are ’called by’ it. The subordinates of a database can be the files that ’compose’ it.\nNOTE 2\tThe subordinates of an object are the objects that are ’used by’ it.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","G.2.1<4>a","Requirement","ECSS-E-ST-40_0860395",1,"Unchanged","The SRelD shall contain a brief description of the information to be associated with a software release, including:\n1.\treference of the corresponding SCF,\n2.\tversion of the delivered software configuration item,\n3.\tstatus of SPRs, SCRs and SW&D related to the software configuration item, and\n4.\tadvice for use of the software configuration item.","NOTE \tThe software release document is a subset of the software configuration file that describes a new version by comparison with “reference” or the previous one. It is used for the delivery of a new version of a software configuration item to a customer.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","H.2.1<5>a","Requirement","ECSS-E-ST-40_0860404",1,"Unchanged","The SUM shall include a description of the intended uses of the software, in terms of capabilities, operating improvements, and benefits expected from its use."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","I.2.1<1>a","Requirement","ECSS-E-ST-40_0860428",1,"Unchanged","The SVerP shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","J.2.1<5>b","Requirement","ECSS-E-ST-40_0860469",1,"Unchanged","The SValP shall list which are the tasks and the items under tests, as well as the criteria to be utilized for the testing activities on the test items associated with the plan. "]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","K.2.1<5.6>a","Requirement","ECSS-E-ST-40_0860493",1,"Unchanged","The SUITP shall list any requirement for software unit testing and integration testing personnel and their training needs."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","K.2.1<9.2.2>a","Requirement","ECSS-E-ST-40_0860518",1,"Unchanged","The SUITP shall list the test items. "]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","K.2.1<10.1>a","Requirement","ECSS-E-ST-40_0860527",2,"Normative Change","The SUITP shall provide an identification of software unit and integration test procedures. "]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","L.2.1<7.2.3>a","Requirement","ECSS-E-ST-40_0860560",1,"Unchanged","The SVS w.r.t. TS or RB shall describe, for each test case, the expected outputs."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","M.2.1<4.5>a","Requirement","ECSS-E-ST-40_0860585",2,"Normative Change","The SVR shall present in gathering all the specific verification reports that have been planned to be provided w.r.t. the SVerP, including:\n1.\tTraceability (when not already included in related software acceptance documents), presenting the following traceability matrices:\no\tSoftware acceptance testing to requirements baseline.\n2.\tFeasibility, presenting in gathering all the specific verification reports that have been planned to be provided w.r.t. the SVerP, including:\no\tStructural code coverage achievement (update for QR and AR);\no\tVerification of software documentation as per 5.8.3.10;\no\tOthers specific verification related to RAMS design (e.g. unit and integration testing coverage ratio)."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","N.2.1<8>a","Requirement","ECSS-E-ST-40_0860606",1,"Unchanged","The SRF shall document any corrective actions identified to ensure that the software intended for reuse meets the applicable project requirements."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","O.2.1<4.6>a","Requirement","ECSS-E-ST-40_0860617",2,"Normative Change","The SDP shall describe the monitoring mechanisms for managing the work. ","NOTE 1\tThe SDP apply to both the customer relationships and the supplier’s relationships.\nNOTE 2\tMonitoring mechanisms include progress report, progress meeting, action item lists.\n"]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","P.2.1<2>a","Requirement","ECSS-E-ST-40_0860649",1,"Unchanged","The SRevP shall list the applicable and reference documents to support the generation of the document."]
["ECSS-E-ST-40C Rev.1","ECSS - Current v1.0","T.2.1<7.4>a","Requirement","ECSS-E-ST-40_0860817",1,"Created","The SMP shall describe the tailoring of the maintenance process by referring to the maintainer’s software maintenance process manual."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.1.1e","Requirement","ECSS-E-ST-40-07_1630007",1,"Created","An SMP Simple Field shall be of simple type."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.1.3b","Requirement","ECSS-E-ST-40-07_1630016",1,"Created","Both Absolute and Relative path strings shall be supported and distinguished as follows:\n1.\tPaths starting with a delimiter are absolute paths from the simulation root object;\n2.\tPaths not starting with a delimiter are relative paths from the current object."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.3.1n","Requirement","ECSS-E-ST-40-07_1630050",1,"Created","The IComponent AddChild method shall add a new child object to the component with the following arguments and behaviour:\n1.\tArguments:\n(a)\t“child” giving the child object to add to the component;\n(b)\t“collection” giving the collection under the component to which the child object is added.\n2.\tBehaviour:\n(a)\tIt returns false if the given collection is not a valid collection under the IComponent object;\n(b)\tIt returns false if the child object is already present in the given collection;\n(c)\tOtherwise, it returns true if the child object is successfully added."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.5.2h","Requirement","ECSS-E-ST-40-07_1630079",1,"Created","The IContainer DeleteComponent method shall delete a component from the collection of contained components, with the following argument and behaviour:\n1.\tArgument: \n(a)\t\"component\" giving a reference to the component to be deleted.\n2.\tBehaviour:\n(a)\tIf the minimum number of component(s) contained by this object is reached, it throws a CannotDelete expection as per CannotDelete.h in [SMP_FILES];\n(b)\tIf the component to delete is not contained, it throws a NotContained exception as per NotContained.h in [SMP_FILES];\n(c)\tIf the component to delete is included, and the minimum number is not reached, then the component is removed from the collection, its Disconnect method is called and finally its destructor is called."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.6.2a","Requirement","ECSS-E-ST-40-07_1630083",1,"Created","All SMP Objects which represent the source of event notifications shall implement the IEventSource interface as per IEventSource.h in [SMP_FILES].","NOTE\tThe specification of event sources ensures that event sinks (see 5.2.6.1) that wish to receive their notifications can subscribe to them.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.8.2b","Requirement","ECSS-E-ST-40-07_1630108",1,"Created","The IRequest GetName method shall return the name of the callable operation if GetType return RT_Invoke or the property name if GetType returns RT_Get or RT_Set.","NOTE\tFor an Operation, requests are usually created by calling the IOperation CreateRequest method  (see 5.2.14.1f) so the name returned is the Operation name. For a Property, the name returned is always the Property name.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.11.4d","Requirement","ECSS-E-ST-40-07_1630142",1,"Created","The ISimpleArrayField SetValue method shall set the corresponding array item value stored with the following arguments and behaviour:\n1.\tArguments:\n(a)\t“index” giving the location of the item for which the value is set;\n(b)\t“value” giving the new value for the array item.\n2.\tBehaviour:\n(a)\tIf the given index is outside the array size, it throws an InvalidArrayIndex as per InvalidArrayIndex.h in [SMP_FILES];\n(b)\tIf the given value simple type kind does not match the simple type kind of the corresponding array item, then it throws an InvalidFieldValue as per InvalidFieldValue.h in [SMP_FILES];\n(c)\tIf the given value simple type kind does match the simple type kind of the corresponding array item, then it stores the given AnySimple value into the item value corresponding to the given index."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.2.13.1e","Requirement","ECSS-E-ST-40-07_1630177",1,"Created","The IProperty GetPrimitiveType method shall return the property equivalent primitive type if it is a simple type property or PTK_None if it is not a simple type property."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.2j","Requirement","ECSS-E-ST-40-07_1630204",1,"Created","The ITimeKeeper GetZuluTime method shall return the Zulu time."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.3i","Requirement","ECSS-E-ST-40-07_1630213",1,"Created","The IScheduler AddImmediateEvent method shall add an immediate simulation time event to the scheduler with the current simulation time as execution time returning an EventId as per Services/EventId.h in [SMP_FILES], with the following argument and behaviour:\n1.\tArgument:\n(a)\t“entryPoint” giving the Entry Point to be called when the Event is executed.\n2.\tBehaviour:\n(a)\tThe scheduled event is inserted at the end of the list of immediate events; the list of immediate events is processed in order of insertion and before any non-immediate event;\n(b)\tAfter adding the new Event to the scheduler, it returns the EventId identifying the added Event.","NOTE\t1\tCalls to AddImmediateEvent differs to calls to AddSimulationTimeEvent method with repeat=0, cycleTime=0 and simulationTime=0 since the event is scheduled at the front instead of the end of the list of scheduled events for the current simulation time.\nNOTE\t2\tIt cannot be assumed that Events added via AddImmediateEvent are the next Event executed, as other Events can have been scheduled with AddImmediateEvent prior to this Event, and hence are executed first.\nNOTE\t3\tTo execute an entry point immediately without going through the scheduler, the Execute() method of the EntryPoint can be called directly.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.4a","Requirement","ECSS-E-ST-40-07_1630234",1,"Created","The simulation environment shall provide an Event Manager component implementing the IEventManager interface as per Services/IEventManager.h in [SMP_FILES]."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.7p","Requirement","ECSS-E-ST-40-07_1630271",1,"Created","The ISimulator AddInitEntryPoint method shall add entry points to be executed in the Initialising state, as per following argument and behaviour:\n1.\tArgument:\n(a)\t “entryPoint” giving a pointer to the entry point interface of the entry point to be added.\n2.\tBehaviour:\n(a)\tIf the simulation is not in Building, Connecting or Standby state, then it throws an InvalidSimulatorState exception as per InvalidSimulatorState.h in [SMP_FILES];\n(b)\tIf the simulation is in Building, Connecting or Standby state, it adds the entry point to the list of entry points to be executed once the simulation reaches Initialising state. \n(c)\tThe ownership of the entry point remains with the caller of AddInitEntryPoint.","NOTE\tThis allows components to subscribe to a callback during initialization phase since there are only explicit methods defined for Publish, Configure and Connect. This simplifies implementation for models that do not require initialization.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.7y","Requirement","ECSS-E-ST-40-07_1630280",1,"Created","The ISimulator GetLinkRegistry method shall return the interface to the mandatory link registry service.","NOTE\tThis is a type-safe convenience method, to avoid having to use the generic GetService() method. For the standardised services, it is recommended to use the convenience methods, which are guaranteed to return a valid reference.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.9.1g","Requirement","ECSS-E-ST-40-07_1630305",1,"Created","The IPublication Unpublish method shall release all data published earlier via the Publish operations.","NOTE\tThis is called prior to deleting the component that has called into a specific IPublication instance.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.3.10.3a","Requirement","ECSS-E-ST-40-07_1630338",1,"Created","The simulation environment shall provide a class implementing the IStructureType interface as per Publication/IStructureType.h in [SMP_FILES]."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.4.1.2.2a","Requirement","ECSS-E-ST-40-07_1630371",1,"Created","The size of an array shall be a positive number."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.4.1.2.5b","Requirement","ECSS-E-ST-40-07_1630396",1,"Created","Enumeration Literal Values shall be unique within an Enumeration."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.4.1.2.7e","Requirement","ECSS-E-ST-40-07_1630404",1,"Created","A Property of an Interface shall not be static."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","5.4.1.3j","Requirement","ECSS-E-ST-40-07_1630429",1,"Created","Each Entry Point of a model or service shall be defined in a catalogue."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.2.4.4c","Requirement","ECSS-E-ST-40-07_1630465",1,"Created","The ByPointer attribute as per ecss.smp.l1.smpcat in [SMP_FILES] shall have the following effect for the Association C++ mapping:\n1.\tIf set to “true”, then the C++ mapping of the type includes the ‘*’ specifier as per “Association” template in Table 6‑1;\n2.\tIf not set, then the C++ mapping of the type includes the specifier corresponding to the type referenced in the Type attribute as per Table 6‑4;\n3.\tIf set to “false”, then the C++ mapping of the type does not include the ‘*’ specifier."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.2.4.6b","Requirement","ECSS-E-ST-40-07_1630476",1,"Created","The access specifier of the Property member methods shall be defined as follows:\n1.\tIf the Operation belongs in an Interface, the member is public;\n2.\tIf the Operation does not belong in an Interface, the mapping of the Visibility attribute is used.","NOTE\tSee clause 6.2.3 for details on the mapping of Visibility attributes.\n"]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.2.4.10a","Requirement","ECSS-E-ST-40-07_1630502",1,"Created","EventSource elements shall be mapped to ISO/ANSI C++ member pointer variables as per “EventSource” template in Table 6‑1."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.2.6.3d","Requirement","ECSS-E-ST-40-07_1630535",1,"Created","If the Class type has the NoConstructor attribute as per ecss.smp.l1.smpcat in [SMP_FILES] set to \"true\", the constructor shall be declared with the delete keyword."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.2.7.2b","Requirement","ECSS-E-ST-40-07_1630552",1,"Created","Interface classes shall have a defaulted virtual destructor."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","6.3.4e","Requirement","ECSS-E-ST-40-07_1630592",1,"Created","A DLL file shall export the function Finalise() with the following DLL Finalise template in Table 6‑8 where DLL_EXPORT is as per DLL_EXPORT template in Table 6‑8."]
["ECSS-E-ST-40-07C Rev.1","ECSS - Current v1.0","B.2.1a","Requirement","ECSS-E-ST-40-07_1630601",1,"Created","The suffix for package files shall be “smppkg”."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.2.2.2a","Requirement","ECSS-E-ST-40-08_1640015",1,"Created","Non-published Field found after unresolved elements processing or found Field with a different value type than the published one shall result in an error in the loading of the Assembly, which specifies the Field Value.","NOTE\tUnresolved elements processing is described in clause 5.5.1.2\n"]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.2.7.2e","Requirement","ECSS-E-ST-40-08_1640048",1,"Created","The BackReference of the Client Model Instance shall be identified by its Name."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.2.7.4e","Requirement","ECSS-E-ST-40-08_1640057",1,"Created","If the Input or Output Field of a Field Link is an Array Item at the index position from an Array Field, the syntax <ArrayFieldName>[index] shall be used in the respective Client and Owner Path."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.2.9i","Permission","ECSS-E-ST-40-08_1640079",1,"Created","The Assembly Instance, or Sub-Assembly, may contain a collection of Component Configurations."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.4.5n","Permission","ECSS-E-ST-40-08_1640114",1,"Created","Execute Task Activity may contain a collection of TemplateArguments to resolve the ones found in the referenced external Schedule."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.5.1.2k","Requirement","ECSS-E-ST-40-08_1640139",1,"Created","When calles, the simulator Configure() method shall attemt to resolve elemeints in UNRESOLVED_LINKS, UNRESOLVED_FIELD_VALUES, UNRESOLVED_OPERATIONS and UNRESOLVED_GEVENT_SUBSCRIPTIONS as follows:\n1.\tEach time before calling a model Configure()method;\n2.\tAfter all model Configure()methods habe ceen called."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.7.2.3g","Permission","ECSS-E-ST-40-08_1640172",1,"Created","A Value may specify paths to elements that do not exist at loading time and that are created dynamically during the simulator Building state or during the simulator Reconnecting state."]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.7.4.2b","Requirement","ECSS-E-ST-40-08_1640181",1,"Created","The Schedule shall be validated at run time in a SMP compliant simulation infrastructure by calling ISimulatorL2.LoadSchedule().","NOTE\tIt is impossible to perform the Schedule semantics validation offline except for Execute Task Activities.\n"]
["ECSS-E-ST-40-08C","ECSS - Current v1.0","5.8.2u","Requirement","ECSS-E-ST-40-08_1640206",1,"Created","Scheduling a Global Event Triggered Event shall subscribe entry points to the Start and Stop global events by calling Subscribe() on the Smp::Services::IEventManager interface."]
["ECSS-M-ST-10-01C","ECSS - Current v1.0","5.4a","Requirement","ECSS-M-ST-10-01_0310027",1,"Created","Prior to starting the review, fulfilment of the review prerequisites defined in the procedure shall be confirmed by the customer and agreed by the review team leader.\n    NOTE See also 5.3.4b."]
["ECSS-M-ST-10-01C","ECSS - Current v1.0","A.2.1<5>a","Requirement","ECSS-M-ST-10-01_0310051",1,"Created","The review procedure shall define the list of the documents required to be delivered for the review."]
["ECSS-M-ST-10C Rev. 1","ECSS - Current v1.0","5.1.2f","Requirement","ECSS-M-ST-10_0010006",1,"Created","Each customer shall verify compliance of his supplier(s) with all project requirements and constraints."]
["ECSS-M-ST-10C Rev. 1","ECSS - Current v1.0","5.2.3.1d","Requirement","ECSS-M-ST-10_0010039",1,"Created","The final audit report shall not be divulged without the agreement of the audited supplier."]
["ECSS-M-ST-10C Rev. 1","ECSS - Current v1.0","5.4a","Requirement","ECSS-M-ST-10_0010064",1,"Created","The customer shall organize the project into sequential phases which include all project specific reviews and decision milestones.\n    ","NOTE Phases and reviews are defined in clause 4.4.3."]
["ECSS-M-ST-10C Rev. 1","ECSS - Current v1.0","C.2.1<3>f","Requirement","ECSS-M-ST-10_0010096",1,"Created","The WBS shall be presented either as a graphical diagram or an indentured structure."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.2.1.3a","Requirement","ECSS-M-ST-40_0320007",1,"Created","Customer and suppliers shall indicate within the CM Plan the classification classes to be applied and the documentation set affected."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.1.3b","Requirement","ECSS-M-ST-40_0320025",1,"Created","The baseline documentation shall reflect the actual configuration of the product, at any given point of the product life cycle."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.2.2i","Requirement","ECSS-M-ST-40_0320064",1,"Created","The evaluation shall be transmitted to the customer for information."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.3.2e","Requirement","ECSS-M-ST-40_0320089",1,"Created","Changes implemented after delivery of the product shall be incorporated in the CIDL."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.4.2b","Requirement","ECSS-M-ST-40_0320098",1,"Created","Configuration in terms of functional and performance characteristics shall be verified at qualification review (QR) for prototype or proto-flight production, and FCV for serial production."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.7.3.1e","Requirement","ECSS-M-ST-40_0320131",1,"Created","The lower tier supplier shall confirm his approval or non-approval with rationale to the relevant customer within the contractually agreed timeframe."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","5.3.7.5e","Requirement","ECSS-M-ST-40_0320156",1,"Created","Access to classified information/documentation shall be restricted to authorized personnel."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","A.2.1<5.1>c","Recommendation","ECSS-M-ST-40_0320243",1,"Created","The configuration management plan should list the codes for companies, information types, models, subsystems, etc. which are applied specifically in the identification method or are in general use during project execution. "]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","C.2.1<3>a","Requirement","ECSS-M-ST-40_0320209",1,"Created","The configuration item data list shall include the following:\n    1. Cover sheets and scope.\n    2. Customer controlled documentation, including\n        (a) customer specifications and ICDs, and\n        (b) support specifications.\n    3. Engineering or design documentation, including\n        (a) verification plans demonstrating compatibility with specified requirements,\n        (b) special instructions or procedures,\n            NOTE For example, transportation, integration, and handling.\n        (c) declared PMP lists,\n        (d) lower level specifications,\n        (e) lower level ICDs,\n        (f) drawings and associated lists,\n        (g) test specifications,\n        (h) test procedures, and\n        (i) users manual or handbook.\n    4. List of applicable changes not yet incorporated into the baselined documentation, and deviations (including status, directly related to the document (e.g. specification) to which the change belongs to).\n    5. CI number breakdown\n        (a) indentured breakdown by part numbers starting from the part number associated with the CI down to the lowest level of composition;\n        (b) quantity of each part number used on the next higher assembly;\n        (c) issue status of the drawings and associated lists applicable to each part number."]
["ECSS-M-ST-40C Rev. 1","ECSS - Current v1.0","E.2.1<6>a","Requirement","ECSS-M-ST-40_0320222",1,"Created","The SCF shall identify all the documents applicable to the delivered software configuration item version."]
["ECSS-M-ST-60C","ECSS - Current v1.0","8.2d","Requirement","ECSS-M-ST-60_0300018",1,"Created","The supplier shall submit the current working schedule to the customer for review and comment."]
["ECSS-M-ST-60C","ECSS - Current v1.0","9.3.1.1c","Requirement","ECSS-M-ST-60_0300043",1,"Created","The OBCP shall be used as the reference for all Control Work Packages."]
["ECSS-M-ST-60C","ECSS - Current v1.0","9.3.4a","Requirement","ECSS-M-ST-60_0300052",1,"Created","The supplier shall provide the customer with the computation of price variation applying the agreed formula and indices and the relevant supporting documentation upon submission of escalation invoices."]
["ECSS-M-ST-60C","ECSS - Current v1.0","F.2.1<3.7>a","Requirement","ECSS-M-ST-60_0300085",1,"Created","The cost estimating plan shall explain how the evolution of the hypothesis is tracked and fed into the cost models.\n    NOTE For example: does the cost engineering entity has an internal information link allowing to respond rapidly to design options that would generate cost over a certain target? "]
["ECSS-M-ST-60C","ECSS - Current v1.0","G.2.1<8>d","Requirement","ECSS-M-ST-60_0300098",1,"Created","The supplier shall provide cost figures associated with confidence level. Unless otherwise agreed with the customer, the supplier shall present ranges at agreed confidence level with the customer. "]
["ECSS-M-ST-80C","ECSS - Current v1.0","7.2.11a","Requirement","ECSS-M-ST-80_0340011",1,"Created","Risks shall be monitored, communicated, and results shall be displayed in conformance with risk assessment report DRD, Annex C.","NOTE The aim is to ensure complete and systematic control of the implementation of risk management activities."]
["ECSS-M-ST-80C","ECSS - Current v1.0","A.2.1<3>a","Requirement","ECSS-M-ST-80_0340020",1,"Created","The risk management policy document shall describe the set of project resources that are affected by risk and thereby have an impact on the project objectives."]
["ECSS-M-ST-80C","ECSS - Current v1.0","B.2.1<8>b","Requirement","ECSS-M-ST-80_0340045",1,"Created","The risk management plan shall summarize the analysis process for each of the risk domain leading to the determination of an overall risk assessment. "]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.2.4c","Requirement","ECSS-Q-ST-20_0380012",2,"Unchanged","The use of acceptance authority media shall be restricted to authorized personnel as identified in the acceptance authority media control system."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.2.6q","Requirement","ECSS-Q-ST-20_0380038",1,"Unchanged","The supplier shall make the measurement design data available to the customer upon request."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.2.8.1a","Requirement","ECSS-Q-ST-20_0380046",1,"Unchanged","Statistical quality control and analysis methods shall be used to maintain or improve the specified control of quality, when statistically significant with respect to the product characteristics and to quantities produced.","NOTE\tExamples of statistical quality control and analysis methods are sample inspection plans, determination of quality levels, statistical process control and process capabilities studies.\n"]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.4.1.3b","Requirement","ECSS-Q-ST-20_0380079",1,"Unchanged","The supplier shall submit to the customer, upon request, the list of procurement sources, including all the information in the records 5.3.1.3a, for information."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.5.1b","Requirement","ECSS-Q-ST-20_0380096",1,"Unchanged","The planning shall include the identification of MIPs in conformance with 5.4.8, together with the reference to the procedures by which the various activities are performed and the required cleanliness levels and temperature and humidity requirements of the facilities."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.5.7.2b","Requirement","ECSS-Q-ST-20_0380129",1,"Unchanged","The required cleanliness levels for all levels of flight hardware shall be indicated on drawings, specifications, procedures, or other documents controlling the manufacture, assembly, integration and test of the items. "]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.5.9.2e","Requirement","ECSS-Q-ST-20_0380152",1,"Unchanged","The receiving organization shall maintain the logbook up-to-date."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.6.3.1b","Requirement","ECSS-Q-ST-20_0380159",1,"Unchanged","The QA organization shall review and approve test procedures."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","5.8.2a","Requirement","ECSS-Q-ST-20_0380191",1,"Unchanged","The supplier shall ensure that GSE is configuration controlled."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","A.2.2a","Permission","ECSS-Q-ST-20_0380246",1,"Created","The response to this DRD may be combined with the response to the product assurance plan, as defined in ECSS-Q-ST-10."]
["ECSS-Q-ST-20C Rev.2 Corr.1","ECSS - Current v1.0","C.2.1g","Requirement","ECSS-Q-ST-20_0380221",1,"Unchanged","The logbook shall contain the records of total operating hours for each limited-life element identified in the test procedures."]
["ECSS-Q-ST-70-54C","ECSS - Current v1.0","5.2.4d","Requirement","ECSS-Q-ST-70-54_1360029",1,"Created","For indirect analytical techniques that involve contamination transfer it shall be ensured that the transfer process is uniform over the entire sample surface."]
["ECSS-Q-ST-10-04C","ECSS - Current v1.0","5.1.1a","Requirement","ECSS-Q-ST-10-04_0180001",1,"Created","The supplier shall uniquely identify critical items."]
["ECSS-Q-ST-10-04C","ECSS - Current v1.0","5.2.5.1a","Requirement","ECSS-Q-ST-10-04_0180034",1,"Created","The supplier shall assess and review all critical items periodically for status."]
["ECSS-Q-ST-10-04C","ECSS - Current v1.0","A.2.1<7>b","Requirement","ECSS-Q-ST-10-04_0180059",1,"Created","This list shall contain the statement of verification of the control implementation as defined in 5.2.4.2."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","5.1.2c","Requirement","ECSS-Q-ST-20-10_1120007",1,"Created","The preliminary equipment specification shall be used as a technical reference for the market investigation and OTS item identification."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","5.3.2.1.4c","Requirement","ECSS-Q-ST-20-10_1120043",1,"Created","The supplier shall verify compatibility of OTS item warm‑up time with respect to system performances."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","5.3.2.3.1c","Requirement","ECSS-Q-ST-20-10_1120064",1,"Created","The supplier shall perform inspection on OTS item to evaluate confidence on provided part list or, if no list is provided, identify constituent EEE parts."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","5.3.2.3.2d","Requirement","ECSS-Q-ST-20-10_1120073",1,"Created","The supplier shall be able to track the supply chain back to the manufacturer of the OTS item."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","5.4.3.2e","Requirement","ECSS-Q-ST-20-10_1120098",1,"Created","Fuses whose performances are not in accordance with the ECSS-E-ST-20 shall be removed and replaced by the supplier with other fuses or other appropriate devices."]
["ECSS-Q-ST-20-10C","ECSS - Current v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-20-10_1120131",1,"Created","The OTS plan shall contain a description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","4.5h","Requirement","ECSS-Q-ST-30-02_0390024",1,"Created","The effect of operational and failure behaviour of specific parts or equipment on other parts or equipment shall be assessed with regard to the physical layout of their mechanical, electrical and thermal interface.\n    NOTE 1 Examples of effects are temperature, vibration, movement, power demand and heat flow.\n    NOTE 2 A graphical representations of requirements 4.5a to 4.5h is given in Figure 4-1                                         "]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","5.2l","Requirement","ECSS-Q-ST-30-02_0390049",1,"Created","The failure probabilities shall be ranked as per Table 5-2 and relevant entry (the PN) listed in the FMECA worksheet column."]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","5.3a","Requirement","ECSS-Q-ST-30-02_0390053",1,"Created","An item shall be considered a critical item if:\n    1. a failure mode has failure consequences classified as catastrophic, or\n    2. a failure mode is classified as CN greater or equal to 6 in conformance with Table 5-3.\n        NOTE The customer can tailor the criteria for critical item identification defining a failure mode as critical according to programme specific needs.                                                                                                                                                                 "]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","8.2a","Requirement","ECSS-Q-ST-30-02_0390091",1,"Created","Process FMECA shall be performed on processes agreed with the customer.\n    NOTE 1 These processes are those considered to have effects as reported in Table 8-1                                         \n    NOTE 2 The inputs needed to start the work depend strongly on the process to be analysed.\nTypical inputs are:\n        a. working and control plan;\n        b. assembly procedure;\n        c. integration procedure;\n        d. test procedure;\n        e. handling procedure (manual). "]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","A.2.1<5>b","Requirement","ECSS-Q-ST-30-02_0390116",1,"Created","The FMEA/FMECA report shall include a functional partition in the design between hardware and software, including a reference to the corresponding HSIA shall be addressed."]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","A.2.1<9>a","Requirement","ECSS-Q-ST-30-02_0390125",1,"Created","The FMEA/FMECA report shall describe the FDIR policy and criteria including reference to relevant documents and to detection reference.\n    NOTE The detection reference includes telemetry, housekeeping data, and health check."]
["ECSS-Q-ST-30-02C","ECSS - Current v1.0","D.2.1<3>a","Requirement","ECSS-Q-ST-30-02_0390150",1,"Created","The HSIA form shall contain the identification of the reference number of the failure mode in the design FMEA/FMECA."]
["ECSS-Q-ST-30-09C","ECSS - Current v1.0","5.1.2a","Requirement","ECSS-Q-ST-30-09_0400001",1,"Created","Availability requirements shall respect the mandatory characteristics defined by the system engineering process.\n    NOTE E.g. traceable, identified, unique, or unambiguous."]
["ECSS-Q-ST-30-09C","ECSS - Current v1.0","6.3g","Requirement","ECSS-Q-ST-30-09_0400033",1,"Created","For flight equipment, the availability analysis shall take into account radiation effects.\n    NOTE For example, upset for logic parts such as SET for opto and linear parts, and latch up."]
["ECSS-Q-ST-40-12C","ECSS - Current v1.0","5.1.1b","Requirement","ECSS-Q-ST-40-12_0430002",1,"Created","The supplier shall perform a FTA for:\n    1. selected undesirable events which could have catastrophic, critical or major consequences;\n        NOTE For definition for the scale of severity, refer to ECSS-Q-ST-30.\n    2. support of failure;\n    3. accident investigations.\n        NOTE This is to limit the amount of effort in performing the analysis."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","5.2.1c","Requirement","ECSS-Q-ST-60-05_0160004",1,"Created","The PID shall contain as a minimum:\n    1. the manufacturing and inspection flow chart;\n    2. the list of applicable documents with approved revision;\n    3. the general organization of the production line;\n    4. the approved domain: authorized parts, materials, processes and reworks;\n    5. the list of manufacturing, inspection and failure analysis equipment;\n    6. the list of hybrids manufactured in conformance with the approved PID."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","7.3.1.2a","Requirement","ECSS-Q-ST-60-05_0160037",1,"Created","Similarity shall be proposed by the manufacturer to the customer by using a similarity form in conformance with Annex C.\n    NOTE Similarity is assessed on the basis of the HTIF and this similarity form."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","8.2.2d","Requirement","ECSS-Q-ST-60-05_0160062",1,"Created","Results shall conform to MIL-STD-883 method 2011 for bond pull strength and MIL-STD-883 method 2019 for die shear strength, with no failure allowed."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","8.3.2c","Requirement","ECSS-Q-ST-60-05_0160071",1,"Created","For bimetallic bonding (gold-aluminium) ageing (1 h at 300 °C or the equivalent time-temperature combination with a 0,92 eV activation energy basis) shall be performed before the pull test."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","10.2.1b","Requirement","ECSS-Q-ST-60-05_0160096",1,"Created","Apart from serialization, all marking shall be clearly visible when normal mounting procedures are followed. "]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","10.3.4b","Requirement","ECSS-Q-ST-60-05_0160121",1,"Created","Magnification shall be such that the layout can be easily identified. "]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","10.5.5a","Permission","ECSS-Q-ST-60-05_0160254",1,"Created","If hybrid circuits may be delidded and relidded for repair:\n    1. The customer is informed before the operation.\n    2. No more than one delid-relid cycle is performed."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","12.3c","Requirement","ECSS-Q-ST-60-05_0160187",1,"Created","The specifications and conditions for the tests specified in Figure 12-1 shall be as given in Table 12-4."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","14a","Requirement","ECSS-Q-ST-60-05_0160196",1,"Created","DPA test sequence depends on the technology and shall be performed in conformance with the following methods: \n    1. External visual inspection, MIL-STD-883 Method 2009.8.\n    2. X-rays (if soldered items or gold wires are present), MIL-STD-883 Method 2012.\n    3. SAM inspection, MIL-STD-883 Method 2030.\n    4. Seal test, MIL-STD-883 Method 1014 Condition A2 - Condition C.\n    5. PIND test, MIL-STD-883 Method 2020 Condition A.\n    6. Internal visual inspection, MIL-STD-883 Method 2017 Class K, MIL-STD-883 Method 2010 Condition A, MIL-STD-750 Method 2072, MIL-STD-750 Method 2073, MIL-STD-883 Method 2032.\n    7. MIL-STD-750 Method 2073.\n    8. SEM inspection, MIL-STD-883 Method 2018 (Provide photos of typical assemblies and possible anomalies).\n    9. Bond pull test, MIL-STD-883 Method 2011 Condition D (Pull all wires).\n    10. Die shear test, MIL-STD-883 Method 2019 (Shear all chips)."]
["ECSS-Q-ST-60-05C Rev. 1","ECSS - Current v1.0","C.2.1a","Requirement","ECSS-Q-ST-60-05_0160221",1,"Created","The Similarity form shall be as in Table C-1."]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","7.2.6b","Requirement","ECSS-Q-ST-60-12_0190032",1,"Created","Yield analysis and estimates based on the design book data shall be carried out to ensure that the circuit operates as specified in the wafer-acceptance criteria (both RF and DC parameters), and that it can withstand uncertainties such as, the accuracy of electrical model parameters and variations.\n    NOTE This includes the choice of, for example, optimum topologies, components, sizes, design centring, worst-case analysis, yield analysis and yield estimate. "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","7.2.11a","Requirement","ECSS-Q-ST-60-12_0190060",1,"Created","The successful output of the design rules checking (DRC) performed at the foundry shall be demonstrated to show conformance with the foundry layout rules (e.g. no errors detected)."]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","7.3.1c","Requirement","ECSS-Q-ST-60-12_0190065",1,"Created","When the design is completed, the designer shall send the file to the manufacturer for assembly of the final reticule and performance of the DRC. "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","8.1a","Requirement","ECSS-Q-ST-60-12_0190098",1,"Created","Application approval shall be carried out on each new designed MMIC in order to validate the compatibility between the MMIC and its specified application. "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","10.2.4.4c","Requirement","ECSS-Q-ST-60-12_0190131",1,"Created","If the test sequence performed is based on the user assembly process and in conformance with the user assembly test defined for the incoming inspection, then this test shall not to be repeated by the user when dies are received. "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","10.4.1.2c","Requirement","ECSS-Q-ST-60-12_0190156",1,"Created","The user LAT shall be performed using TCV, DEC or MMICs as per Figure 10-4 in conformance with ESCC 2439010."]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","10.4.2e","Requirement","ECSS-Q-ST-60-12_0190165",1,"Created","The duration of the test shall be 168 hours for high-grade level (failure criteria A=0, R=1). "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","10.4.5b","Requirement","ECSS-Q-ST-60-12_0190190",1,"Created","A test plan shall be issued and agreed upon by the customer. "]
["ECSS-Q-ST-60-12C","ECSS - Current v1.0","B.2.1a","Requirement","ECSS-Q-ST-60-12_0190210",1,"Created","The compliance matrix shall summarise the following:\n    1. The function description and associated main characteristics.\n    2. The software or hardware used for the design.\n    3. Verification that the circuit belongs to the specified functional domain and is designed using, for example, the models and cells, described in the design manual. If not, an extension of the qualification domain shall be provided.\n    4. The results of the sensitivity and stability analyses.\n    5. The derating of the elementary parts.\n    6. The DRC results.\n    7. The ERC results.\n    8. Verification from the manufacturer that he can perform the set of tests specified by the designer for the wafer or dies release."]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-70-02_0510013",1,"Created","Samples shall only be handled with clean nylon or lint-free gloves."]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","5.2.4.2m","Requirement","ECSS-Q-ST-70-02_0510038",1,"Created","A pressure of 10-4 Pa shall be reached within one hour with an unloaded system. "]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","5.3.2.14a","Recommendation","ECSS-Q-ST-70-02_0510155",1,"Created","In cases where the CVCM outgassing requirements are more stringent than the standard detection limits, a quartz crystal microbalance should be installed as a fourth collector plate. \n    NOTE 1 See clause 5.5.2\n    NOTE 2 The infrared transmission data (see 5.3.2.12) can also be used for equivalent mass determination as the intensities of the infrared absorption bands are related to the mass of the contaminants by the law of Lambert-Beer."]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","5.7.2.4b","Requirement","ECSS-Q-ST-70-02_0510104",1,"Created","The supplier shall perform the actual test with identical conditions and procedure as the normal Micro-VCM-test as described in clause 5.3.2."]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","B.2.1<5>a","Requirement","ECSS-Q-ST-70-02_0510129",1,"Created","The Micro-VCM worksheet shall contain a test reference number."]
["ECSS-Q-ST-70-02C","ECSS - Current v1.0","C.2.1<7>a","Requirement","ECSS-Q-ST-70-02_0510138",1,"Created","The Micro-VCM datasheet shall describe the use and location of the materials in the spacecraft."]
["ECSS-Q-ST-70-03C","ECSS - Current v1.0","5.2i","Requirement","ECSS-Q-ST-70-03_0520013",1,"Created","Lint-free gloves or surgical latex talc-free gloves shall be worn during selection and preparation of the parts.\n    NOTE 1 Other surface treatments can be applied to the part to improve the quality of the surface or increase its roughness.\n    NOTE 2 Masking can be applied to the parts not to be anodized."]
["ECSS-Q-ST-70-03C","ECSS - Current v1.0","5.6.3.2a","Requirement","ECSS-Q-ST-70-03_0520043",1,"Created","Thermo-optical properties of the parts shall be measured according to ECSS-Q-ST-70-09 to verify the following requirements:\n    1. Solar absorptance (as) at least 0,93, and\n    2. Normal emittance (en) at least 0,90.\n        NOTE The colour uniformity assessed by visual inspection is not directly linked to the above measurements, as the wavelengths of interest are not the same. The absorbtance and emittance uniformity is therefore often verified using the visual colour uniformity as input."]
["ECSS-Q-ST-70-03C","ECSS - Current v1.0","5.6.3.3e","Requirement","ECSS-Q-ST-70-03_0520052",1,"Created","The welding process shall be verified during production with dedicated engineering samples."]
["ECSS-Q-ST-70-04C","ECSS - Current v1.0","5.1.3.1d","Requirement","ECSS-Q-ST-70-04_0530013",1,"Created","The test procedure for controlling and monitoring the contamination shall contain the following information:\n    1. contamination check methods used during tests,\n    2. contamination results."]
["ECSS-Q-ST-70-04C","ECSS - Current v1.0","5.3.3a","Requirement","ECSS-Q-ST-70-04_0530046",1,"Created","Acceptance criteria shall be defined (beforehand) in common agreement between the test authority and the customer."]
["ECSS-Q-ST-70-06C","ECSS - Current v1.0","5.1.2.4c","Requirement","ECSS-Q-ST-70-06_0550013",1,"Created","Depending on the properties to be measured, the supplier shall use a particles fluxes or an absorbed based simulation."]
["ECSS-Q-ST-70-06C","ECSS - Current v1.0","5.1.4.2e","Requirement","ECSS-Q-ST-70-06_0550029",1,"Created","Thermal effects on the sample shall be assessed during radiation to ensure that the maximum temperature is not exceeded."]
["ECSS-Q-ST-70-06C","ECSS - Current v1.0","5.3.1a","Requirement","ECSS-Q-ST-70-06_0550054",1,"Created","The test records of the radiation test shall be retained for, at least, ten years or in accordance with project contract requirements."]
["ECSS-Q-ST-70-06C","ECSS - Current v1.0","C.2.1a","Requirement","ECSS-Q-ST-70-06_0550079",1,"Created","The radiation test report shall include or refer to the following information:\n    1. description of the purpose, objective, content and the reason prompting its preparation,\n    2. description of the radiation test facility,\n    3. description of the item to be tested or a reference to the document containing its identification characteristics (e.g. request for radiation testing),\n    4. calibration tools, flux monitoring method, (periodic adjustments or controlled constant flux),\n    5. the test procedure or a reference to the document containing the description of the test procedure ( e.g. radiation test specifications and procedure DRD),\n        NOTE It often consist in describing the as- run test procedure as well as any deviation from the initial test procedure (including a discussion of possible effect on test).\n    6. the irradiation source characterization (or a reference to the document containing this information,\n    7. the test results,\n    8. discussion about the tests results,\n    9. conclusion and recommendations."]
["ECSS-Q-ST-70-09C","ECSS - Current v1.0","A.2.1b","Requirement","ECSS-Q-ST-70-09_0580032",1,"Created","The report shall contain the name of the supplier through whom the purchase was made."]
["ECSS-Q-ST-70-09C","ECSS - Current v1.0","B.2.1e","Requirement","ECSS-Q-ST-70-09_0580041",1,"Created","The audit / review report shall contain the audit findings."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.1.4.4a","Requirement","ECSS-Q-ST-70-18_0620025",1,"Created","The supplier shall use bending jigs to form the cable to predetermined shapes as identified by the engineering drawing.\n    NOTE An example of such a bending jig is shown in Figure C-2."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.2.5f","Requirement","ECSS-Q-ST-70-18_0620058",1,"Created","The supplier shall not use pure tin or cadmium finishes."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.3.5.2d","Requirement","ECSS-Q-ST-70-18_0620081",1,"Created","The rate of change of temperature shall not exceed 2 °C per minute.\n    NOTE Recommendations for dealing with special requirements (e.g. higher operating temperature extremes) can be obtained from cable manufacturers."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.5.1.1.1e","Requirement","ECSS-Q-ST-70-18_0620115",1,"Created","After the solder has solidified and cooled, the supplier shall clean the joint with one of the solvent cleaners specified in clause 5.2.3."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.5.1.2a","Requirement","ECSS-Q-ST-70-18_0620124",1,"Created","The supplier shall assemble the connector to the cable-end in conformance with the requirements 5.5.1.2b to 5.5.1.2r."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.5.3e","Requirement","ECSS-Q-ST-70-18_0620149",1,"Created","The supplier shall store the cable in a suitable container inside a sealed bag with an inert atmosphere."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","5.7.3c","Requirement","ECSS-Q-ST-70-18_0620182",1,"Created","The severity of the vibration tests shall not be inferior to that shown in the following tables of ECSS-Q-ST-70-08:\n    1. Sine survey\n    2. Minimum severity for sine vibration testing\n    3. Minimum severity for random vibration testing for all applications except launchers\n    4. Minimum severity for random vibration testing for launchers."]
["ECSS-Q-ST-70-18C","ECSS - Current v1.0","A.2.1f","Requirement","ECSS-Q-ST-70-18_0620207",1,"Created","The logbook shall contain the finding and related corrective action raised during the audit."]
["ECSS-Q-ST-70-20C","ECSS - Current v1.0","5.2.1g","Requirement","ECSS-Q-ST-70-20_0630012",1,"Created","The supplier shall prepare the second test sample for the corrosion test by removing the outer insulation jacket partially by using the scalpel blade."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","5.1.1.2.2a","Requirement","ECSS-Q-ST-70-21_0640007",1,"Created","The supplier shall avoid contamination of the sample during handling.\n    NOTE This can be achieved by the use of, for instance, suitable protective gloves."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","5.1.2.2.4d","Requirement","ECSS-Q-ST-70-21_0640032",1,"Created","Feed-throughs shall be available for gas inlets, evacuation, venting to air, and electricity for ignition."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","5.1.2.3.4c","Requirement","ECSS-Q-ST-70-21_0640065",1,"Created","The sheet shall be rolled into a compact roll, and shall be surround with glass fibre to form a bar."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","5.1.2.4.1a","Requirement","ECSS-Q-ST-70-21_0640074",1,"Created","The supplier shall use the electrical wire insulation flammability test only for gauges AWG 20 to AWG 10 with copper conductors and for normal pressures with a maximum oxygen concentration of volume fraction 25 %."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","5.1.2.4.12a","Recommendation","ECSS-Q-ST-70-21_0640156",1,"Created","The supplier should run the pre-test procedure as described in annex B.3.1."]
["ECSS-Q-ST-70-21C","ECSS - Current v1.0","A.2.1<1.7>a","Requirement","ECSS-Q-ST-70-21_0640132",1,"Created","The test report shall describe the test atmosphere."]
["ECSS-Q-ST-70-22C","ECSS - Current v1.0","4.1.2.2a","Requirement","ECSS-Q-ST-70-22_0170004",1,"Created","Materials shall be labelled with the shelf-life and the date of the beginning of life or the date of manufacture (see clause 4.1.3).\n    NOTE In some critical applications, the project can reduce the shelf-life as originally stated by the manufacturer or supplier in order to meet particularly stringent product assurance requirements."]
["ECSS-Q-ST-70-22C","ECSS - Current v1.0","4.1.6a","Requirement","ECSS-Q-ST-70-22_0170018",1,"Created","Re-certification of material shelf-life shall be achieved by retesting the material to verify that its properties are still within their specified limits."]
["ECSS-Q-ST-70-28C","ECSS - Current v1.0","4.5b","Requirement","ECSS-Q-ST-70-28_0150023",1,"Created","The supplier shall remove components only if the mounting density is such that the integrity of other components in the vicinity can be ensured."]
["ECSS-Q-ST-70-28C","ECSS - Current v1.0","4.9.2b","Requirement","ECSS-Q-ST-70-28_0150048",1,"Created","The maximum wire diameter shall not be greater than two thirds of the width of the conductor."]
["ECSS-Q-ST-70-28C","ECSS - Current v1.0","4.14.1.2b","Requirement","ECSS-Q-ST-70-28_0150081",1,"Created","The supplier shall cover the wires with space-approved insulation. "]
["ECSS-Q-ST-70-28C","ECSS - Current v1.0","4.14.3a","Requirement","ECSS-Q-ST-70-28_0150090",1,"Created","After repair, the supplier shall inspect the soldered joints in conformance with the accept/reject criteria of clause 12 in ECSS-Q-ST-70-08. \n    ","NOTE For example: Inspection of the pad or track area to ensure that no lifting has occurred and that no damage has been sustained by the base material is one of the required inspections."]
["ECSS-Q-ST-70-28C","ECSS - Current v1.0","4.19.2a","Requirement","ECSS-Q-ST-70-28_0150114",1,"Created","The supplier shall retain the quality records (e.g. logbooks) for at least ten years or in conformance with project business agreement requirements,"]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","5.7.1.1a","Requirement","ECSS-Q-ST-40_0440024",1,"Unchanged","Safety analysis shall support the identification of sources of safety risk as well as the performance of preliminary trade-off analyses between alternative system concepts."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","5.8b","Requirement","ECSS-Q-ST-40_0440049",1,"Unchanged","The supplier shall include in his statement of compliance a statement that open verifications are followed up in the safety verification tracking log (SVTL), as defined in clause 8.5.1, and do not affect further safe processing."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","5.9.5a","Requirement","ECSS-Q-ST-40_0440058",1,"Unchanged","The supplier shall maintain records of personnel having received safety training in accordance with ECSS-Q-ST-20."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.3.3.4.2b","Requirement","ECSS-Q-ST-40_0440091",1,"Unchanged","The design shall tolerate a minimum number of credible failures and/or operator errors determined by the hazard consequence."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.3.6j","Requirement","ECSS-Q-ST-40_0440117",1,"Unchanged","A single failure shall not cause loss of the emergency and warning function."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.4.1m","Requirement","ECSS-Q-ST-40_0440324",1,"Created","The function criticality shall be assigned without taking into account any compensating provisions.","NOTE \tContinuing functional decomposition into lower-level functions, to distinguish between functions that could lead to different hazardous events, is not considered as creating compensating provisions.\n"]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.4.3.4a","Requirement","ECSS-Q-ST-40_0440160",1,"Unchanged","Materials shall be selected and controlled in accordance with ECSS-Q-ST-70."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.5.6.3d","Requirement","ECSS-Q-ST-40_0440328",1,"Created","In all situations there shall be sufficient time for the compensating provisions to intervene in order to prevent or mitigate the subject failure."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","6.6.3.4c","Requirement","ECSS-Q-ST-40_0440205",1,"Unchanged","The safety manager or safety relevant authority shall have the authority to stop any operation that does not conform to safety requirements. "]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","7.5.3a","Requirement","ECSS-Q-ST-40_0440230",1,"Informative Change","Safety risk assessment shall \n1.\tcomprise the identification, classification and ranking of safety risks and their contributors,\n2.\tbe based on deterministic hazard analysis by combining the consequence severity and the likelihood of occurrence of the consequence,\n3.\tbe used to facilitate effective and efficient safety risk reduction and control, \n4.\tsupport project risk management as defined in ECSS-M-ST-80, \n5.\tassess compliance with probabilistic safety targets.","NOTE \t1\tThe estimation of event likelihoods is based on the use of different sources of data i.e.: \n·\tprevious experience on the particular system (i.e. measured or observed directly relevant test or experience data), \n·\tdata from other systems or projects (i.e. extrapolation from generic data, similarity data, or physical models), and \n·\texpert judgment (i.e. direct estimation of likelihoods by domain specialists).\nNOTE \t2\tThe determination of likelihood is not a mean to downgrade the criticality of function.\n"]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","7.5.4.4.1a","Requirement","ECSS-Q-ST-40_0440239",1,"Unchanged","Multiple failures, which result from common-cause or common-mode failure mechanisms, shall be analysed as single failures for determining failure tolerance. "]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","8.3.4.2c","Requirement","ECSS-Q-ST-40_0440272",1,"Unchanged","The closeout shall be given by the approved launch authority procedure."]
["ECSS-Q-ST-40C Rev.1","ECSS - Current v1.0","8.6a","Requirement","ECSS-Q-ST-40_0440292",2,"Normative Change","All ground equipment that falls into the scope of an applicable ‘New Approach directive’ shall be ‘CE’ marked and supplied with a supporting ‘Declaration of Conformity’ and User Manual detailing all safety warnings.","NOTE \tAdditional information is provided in Informative Annex G.  \n"]
["ECSS-Q-ST-70-29C","ECSS - Current v1.0","4.1.1.3d","Requirement","ECSS-Q-ST-70-29_0650011",1,"Created","The supplier shall use all surfaces, tops, bottoms and sides to calculate the total surface area."]
["ECSS-Q-ST-70-29C","ECSS - Current v1.0","4.1.1.3e","Requirement","ECSS-Q-ST-70-29_0650012",1,"Created","In cases where the cut pieces of the sample do not fit into the container because of its size, the supplier shall cut two or more pieces, as long as 4.1.1.3d. is met."]
["ECSS-Q-ST-70-29C","ECSS - Current v1.0","4.4.1a","Requirement","ECSS-Q-ST-70-29_0650045",1,"Created","The test conditions shall be as follows:\n    1. Temperature: 50 °C ± 2 °C.\n    2. Atmosphere: at least 20,9 % oxygen, with the balance nitrogen or argon.\n    3. Pressure: 1 atmosphere pressure (1 013 hPa at 50 °C).\n    4. Duration: 72 hours ± 1 hour."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.1.3.3b","Requirement","ECSS-Q-ST-70-30_0120011",1,"Created","The following power-driven wire-wrapping tools shall be used:\n    1. electrical tool with mains supply,\n    2. pneumatic tool, supplied with regulated, lubricated and filtered air. \n        NOTE Figure A-1 shows examples of power-driven wire-wrapping tools."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.1.6.3a","Requirement","ECSS-Q-ST-70-30_0120038",1,"Created","After completion of the temperature cycling, the test samples shall be subjected to vibration."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.2.1.2d","Requirement","ECSS-Q-ST-70-30_0120047",1,"Created","The conductor diameter shall be within the range 0,25 mm to 0,51 mm nominal (30 AWG to 24 AWG), and from the following material:\n    1. soft-annealed, high-conductivity copper having an elongation at fracture of not less than 15 %, for wire gauges 24 AWG and 26 AWG, or\n    2. high-strength, high-conductivity copper alloy with less than 2 % strengthening elements, having an elongation at fracture of not less than 7 %, for wire gauges 28 AWG and 30 AWG.\n        NOTE These materials are suitable for use within the temperature range -55 °C to +100 °C."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.3.2.1b","Requirement","ECSS-Q-ST-70-30_0120082",1,"Created","Spacing between adjacent turns, the sum of all spaces within one wrap, and the distances for positioning wraps on the terminal post shall be as detailed in Figure 5-3. \n    NOTE This also gives the dimension limits for the minimum number of turns required."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.4.2a","Requirement","ECSS-Q-ST-70-30_0120104",1,"Created","Stripping force test shall be performed to determine adequate tightness of the wire around the terminal post. "]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.5.1e","Requirement","ECSS-Q-ST-70-30_0120137",1,"Created","The operator shall confirm that during visual inspection, the following criteria are met.\n    1. The silver plating on the conductor has no nicks or scratches exposing the base material (refer also to the requirements of clause 5.2.1).\n    2. The terminal posts conform with the requirements of clause 5.2.2.\n    3. Wire-wrap connections are clean and free of foreign material.\n    4. There is no evidence that the connection has been disturbed after manufacture.\n    5. The wire insulation makes captive contact with at least three corners of the terminal. \n    6. There is no overlapping between two adjacent connections on the same terminal post (see Figure 5-4, case B).\n    7. Uniformity and correct positioning of the wrap on the terminal post conform with the requirements of clause 5.3.2.1 and Figure 5-3.\n    8. The number of turns of conductor conforms to the requirements of clause 5.3.3 and Table 5-2.\n    9. The end tail conforms to the requirements of clause 5.3.3 (see Figure 5-4, case E).\n    10. No overlapping turns are present within the wrap joint (see Figure 5-4, case F).\n    11. The conductor is tightly wrapped onto the terminal post. \n    12. The maximum spacing between adjacent turns does not exceed 1/2 the diameter of the uninsulated conductor, and, excluding first and last turns, the sum of all gaps does not exceed the conductor diameter (see Figure 5-3).\n    13. The insulated wire is routed in a manner which does not tend to unwrap the wire on the terminal post."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.5.2a","Requirement","ECSS-Q-ST-70-30_0120138",1,"Created","Defective wire and posts shall be replaced."]
["ECSS-Q-ST-70-30C","ECSS - Current v1.0","5.6.7b","Requirement","ECSS-Q-ST-70-30_0120171",1,"Created","A training programme shall be developed, maintained and implemented to provide for excellence of workmanship and personnel skill, careful and safe operations, and improvement of the quality of wrapped joints."]
["ECSS-Q-ST-70-36C","ECSS - Current v1.0","5.3b","Requirement","ECSS-Q-ST-70-36_0670018",1,"Created","The supplier shall include both the residual stress distribution and the grain orientation in designing a part to be machined from wrought aluminium."]
["ECSS-Q-ST-70-36C","ECSS - Current v1.0","C.2.1<12>a","Requirement","ECSS-Q-ST-70-36_0670043",1,"Created","Any processes used for reducing tensile stresses shall be noted, if relevant.\n    NOTE For example: Shot peening or stress-relief treatments."]
["ECSS-Q-ST-70-37C","ECSS - Current v1.0","5.1b","Requirement","ECSS-Q-ST-70-37_0680002",1,"Created","The test solution shall be 3.5 weight percent sodium chloride in water."]
["ECSS-Q-ST-70-37C","ECSS - Current v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-70-37_0680021",1,"Created","For specimens to be taken from material less than 12 mm thick, the supplier shall use flat specimens of the type shown in Figure 5-2."]
["ECSS-Q-ST-70-37C","ECSS - Current v1.0","5.3.3.3a","Requirement","ECSS-Q-ST-70-37_0680054",1,"Created","The supplier shall classify alloys or weldments as moderate if the following applies:\n    1. none of the three stress-corrosion specimens fails in the thirty-day test. Any failure is disregarded if the tensile strength of the unstressed control specimen removed from test at the time of failure of the stress-corrosion specimen does not exceed the stress-corrosion test stress; and\n    2. the average tensile strength of the two stress-corrosion specimens after the thirty-day test is not less than 90 % of that of the unstressed control specimens; and\n    3. metallographic examination at ×50 magnification shows evidence of stress-corrosion in any of the three stress-corrosion specimens."]
["ECSS-Q-ST-70-45C","ECSS - Current v1.0","5.3.4b","Requirement","ECSS-Q-ST-70-45_0690016",1,"Created","A minimum number of three valid tests, in conformance with the validity criteria of ASTM E 1290, shall be carried out for each set of material and test condition."]
["ECSS-Q-ST-70-45C","ECSS - Current v1.0","5.4.1a","Requirement","ECSS-Q-ST-70-45_0690017",1,"Created","Test apparatus, specimens, test procedures, precision and bias shall be in conformance with ASTM E 466."]
["ECSS-Q-ST-70-45C","ECSS - Current v1.0","5.9c","Requirement","ECSS-Q-ST-70-45_0690050",1,"Created","Statistical analysis of numerical results of fatigue tests shall be conducted in conformance with clause 5.4.1g."]
["ECSS-Q-ST-70-45C","ECSS - Current v1.0","5.12.5d","Requirement","ECSS-Q-ST-70-45_0690069",1,"Created","The customer shall authorize disposal of materials and specimens."]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.1.3a","Requirement","ECSS-Q-ST-70-46_0700009",1,"Created","Fastener heads shall be formed by hot or cold forging before heat treating.","NOTE Driving recesses and lightening holes in double hexagon design can be forged or machined."]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.1.5d","Requirement","ECSS-Q-ST-70-46_0700018",1,"Created","There shall be no machining or etching of the fillet radius after rolling."]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.2.2a","Requirement","ECSS-Q-ST-70-46_0700043",1,"Created","Nominal dimensions shall be in accordance with the detail drawings of the customer specification document for threaded fasteners. "]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.3.2.2b","Requirement","ECSS-Q-ST-70-46_0700076",1,"Created","For fasteners with nominal diameter greater than 6 mm, hardness shall be measured in the centre of the circular surface and at two other locations at different distances from the centre of the surface, Figure 4-5."]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.3.6.2a","Requirement","ECSS-Q-ST-70-46_0700109",1,"Created","The percent elongation after fracture, the reduction of area at failure and the time to fracture shall be within the values specified in the customer specification document for threaded fasteners."]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.3.7.1a","Requirement","ECSS-Q-ST-70-46_0700110",1,"Created","Fasteners shall be tested for corrosion in accordance with ASTM B 117-07a. "]
["ECSS-Q-ST-70-46C Rev. 1","ECSS - Current v1.0","4.4.2.6f","Requirement","ECSS-Q-ST-70-46_0700144",1,"Created","Only qualified test laboratories shall carry out the tests."]
["ECSS-Q-ST-70-53C","ECSS - Current v1.0","5.2.2.2b","Requirement","ECSS-Q-ST-70-53_0990020",1,"Created","Further cleaning or other treatments require customer approval."]
["ECSS-Q-ST-70-53C","ECSS - Current v1.0","B.2.1b","Requirement","ECSS-Q-ST-70-53_0990053",1,"Created","A financial and administrative proposal including:\n    1. Responsible person for the activity.\n    2. List of deliverable items.\n    3. Work breakdown structure defining the required operations and responsibilities.\n        NOTE I.e. preparation of specimens, testing, evaluation of results, reporting.\n    4. Time schedule.\n    5. Travel and subsistence plan (if applicable).\n    6. Itemized cost list.\n    7. Milestone payment plan."]
["ECSS-Q-ST-70-55C","ECSS - Current v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-70-55_1030007",1,"Created","The work area shall comply to the rules and guidelines of good laboratory practice."]
["ECSS-Q-ST-70-55C","ECSS - Current v1.0","5.4.3e","Requirement","ECSS-Q-ST-70-55_1030032",1,"Created","Traceability shall be maintained throughout the process from incoming inspection to final measurements and calculations, including details of the test equipment and personnel employed in performing the task."]
["ECSS-Q-ST-70-58C","ECSS - Current v1.0","5.2.4a","Requirement","ECSS-Q-ST-70-58_1040029",1,"Created","The biodiversity in bioburden controlled environments shall be characterized at the commissioning phase."]
["ECSS-Q-ST-70-58C","ECSS - Current v1.0","5.2.5.4b","Requirement","ECSS-Q-ST-70-58_1040044",1,"Created","The labelling of each sample shall include the following information as a minimum:\n    1. Collection site (facility).\n    2. Sampling location within facility.\n    3. Occupancy state at time of sampling.\n    4. No. of personnel present at time of sampling.\n    5. Date and time of collection.\n    6. Name of person collecting the sample.\n    7. Size of sample in units of m3 (volume) or cm2 (surface area).\n    8. Details of all activities being performed at the time of sampling.\n    9. Sampling method(s), in conformance with ECSS-Q-ST-70-55.\n    10. Analysis method(s), in conformance with ECSS-Q-ST-70-55.\n    11. Any deviations from the requirements of the sampling plan."]
["ECSS-Q-ST-70-58C","ECSS - Current v1.0","5.3e","Requirement","ECSS-Q-ST-70-58_1040062",1,"Created","The supplier shall submit the Cleanroom commissioning report in conformance with Annex D to the customer for approval "]
["ECSS-Q-ST-70-13C Rev. 1","ECSS - Current v1.0","5.1.3.2a","Requirement","ECSS-Q-ST-70-13_0610025",1,"Unchanged","The supplier shall environmentally condition the sample for a nominal 24 hour period at (22 ± 3) °C with a relative humidity of (55 ± 10) %.\n    ","NOTE 1 The humidity requirement can be achieved either in a conditioning room, or by dessicators filled with silica gel or a saturated salt solution.\nNOTE 2 A saturated salt solution of calcium nitrate gives approximately 51 % relative humidity at the testing temperature.\n"]
["ECSS-Q-ST-70-13C Rev. 1","ECSS - Current v1.0","5.3e","Requirement","ECSS-Q-ST-70-13_0610050",1,"Unchanged","The supplier shall report defects and the appearance of the fracture.\n    ","NOTE 1 Defects for instance can be air bubbles or material inclusions.\nNOTE 2 Appearance of the fracture for instance can be rough, ductile, smooth or brittle."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.1.1.3a","Requirement","ECSS-Q-ST-70-50_1140009",1,"Created","The following apparatus shall be used to perform a tape-lift analysis:\n    1. A low-tack, transparent adhesive tape with an adhesive force of less than 0,3 N/mm.\n    2. A tape that is free of particles, voids, bubbles, and other artefacts detrimental to the counting of particles.\n    3. A membrane filter with a pore size less than 1 µm, and a minimum diameter of 5 cm, which provides contrast with the particulate contaminants being analyzed.\n        NOTE The choice of the membrane filter depends upon the nature of the particles being analysed (e.g. a white membrane filter in the case of black particles and a black membrane filter in the case of white particles). Membrane filters can have grids when statistical counting is used.\n    4. A mask or gridded membrane filter to perform statistical counting on squares of pre-defined area.\n    5. Non-shedding and lint-free gloves.\n    6. Tweezers.\n    7. Scissors or a scalpel.\n    8. A clean container for the transport of the tape-lift sample to the measurement facility.","NOTE 1 A clean container is a container devoid of particulate that could influence the measurement of the tape-lift sample.\nNOTE 2 The container can be sealed to prevent external contamination from reaching the internal parts of the container."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.1.1.4i","Requirement","ECSS-Q-ST-70-50_1140018",1,"Created","The membrane filter/tape assembly shall be placed into the tape-lift sample holder and the sample holder lid closed."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.1.2.7a","Requirement","ECSS-Q-ST-70-50_1140042",1,"Created","The silicon wafer witness shall be analysed with the microscope counting method as specified in see 5.3."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.2.2.2b","Requirement","ECSS-Q-ST-70-50_1140069",1,"Created","The gas shall be chemically compatible with the membrane filter."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.4.5a","Requirement","ECSS-Q-ST-70-50_1140098",1,"Created","The cleaned sensor shall be packed in a re-useable self-sealing and clean antistatic bag, and returned after exposure."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","5.4.5b","Recommendation","ECSS-Q-ST-70-50_1140214",1,"Created","The bag specified in 5.4.5a should be made of polyethylene."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","6.2j","Requirement","ECSS-Q-ST-70-50_1140128",1,"Created","Any anomalies or observations shall be noted on a dedicated inspection sheet in the form of a sketch or photograph."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","6.4.3b","Requirement","ECSS-Q-ST-70-50_1140149",1,"Created","A risk assessment shall be made prior to the inspection to assess any risks of damage to the spacecraft hardware taking into account the accessibility of the area to be inspected."]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","C.2.1<14>a","Requirement","ECSS-Q-ST-70-50_1140181",1,"Created","The report shall contain the results of all particle contamination measurements carried out. "]
["ECSS-Q-ST-70-50C","ECSS - Current v1.0","D.2.1<8>a","Requirement","ECSS-Q-ST-70-50_1140192",1,"Created","The report shall define what specific inspection method has been used."]
["ECSS-Q-ST-70-56C","ECSS - Current v1.0","5.2.4c","Requirement","ECSS-Q-ST-70-56_1230014",1,"Created","Positive controls shall be used to ensure that the BIs and the growth medium used for the bioburden reduction process control are in good order."]
["ECSS-Q-ST-70-57C","ECSS - Current v1.0","5.1d","Requirement","ECSS-Q-ST-70-57_1240004",1,"Created","Upon approval by the customer, the supplier shall implement the dry heat bioburden reduction."]
["ECSS-Q-ST-70-57C","ECSS - Current v1.0","5.4e","Requirement","ECSS-Q-ST-70-57_1240029",1,"Created","The equipment used for bioburden reduction shall include instrumentation to monitor, control and record the following process parameters:\n    1. Temperature\n    2. Time\n    3. Chamber pressure and airflow\n    4. Humidity, if applicable"]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.1a","Requirement","ECSS-Q-ST-20-07_0370001",1,"Created","The space test centre shall operate a quality management system in compliance with requirements from the EN 9100:2009."]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.4.2d","Requirement","ECSS-Q-ST-20-07_0370034",1,"Created","The space test centre shall establish and implement criteria for managing the competences and the authorisation to perform the test centre activities."]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.5.3g","Requirement","ECSS-Q-ST-20-07_0370059",1,"Created","For a space test centre where flight hardware is exposed, the minimum cleanliness level of the environment for airborne particles shall be ISO class 8."]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.6.3e","Requirement","ECSS-Q-ST-20-07_0370084",1,"Created","The Calibration Plan specified in the requirement 5.6.3d shall include: \n1.\ta unique identification of the equipment to be calibrated,\n2.\tthe calibration activities with their periodicity, \n3.\tthe applicable specification, \n4.\tthe identified resources."]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.6.4f","Requirement","ECSS-Q-ST-20-07_0370099",1,"Created","Records of the performance of the maintenance activities shall be available. "]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.7.4.1a","Requirement","ECSS-Q-ST-20-07_0370124",1,"Created","The space test centre shall ensure that all tests are documented in test reports. "]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","5.8.2e","Requirement","ECSS-Q-ST-20-07_0370157",1,"Created","Space test centre NCRs affecting the test specimen and any other customer property or the test programme shall be notified to the customer. "]
["ECSS-Q-ST-20-07C","ECSS - Current v1.0","A.2.1<3>a","Requirement","ECSS-Q-ST-20-07_0370182",1,"Created","In case of the answer \"Yes\" in Questionnaire Part 1 and Part 2 the customer shall provide the following:\n1.\tBrief description of each task or operation with identification of hazardous operations.\n2.\tIdentification of the operating location for the hazardous operations within the testing area or departing and arriving areas.\n3.\tSpecific hazards to which personnel are exposed during the operation.\n4.\tConfiguration of the test specimen prior to, during, and at completion of each hazardous operation, including all the GSE.\n5.\tIdentification of the failure tolerances  and the means for verifying that the failure tolerances are in place and operational.\n6.\tIdentification of any conditions that cause the operation to be considered hazardous.\n7.\tIdentification, of the safety precautions to be taken for each activity, hazardous or not, where specific guidelines are observed or actions are taken to prevent or limit hazards.\n8.\tIdentification, of procedures involving manually controlled pressurization of systems where the maximum operating pressure is reached.\n9.\tIdentification of organizational elements and facilities applicable to support the operations.\n10.\tIdentification of tools, equipment, and clothing for the safe performance of a hazardous operation or for emergency procedures associated with the operation. \n11.\tInitial identification of the emergency or contingency actions for each hazardous operation. \n12.\tInitial identification of the emergency or contingency actions specified in the requirement A.2.1<3>a.11 contains the following information: \n(a)\tspecific actions to cope with emergency or contingency conditions and identification of the individuals directing the actions; \n(b)\thazards unique to the operation and steps for rendering safe  to protect personnel and equipment.\n13.\tEvidence of customer’s past experience in the handling of hazardous items. \n14.\tReference to previous safety procedures and hazard analyses carried out for other projects.\n15.\tRecommendation of special provisions to be furnished the space test centre or possible test facility upgrading to minimize risk.","NOTE 1\tExamples of specific hazards for 3 are: pyrotechnics, and propellants. \nNOTE 2\tExamples of failure tolerances for 5 are: redundancies, safety devices, inhibits.\nNOTE 3\tExamples of support to operations for 9 are: safety officer, security, and medical.\nNOTE 4\tExamples of hazards for 12 are: pressure relief, and operation abort."]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","4.2g","Requirement","ECSS-Q-ST-20-08_1170008",1,"Created","Test or stimulus points shall be accessible without the need to disconnect or deroute flight harness of an item of equipment."]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","5.5.1b","Requirement","ECSS-Q-ST-20-08_1170038",1,"Created","The Pre-storage review shall:\n1.\tconfirm the configuration of the item to be stored as agreed in the Storage Plan in conformance with DRD from Annex A including status of all RFD or RFWs, NCRs and open work;\n2.\tensure that storage documentation, specified in the requirements from the clause 5.2, is available and covers all storage activities and duration;\n3.\tensure that storage resources are available in terms of tools, storage support equipment’s, facilities and personnel and fulfil the conditions documented in the storage plan;\n4.\tconclude on the acceptability to start the storage;\n5.\tidentify periodic inspection and testing."]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","6.2.6a","Requirement","ECSS-Q-ST-20-08_1170063",1,"Created","History of MGSE shall be recorded in its log book in conformance with the DRD from the Annex C of the ECSS-Q-ST-20 and made available to the user."]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","7.3d","Requirement","ECSS-Q-ST-20-08_1170096",1,"Created","Each supplier responsible for the transport shall nominate a person responsible for all transport activities."]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","7.8.1d","Requirement","ECSS-Q-ST-20-08_1170124",1,"Created","For P3 products, the packaging shall protect them against the risks of T3 transports. "]
["ECSS-Q-ST-20-08C","ECSS - Current v1.0","7.8.2d","Requirement","ECSS-Q-ST-20-08_1170133",1,"Created","The container for the units shall be labelled, tagged or marked to allow detailed identification of the contents of the container, with at least the following:\n1.\tName of manufacturer and customer of the flight hardware\n2.\tProject name\n3.\tUnit name and model\n4.\tConfiguration Item number\n5.\tPart number\n6.\tQuantity or weight (kg)"]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","7.1.1a","Requirement","ECSS-Q-ST-70-39_1280025",1,"Created","The manufacturer of welded joints shall be audited by the welding supervisor to demonstrate that the workshop facilities and equipment are capable of performing the welding operation."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","7.3.4d","Requirement","ECSS-Q-ST-70-39_1280049",1,"Created","Tooling and fixtures shall not be a source of contamination to the joint. "]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","8.1.5c","Requirement","ECSS-Q-ST-70-39_1280070",1,"Created","Pre-weld cleaning of contaminants detrimental to weld quality on filler materials and surfaces to be welded shall be performed in an environment which cannot degrade the quality of the weld. "]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","9.1.2f","Requirement","ECSS-Q-ST-70-39_1280087",1,"Created","Welded titanium joints shall be acceptable in the following cases:\n1.\twhen the colour of the joint is equal or better than brown in conformance with the colours from the Table 9-1,\n2.\tdiscoloration is removed prior to additional welding,\n3.\tat least 25 μm thickness of material is removed.\n","NOTE\tExamples of weld discoloration for titanium welds are shown in the Table 9-2."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","9.2.2b","Requirement","ECSS-Q-ST-70-39_1280113",1,"Created","Measurements for arc welds shall be made in accordance with ISO 9015-1:2001 and ISO 9015-2:2003.","NOTE\tASTM E384 is an equivalent standard."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","11.4c","Requirement","ECSS-Q-ST-70-39_1280150",1,"Created","When a delta verification is performed, two additional welds shall be produced for re-welding."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","12.2.1i","Requirement","ECSS-Q-ST-70-39_1280175",1,"Created","Malfunctions of the welding equipment shall be documented in the Logbook in conformance with the DRD from Annex C from ECSS-Q-ST-20."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","13.1a","Requirement","ECSS-Q-ST-70-39_1280185",1,"Created","All changes to the WPS from DRD from Annex A shall be controlled in conformance with t ECSS-M-ST-40."]
["ECSS-Q-ST-70-39C","ECSS - Current v1.0","A.2.1<2.1>a","Requirement","ECSS-Q-ST-70-39_1280218",1,"Created","In addition to the requirements specified in the clause A.2.1<1>, the WPS for mechanised arc welding shall contain as a minimum, the following additional information:\n1.\tElectrical parameters:\n(a)\tType of current: AC or DC and polarity,\n(b)\tPulse welding details: machine settings, programme selection,\n(c)\tCurrent range,\n(d)\tVoltage range,\n(e)\tSlope profile.\n2.\tMechanical parameters:\n(a)\tTravel speed range,\n(b)\tWire or strip feed speed range.\n3.\tIn case the equipment does not permit control of one of either variable specified in the requirements A.2.1<2.1>a1 and A.2.1<2.1>a2, the machine settings are specified instead.\n4.\tOther parameters:\n(a)\tTorch, electrode or wire angle,\n(b)\tFor mechanized and automatic welding maximum weaving or amplitude, frequency and dwell time of oscillation.","NOTE\tFor the requirement A.2.1<2.1>a3 the range of application for the WPS is then limited to equipment of that particular type."]
["ECSS-Q-ST-10C Rev.1","ECSS - Current v1.0","5.1.1.3c","Requirement","ECSS-Q-ST-10_0360010",1,"Unchanged","Reviews and audits of the product assurance programme, of processes or of product shall be carried out by personnel not directly involved in the work being performed."]
["ECSS-Q-ST-10C Rev.1","ECSS - Current v1.0","5.1.2d","Requirement","ECSS-Q-ST-10_0360014",1,"Unchanged","The PA manager shall interface with lower-tier suppliers regarding all Product Assurance matters."]
["ECSS-Q-ST-10C Rev.1","ECSS - Current v1.0","5.2.5d","Requirement","ECSS-Q-ST-10_0360043",1,"Unchanged","The PA manager shall identify the project documents requiring approval including those requiring approval by PA."]
["ECSS-Q-ST-70-14C","ECSS - Current v1.0","5.1a","Requirement","ECSS-Q-ST-70-14_1340001",1,"Created","The supplier shall identify, the applicable classes of environments from the list specified in the Table 5-1 to which space flight hardware materials are exposed during hardware life cycle on ground or during mission.","NOTE \tA non-exhaustive list of standards that can be agreed between customer and supplier is given in the bibliography of this standard.\n"]
["ECSS-Q-ST-70-14C","ECSS - Current v1.0","5.5.2f","Permission","ECSS-Q-ST-70-14_1340070",1,"Created","Austenitic stainless steel brushes may be used on other alloy classes provided that:\n1.\tuse of the brush is restricted to a single alloy, or\n2.\tthe brush is cleaned, rinsed, and dried before use on a different alloy."]
["ECSS-Q-ST-70-14C","ECSS - Current v1.0","5.7.1a","Requirement","ECSS-Q-ST-70-14_1340055",1,"Created","All inorganic finishes shall be verified in compliance with requirements from clause 5.5."]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","4.3b","Requirement","ECSS-Q-ST-30_0410005",2,"Normative Change","The plan shall address the dependability requirements applicable to the project."]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","5.2b","Requirement","ECSS-Q-ST-30_0410027",1,"Unchanged","Dependability requirements shall be apportioned, in a top-down process, to establish dependability requirements for lower level elements. "]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","5.4.1f","Requirement","ECSS-Q-ST-30_0410130",1,"Created","The criticality of hardware and operations shall be determined in accordance with the highest criticality of functions implemented.","NOTE \tFor the criticality categorization of software, see clause 5.4.2.\n"]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","5.5a","Requirement","ECSS-Q-ST-30_0410047",1,"Unchanged","The supplier shall ensure that dependability aspects are covered in all development, qualification and acceptance test planning and reviews, including the preparation of test specifications and procedures and the evaluation of test results. "]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","6.4.2.1b","Requirement","ECSS-Q-ST-30_0410072",1,"Unchanged","The reliability data sources and methods used in reliability predictions shall be as specified by the customer. "]
["ECSS-Q-ST-30C Rev.1","ECSS - Current v1.0","6.5c","Requirement","ECSS-Q-ST-30_0410105",2,"Deleted","<<deleted>>."]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.1.1.3d","Requirement","ECSS-Q-ST-70-26_0130009",1,"Unchanged","Fresh air shall be supplied to the room through a filtering system with positive pressure difference with regard to adjacent rooms."]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.1.2.4a","Requirement","ECSS-Q-ST-70-26_0130032",2,"Normative Change","The supplier shall provide the equipment specified in Table 5-1 necessary for verification activities specified in clause 5.4.3. "]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.2.1h","Requirement","ECSS-Q-ST-70-26_0130040",2,"Normative Change","The supplier shall use tools as specified in SAE-AS-22520 for the crimp contact configuration.","NOTE \tExamples of crimping parameters are given in Table A-1 to Table A-6\n"]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.2.6d","Requirement","ECSS-Q-ST-70-26_0130174",1,"Created","Only one braided shield shall be crimped in one ferrule connection."]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.3.4.1a","Permission","ECSS-Q-ST-70-26_0130223",1,"Created","For wires qualified by ESCC the qualified tool set-up may be used without additional validation when different batches of wires are used."]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.4.2c","Requirement","ECSS-Q-ST-70-26_0130088",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.4.4e","Requirement","ECSS-Q-ST-70-26_0130100",1,"Unchanged","The specimen shall be ground with the aid of appropriate grades of silicon carbide papers, in order to expose the mid-section of the joint. "]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.5.5g","Requirement","ECSS-Q-ST-70-26_0130133",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-26C Rev.1 Corr.1","ECSS - Current v1.0","5.5.8a","Requirement","ECSS-Q-ST-70-26_0130155",2,"Normative Change","The QA organization of the supplier shall disposition any nonconformance which is observed in respect of the process in conformance with the quality assurance requirements, in conformance with ECSS-Q-ST-10-09. "]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","5.2.2.1a","Requirement","ECSS-Q-ST-10-09_0350011",1,"Unchanged","The supplier shall nominate and authorize the internal NRBs core members for the business agreement."]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","5.2.2.3c","Requirement","ECSS-Q-ST-10-09_0350020",1,"Unchanged","The internal NRB shall analyse whether human error or poor workmanship are the primary or secondary cause for the nonconformance."]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","5.3b","Requirement","ECSS-Q-ST-10-09_0350045",1,"Unchanged","The NRB shall determine also preventive actions to avoid the occurrence of the nonconformance on similar items."]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","6.3.1a","Requirement","ECSS-Q-ST-10-09_0350078",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","6.3.2.3a","Requirement","ECSS-Q-ST-10-09_0350087",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-10-09C Rev. 1","ECSS - Current v1.0","A.2.1<39>a","Recommendation","ECSS-Q-ST-10-09_0350148",1,"Created","The NCR should additionally contain the following information: \n    1. Related internal NCR\n    2. NCR title\n    3. Next higher assembly\n    4. Subsystem / Model reference \n    5. Identification of violated requirements \n    6. Customer notification (date and reference ) \n    7. Alert identification "]
["ECSS-Q-ST-70-17C","ECSS - Current v1.0","5.1b","Requirement","ECSS-Q-ST-70-17_1380002",1,"Created","The substrate material and surface finish shall be representative of the final product."]
["ECSS-Q-ST-70-17C","ECSS - Current v1.0","6.2d","Requirement","ECSS-Q-ST-70-17_1380037",1,"Created","For ceramic coatings the adhesion test shall be performed in compliance with the requirements in ISO 2409:2007, without cross cut."]
["ECSS-Q-ST-70-17C","ECSS - Current v1.0","6.5b","Requirement","ECSS-Q-ST-70-17_1380062",1,"Created","Test solvents shall be agreed between customer and supplier.","NOTE\t1\tThese solvents are normally agreed taking into account any restrictions due to compatibility with substrate.\nNOTE\t2\tCommon test solvents are deionized water, acetone, MEK, IPA, methyl/ethyl alcohol\n"]
["ECSS-Q-ST-70-17C","ECSS - Current v1.0","6.7e","Permission","ECSS-Q-ST-70-17_1380086",1,"Created","For very low dose the radiation test need not be performed if so agreed with the customer.","NOTE\tFor example, in category A and B.\n"]
["ECSS-Q-ST-70-31C Rev.1","ECSS - Current v1.0","4.2.2.1a","Requirement","ECSS-Q-ST-70-31_0660012",1,"Unchanged","The conditions for handling and storage of materials used in this process shall be clearly indicated to all operators and supervising staff."]
["ECSS-Q-ST-70-31C Rev.1","ECSS - Current v1.0","4.3.1.2b","Requirement","ECSS-Q-ST-70-31_0660046",1,"Unchanged","Surfaces shall be free of dust and grease.","NOTE \tThis can be achieved by standard cleaning procedures or by the manufacturer cleaning method.\n"]
["ECSS-Q-ST-70-31C Rev.1","ECSS - Current v1.0","4.3.1.3d","Requirement","ECSS-Q-ST-70-31_0660053",1,"Unchanged","The hardware shall be protected from random temperature extremes, high humidity and physical damage."]
["ECSS-Q-ST-70-31C Rev.1","ECSS - Current v1.0","4.3.4.2c","Requirement","ECSS-Q-ST-70-31_0660078",1,"Unchanged","Unmasking shall be performed carefully to avoid the starting of pulling stresses in the paint."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.2b","Requirement","ECSS-Q-ST-70-71_1260004",1,"Unchanged","Wrought alloys 5456, 5083 and 5086 shall be used only in controlled tempers for resistance to SCC and exfoliation.","NOTE\tExamples of controlled tempers are H111, H112, H116, H117, H323, H343.\n"]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.9d","Requirement","ECSS-Q-ST-70-71_1260037",1,"Unchanged","Alloys containing Beryllium higher than 4 % by weight shall not be used."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.11n","Requirement","ECSS-Q-ST-70-71_1260062",1,"Unchanged","Where void free application is used on coatings and varnishes the supplier shall apply a debubbling process, defined in a dedicated procedure."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.12i","Requirement","ECSS-Q-ST-70-71_1260070",1,"Unchanged","The exposure to the space environment shall not impair the function of the tape."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.17i","Requirement","ECSS-Q-ST-70-71_1260111",1,"Unchanged","Materials that liberate acetic acid shall be assessed before use."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.18l","Requirement","ECSS-Q-ST-70-71_1260126",1,"Unchanged","Materials that absorb and release water shall be assessed with respect to the effect on the performance of the material and for contamination risk."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.2.19c","Requirement","ECSS-Q-ST-70-71_1260135",1,"Unchanged","Curing processes shall be assessed by means of a preliminary test programme using thermal-analysis equipment."]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.3.4b","Requirement","ECSS-Q-ST-70-71_1260160",1,"Unchanged","Process conditions and environments shall be specified and controlled during all stages of painting, coating.","NOTE\tStages of painting, coating include for example preparation, application, curing or drying, inspection or testing and storage.\n"]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.3.9.2b","Requirement","ECSS-Q-ST-70-71_1260193",1,"Unchanged","The supplier shall demonstrate that when anodizing processes are applied to thin foils the complete removal of process chemicals in complex parts is ensured.","NOTE\tThin foils include for example honeycomb cores.\n"]
["ECSS-Q-ST-70-71C Rev.1","ECSS - Current v1.0","4.3.13a","Requirement","ECSS-Q-ST-70-71_1260218",1,"Unchanged","Heat treatment of metals and alloys shall conform to national or international specifications for aerospace applications approved by the customer."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","4.1.3c","Requirement","ECSS-Q-ST-70_0490194",1,"Unchanged","The supplier shall appoint a MMPP manager."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","4.2.2e","Requirement","ECSS-Q-ST-70_0490009",2,"Unchanged","The following constraints shall be assessed: \n1.\trequirements originating from the initial technical specification.\n2.\tprogrammatic project requirements and conditions."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","4.4c","Requirement","ECSS-Q-ST-70_0490031",2,"Unchanged","For cleanliness­ or contamination­critical applications, a chemical and particle requirement specification and a specific cleanliness control plan shall be established in conformance with DRDs from Annex A and Annex B of ECSS-Q-ST-70-01."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","5.1.11c","Requirement","ECSS-Q-ST-70_0490216",1,"Informative Change","The compatibility of materials which are or can come into contact with LOX or GOX shall be evaluated except the case specified in the requirement 5.1.11d.","See NASA-STD-6001 Tests No. 13 and No. 14."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","5.1.14b","Requirement","ECSS-Q-ST-70_0490219",1,"Unchanged","Use of materials shall comply with safety evaluation and assessment results concerning design and application criteria or details."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","5.2.2a","Requirement","ECSS-Q-ST-70_0490061",1,"Informative Change","Pure tin finish with more than 97 % purity shall not be used.","This is due to the possibility of whisker growth and transformation to grey tin powder at low temperatures."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","5.7.1b","Requirement","ECSS-Q-ST-70_0490087",1,"Unchanged","Any modification, change of condition or configuration of application shall lead to a re-evaluation in conformance with the process shown in Figure 4-1."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","6.2d","Requirement","ECSS-Q-ST-70_0490248",1,"Unchanged","The supplier shall be responsible for storing and maintain all mechanical parts data in an internal database."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","7.3d","Requirement","ECSS-Q-ST-70_0490253",1,"Unchanged","The access to the data, from requirement 7.3c, shall be granted to the customer."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","7.3m","Requirement","ECSS-Q-ST-70_0490262",1,"Unchanged","In the case of a process suspension for four months continuously, retraining and recertification shall be performed."]
["ECSS-Q-ST-70C Rev.2","ECSS - Current v1.0","7.7.3a","Requirement","ECSS-Q-ST-70_0490161",2,"Unchanged","Before implementation of a process, the supplier shall ensure that personnel are trained in accordance with the training and certification programme specified in 7.3f, 7.3g and 7.3h and that environment, means and documentation are adequate."]
["ECSS-Q-ST-60-14C Rev.1 Corr.1","ECSS - Current v1.0","4.1.6a","Requirement","ECSS-Q-ST-60-14_0470009",2,"Normative Change","EEE parts manufacturers requirements or, by default, ESCC 20600 or IPC/JEDEC J-STD-033D (April 2018) shall apply for packing, packaging and handling.\n"]
["ECSS-Q-ST-60-14C Rev.1 Corr.1","ECSS - Current v1.0","5d","Requirement","ECSS-Q-ST-60-14_0470016",2,"Normative Change","In absence of EEE manufacturer's lifetime limitation and when required, relifing shall be performed between T1 and T2 according to the timing parameters given in Table 5‑1.\n","NOTE \t1\tRelife can be anticipated before T1, provided dT remains applicable.\nNOTE \t2\tFor parts not planned to be mounted and to be kept in stock, relifing is not mandatory.\n"]
["ECSS-Q-ST-60-14C Rev.1 Corr.1","ECSS - Current v1.0","6.1.4d","Requirement","ECSS-Q-ST-60-14_0470066",1,"Created","External Visual Inspection shall be done in accordance with applicable procurement specifications.\n"]
["ECSS-Q-ST-60-14C Rev.1 Corr.1","ECSS - Current v1.0","7.5b","Requirement","ECSS-Q-ST-60-14_0470092",1,"Created","The Certificate of Conformity shall be attached with the components during their delivery.\n"]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","5.3.3a","Requirement","ECSS-Q-ST-30-11_0140010",1,"Informative Change","For a particular type or manufacturer, when a specific derating rule is defined in the appendix of the approved ESCC detail specification issued by the ESCC Executive, it shall take precedence over the generic requirement of this standard. ","NOTE \tThere are many misunderstandings about ratings vs derating. Specifications normally only contain ratings. The exceptions are listed in 5.3.3b.\n"]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.5.2a","Requirement","ECSS-Q-ST-30-11_0140036",1,"Unchanged","Parameters of capacitors from family-group code 01-05 shall be derated as per Table 6‑4."]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.8.1a","Recommendation","ECSS-Q-ST-30-11_0140171",2,"Normative Change","Internal heating due to ESR can increase ageing and should be taken into account by applying a margin in temperature."]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.15.2a","Requirement","ECSS-Q-ST-30-11_0140070",1,"Unchanged","Parameters of Diodes from family-group code 04-05, 04-11 to 04-13, 04-15, 04-16 and 04‑17 shall be derated as per Table 6‑15."]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.25.1i","Requirement","ECSS-Q-ST-30-11_0140196",1,"Created","When no minimum coil voltage is provided, the coil voltage shall be between 110 % of the maximum latch or reset or pick-up voltage over the full temperature range and the maximum coil voltage.","NOTE \tLatch or reset voltage are specified for latching device, pick-up voltage is specified for non-latching devices.\n"]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.26.2.2a","Requirement","ECSS-Q-ST-30-11_0140114",2,"Normative Change","Parameters of Metal film semi-precision resistor (type RLR) shall be derated as per Table 6‑26."]
["ECSS-Q-ST-30-11C Rev.2","ECSS - Current v1.0","6.31.2a","Requirement","ECSS-Q-ST-30-11_0140140",2,"Normative Change","Parameters of Transistors from family-group code 12-12, 12-14, 12-15(FET) and 12-16(FET) shall be derated as per Table 6‑38."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","5.1c","Requirement","ECSS-Q-ST-70-15_1470003",1,"Created","The design definition authority shall specify NDT acceptance criteria.","NOTE\tIt is assumed that accept and reject criteria reflect the possible need to ensure that cracks smaller than the targeted crack size are reported as “detected cracks” in line with ECSS-E-ST-32-01 clause 10.7 (for example > 50 % of the targeted crack size).\n"]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","5.4b","Requirement","ECSS-Q-ST-70-15_1470028",1,"Created","Configuration control shall be performed in compliance with ECSS-M-ST-40 for the following:\n1.\tPersonnel qualification and certification\n2.\tNDT specification\n3.\tNDT standards\n4.\tPart specific NDT procedures","NOTE\tIt is important that the meaning of NDT procedure, instruction, and specification is clarified between customer and supplier.\n"]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.2.2c","Requirement","ECSS-Q-ST-70-15_1470061",1,"Created","Inspection personal shall be qualified in accordance with the company written practice or EN ISO 9712:2012."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.3.2g","Requirement","ECSS-Q-ST-70-15_1470070",1,"Created","Penetrant testing shall be performed before any surface treatments, because they can have an unacceptable impact upon the sensitivity of the testing."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.4.2a","Requirement","ECSS-Q-ST-70-15_1470095",1,"Created","Except the cases specified in the requirements 6.4.2b and 6.4.2c, eddy current inspections shall be performed in accordance with EN ISO 15549:2019 or a standard approved by the customer."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.5.3.3c","Requirement","ECSS-Q-ST-70-15_1470131",1,"Created","The checking of wet particles concentration shall be performed in accordance with requirements from EN ISO 9934-1:2016, EN ISO 9934-2:2015, EN ISO 9934-3:2015."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.6.6b","Requirement","ECSS-Q-ST-70-15_1470152",1,"Created","The application of RT discontinuity detection shall be qualified in agreement with the customer as follows: \n1.\tOn pre-cracked specimens X-ray tests are performed in order to verify the sensitivity of the testing with respect to a discontinuity located in specific parts;\n2.\tSpecimen definition and selection is agreed with the customer."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.7.3.2b","Requirement","ECSS-Q-ST-70-15_1470161",1,"Created","Water based couplants shall not be used with materials prone to corrosion."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","6.7.7.2f","Requirement","ECSS-Q-ST-70-15_1470194",1,"Created","Ultrasonic testing for surface or embedded discontinuities in welds or in parent material surrounding the welds shall be in conformance with ASTM E 164:2019 or supplier internal specifications approved by the customer."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","8.6.2.2a","Requirement","ECSS-Q-ST-70-15_1470219",1,"Created","The NDT of a composite laminate or part that is cured and ready for further assembly or use shall be conducted using ultrasonic techniques to check for delamination cracks or voids which can reduce material performance."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","9.1.5b","Requirement","ECSS-Q-ST-70-15_1470252",1,"Created","Items to be tested using penetrant, shall have their mechanically disturbed surfaces etched prior to testing.","NOTE\tSee also clause 6.3 for the case of standard penetrant testing.\n"]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","9.2.1c","Requirement","ECSS-Q-ST-70-15_1470258",1,"Created","Personnel performing Special fracture control NDT activities shall be qualified and certified for each Special fracture control NDT method in accordance with NAS 410:2014 Level 2 and EN 4179:2017. "]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","9.2.3.2d","Requirement","ECSS-Q-ST-70-15_1470285",1,"Created","Standard X-ray radiographic fracture control NDT shall be performed in accordance with requirements from clause 6.6.7."]
["ECSS-Q-ST-70-15C","ECSS - Current v1.0","C.2.1a","Requirement","ECSS-Q-ST-70-15_1470318",1,"Created","The NDT Procedure shall include, date, issue and revision number."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","6.4d","Requirement","ECSS-Q-ST-70-12_1200018",1,"Unchanged","The serial number shall identify the position of the PCB on the panel."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.1.2c","Requirement","ECSS-Q-ST-70-12_1200023",1,"Informative Change","Except the case specified in the requirement 11.4.1e, the external and internal layers shall use basic copper thickness 70 µm, 35 µm or 17 µm.","NOTE \t1\tCopper layers can be implemented as copper clad laminate or as separate copper foils.\nNOTE \t2\tRequirement 11.4.1e specifies microvia layers on HDI PCBs.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.4.2c","Requirement","ECSS-Q-ST-70-12_1200044",1,"Unchanged","The use of planarization, copper reduction or surface preparation processes shall be excluded in the definition of the total copper thickness.","NOTE \t1\tPlating of sequential half stacks can be done with different plating methods, like panel plating, selective pattern plating or a combination and can include copper surface reduction processes to reduce copper surface thickness and give best options for fine pitch etching.\nNOTE \t2\tThe plated copper thickness as-designed is 25 µm. This can be a thicker layer as-manufactured.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.5.2a","Requirement","ECSS-Q-ST-70-12_1200065",2,"Normative Change","Non-functional pads in PTH shall be present on all layers, except two cases specified in the requirement 7.5.2b.","NOTE \tThe presence of non-functional pads reduce the risk of hole wall pull-away and reduce the risk of cracks in resin-rich areas.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.8.1f","Permission","ECSS-Q-ST-70-12_1200414",1,"Unchanged","Other surface finishes than the ones specified in the requirements from 7.8.1a to 7.8.1d may be used for non-soldering purpose."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.4a","Requirement","ECSS-Q-ST-70-12_1200091",1,"Unchanged","Tolerances on track width and spacing shall be as specified in the Table 7‑3."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.4j","Recommendation","ECSS-Q-ST-70-12_1200422",1,"Unchanged","The edge of the PCB should include on one side of the laminate a non-functional track as mechanical reinforcement with a width of ≥ 0,3 mm. ","NOTE \t1\tThis is indicated as “Ir” in Figure 8‑2.\nNOTE \t2\tThe non-functional track for mechanical reinforcement is named reinforcement strip.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.7.5e","Permission","ECSS-Q-ST-70-12_1200430",2,"Normative Change","The minimum as-manufactured annular ring on the component side may be 0.","NOTE \tThe as-manufactured annular ring is indicated with the red arrow in Figure 8‑8.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","9.5c","Requirement","ECSS-Q-ST-70-12_1200145",1,"Unchanged","Bending of the flex section shall be performed in conformance with the requirements from the clause 8.6."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","10.3.2b","Requirement","ECSS-Q-ST-70-12_1200152",1,"Unchanged","The copper or aluminium core shall have a protective layer to prevent corrosion.","NOTE \tThe type of protective layer is specified in the PCB definition dossier. Examples of protective layers to prevent corrosion are anodization, alodine, nickel plating, gold plating. These corrosion protections can have specific drawbacks for further PCB processing.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","10.4.4d","Requirement","ECSS-Q-ST-70-12_1200180",2,"Normative Change","The distance between a plated hole and the heat sink or insert shall be in conformance with the requirement 13.8.2k and values specified in the Table 13‑3."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","11.4.1m","Requirement","ECSS-Q-ST-70-12_1200552",1,"Created","For polyimide HDI technology as specified in 11.6a, the build-up of full microvia layers shall be maximum 2 on each side of the PCB."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","11.5.4a","Requirement","ECSS-Q-ST-70-12_1200450",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","12.3j","Requirement","ECSS-Q-ST-70-12_1200221",2,"Normative Change","The width of an embedded film resistor shall be ≥ 200 µm."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","12.5.1a","Requirement","ECSS-Q-ST-70-12_1200226",1,"Unchanged","The spacing and width for external layers of RF PCBs shall be in conformance with the values from Table 7‑4."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.6.2a","Requirement","ECSS-Q-ST-70-12_1200240",1,"Unchanged","The temperature increment of tracks with respect to the dielectric substrate shall be ≤ 10 °C."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.8.2e","Requirement","ECSS-Q-ST-70-12_1200258",1,"Unchanged","Insulation distance in Z direction for superimposed conductors shall be in conformance with values specified in Table 13‑3 and Table 13‑4.","NOTE \tThe requirements 7.1.3e and 10.3.1 also specify insulation distance of superimposed conductors, as explained in the clause 13.8.1.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.9.3.2c","Requirement","ECSS-Q-ST-70-12_1200285",1,"Unchanged","The insulation distance from a conductor to the PCB edge in conformance with the requirement 13.8.2h shall be doubled in case the PCB edge faces an external conductive element within a distance of less than 1 mm."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.9.3.3c","Requirement","ECSS-Q-ST-70-12_1200289",1,"Unchanged","A critical net shall be covered with conformal coating including the track, pads and component leads."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.12.3.1c","Recommendation","ECSS-Q-ST-70-12_1200496",1,"Unchanged","Direct coupling between bundles of non-critical signals specified in the requirement 13.12.3.1a should be avoided."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.3.2b","Requirement","ECSS-Q-ST-70-12_1200323",1,"Unchanged","The distance of components to adjacent surroundings shall be in conformance with values specified in Table 14‑2.","NOTE \tAn illustration is given in Figure 14‑2.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.5.2c","Permission","ECSS-Q-ST-70-12_1200516",2,"Normative Change","Pad designs may deviate from the requirements of clauses 14.5.3 to 14.5.7, in case the following conditions are met:\n1.\tthe existing pad designs are verified in accordance with clause 13 of ECSS-Q-ST-70-61, and\n2.\tinsulation distance is in conformance with requirement 14.5.2a.","NOTE \tThis requirement is defined to enable best practices as per recommendations from the EEE component manufacturer, and optimisation for assembly and PCB manufacturing.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.5.8c","Recommendation","ECSS-Q-ST-70-12_1200519",1,"Unchanged","The pad design for components of type AAD should be with via-in-pad technology."]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","5.2g","Recommendation","ECSS-Q-ST-70-16_1460007",1,"Created","The assessment should include, but is not limited to:\n1.\tJoints design \n(a)\tMechanical loads\n(b)\tThermo-mechanical loads\n(c)\tAdherends \n(d)\tGeometrical Configuration\n(e)\tShape of the bondline\n(f)\tNeed of NDI\n2.\tAdhesives properties\n(a)\tMechanical properties\n(b)\tThermo-mechanical properties\n(c)\tOffgassing\n(d)\tMoisture sensitivity\n(e)\tAppearance\n(f)\tSpecific properties \n3.\tProcessing\n(a)\tSurface preparation of adherends\n(b)\tCuring conditions: time to full cure, temperature, pressure, humidity, time to handling strength\n(c)\tAdhesive conditioning\n(d)\tViscosity\n(e)\tPot life \n(f)\tManual or machine processing \n(g)\tAdhesive filet removal (excess adhesive)\n(h)\tPackaging and storage\n4.\tGround, launch, and in-orbit environment\n(a)\tRadiation\n(b)\tVacuum\n(c)\tTemperature range\n(d)\tThermal cycling\n(e)\tChemical compatibility\n(f)\tStorage time and storage conditions\n5.\tProcurement\n(a)\tCost factors \n(b)\tLead time\n(c)\tExport control\n(d)\tObsolescence risk\n6.\tHealth and safety\n","NOTE\t1\tFor requirement 5.2g.1(e): The shape of the bondline refers, for example, to the presence/absence of an outer fillet (excess glue) \nNOTE\t2\tFor requirement 5.2g.2(d): Sensitivity can be related to water absorption, water content in the adhesive, water desorption, CME, water diffusion.\nNOTE\t3\tFor requirement 5.2g.2(d): Accelerated hot-wet tests can be performed within screening activities in order to determine the moisture sensitivity of representative assembly.\nNOTE\t4\tFor requirement 5.2g.2(e): Optical applications can require either transparent or dark glues. \nNOTE\t5\tFor requirement 5.2g.2(f): Specific properties include electrical, thermal, optical, thermo-optical properties. \nNOTE\t6\tFor requirement 5.2g.3(g)variations in adhesive processing can modify final adhesive properties \nNOTE\t7\tFurther information about selection of adhesives can be found in section 7 of ECSS-E-HB-32-21.\n"]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","7.4c","Requirement","ECSS-Q-ST-70-16_1460031",1,"Created","Any deviation between test items and flight hardware bonding procedure shall be justified and submitted for the customer approval.\n","NOTE\tDeviations can be related to differences in adhesive application, tooling manufacturing environment and to upscaling of in production.\n"]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","7.7.1c","Recommendation","ECSS-Q-ST-70-16_1460040",1,"Created","After each environmental exposure step, inspection of the test item set should be performed.\n"]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","7.12.2f","Requirement","ECSS-Q-ST-70-16_1460065",1,"Created","In addition to requirement 7.12.2b additional thermal cycles shall be performed to cover mission lifetime.\n","NOTE\t1\tThe additional thermal cycles are typically performed to simulate ageing effects (thermo-chemical, creep and fatigue phenomena).\nNOTE\t2\tThe additional thermal cycles can contain long term thermal endurance exposure, for example cruise phases of probes.\n"]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","8.8b","Requirement","ECSS-Q-ST-70-16_1460098",1,"Created","Bonded assemblies shall be free of defects that affect the intended use. \n","NOTE\tFor example cracks, entrapped air, kissing bonds, discoloration and particles can all affect bonding performance.\n"]
["ECSS-Q-ST-70-16C","ECSS - Current v1.0","B.2.1a","Requirement","ECSS-Q-ST-70-16_1460131",1,"Created","The adhesive bonding test plan shall contain the following information\n1.\tTest objective\n2.\tTest items \n(a)\tAdhesive and adherend materials\n(b)\tRepresentativeness of test items vs flight configuration\n(c)\tReference to the adhesive bonding procedure in conformance with DRD in Annex A\n(d)\tNumber of test sets and test items quantity in each set\n3.\tVerification Test sequence\n(a)\tList and designation of test item sets\n(b)\tApplicable test procedures\n(c)\tApplicable test standards\n(d)\tApplicable inspection procedures\n(e)\tSequence of consecutive exposures\n(f)\tInspections performed during verification sequence on each item set\n4.\tPass-fail criteria\n"]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","7.3a","Requirement","ECSS-Q-ST-70-80_1480026",1,"Created","The AM verification phase shall be split into two phases:\n1.\tAM verification on metallurgical and mechanical standard test specimens, in compliance with clause 7.4, and\n2.\tAM verification on prototypes: in compliance with clause 7.5."]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","7.5.2a","Requirement","ECSS-Q-ST-70-80_1480051",1,"Created","A prototype shall be built and tested for every new part design.","NOTE\tTesting of prototypes is done for manufacturing validation.\n"]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","7.8a","Requirement","ECSS-Q-ST-70-80_1480070",1,"Created","No repair of the manufactured part(s) or specimens shall be permitted during the verification phase."]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","8.3.2.1c","Requirement","ECSS-Q-ST-70-80_1480096",1,"Created","Metallography shall be performed for class 1.1 and 1.2 parts on the full height blanks in accordance with clause 12.5.1.1."]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","8.4.1d","Requirement","ECSS-Q-ST-70-80_1480105",1,"Created","If required in Table 8‑2 for the respective safety class, X-Ray CT testing shall be performed after the last heat- or HIP-treatment."]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","10.5.2b","Requirement","ECSS-Q-ST-70-80_1480130",1,"Created","Maintenance activities shall include:\n1.\tAfter each build\n(a)\tCheck log and analyse results from build done,\n(b)\tVisual inspection of the system,\n(c)\tVacuum clean the powder basin centre area with clean vacuum cleaner,\n(d)\tCheck the chamber interior for metallisation and clean if polluted,\n(e)\tCheck or change protections foils of beam column, chamber,\n(f)\tCheck or change observation window protection glass,\n(g)\tVacuum clean the chamber from loose particles with dirty vacuum cleaner,\n(h)\tRemove tank and sandblast cake in dedicated sandblaster,\n(i)\tSieve powder contents in sandblaster and clean vacuum cleaner,\n(j)\tFill hoppers with sieved powder,\n(k)\tClean seals and door,\n(l)\tClose the chamber and start vacuum.\n2.\tBefore a build\n(a)\tCheck that the rake is properly attached and the condition of rake teeth,\n(b)\tCheck amount of powder according to height of next job,\n(c)\tCheck or trim the powder dispatcher in accordance with OEM equipment handbook.\n3.\tWeekly\n(a)\tCheck of safety equipment,\n(b)\tCheck filter on personal protection for impurities and clean or replace if polluted,\n(c)\tClean floor of laboratory.\n4.\tMonthly\n(a)\tClean areas: Cabinet, computer, behind the side walls,\n(b)\tCheck coolant filling level and fill it if level is low,\n(c)\tCheck Helium filling level and fill it if level is low,\n(d)\tTesting emergency shutdown, emergency stop,\n(e)\tCheck / clean the sieving equipment for damage.\n5.\tYearly\n(a)\tCheck fire extinguisher,\n(b)\tInspect air dryer and filters,\n(c)\tInspect sandblaster and change filters.\n6.\tA – Maintenance: See OEM handbook for frequency\n(a)\tCheck electron beam unit: cathode, top column, sensors,\n(b)\tCheck vacuum chamber,\n(c)\tCheck camera system,\n(d)\tCheck mechanical drives, guides and bearings,\n(e)\tCheck / adjust powder dispatcher system,\n(f)\tCheck seals.\n7.\tB – Maintenance: See OEM handbook for frequency\n(a)\tChange cathode,\n(b)\tCheck electron beam unit: top column, sensors,\n(c)\tCheck vacuum chamber,\n(d)\tCheck camera system,\n(e)\tCheck mechanical drives, guides and bearings,\n(f)\tChange rake arm,\n(g)\tCheck / adjust powder dispatcher system,\n(h)\tCheck / adjust build tank and table,\n(i)\tCheck seals.","NOTE\tSafety equipment can refer to devices which trigger e.g. emergency stops, etc.\n"]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","12.3g","Requirement","ECSS-Q-ST-70-80_1480163",1,"Created","X-Ray CT shall be applied to detect internal defects in accordance with ASTM E 1570 and ASTM E 1441 unless otherwise specified.","NOTE\tTypical internal defects for mPBF processes are pores, lack of fusion, cracks, or inclusions. X-Ray CT can also provide the porosity level, the defect’s size, shape, and location.\n"]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","13.4b","Requirement","ECSS-Q-ST-70-80_1480196",1,"Created","Powder, containers shall be stored in humidity and temperature controlled area."]
["ECSS-Q-ST-70-80C","ECSS - Current v1.0","A.2.1a","Requirement","ECSS-Q-ST-70-80_1480204",1,"Created","The supplier shall present the preliminary manufacturing concept, including as a minimum:\n1.\tAn overview of all applicable, application-specific requirements\n2.\tThe safety class\n3.\tThe selected AM end to end manufacturing process\n4.\tDesign allowables from a MPD (if available)\n5.\tAMP (if available and verifiable)"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.1.3d","Requirement","ECSS-Q-ST-60_0480010",3,"Normative Change","Depending on the progress of the program, the main PCB activities shall be:\n1.\tTo manage and control the part procurement programmes at all levels including the review and approval of the supplier’s EEE component control plan and associated documents,\n2.\tTo implement the Parts Approval cycle through PAD approval including review of part/manufacturer evaluation/qualification plan and test reports, status of qualification, approval of procurement specifications, quality and lot acceptance levels and procurement inspections, DPA, radiation sensitivity assessment information,\n3.\tTo assess parts technical issues such as Non-conformances, Waivers, Deviations and alerts and verify the implementation of mitigation measures,\n4.\tUpon customer’s request, assessment activities (by sampling) including:\n(a)\tconformity of procurement conditions, \n(b)\tconformity of procurement data,\n(c)\tpost-procurement data, and\n(d)\tapplication of alerts recommendations.","NOTE\t1\t Customer request depends on from the criticality of the equipment or supplier.\nNOTE\t2\tFor (a) to (c), assessment of the procurement conditions, conformity of procurement and post-procurement data is performed versus approval document.\nNOTE\t3\tThe risks like parts under Export license restrictions (eg. EAR/ITAR), all Long Lead Time Items are listed in the Critical Item List as per ECSS-Q-ST-10-04.\n"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.2.2.2h","Requirement","ECSS-Q-ST-60_0480035",2,"Unchanged","The use of pure tin (inside or outside the part) shall be declared in the PAD or in the JD."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.2.3.2.2a","Requirement","ECSS-Q-ST-60_0480060",1,"Unchanged","The supplier shall perform an evaluation against the ESCC basic specification no. 20200 and the ancillary specifications for dedicated component families and shall include, but not necessarily be limited to, a survey of:\n1.\tThe overall manufacturing facility and its organization and management,\n2.\tThe manufacturer’s system for inspection and manufacturing control including all relevant specifications, procedures, and internal documents,\n3.\tThe production line used for the component."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.2.4c","Requirement","ECSS-Q-ST-60_0480069",1,"Unchanged","The supplier shall maintain a system of traceability of the acceptance and approval of each component used in flight products."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.3.3b","Requirement","ECSS-Q-ST-60_0480087",2,"Unchanged","The screening test requirements shall be defined such that accumulated stress does not jeopardize component reliability. "]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.4c","Requirement","ECSS-Q-ST-60_0480127",1,"Unchanged","On request, handling and storage procedures shall be sent to the customer for review."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","4.6.1a","Requirement","ECSS-Q-ST-60_0480144",2,"Unchanged","<<deleted>>"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.1.3c","Permission","ECSS-Q-ST-60_0480503",1,"Unchanged","Other pertinent experts from the customer or suppliers may also participate, on request."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.1.4h","Requirement","ECSS-Q-ST-60_0480172",1,"Unchanged","The content of the DCL shall be in conformance with its DRD in Annex B."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.2.2.4a","Requirement","ECSS-Q-ST-60_0480188",4,"Normative Change","The radiation requirements for the EEE components and the mission radiation environment specification are project specific and shall be derived from the ECSS-Q-ST-60-15."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.2.4g","Requirement","ECSS-Q-ST-60_0480564",1,"Created","The previous use or approval of a part, via PAD or JD, in any other project shall not be considered as an automatic approval for the present program.","NOTE \tThe pertinence of the heritage in terms of mission profile and requirements can be assessed as well as all the deviations (e.g. RFDs, RFWs, special dispositions for a specific space program) previously accepted.\n"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.3.1f","Requirement","ECSS-Q-ST-60_0480225",2,"Normative Change","In case of documentation update, the change shall be submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.3.7a","Requirement","ECSS-Q-ST-60_0480247",1,"Unchanged","The procurement entity shall perform incoming inspection at his premises on all components to verify conformance with the purchase order requirements."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.4f","Requirement","ECSS-Q-ST-60_0480571",1,"Created","An ESD Control Programme in accordance with EN 61340-5-1 shall be developed and implemented by the supplier.","NOTE \tEN 61340-5-1 guideline can be used for editing the ESD Control Programme.\n"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","5.6.4d","Requirement","ECSS-Q-ST-60_0480294",1,"Unchanged","One time programmable components shall be submitted to a post-programming sequence. "]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.2.1b","Requirement","ECSS-Q-ST-60_0480464",1,"Unchanged","The selection, evaluation and approval of commercial EEE components for class 3 programmes shall be performed in conformance with clause 6.2 from ECSS-Q-ST-60-13 standard."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.2.2.2g","Requirement","ECSS-Q-ST-60_0480326",2,"Unchanged","As per 6.2.2.2f, the justification of the use of pure tin shall be sent to the customer for approval."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.2.3.1e","Requirement","ECSS-Q-ST-60_0480344",2,"Unchanged","In the definition of the evaluation programme any information including pertinent reliability, analysis and test data from the manufacturer of the component and previous use in comparable application shall be considered and their relevance justified."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.2.4e","Requirement","ECSS-Q-ST-60_0480361",2,"Unchanged","In case the evaluation results (as per clause 6.2.3.1) are changing the procurement conditions documented in the PAD or the JD, a new revision of the PAD or the JD shall be submitted to the customer for approval."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.3.3f","Requirement","ECSS-Q-ST-60_0480466",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.3.9h","Requirement","ECSS-Q-ST-60_0480400",3,"Unchanged","For health and safety reasons, any test producing beryllium oxide dust shall be omitted."]
["ECSS-Q-ST-60C Rev.4","ECSS - Current v1.0","6.6.3c","Requirement","ECSS-Q-ST-60_0480471",2,"Normative Change","The list of add-on parts shall be provided to the customer.."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.1d","Requirement","ECSS-Q-ST-70-61_1510004",1,"Created","Working areas shall be kept free from any tools or equipment not used for the current task."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.4.5a","Requirement","ECSS-Q-ST-70-61_1510038",1,"Created","All ESD-sensitive items shall be contained within ESD-protective containers for movement between and within ESD-protected areas. "]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.5.1a","Requirement","ECSS-Q-ST-70-61_1510047",1,"Created","Equipment and tools shall be inspected to meet requirements from respective clauses 5.5.2 to 5.5.19."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.5.6.2b","Requirement","ECSS-Q-ST-70-61_1510072",1,"Created","Stripping tools or machines shall fit the size of the wire conductor.","NOTE\tIt is good practice to mask off the die openings for wire sizes not in use.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.5.10e","Requirement","ECSS-Q-ST-70-61_1510105",1,"Created","Solder paste deposition procedures and associated acceptance criteria shall be controlled and documented."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","5.5.14.1b","Requirement","ECSS-Q-ST-70-61_1510114",1,"Created","Reflow process parameters for condensation reflow machines shall be controlled and documented according to clause 5.5.14.5."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","6.2.1a","Requirement","ECSS-Q-ST-70-61_1510139",1,"Created","For soldering, solder paste, ribbon, wire and preforms shall be used provided that the alloy and flux meet the requirements of this standard."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","6.7c","Requirement","ECSS-Q-ST-70-61_1510174",1,"Created","Wires shall be stripped of their insulation in accordance with clause 7.5.1."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","6.11c","Requirement","ECSS-Q-ST-70-61_1510199",1,"Created","Materials covered by this clause shall be individually assessed in accordance with clause 4.2.11 and 4.2.15 of ECSS-Q-ST-70-71 when flammability requirements are applicable."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","7.2.3c","Requirement","ECSS-Q-ST-70-61_1510212",1,"Created","Solvents that do not conform to clause 6.4 shall be removed from the work area.","NOTE\tExample: Solvents contaminated with impurities such as inorganic acids.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","7.6.1a","Requirement","ECSS-Q-ST-70-61_1510241",1,"Created","Gold plated terminations of component shall be degolded and pretinned."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","7.6.3.2a","Requirement","ECSS-Q-ST-70-61_1510267",1,"Created","For degolding, solder shall be melted onto the component termination using a soldering iron tip with temperature either lower than or equal to 330 °C or maximum temperature recommended by the component manufacturer."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","7.7h","Requirement","ECSS-Q-ST-70-61_1510300",1,"Created","Soldering iron tip shall be pretinned before soldering.","NOTE\tPretinning prevents oxidation of the tip.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","8.2.5h","Requirement","ECSS-Q-ST-70-61_1510325",1,"Created","Solder fillets shall not impair stress relief bends."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","8.2.7e","Requirement","ECSS-Q-ST-70-61_1510337",1,"Created","Where the component lead is welded the minimum distance to the bend shall be measured from the weld in accordance with Figure 8-5(b).","NOTE\tExample: Tantalum capacitors.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","8.2.10g","Permission","ECSS-Q-ST-70-61_1510374",1,"Created","After swaging, the terminal may have a maximum of three radial splits or cracks, provided that the splits or cracks do not extend beyond the swaged area of the terminal and are a minimum of 90° apart."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","8.3.3b","Requirement","ECSS-Q-ST-70-61_1510397",1,"Created","The inspection shall be performed on the whole surface of the PCB with a microscope or a magnifying tool with a magnification of 4x as a minimum."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","9.4.4a","Requirement","ECSS-Q-ST-70-61_1510435",1,"Created","The top route shall not be used where side entry is possible."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","9.5b","Requirement","ECSS-Q-ST-70-61_1510445",1,"Created","The bend to attach conductors to hook terminals shall be:\n1.\ta minimum of 1/2 turn,\n2.\ta maximum of 3/4 turn."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","9.8h","Requirement","ECSS-Q-ST-70-61_1510473",1,"Created","The heat-shrinkable insulation sleeving shall be centred over the cleaned and inspected interconnection."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","9.9.4h","Requirement","ECSS-Q-ST-70-61_1510506",1,"Created","Bending tools for the preforming of conductors shall be in accordance with clause 5.5.4."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.2.1e","Requirement","ECSS-Q-ST-70-61_1510536",1,"Created","The solder fillet shall not be in contact with any remaining gold-plated area on the termination."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.2.2b","Requirement","ECSS-Q-ST-70-61_1510545",1,"Created","Conductors shall not be temporarily constrained against spring-back force during solder solidification, to prevent residual stresses in the solder joints, leads and terminals.","NOTE\tResidual stresses are produced in the lead material or solder joint.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.2.5o","Requirement","ECSS-Q-ST-70-61_1510579",1,"Created","The process of additional heating shall be documented."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.3.3h","Requirement","ECSS-Q-ST-70-61_1510604",1,"Created","The solder fillets for clinched leads shall meet the visual workmanship standards as illustrated in Figure E-2."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.4.9f","Permission","ECSS-Q-ST-70-61_1510654",1,"Created","X-ray inspection may be omitted providing justification and approval of Approval Authority."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.5.2f","Requirement","ECSS-Q-ST-70-61_1510690",1,"Created","The number of reworked solder joints shall not exceed 10 % of the total number of solder joints on a board with the exception specified in requirements 10.5.2g and 10.5.2h."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","10.5.2o","Requirement","ECSS-Q-ST-70-61_1510699",1,"Created","Wiring a tantalum capacitor bonded on PCB as described in clause I.3.7 of ECSS-Q-ST-70-28 shall not be performed."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","11.2b","Requirement","ECSS-Q-ST-70-61_1510733",1,"Created","Adhesive shall be mixed and cured in accordance with the manufacturer’s recommendations. "]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","12.1b","Requirement","ECSS-Q-ST-70-61_1510749",1,"Created","Components and conductors shall not be physically moved prior or during visual inspection."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.1.2.1a","Requirement","ECSS-Q-ST-70-61_1510766",1,"Created","Technology sample shall be made when introducing a new assembly process or new supplier."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.1.6c","Requirement","ECSS-Q-ST-70-61_1510799",1,"Created","The supplier shall organise with the Approval Authority a final verification review.","NOTE\tThe assembly processes can be reviewed during the meeting to issue the PID. Verification of closure of the actions identified during the audit of the manufacturing line.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.2.1m","Requirement","ECSS-Q-ST-70-61_1510824",1,"Created","Rework of components, other than manually soldered, shall be decided during the MIP1 "]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.2.3h","Requirement","ECSS-Q-ST-70-61_1510858",1,"Created","More than 5 % of reworked soldered joints per component shall not be accepted."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.4b","Requirement","ECSS-Q-ST-70-61_1510884",1,"Created","Leadless chip capacitors and leadless components with plane termination shall not be assembly verified through electrical testing procedure.","NOTE\tCapacitor and TO276 packages such as SMD05, SMD1, SMD2 and SMD5C, are excluded as the failure mechanism is crack in ceramic.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.4k","Requirement","ECSS-Q-ST-70-61_1510893",1,"Created","The electrical value of components for electrical monitoring shall be selected to be able to detect anomalies in the solder joint:\n1.\tfor resistor zero ohm or the lowest value in the procurement specification,\n2.\tfor other types, custom daisy chain."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","13.6h","Requirement","ECSS-Q-ST-70-61_1510913",1,"Created","The samples for environmental testing shall be submitted to 500 thermal cycles with temperature conditions in conformance with clause 14.11 and with continuous electrical monitoring in accordance with clause 14.6. "]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","14.6d","Requirement","ECSS-Q-ST-70-61_1510953",1,"Created","Continuous electrical monitoring of daisy chain shall be performed during the thermal cycling. ","NOTE\t1: The number of thermal cycles for each verification is defined in the respective clause for each type of verification programme. \nNOTE\t2: Alternative electrical monitoring methods can be agreed with the Approval Authority.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","14.7e","Requirement","ECSS-Q-ST-70-61_1510962",1,"Created","Electrical continuity measurements shall be performed by continuous electrical monitoring of the daisy chain resistance during the first 5 (five) thermal cycles and the last 10 (ten) thermal cycles."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","14.11h","Requirement","ECSS-Q-ST-70-61_1510999",1,"Created","The monitoring thermocouple shall be attached to the surface of the printed circuit board."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","14.15.2e","Permission","ECSS-Q-ST-70-61_1511024",1,"Created","Additional microsections may be requested by the Approval Authority in case of cracks or other features detected during the first microsection sampling.."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","15.1g","Requirement","ECSS-Q-ST-70-61_1511059",1,"Created","The supplier shall be informed about assembly NCRs in the customer assembly line."]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","16.3b","Requirement","ECSS-Q-ST-70-61_1511071",1,"Created","The Approval Authority shall approve the PID.","NOTE\tThe approval can be achieved by PID signature or minutes of meeting being signed by the Approval Authority.\n"]
["ECSS-Q-ST-70-61C","ECSS - Current v1.0","17.8b","Requirement","ECSS-Q-ST-70-61_1511092",1,"Created","A training programme shall be developed, maintained and implemented by the supplier to provide excellence of workmanship and personnel skills in soldering."]
["ECSS-Q-ST-70-40C","ECSS - Current v1.0","6.2a","Requirement","ECSS-Q-ST-70-40_1500008",1,"Created","Brazers performing brazing processes requiring manual interaction shall be trained and certified."]
["ECSS-Q-ST-70-40C","ECSS - Current v1.0","9.1c","Requirement","ECSS-Q-ST-70-40_1500033",1,"Created","Any acceptance criteria for the NDT, not covered in clause 10.3, shall be agreed with the customer."]
["ECSS-Q-ST-70-40C","ECSS - Current v1.0","10.4a","Requirement","ECSS-Q-ST-70-40_1500042",1,"Created","For the selection of the quality levels from Table 10-1 the following rule shall apply:\n1.\tFor Safety Class 1: Quality Level A,\n2.\tFor Safety Class 2: Quality Level B as a minimum,\n3.\tFor Safety Class 3: Quality Level C as a minimum."]
["ECSS-Q-ST-70-40C","ECSS - Current v1.0","11.7c","Requirement","ECSS-Q-ST-70-40_1500068",1,"Created","Documents specified in the requirements from 11.7a.1 to 11.7a.3 and 11.7b shall be controlled in conformance with ECSS-M-ST-40."]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.1.1b","Requirement","ECSS-Q-ST-70-05_0540002",1,"Unchanged","Hazardous substances, items and operations shall be isolated from other activities."]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.1.5.1b","Requirement","ECSS-Q-ST-70-05_0540015",1,"Unchanged","Interferences of environmental components shall be eliminated","NOTE \tMajor environmental interferences are caused by H2O and CO2. Elimination of H2O and CO2 is possible by flushing with the proper gases or applying a vacuum.\n"]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.4.3.2a","Requirement","ECSS-Q-ST-70-05_0540056",1,"Unchanged","The calibration shall be performed covering the required concentration range.","NOTE \tTypical range is 5 ´ 10-8 g/cm2   to  5 ´ 10-6 g/cm2.\n"]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.4.3.3f","Requirement","ECSS-Q-ST-70-05_0540065",2,"Normative Change","For the direct method, the detection limit shall be calculated using methodology given in 5.4.3.6."]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.4.3.7.3h","Requirement","ECSS-Q-ST-70-05_0540127",1,"Created","Methyl silicones and methyl-phenyl silicones shall be below the LOD of the direct method in all five blank spectra.","NOTE \tThe possible source of siloxanes in blank spectra is the entire set of tools and solvents used for sample preparation.\n"]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.4.5.3a","Requirement","ECSS-Q-ST-70-05_0540082",3,"Normative Change","Operators shall be trained by preparing a hydrocarbon standard solution by the following procedure:\n1.\tA gas-tight syringe is filled with the standard solution containing an equivalent of 1 ´ 10-6 g analyte and put in the Petri dish.\n2.\tThe sample is transferred drop-wise with the glass rod or micro-syringe from the Petri dish onto the IR-window within the area of the IR-beam.\n3.\tAfter all droplets are transferred to the window, the Petri dish is rinsed with a few droplets of fresh chloroform and transferred again according to step 2.\n4.\tStep 3 is repeated at least twice.\n5.\tThe IR-transparent window is placed on the sample holder in the sample compartment of the pre-aligned spectrometer.\n6.\tThe spectrum is recorded and the transmission loss for hydrocarbons at about 2 920 cm-1 is measured.\n7.\tSteps 1 to 6 are repeated 10 times."]
["ECSS-Q-ST-70-05C Rev.2","ECSS - Current v1.0","5.5.3c","Requirement","ECSS-Q-ST-70-05_0540091",1,"Unchanged","The supplier shall deliver the review report to all customers within six weeks after the end of the regular review or evaluation testing."]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","5.2.6a","Requirement","ECSS-Q-ST-60-03_1590025",1,"Created","For DEVICE nonconformance handling, ECSS-Q-ST-10-09 shall apply. "]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","6.2.1.2a","Requirement","ECSS-Q-ST-60-03_1590050",1,"Created","The supplier shall perform a dependability and safety analysis at the DEVICE level, using the results of system-level safety and dependability analyses, in order to determine the criticality of each DEVICE function in compliance with ECSS-Q-ST-30 clause 5.4."]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","6.2.5d","Requirement","ECSS-Q-ST-60-03_1590083",1,"Created","The supplier shall report on conformance to the project security requirements in the DEVICE Product Assurance Report in compliance with DRD in Annex B."]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","6.3.4q","Requirement","ECSS-Q-ST-60-03_1590108",1,"Created","DEVICE containing deactivated functions shall be verified and validated to ensure that the deactivated functions cannot be activated or that their accidental activation cannot harm the operation of the system. "]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","6.3.4.4c","Requirement","ECSS-Q-ST-60-03_1590117",1,"Created","The customer shall ensure that the acceptance tests are performed in accordance with the approved acceptance test plan. "]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","8.2.2g","Requirement","ECSS-Q-ST-60-03_1590150",1,"Created","The supplier shall ensure that all authorized changes are implemented in accordance with the configuration management plan. "]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","A.2.1<5.7>b","Requirement","ECSS-Q-ST-60-03_1590175",1,"Created","The DPAP shall define the method and tools used for the DEVICE criticality analysis."]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","A.2.1<6.5>b","Requirement","ECSS-Q-ST-60-03_1590186",1,"Created","The DPAP shall define the methods and tools used for process assessment and improvement."]
["ECSS-Q-ST-60-03C","ECSS - Current v1.0","B.2.1<4>b","Requirement","ECSS-Q-ST-60-03_1590208",1,"Created","The DPAR shall contain reporting on the verification of the measures applied for the handling of critical DEVICE. "]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","5.1.5.2a","Requirement","ECSS-Q-ST-80_0720010",1,"Informative Change","The supplier shall maintain training records.\nEXPECTED OUTPUT:\tRecords of training and experience [PAF, -; -]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","5.4.2.2a","Requirement","ECSS-Q-ST-80_0720040",1,"Normative Change","The supplier shall provide the software product assurance requirements applicable to the next level suppliers for customer’s acceptance.\nEXPECTED OUTPUT:\tSoftware product assurance requirements for suppliers [PAF, -; SRR]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","5.7.3.1b","Requirement","ECSS-Q-ST-80_0720064",1,"Informative Change","The suppliers shall ensure that the results of previous assessments are used in its project activity \nEXPECTED OUTPUT:\tSoftware process assessment records: improvement plan [PAF, -; -]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.1.5a","Requirement","ECSS-Q-ST-80_0720072",2,"Informative Change","A mandatory TRR, as specified in clause 5.3.5.1 of ECSS-E-ST-40, shall be held, in the form of a Project Review as specified in clause 5.3.3.2 ECSS-E-ST-40, before the beginning of the validation against the requirements baseline, to check that:\n1.\tthe software status is compatible with the commencement of validation activities;\n2.\tthe necessary resources, software product assurance plans, test and validation documentation, simulators or other technical means are available and ready for use.\nEXPECTED OUTPUT:\tConfirmation of readiness of test activities [DJF; TRR]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.2.3.7a","Requirement","ECSS-Q-ST-80_0720099",1,"Unchanged","Unit and integration testing shall be (re-)executed on non-instrumented code."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.2.6.7a","Requirement","ECSS-Q-ST-80_0720125",1,"Informative Change","The supplier shall ensure that:\n1.\tthe planned verification activities are adequate to confirm that the products of each phase are conformant to the applicable requirements;\n2.\tthe verification activities are performed according to the plan. \nEXPECTED OUTPUT:\tSoftware product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.2.7.2a","Requirement","ECSS-Q-ST-80_0720133",2,"Normative Change","Analyses of the advantages to be obtained with the selection of existing software (ref. 3.2.9) instead of new development shall be carried out.\nEXPECTED OUTPUT:\tThe following outputs are expected:\na.\tSoftware reuse approach, including approach to delta qualification [PAF, SPAP; SRR, PDR];\nb.\tSoftware reuse file [DJF, SRF; SRR, PDR]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.2.9.6a","Requirement","ECSS-Q-ST-80_0720329",1,"Created","The supplier shall update the software security analysis at each software development milestone, to confirm the security sensitivity and related security risks of software components.\nEXPECTED OUTPUT:\tSoftware security analysis report [SF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.3.4.8a","Requirement","ECSS-Q-ST-80_0720175",1,"Unchanged","The code shall be put under configuration control immediately after successful unit testing."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.3.5.30a","Requirement","ECSS-Q-ST-80_0720206",1,"Informative Change","Software containing deactivated code shall be validated specifically to ensure that the deactivated code cannot be activated or that its accidental activation cannot harm the operation of the system.\nEXPECTED OUTPUT:\tTesting and validation reports [DJF, -; CDR, QR, AR]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","6.3.9.6a","Requirement","ECSS-Q-ST-80_0720226",1,"Informative Change","All maintenance activities shall be logged in predefined formats and retained. \nEXPECTED OUTPUT:\tMaintenance records [MF, -; -]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","7.1.6a","Requirement","ECSS-Q-ST-80_0720233",1,"Informative Change","The results of metrics collection and analysis shall be included in the software product assurance reports, in order to provide the customer with an insight into the level of quality obtained.\nEXPECTED OUTPUT:\tSoftware product assurance reports [PAF, -; -]."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","7.4.5a","Requirement","ECSS-Q-ST-80_0720259",1,"Unchanged","Taking account of the provider’s maintenance and product policy, it shall be ensured that the hardware and support services can be maintained throughout the specified life of the software product within the operational constraints."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","B.2.1<6.6>a","Requirement","ECSS-Q-ST-80_0720289",1,"Unchanged","The SPAP shall describe the process metrics derived from the defined quality models, the means to collect, store and analyze them, and the way they are used to manage the development processes."]
["ECSS-Q-ST-80C Rev.2","ECSS - Current v1.0","B.2.1<8>b","Requirement","ECSS-Q-ST-80_0720298",1,"Unchanged","For each software product assurance requirement, the following information shall be provided:\n1.\trequirement identifier;\n2.\tcompliance \n(C = compliant, NC = non–compliant, NA = not applicable);\n3.\treference to the project documentation covering the requirement (e.g. section of the software product assurance plan);\n4.\tremarks."]
["ECSS-Q-ST-60-15C Rev.1","ECSS - Current v1.0","5.1l","Requirement","ECSS-Q-ST-60-15_1620013",1,"Created","Component type TIDS shall be based on the parametric and functional limits given in component detail specification or manufacturer data sheet, or on the maximum parameter degradation acceptable to ensure equipment operation in compliance with equipment performance specification at the end of its radiation design lifetime.","NOTE \tTIDS is defined by comparing part parametric/functional requirements with TID test data.\n"]
["ECSS-Q-ST-60-15C Rev.1","ECSS - Current v1.0","5.2p","Requirement","ECSS-Q-ST-60-15_1620047",1,"Created","Calculation of TNIDL through ray-tracing analysis shall be submitted to the customer for approval and implemented as follows:\n1.\tSLANT technique is used with the solid sphere non-ionizing dose-depth curve;\n2.\tthe non-ionizing dose is calculated at the centre (called the detector in the following) of a sphere: The 4π spherical surface surrounding the detector is then be sectored into N elementary solid angles equally distributed over the full space solid angle (4π). The minimum number of sectors is 2000; or\n3.\tthe non-ionizing dose is calculated at the centre (called the detector in the following) of a parallelepiped with each face meshed with quadrilaterals and rays are launched from the detector within each cell. The number of cells per face is greater than 400 and at least 20 rays are launched per cell."]
["ECSS-Q-ST-60-15C Rev.1","ECSS - Current v1.0","5.3k","Requirement","ECSS-Q-ST-60-15_1620074",1,"Created","All SEE testing shall be performed in conformance to requirements of clause 5.3f."]
["ECSS-Q-ST-60-15C Rev.1","ECSS - Current v1.0","A.2.1<3>b","Requirement","ECSS-Q-ST-60-15_1620108",1,"Created","Solar particle event ion fluxes versus LET spectrum for a given Aluminium shield thickness (e.g. 1 g/cm2) shall be presented with figure and table."]
["ECSS-Q-ST-60-15C Rev.1","ECSS - Current v1.0","B.2.1<3>a","Requirement","ECSS-Q-ST-60-15_1620117",1,"Created","The radiation analysis report shall provide TNID tolerance of each sensitive component with reference of test report."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","5.5d","Requirement","ECSS-Q-ST-70-60_1390017",1,"Unchanged","The PCB manufacturer shall provide a letter of support from the main industrial space customers."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","5.9m","Requirement","ECSS-Q-ST-70-60_1390048",1,"Unchanged","The final conclusion of the audit process shall be provided in the final audit report or minutes of meeting."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","5.12b","Requirement","ECSS-Q-ST-70-60_1390056",1,"Unchanged","The qualification authority shall publish the qualification status."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.2.2a","Requirement","ECSS-Q-ST-70-60_1390073",1,"Unchanged","ECSS-Q-ST-70-60 shall be used as the PCB procurement specification.","NOTE \tIt is not good practice that the procurement authority issues his own procurement specification in which he refers to ECSS-Q-ST-70-60 as an applicable or a reference document. A reason for this is because traceability of compliance to ECSS-Q-ST-70-60 can be lost. Another reason for this is because the PCB manufacturer issues its CoC against the procurement standard and he categorises his KPIs according to the used procurement standard. In case the procurement authority desires specific additional requirements that are not covered by ECSS-Q-ST-70-60, it is good practice to include these in the PCB definition dossier or in the purchase order.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.4a","Requirement","ECSS-Q-ST-70-60_1390095",1,"Unchanged","The PCB manufacturer shall retain the quality records for at least ten years and in accordance with business agreement requirements."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.6i","Requirement","ECSS-Q-ST-70-60_1390116",1,"Unchanged","ENIG, ENEPIG and ENIPIG finish plating thickness shall be verified once per panel in conformance with Table 10‑13."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.10.2a","Requirement","ECSS-Q-ST-70-60_1390140",1,"Unchanged","Repair operations shall be documented and justified in a work instruction by the PCB manufacturer and referenced in the PCB manufacturer’s PID."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.10.2j","Requirement","ECSS-Q-ST-70-60_1390146",2,"Normative Change","The total number of repairs in conformance with the requirements 6.10.2g, 6.10.2h, 6.10.2i and 6.10.2q shall not exceed 6 per 50 cm2 and 6 per PCB.","NOTE \tThis is based on ECSS-Q-ST-70-28 considering a maximum per PCB and per surface area, whichever is more restrictive.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","6.12d","Permission","ECSS-Q-ST-70-60_1390756",1,"Informative Change","Spare coupons may be stored in an uncontrolled environment.","NOTE \tThis is acceptable because it is considered worst-case. However, it is good practice to store coupons together with PCBs as this ensures representativity in case any test, such as relife testing, is undertaken.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","7.2d","Requirement","ECSS-Q-ST-70-60_1390188",1,"Unchanged","For delta qualification of a process or equipment change that affects the properties of the dielectric material, the following tests shall be performed on PCB and coupons:\n1.\tGroup 1, 3, 5: all;\n2.\tGroup 4 or 6: all;\n3.\tGroup 2: peel strength, flexural fatigue, bending test, outgassing, thermal analysis."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","7.3b","Requirement","ECSS-Q-ST-70-60_1390194",1,"Unchanged","The test selection for initial qualification of PCB manufacturer shall be in conformance with requirement 7.2b."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","8.1d","Requirement","ECSS-Q-ST-70-60_1390218",2,"Normative Change","The PCB manufacturer shall perform referee testing on a spare PCB in case this is specified in Table 10‑27 and 10.6.3c.","NOTE \tReferee testing is specified in Ref. b and c from Table 10‑27.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","8.2.3j","Requirement","ECSS-Q-ST-70-60_1390243",1,"Unchanged","A coupon shall be present that includes patterns for electrical tests in conformance with requirement 15.2f.3 of ECSS-Q-ST-70-12.","NOTE \tElectrical tests include insulation resistance, dielectric withstanding voltage. Specific electrical test conditions can be specified by the procurement authority in conformance with requirement 9.6.3d.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","8.3b","Requirement","ECSS-Q-ST-70-60_1390257",1,"Unchanged","The CoC and its lab reports shall be delivered to the procurement authority."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.2.4h","Requirement","ECSS-Q-ST-70-60_1390283",1,"Unchanged","After removing the specimens from the steam generator machine, they shall be dried."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.3.3.1d","Requirement","ECSS-Q-ST-70-60_1390292",1,"Unchanged","The diameter of plated and non-plated holes shall be verified for all hole diameters."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.3.4a","Requirement","ECSS-Q-ST-70-60_1390315",1,"Unchanged","Impedance test for controlled impedance lines shall be performed using TDR in conformance with test method 2.5.5.7a of IPC-TM-650."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.3.8.2a","Requirement","ECSS-Q-ST-70-60_1390333",1,"Unchanged","Resistive continuity testing shall be performed on final PCBs using flying probe equipment."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.4.4b","Requirement","ECSS-Q-ST-70-60_1390364",1,"Unchanged","Bending test shall cover only static applications.","NOTE \tDynamic applications are project qualified in conformance with requirement 8.6.2b of ECSS-Q-ST-70-12.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.4.5e","Requirement","ECSS-Q-ST-70-60_1390373",1,"Unchanged","The tape shall have an adhesion of at least 4,4 N/cm.","NOTE \tExample of tape that can be used is 3M Brand 600 with a width of 13 mm.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.4.11.4c","Requirement","ECSS-Q-ST-70-60_1390394",1,"Unchanged","Flux shall be applied to the test area and drained on absorbent, clean material prior to solderability test."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.5.2.5c","Permission","ECSS-Q-ST-70-60_1390806",1,"Unchanged","The magnification for microscopic inspection may be 50x to 1000x."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.5.5.2.1c","Requirement","ECSS-Q-ST-70-60_1390440",1,"Unchanged","The PCB manufacturer shall specify the IST coupon design and IST test method to be used.","NOTE \tThis can deviate from the IST test parameters from clause 9.5.5.4.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.5.5.3c","Permission","ECSS-Q-ST-70-60_1390811",1,"Unchanged","The plating sequence to manufacture a buried via across top and bottom layer of a single laminate need not to be included in the IST coupon."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.5.5.4.4a","Recommendation","ECSS-Q-ST-70-60_1390821",1,"Unchanged","After IST testing, the coupon should be submitted to microsectioning."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.6.3g","Requirement","ECSS-Q-ST-70-60_1390477",1,"Unchanged","The test pattern for intralayer insulation resistance shall have at least 25 mm parallel conductors.","NOTE \tInsulation distance between tracks or between layers is representative of the PCB, as specified in clause 15.2a of ECSS-Q-ST-70-12.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.7.2.3f","Requirement","ECSS-Q-ST-70-60_1390502",1,"Unchanged","It shall be determined if a breach of insulation occurred in prepreg or in laminate layers.","NOTE \tThe cleanliness of prepreg layer is under control by the PCB manufacturer. The cleanliness of laminate layers is under control by the laminate supplier.\n"]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.7.3.2f","Recommendation","ECSS-Q-ST-70-60_1390834",1,"Unchanged","Registration should be ≤ 80 μm."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","9.8.4i","Requirement","ECSS-Q-ST-70-60_1390538",1,"Unchanged","The temperature range shall be at least 200 °C."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","10.3g","Requirement","ECSS-Q-ST-70-60_1390578",1,"Informative Change","For the technological feature resin voids, the acceptance criteria, the inspection samples and the measurement method shall be in conformance with Table 10‑24."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","10.4b","Requirement","ECSS-Q-ST-70-60_1390615",2,"Normative Change","For the technological feature conductor spacing, the acceptance criteria, the inspection samples and the measurement method shall be in conformance with Table 10‑43."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","10.6.2f","Requirement","ECSS-Q-ST-70-60_1390679",2,"Normative Change","The parts of cracks or voids protruding from underneath the pad shall be evaluated as dielectric cracks in conformance with the Table 10‑27."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","10.6.3d","Requirement","ECSS-Q-ST-70-60_1390688",1,"Unchanged","Remaining insulation distance shall be the sum of insulation distances to conductors that are not affected by cracks."]
["ECSS-Q-ST-70-60C Rev.1","ECSS - Current v1.0","E.2.1a","Requirement","ECSS-Q-ST-70-60_1390717",1,"Unchanged","Process changes shall include process parameters, chemistry, material, equipment, process flow and inspections."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","6.3b","Requirement","ECSS-Q-ST-70-12_1200014",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.1.1d","Permission","ECSS-Q-ST-70-12_1200528",1,"Created","Blind and buried vias may be filled with prepreg resin or plugging paste.","NOTE \tPlugging paste is a dielectric material applied in a dedicated filling process, usually a type of epoxy paste applied with a squeegee.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.3.5a","Requirement","ECSS-Q-ST-70-12_1200041",2,"Normative Change","Except the case specified in the recommendation 11.6d, the aspect ratio of vias on a rigid and rigid-flex PCB shall be ≤ 7.","NOTE \tThere is no additional requirement for the minimum diameter of plated via in case the diameter conforms to the aspect ratio of ≤ 7.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.4.6c","Recommendation","ECSS-Q-ST-70-12_1200064",2,"Normative Change","Widening of tracks should occur close to AAD footprint to provide a wider track where no other circuitry is adjacent that requires the use of fine pitch.","NOTE \tSee example of nonconformance indicated by yellow arrow in Figure 7‑1.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","7.8.1b","Requirement","ECSS-Q-ST-70-12_1200074",1,"Unchanged","Except cases specified in the requirement 7.8.1d, each finish shall be on separate outer layer nets when a single PCB uses a mixed surface finish of electrolytic gold and fused tin-lead."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.3.3e","Requirement","ECSS-Q-ST-70-12_1200089",1,"Unchanged","Copper cladding on flex laminate of 17 µm shall be the type “rolled and annealed” or “electrodeposited”."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.4f","Permission","ECSS-Q-ST-70-12_1200419",1,"Unchanged","Non-functional tracks may be used to achieve an even distribution of tracks over the entire width of the PCB."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","8.7.5a","Requirement","ECSS-Q-ST-70-12_1200122",1,"Unchanged","Through-holes shall be manufactured by drilling into the initial copper thickness."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","9.4d","Recommendation","ECSS-Q-ST-70-12_1200433",1,"Unchanged","In a multilayer rigid-flex PCB where flex laminates are bonded together with bondply, the ends of the cover layers and bondply should be off-set in the rigid section by 1 mm to prevent a line of weakness."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","10.3.2d","Requirement","ECSS-Q-ST-70-12_1200154",1,"Unchanged","The PCB manufacturer shall inform the supplier of the method of bonding the heat sink.","NOTE \tThis is done to verify the thermal properties of the assembly.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","10.4.3h","Requirement","ECSS-Q-ST-70-12_1200176",1,"Unchanged","The molybdenum inserts shall have a tolerance of ≤ ± 0,035 mm."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","11.4.1i","Recommendation","ECSS-Q-ST-70-12_1200192",2,"Normative Change","The as-designed insulation in Z direction in microvia layers should be 100 µm.","NOTE \tThe typical build-up to achieve ≥ 60 µm as-manufactured and a designed insulation of 100 µm, is by using 2 sheets of polyimide prepreg type 106. For high speed HDI other prepreg styles can be considered, such as 1035 or 1027.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","11.5.2a","Requirement","ECSS-Q-ST-70-12_1200447",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","12.3f","Recommendation","ECSS-Q-ST-70-12_1200456",1,"Unchanged","Layers that include embedded film resistors should not be plated.","NOTE \tThis is done to achieve the best accuracy of etching and resistor value as-manufactured.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","12.4a","Recommendation","ECSS-Q-ST-70-12_1200458",1,"Unchanged","The thickness of RF PCB as-designed should be ≤ 3 mm."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.4d","Requirement","ECSS-Q-ST-70-12_1200238",2,"Deleted","<<deleted>>"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.7.2b","Recommendation","ECSS-Q-ST-70-12_1200473",1,"Unchanged","Critical tracks should be routed on a single layer."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.8.2i","Requirement","ECSS-Q-ST-70-12_1200262",1,"Unchanged","The insulation distance between hole wall of vias on different nets shall be in conformance with the values specified in the Table 13‑3.","NOTE \tThe as-manufactured distance is not affected by the number of bond sequences. However, the tolerance on the as-designed distance increases with the number of bond sequences, as specified in the Table 13‑7.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.9.3.2d","Requirement","ECSS-Q-ST-70-12_1200286",1,"Unchanged","Flexible PCB sections that include critical tracks and that face other conductive elements with an insulation distance of < 1 mm shall include an additional insulation layer of ≥ 25 µm on the conductive element.","NOTE \tAdditional insulation can be provided by 25 µm Kapton tape.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","13.12.2h","Recommendation","ECSS-Q-ST-70-12_1200493",1,"Unchanged","Circuitry and components for high speed signals should be kept close together."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.2g","Requirement","ECSS-Q-ST-70-12_1200593",1,"Created","The method of depanneling a PCB from its support frame shall be included in the PCB definition dossier."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.4a","Recommendation","ECSS-Q-ST-70-12_1200515",1,"Unchanged","Adhesive bonding should not be performed on fused tin-lead."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","14.5.6a","Requirement","ECSS-Q-ST-70-12_1200350",1,"Unchanged","The pad design for components of type LCC shall be in conformance with the as-manufactured values specified in the Table 14‑9, except for the case specified in 14.5.2c.","NOTE \t1\tAn illustration is given in Figure 14‑11.\nNOTE \t2\tLCC means leadless chip carrier.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-70-12_1200361",1,"Unchanged","The PCB definition dossier shall include the following data:\n1.\tDescription, as specified in A.2.1<2>,\n2.\tMechanical layout, as specified in A.2.1<3>,\n3.\tArtwork data , as specified in A.2.1<4>,\n4.\tDrawing, as specified in A.2.1<5>,\n5.\tSpecific electrical test, as specified in A.2.1<6>,\n6.\tReview Items , as specified in A.2.1<7>,\n7.\tCheck list, as specified in A.2.1<8>,"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<2>a","Requirement","ECSS-Q-ST-70-12_1200362",1,"Unchanged","The PCB definition dossier shall include a description containing at least the following data:\n1.\tBase material,\n2.\tFinishes,\n3.\tNumber of layers,\n4.\tSize,\n5.\tThickness and tolerance,\n6.\tPart number of PCB design: specified by supplier,\n7.\tRevision number of PCB design,\n8.\tHeat sink including:\n(a)\tHeat sink thickness,\n(b)\tTolerances permitted,\n(c)\tMaterial used,\n(d)\tType of protective surface coating.","NOTE \tSynonyms of revision number in requirement 7 are issue number and version number.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<3>a","Requirement","ECSS-Q-ST-70-12_1200363",1,"Unchanged","The PCB definition dossier shall include the mechanical layout containing at least the following data:\n1.\tOne or more mechanical drawings including a dimensioning system,\n2.\tLocation and form for the PCB manufacturer to place date code and serialization.","NOTE 1\tIt is recommended in the requirement 1 to use a reference hole as datum point. The reference hole is recommended to be drilled in the first drill cycle.\nNOTE 2\tThe form of numbering as specified in requirement 2 can be in ink or conductive pattern.\nNOTE 3\tAn example of mechanical layout is shown in Figure A-1.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<4>a","Requirement","ECSS-Q-ST-70-12_1200364",1,"Unchanged","The PCB definition dossier shall include the artwork data containing at least the following information:\n1.\tArtwork data of each conductive PCB layer,\n2.\tArtwork data for non-conductive layers,\n3.\tDrilling and milling files.","NOTE 1\tExamples of conductive layers for the requirement 1 are circuitry and selective finishes.\nNOTE 2\tExamples of non-conductive layers for the requirement 2 are solder mask and silk screen \nNOTE 3\tIt is preferred in the requirement 3 to distinguish by different tool codes the plated and non-plated holes in the drill file even if they have identical diameter.\nNOTE 4\tFor example, ODB++ is a format that describes all artwork of all layers in one file.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<5>a","Requirement","ECSS-Q-ST-70-12_1200365",1,"Informative Change","The PCB definition dossier shall include the drawings containing at least the following:\n1.\tDrilling drawing,\n2.\tDrilling tables, including:\n(a)\tSymbol, \n(b)\tDiameter of as-manufactured holes,\n(c)\tTolerance,\n(d)\tPlated or not plated,\n(e)\tQuantity. \n3.\tBuild-up data, including:\n(a)\tNumbered conductive layers from top to bottom,\n(b)\tTotal copper thickness, basic + plated, for each layers with tolerances,\n(c)\tPresence of planes: ground and supply, mesh plane or full copper,\n(d)\tPresence of layers with controlled impedance,\n(e)\tThickness tolerance of laminate and prepreg, including minimum as-manufactured insulation distances,\n(f)\tTotal PCB thickness and tolerance,\n(g)\tSpecification if thickness is measured over bare laminate or over conductive pattern,\n(h)\tSpecific requirements for build-up.","NOTE 1\tExamples of specific requirements for build-up are:\n·\tstyle of prepreg and laminate,\n·\tuse of separate copper foil or copper cladding on laminate for external layers,\n·\tuse of single or double sided laminate,\n·\tuse of two individually cured insulators to achieve reliable insulation.\nNOTE 2\tExamples of Drilling drawing, Drilling table and Build-up data are given in Figure A-2, Figure A-3, Figure A-4.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<6>a","Requirement","ECSS-Q-ST-70-12_1200366",1,"Unchanged","The PCB definition dossier shall include the electrical test description containing at least the following data:\n1.\tNetlist,\n2.\tDefinition of any electrical tests that are specific to the PCB design and in addition to the standard set of electrical tests,\n3.\tIdentification of conductive lines that are designed to be of higher DC resistance that are at risk not to pass standard continuity testing,\n4.\tThe definition of controlled impedance tracks including:\n(a)\tReference planes,\n(b)\tType of coupling,\n(c)\tTrack dimensions, including height, width, cross section,\n(d)\tSpacing dimensions in X,Y and in Z direction,\n(e)\tImpedance value, tolerance and method of measurement.\n5.\tIdentification of any deliberate errors.","NOTE 1\tExample for requirement 4(b): broadside coupled, edge coupled.\nNOTE 2\tIn the requirement 4(e) the standard method for measuring impedance and tolerance is TDR in case the method is not specified\nNOTE 3\tExample for the requirement 5 are differences between artwork and net list such as star points.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<7>a","Requirement","ECSS-Q-ST-70-12_1200367",1,"Informative Change","The PCB definition dossier shall include all Review Items.","NOTE \tThe following design features are required to be recorded as Review Items by the present standard:\n1.\tAsymmetric build-up as specified in 7.1.1b,\n2.\tMolybdenum, CIC layers and AlN as specified in 7.1.1c\n3.\tAsymmetric copper cladding as specified in 7.1.2b,\n4.\tTotal copper thickness >700 µm as specified in 7.1.2g, \n5.\tSingle sheet of glass reinforcement in laminate as specified in 7.1.3c,\n6.\t4 mil laminate as specified in 7.1.3f,\n7.\t5 mil laminate at >30V as specified in 7.1.3g,\n8.\tTotal PCB thickness as specified 7.3.2c and 7.3.3c,\n9.\tReduced as-designed track width and spacing as specified in 7.4.3c and 7.4.4c,\n10.\tFine pitch tracks as specified in 7.4.3g, and 7.4.5b,\n11.\tRemoval of non-functional pads as specified in 7.5.2c for PTH and 7.5.2e for core vias, buried vias and through-going vias,\n12.\tReduced as-designed pad dimensions on solder side and component side as specified 7.5.3e and 7.5.3g,\n13.\tPad diameter on rigid laminate <0,3mm larger than drilled hole as specified in 7.5.3j,\n14.\tReduced diameter of internal pads as specified in 7.5.3l,\n15.\tNon-circular pads as specified in 7.5.4b\n16.\tAsymmetric copper planes as specified in 7.6e,\n17.\tMixed surface finish as specified in 7.8.1e,\n18.\t70 µm copper cladding in flex laminate as specified in 8.3.3c,\n19.\tFull copper planes in flex laminate as specified in 8.3.4b,\n20.\t70 µm copper foil in combination with no-flow prepreg as specified in 9.3d,\n21.\tMore than 2 flex laminates as specified in 9.3f, \n22.\tPad diameter on flex laminates <0,6 mm larger than diameter of drilled hole as specified in 9.6b,\n23.\tHeat sinks and their mechanical stability as specified in 10.2a, 10.3.3a and 10.4.4a.\n24.\tConductive surface pattern below external heat sink as specified in 10.3.2g,\n25.\tHDI as specified in 11.2c,\n26.\tBasic copper layer thickness <17 µm as specified in 11.4.1e,\n27.\tDiameter of external capture pad or internal landing pad of microvias that are <0,175 mm larger than the ablated hole for polyimide HDI or <0,15 mm larger for high speed HDI as specified in 11.4.3b,\n28.\tReduced annular ring with teardrop reinforcement as specified in 11.5.2a,\n29.\tDifferential pair routed in AAD footprint as specified in 11.5.5a,\n30.\tAspect ratio of vias >7 as specified in 11.1e,\n31.\tEmbedded film resistors as specified in the requirements 12.3a and 12.3i,\n32.\tThickness of RF PCB >3mm as specified in 12.4b,\n33.\tNumber of layers in RF PCB >8 as specified in 12.4d,\n34.\tReduced insulation distance for RF elements as specified in 12.5.1b,\n35.\tZ-controlled backdrilling as specified in 12.9a,\n36.\tProfiled top layers as specified in 12.8b,\n37.\tProfiled aluminium backing as specified in 12.8c,\n38.\tReduced as–designed insulation distance as specified in 13.10c,\n39.\tControlled impedance tracks as specified in 13.11.2,\n40.\tDesign of test coupon as specified in 15.1b.\n41.\tCopper distribution and thickness after plating of microvia layers with 1 sheet of prepreg as specified in 11.4.1k.7,\n42.\tPossible coverage with SnPb on the side of small SMT pads as specified in 14.2e,\n43.\tPossible tighter tolerances for scaling of external conductors as specified in 6.2.3g of ECSS-Q-ST-70-60,\n44.\tPossible maximum thickness of solder mask on conductor as specified in 8.2.4p of ECSS-Q-ST-70-60,\n45.\tPossible tape testing on PCB as specified in 9.4.5g of ECSS-Q-ST-70-60.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<7>b","Requirement","ECSS-Q-ST-70-12_1200368",1,"Unchanged","The PCB definition dossier shall include all specific inspections required for the Review Items."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.1<8>a","Requirement","ECSS-Q-ST-70-12_1200369",1,"Unchanged","The PCB definition dossier shall include a check list containing at least the following data:\n1.\tall file names included in the archive,\n2.\tlast modified data of each file,\n3.\tsize of the file,\n4.\tCRC.","NOTE \tThe purpose of the check list is to define the content of the archive file to prevent transmission of wrong data. In Figure A-5 an example of a check list is shown. The check list indicates the content of the archive file by the four items mentioned in A.2.1<8>.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.2a","Requirement","ECSS-Q-ST-70-12_1200370",1,"Unchanged","The format of the data of the PCB definition dossier shall be agreed between supplier and PCB manufacturer."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.2b","Recommendation","ECSS-Q-ST-70-12_1200525",1,"Unchanged","One single file should be used for transferring the data between supplier and PCB manufacturer."]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.2c","Recommendation","ECSS-Q-ST-70-12_1200526",1,"Unchanged","The transmitted file should be an archive with lossless compression.","NOTE \tExamples of file extensions of archives with lossless compression are: .zip, .rar,.7z, .tar.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","A.2.2d","Requirement","ECSS-Q-ST-70-12_1200371",1,"Unchanged","The supplier shall ensure the file format enables verification of file integrity to prevent corruption.","NOTE \tFor example verification by CRC.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","B.2.1a","Requirement","ECSS-Q-ST-70-12_1200372",1,"Unchanged","The PCB manufacturing dossier shall contain following information:\n1.\tReference to the purchase order including the following items:\n(a)\tID number\n(b)\tLine item numbers for each required PCB type\n(c)\tLine item numbers for each required PCB tooling\n(d)\tLine item numbers for other required services like FAI\n(e)\tRequired quantities for each line item\n(f)\tRequired delivery dates for each line item\n2.\tReference to the PCB definition dossier for each PCB type.\n3.\tTooling files\n(a)\tImaging\n(b)\tDrilling\n(c)\tMilling or routing\n(d)\tPlating\n(e)\tLamination\n(f)\tAOI\n(g)\tElectrical testing\n(h)\tProcess route card or traveller information\n(i)\tInspection drawings\n4.\tMRR checklist","NOTE \tAn example of an MRR checklist is provided in Annex G.\n"]
["ECSS-Q-ST-70-12C Rev.1","ECSS - Current v1.0","B.2.1b","Requirement","ECSS-Q-ST-70-12_1200373",1,"Unchanged","The supplier and PCB manufacturer shall document in the MRR checklist their approval of the PCB manufacturing dossier, the PCB definition dossier and all Review Items."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","5a","Requirement","ECSS-Q-ST-20-30_1660001",1,"Created","The use of any technique or technology involved in harness manufacturing shall be agreed upon between customer and manufacturer.","NOTE\tExamples for techniques (non-exhaustive) are crimping, soldering, splicing, welding and potting.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","5b","Requirement","ECSS-Q-ST-20-30_1660002",1,"Created","The manufacturer shall establish a qualified process in accordance with ECSS‑Q‑ST‑70 for each technique used for the harness manufacturing.","NOTE\tAll processes are expected to be listed and approved via the DPL issued by the manufacturer in accordance with ECSS‑Q‑ST‑70, Annex C.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","5c","Requirement","ECSS-Q-ST-20-30_1660003",1,"Created","IPC/WHMA-A-620E-S (Addendum for Space and Military Applications Requirements) and IPC/WHMA-A-620E shall apply with the conventions for ‘Applicable as is’, ‘Applicable with modification’, ‘Applicable with amendment’ and ‘Not applicable’ defined in clause 3.4. "]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.0.1.6a","Permission","ECSS-Q-ST-20-30_1660004",1,"Created","For wires and cables, which are manufactured, qualified, procured and handled in accordance with ESCC specifications, a Red Plague control plan may be omitted."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.0.1.7a","Permission","ECSS-Q-ST-20-30_1660005",1,"Created","For wires and cables, which are manufactured, qualified, procured and handled in accordance with ESCC specifications, a White Plague control plan may be omitted."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.9a","Requirement","ECSS-Q-ST-20-30_1660006",1,"Created","Requirement flow down shall be performed in accordance with ECSS‑M‑ST‑10."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.10a","Requirement","ECSS-Q-ST-20-30_1660007",1,"Created","Modifications and amendments made to the IPC baseline by this standard shall be covered by a supplier developed program that is provided to the customer for review and approval.","NOTE\tFor a manufacturer developed program it is still recommended, but not mandatory, that the training of personnel related to the IPC/WHMA-A-620-Space Addendum Training and Certification Program is traceable to a Master IPC trainer.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.16a","Requirement","ECSS-Q-ST-20-30_1660008",1,"Created","Materials and Processes shall be handled in accordance with ECSS‑Q‑ST‑70."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.19.1a","Requirement","ECSS-Q-ST-20-30_1660009",1,"Created","Rework shall be documented."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.19.1b","Requirement","ECSS-Q-ST-20-30_1660010",1,"Created","Rework shall be performed in accordance with the applicable requirements in this standard. "]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.19.2a","Requirement","ECSS-Q-ST-20-30_1660011",1,"Created","Repair shall be documented."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.19.2b","Requirement","ECSS-Q-ST-20-30_1660012",1,"Created","Repair shall be performed in accordance with documented procedures agreed between the manufacturer and the customer."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.1.19.2c","Requirement","ECSS-Q-ST-20-30_1660013",1,"Created","Any deviation of the repair procedure to the requirements in this standard and any deviation of the final product as consequence of the repair procedure to the requirements in this standard shall be highlighted by the manufacturer and agreed with the customer prior to performing.","NOTE\tFor deviations a “Request for Deviation” or “Waiver” can be used.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.3.1a","Requirement","ECSS-Q-ST-20-30_1660014",1,"Created","[Not applicable]"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.3.2a","Requirement","ECSS-Q-ST-20-30_1660015",1,"Created","[Not applicable]"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.3.3a","Requirement","ECSS-Q-ST-20-30_1660016",1,"Created","[Not applicable]"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.3.4a","Requirement","ECSS-Q-ST-20-30_1660017",1,"Created","[Applicable as is]"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.3.5a","Requirement","ECSS-Q-ST-20-30_1660018",1,"Created","[Not applicable]"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.8.4a","Requirement","ECSS-Q-ST-20-30_1660019",1,"Created","The minimum sleeving overlap shall be 3 mm."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.9.2.1a","Requirement","ECSS-Q-ST-20-30_1660020",1,"Created","The use of build‑up material shall be agreed between manufacturer and customer prior to use. "]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.9.2.1b","Requirement","ECSS-Q-ST-20-30_1660021",1,"Created","Wires and cables under a cable clamp shall be protected against mechanical damages induced by the cable clamp by means of a dedicated layer of protective material.","NOTE\tTypical protective, build-up materials utilised for that purpose are sleeves or tapes (e.g. Polyimide/Kapton or Aluminium)\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.12.3a","Requirement","ECSS-Q-ST-20-30_1660022",1,"Created","Marking and colour-coding shall be resistant to solvents as specified in ESCC 24800."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.12.6.2a","Requirement","ECSS-Q-ST-20-30_1660023",1,"Created","Marking sleeves shall be free from burn marks or charring due to excessive overheating (see Figure 6‑2Figure 6‑1)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.12.6.2b","Requirement","ECSS-Q-ST-20-30_1660025",1,"Created","Slight discoloration due to minor overheating shall not be a cause of rejection but be treated as process indicator in accordance with the IPC/WHMA-A-620 (see Figure 6‑3)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.14.1a","Requirement","ECSS-Q-ST-20-30_1660027",1,"Created","Cut end protrusion shall be 0 mm to 0,5 mm and square to the face of the tie wrap.","NOTE\tA receded tie-wrap tail with regards to the collar head (see Figure 6‑4) is considered as a negative protrusion as thus not acceptable.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0",null,"Requirement","ECSS-Q-ST-20-30_1660028",1,"Created"," \nFigure 6‑3: Tie-wrap – acceptable cut end protrusion\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.14.1b","Requirement","ECSS-Q-ST-20-30_1660029",1,"Created","Where a tie wrap is used to fix a harness bundle to a structural element, a dedicated layer of protection shall be applied onto the bundle under the tie wrap.","NOTE\tThe term structural element here means any element that prevents the tie-wrap from moving with the harness under mechanical loads.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.14.1.1a","Requirement","ECSS-Q-ST-20-30_1660030",1,"Created","The insulation shall not be damaged by the restraining device "]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.14.1.1b","Requirement","ECSS-Q-ST-20-30_1660031",1,"Created","Compression of the insulation shall not degrade the performance of the cables and is controlled by a qualified process in accordance with requirement 5b.","NOTE\tCompression of insulation can lead to reduction in insulation thickness and thus affect performance parameters such as insulation resistance and insulation breakdown voltage.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.14.1.1c","Requirement","ECSS-Q-ST-20-30_1660032",1,"Created","For insulation materials sensitive to creeping (cold-flow), measures shall be taken to protect the respective material from compressive stress induced by the restraining device.","NOTE\tExample for materials sensitive to creeping (cold-flow) are PTFE and FEP.\nNOTE\tMeasures can include the addition of local cable protection under the restraining device\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.1a","Requirement","ECSS-Q-ST-20-30_1660033",1,"Created","Table 15-1 of IPC/WHMA-A-620E-S is not applicable. Any broken strand shall be considered as a defect."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.2.1.2.1a","Requirement","ECSS-Q-ST-20-30_1660034",1,"Created","Any broken strand shall be considered as a defect"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.2.2.1a","Requirement","ECSS-Q-ST-20-30_1660035",1,"Created","An additional insulation layer shall be added between the exposed shielding and the wire insulation and shall extend beyond the end of the exposed shield by at least 2 mm to prevent the sharp braid ends from damaging the wire insulation."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.3.2a","Requirement","ECSS-Q-ST-20-30_1660036",1,"Created","The crimp ring shall not extend beyond the crimp area."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.3.2b","Requirement","ECSS-Q-ST-20-30_1660037",1,"Created","The number of shield strands not contained under the crimp ring shall be less than 6% of the total number of strands within the shield."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.15.3.2c","Requirement","ECSS-Q-ST-20-30_1660038",1,"Created","Trimmed strand ends shall be covered by a protective insulation layer."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.19.4a","Requirement","ECSS-Q-ST-20-30_1660039",1,"Created","The manufacturer shall maintain a mating and de-mating logbook for each connector, including at a minimum\n1.\tProject designation\n2.\tHarness / HMU identifier\n3.\tCI number of the Harness / HMU\n4.\tSerial number (SN) of the Harness / HMU\n5.\tConnector identifier","NOTE\tConnectors are typically identified using the scheme UNIT_A000, where:\n·\t‘UNIT’ denotes the name of the unit (e.g. PCDU)\n·\t‘A’ denotes the connector gender with P for Plug and J for Jack \n·\t‘000’ denotes a sequential number unique to the unit, starting with 001\n1.\tDedicated record of each mating and de-mating operation\n2.\tDate and signature for each mating and de-mating operation by the respective operator or inspector\n3.\tMaximum number of allowed mating cycles\nNOTE\t1\tA mating cycle is defined as one (1) mating and one (1) de-mating operation\nNOTE\t2\tThe maximum number of allowed cycles is typically specified in the engineering documentation, manufacturer datasheet or applicable standards\n4.\t(De-)Mating justification\nNOTE\t1\tTypically includes the reason for the mating operation (e.g. electrical testing, electrical AIT) and indicates the use of savers or mating to flight equipment\nNOTE\t2\tAnnex B can be used as template for the mating logbook.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.19.4b","Requirement","ECSS-Q-ST-20-30_1660040",1,"Created","The test procedure shall ensure that the harness is fully discharged at the end of each test and prior to disconnecting the harness from the test equipment."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.19.4.1a","Requirement","ECSS-Q-ST-20-30_1660041",1,"Created","The ‘Shorts’ test is not required by default and shall only be performed when specified by the customer."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.19.5.1a","Requirement","ECSS-Q-ST-20-30_1660042",1,"Created","Continuity testing shall be performed on any intentionally conductive paths, including shielding."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.19.6.1a","Requirement","ECSS-Q-ST-20-30_1660043",1,"Created","Contact Retention Verification shall be performed in accordance with IPC/WHMA‑A‑620E‑S, section 19.7.5."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","6.20a","Requirement","ECSS-Q-ST-20-30_1660044",1,"Created","Soldering requirements for high voltage applications are specified in ECSS-Q-ST-70-61."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.2a","Requirement","ECSS-Q-ST-20-30_1660045",1,"Created","Any bare conductor at the back of a connector shall be insulated.","NOTE\tThe back of a connector is where the contact, crimped to a wire, enters the connector insulator as opposed to the front of the connector which mated the respective interface counterpart.\nNOTE\tCommon means to implement insulation are:\n- Application of insulation sleeves\n- Potting\n- Use of grommets\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.3a","Requirement","ECSS-Q-ST-20-30_1660046",1,"Created","All processes related to soldering operations shall be performed in accordance with ECSS-Q-ST-70-61."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.4a","Requirement","ECSS-Q-ST-20-30_1660047",1,"Created","All processes related to crimping operations shall be performed in accordance with ECSS-Q-ST-70-26."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5a","Requirement","ECSS-Q-ST-20-30_1660048",1,"Created","Insulation sleeving shall overlap the contact barrel and the wire insulation by a minimum of two times the wire diameter or 3 mm, whichever is greater."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5b","Requirement","ECSS-Q-ST-20-30_1660049",1,"Created","Insulation sleeving shall not prevent the movement of the contact inside connector insulator."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5c","Requirement","ECSS-Q-ST-20-30_1660050",1,"Created","Insulation sleeve shall not slide or vibrate off.","NOTE\tAdditional shrinking sleeves can be added to build up the diameter of the wire so the outer shrinking sleeve is tight on the assembly from one end to the other as illustrated in Figure 7‑1.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5d","Requirement","ECSS-Q-ST-20-30_1660051",1,"Created","Insulation sleeve shall not cover the inspection hole as illustrated in Figure 7‑2."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5e","Requirement","ECSS-Q-ST-20-30_1660053",1,"Created","In case the geometry of the connector allows, the insulation sleeve shall enter into the insulator cavity of the connector, not leaving any exposed conductor detectable by visual inspection at a 45° angle to the cavity axis as illustrated in Figure 7‑3.","NOTE\tVerification can be done by visual inspection only.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5f","Requirement","ECSS-Q-ST-20-30_1660054",1,"Created","In case the geometry of the connector does not allow the insulation sleeve to enter into the insulator cavity of the connector, the gap between the insulator and the sleeve shall be 0,5 mm or less from the point where the connector terminal enters the connector insert.","NOTE\tExamples of acceptable and unacceptable gaps are depicted in Figure 7‑4.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5g","Requirement","ECSS-Q-ST-20-30_1660055",1,"Created","In case the connector is subject to reliable insulation, clause 4.2.1.2 of ECSS-E-ST-20 shall be applied instead of requirement 7.5e and 7.5f."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5h","Requirement","ECSS-Q-ST-20-30_1660056",1,"Created","There shall be no foreign particles entrapped underneath the shrinking sleeve.","NOTE\tExamples of a foreign particle trapped underneath a shrinking sleeve is shown in Figure 7‑5.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.5i","Requirement","ECSS-Q-ST-20-30_1660057",1,"Created","Shrinking sleeve shall not show any signs of excessive deformation or stress.","NOTE\tFor example whitening as shown in Figure 7‑6\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.6a","Requirement","ECSS-Q-ST-20-30_1660058",1,"Created","For connector identification labels applied longitudinally to the harness bundle the read direction of the marking on the label shall be towards connector (see Figure 7‑7)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.6b","Requirement","ECSS-Q-ST-20-30_1660060",1,"Created","For connector identification labels applied perpendicular to the harness bundle the marking on the label shall be readable upright looking from harness side towards connector (see Figure 7‑8)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7a","Requirement","ECSS-Q-ST-20-30_1660062",1,"Created","An additional insulation layer shall be positioned under shielding and shall extend beyond shielding termination to prevent sharp edges from cut braid ends to damage the underlying wire and cable insulation (see Figure 7‑9)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7b","Requirement","ECSS-Q-ST-20-30_1660063",1,"Created","Overlapping braids shall be secured on all branches over the full length of the overlap (see Figure 7‑10)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7c","Requirement","ECSS-Q-ST-20-30_1660064",1,"Created","The required optical coverage of the braided shield shall be maintained across the entire branching area (see Figure 7‑11)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7d","Requirement","ECSS-Q-ST-20-30_1660065",1,"Created","The ends of the braid shall be secured."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7e","Requirement","ECSS-Q-ST-20-30_1660066",1,"Created","The braids of the different branches shall overlap for at least 30 mm or two times the diameter of the largest bundle, whichever is longer, at the breakout."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7f","Requirement","ECSS-Q-ST-20-30_1660067",1,"Created","The open ends of the braid shall be cut in a uniform manner."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7g","Requirement","ECSS-Q-ST-20-30_1660068",1,"Created","The open ends of the braid shall be free of fraying, unraveling and pulled loops (see Figure 7‑11)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7h","Requirement","ECSS-Q-ST-20-30_1660069",1,"Created","The braid shall be free of bulges and dents."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.7i","Requirement","ECSS-Q-ST-20-30_1660070",1,"Created","The braid shall be free of tears and cuts (see Figure 7‑11)."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8a","Requirement","ECSS-Q-ST-20-30_1660074",1,"Created","Shielding of harness bundles with conductive, metal foil to achieve Electromagnetic Compatibility shall be performed by helicoidal wrapping around the bundle as depicted in Figure 7‑12."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8b","Requirement","ECSS-Q-ST-20-30_1660076",1,"Created","The wrapping shall be performed with an overlap of at least 50 %.","NOTE\tHandling and in particular bending of harness bundles can alter the overlap of the wrapping locally when using non-adhesive foils.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8c","Requirement","ECSS-Q-ST-20-30_1660077",1,"Created","The harness manufacturer shall ensure the electrical continuity of the shield along the entire harness.","NOTE\tFor example by wrapping using a single, continuous piece of foil or utilizing a drain wire.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8d","Requirement","ECSS-Q-ST-20-30_1660078",1,"Created","Wrapping shall be tight to the bundle as shown in Figure 7‑13 and not slide along the bundle as indicated in Figure 7‑14."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8e","Requirement","ECSS-Q-ST-20-30_1660081",1,"Created","The ends of the foil pieces shall be secured."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8f","Requirement","ECSS-Q-ST-20-30_1660082",1,"Created","The foil shall be free of tears, cracks and holes as shown in Figure 7‑15."]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8g","Requirement","ECSS-Q-ST-20-30_1660084",1,"Created","The foil shall be free of wrinkles that jeopardize shield continuity and proper shield function or are prone to tearing.","NOTE\tMinor wrinkles are considered unavoidable and acceptable.\n"]
["ECSS-Q-ST-20-30C","ECSS - Current v1.0","7.8h","Requirement","ECSS-Q-ST-20-30_1660085",1,"Created","Foil wrappings of the different branches shall overlap at the breakout for at least 30 mm or two times the diameter of the largest bundle, whichever is longer."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.1a","Requirement","ECSS-Q-ST-70-01_1650001",1,"Created","The supplier shall define and implement a cleanliness and contamination control programme for each level of configuration. ","NOTE \t1\tSurveys can also be made to determine the contamination control requirements, based on mission objectives and scenarios.\nNOTE \t2\tThe objective of this programme is, starting from the mission performance requirements, to establish cleanliness and contamination levels to be achieved at different manufacturing, AIT and mission stages. \nNOTE \t3\tIn general, the organization of regular workshops dedicated to cleanliness and contamination control for a specific programme is a good practice.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.1b","Requirement","ECSS-Q-ST-70-01_1650002",1,"Created","The supplier shall establish measures for the coordination and resolution of cleanliness and contamination control issues among the parties involved in the project."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.1c","Requirement","ECSS-Q-ST-70-01_1650003",1,"Created","The supplier shall appoint a C&CC responsible."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.1d","Requirement","ECSS-Q-ST-70-01_1650004",1,"Created","The C&CC responsible shall define contamination sensitivity of the programme for each level of configuration.","NOTE \tContamination sensitivity is driven by the design, program phases depending on mission, and involved technologies.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.1a","Requirement","ECSS-Q-ST-70-01_1650005",1,"Created","The supplier shall define and document the cleanliness levels applicable to the contamination critical and contamination sensitive items, and any other needs and provisions for contamination control, in a cleanliness requirement specification (CRS), in conformance with the DRD in Annex A.","NOTE \t“Cleanliness levels” are intended as:\n·\tThe maximum level of contamination for acceptable mission performances until EOL, and\n·\tThe maximum level of contamination applicable at the delivery of hardware from lower-tier suppliers.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.1b","Requirement","ECSS-Q-ST-70-01_1650006",1,"Created","The CRS shall be defined as early as possible in the programme to ensure proper consideration during the design phase.","NOTE \tCleanliness is of fundamental importance for the space system’s performance.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.1c","Requirement","ECSS-Q-ST-70-01_1650007",1,"Created","The CRS shall be reviewed and approved by users and engineers from all applicable and impacted disciplines.","NOTE \t1\tUsers can be, for example, experimenters or scientists.\nNOTE \t2\tEngineers can be, for example, payload, instrument, optics, mechanisms, thermal, structural engineers.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.1d","Requirement","ECSS-Q-ST-70-01_1650008",1,"Created","The CRS shall be provided by the SRR as part of the review data package."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.1e","Requirement","ECSS-Q-ST-70-01_1650009",1,"Created","The C&CC responsible shall ensure compliance to both the ground and flight functional requirements and constraints of the project for each level of configuration.","NOTE \tTypical good practices e.g. Preparing a C&CC coordination plan, organising and supporting co-engineering activities starting before SRR, establishing and maintaining cleanliness and contamination control boards starting no later than PDR.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.1a","Requirement","ECSS-Q-ST-70-01_1650010",1,"Created","The supplier shall establish a Cleanliness and Contamination Control Plan (C&CCP) in conformance with the DRD outlined in Annex B (C&CCP DRD) and to be provided no later than the PDR."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.2a","Requirement","ECSS-Q-ST-70-01_1650011",1,"Created","As part of the C&CCP (see Annex B), a contamination budget and allocations shall be established."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.2b","Requirement","ECSS-Q-ST-70-01_1650012",1,"Created","The contamination budgets shall allocate the applicable cleanliness levels to the activities along the lifetime, at different MAIT, launch and mission phases.","NOTE \tAs an example for reusable vehicles mission phases are on ground, launch, in-flight and atmospheric entry and re-entry to a planet, dwarf planet or a natural satellite.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.3a","Requirement","ECSS-Q-ST-70-01_1650013",1,"Created","As part of the C&CCP (see Annex B), prediction tables shall be established including MAIT, launch campaign and all mission phases for the following:\n1.\tParticulate contamination;\n2.\tMolecular contamination."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.3b","Requirement","ECSS-Q-ST-70-01_1650014",1,"Created","The contamination predictions shall demonstrate the accumulation of molecular and particulate contaminants expected at MAIT, launch campaign and all mission phases."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.3c","Requirement","ECSS-Q-ST-70-01_1650015",1,"Created","An analysis shall be performed to predict particulate and molecular deposition on sensitive items and documented in agreement with the customer, including:\n1.\tIn-flight molecular contamination (e.g. organic contaminants, water ice):\n(a)\tKinetic parameters for in-flight molecular contamination modelling obtained as per ECSS-Q-TM-70-52.\n2.\tParticulate and molecular contamination during launch campaign including lift off until separation.\n3.\tParticulate and molecular contamination during atmospheric entry, re-entry and landing.\n4.\tParticulate and molecular contamination on sensitive items during mission phases such as on orbit servicing, in orbit manufacturing, docking.","NOTE \t1\tto item c: Examples of modelling techniques are given in Annex G.\nNOTE \t2\tto item c: Heritage data can be used for predictions of particulate and molecular deposition on sensitive items.\nNOTE \t3\tto item 1: Mathematical models and test methodology outlined in the ECSS-Q-TM-70-52 can be modified to increase accuracy by obtaining more parameters to increase the accuracy of the simulation.\nNOTE \t4\tto item 3: An example for reusable vehicles mission phases are on ground, launch, in-flight and atmospheric entry and re-entry to a planet, dwarf planet or a natural satellite.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.2.3d","Requirement","ECSS-Q-ST-70-01_1650016",1,"Created","Contamination corrective, mitigation and preventative actions to reduce contamination shall be investigated and implemented including their predicted efficiencies:\n1.\tIf contamination predictions or when available actual measurements, result in a higher than the specified level,\n2.\tIf models used for analysis in the early project phases are preliminary and considered high risk by the customer.","NOTE \tThe cleanliness verification activities can be specified in the C&CCP. The C&CCP as per Annex B can be tailored for test facilities with a particular view to their cleanliness and contamination control policy.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.1a","Requirement","ECSS-Q-ST-70-01_1650017",1,"Created","The supplier shall establish a Cleanliness and Contamination Control Verification Report (C&CCV) in conformance with the DRD outlined in Annex C (C&CCV DRD), to be provided no later than the PDR."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.2a","Requirement","ECSS-Q-ST-70-01_1650018",1,"Created","The supplier shall verify the fulfilment of the applicable cleanliness levels.","NOTE \t1\tCleanliness requirements are the maximum level of contamination for acceptable mission performances until EOL, and/or the maximum level of contamination applicable at the delivery of hardware.\nNOTE \t2\tThe demonstration as requirement 5.1.2.2.3b, with predictions updated using the actual measurements, is part of the verification.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.2b","Requirement","ECSS-Q-ST-70-01_1650019",1,"Created","The cleanliness verification of all activities specified in the C&CCP shall be demonstrated in the C&CCV."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.2c","Requirement","ECSS-Q-ST-70-01_1650020",1,"Created","On-ground cleanliness and contamination predictions shall be regularly updated with actual data from ground activities, including contamination monitoring measurements, the actual duration of activities, and other relevant factors affecting the predictions.","NOTE \t1\tUpdates of the predictions can be documented in the Cleanliness and Contamination Control Verification Report as per 5.1.2.3.2, or in a separate document referenced by the Contamination Control Verification Report.\nNOTE \t2\tRequirement 5.3.1.6a applies until the measurements from contamination monitoring are available.\nNOTE \t3\tThe document delivery schedule can be established in agreement with the customer.\nNOTE \t4\tSome examples of “other relevant factors” are e.g., performed anomalies, deviations, bakeouts, hardware orientation, applied protections.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.2d","Requirement","ECSS-Q-ST-70-01_1650021",1,"Created","Predictions for contamination sensitive and contamination critical items based on modelling analysis shall be verified and corrected against experimental data.\n1.\tFor in-flight molecular contamination via dedicated or as a part of planned testing activities during MAIT, or in-orbit measurements;\n2.\tFor particulate and molecular contamination during launch via dedicated tests, in situ data provided by the launch provider or heritage data."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.1.2.3.3a","Requirement","ECSS-Q-ST-70-01_1650022",1,"Created","A cleanliness declaration of conformity shall be delivered for space hardware at DRB together with the C&CCV."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.1a","Requirement","ECSS-Q-ST-70-01_1650023",1,"Created","The level of sensitivity to contamination shall be one of the drivers in the initial design."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.1b","Requirement","ECSS-Q-ST-70-01_1650024",1,"Created","The design shall be cleanliness oriented.","NOTE \t1\tA way to implement a cleanliness-oriented design is given in Annex F.\nNOTE \t2\tSuch design can contribute to achieve the contamination levels defined by the CRS on ground as well during the launch and mission.\nNOTE \t3\tA way to achieve the target contamination levels can be found in Annex E.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.1c","Requirement","ECSS-Q-ST-70-01_1650025",1,"Created","When the design baseline is incompatible with cleanliness requirements, the design changes shall be identified, and corrective actions be taken in close cooperation with all levels involved."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2a","Requirement","ECSS-Q-ST-70-01_1650026",1,"Created","When the offgassing effect of a material is a selection criterion, the supplier shall apply ECSS-Q-ST-70-29.","NOTE \tFor modelling the molecular contamination during on-ground activities, when outgassing data are too conservative, offgassing data are advisable.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2b","Requirement","ECSS-Q-ST-70-01_1650027",1,"Created","For the particulate contamination monitoring, inspection and quantification the supplier shall apply ECSS-Q-ST-70-50."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2c","Requirement","ECSS-Q-ST-70-01_1650028",1,"Created","When the microbiological contamination effect is a selection criterion, the supplier shall apply ECSS-Q-ST-70-55."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2d","Requirement","ECSS-Q-ST-70-01_1650029",1,"Created","When sterilization and material compatibility are selection criteria, the supplier shall apply ECSS-Q-ST-70-53. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2e","Requirement","ECSS-Q-ST-70-01_1650030",1,"Created","The outgassing screening test of materials shall be performed in accordance with ECSS-Q-ST-70-02 including the following conditions:\n1.\toutgassing data older than 10 years is not admissible for material selection;\n2.\tscreening outgassing tests is performed by a trusted test house.","NOTE \t1\tMODESA outgassing database can be referred to obtain updated list of the trusted test houses and reach the outgassing data.\nNOTE \t2\tTrusted test houses are those that can provide a Certificate of Conformity in compliance with ECSS-Q-ST-70-02 standards.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2f","Requirement","ECSS-Q-ST-70-01_1650031",1,"Created","Outgassing requirements shall be based on the quantity of material concerned, and the specific environmental conditions.","NOTE \tSpecific environmental conditions can be available volumes and temperatures.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2g","Requirement","ECSS-Q-ST-70-01_1650032",1,"Created","The outgassing criteria for materials within the direct and indirect view of sensitive items shall conform to following tables based on defined temperatures:\n1.\tat RT to Table 5‑1;\n2.\tat temperature below RT to Table 5‑2.","NOTE \t1\t“Indirect view” in a vacuum environment refers not only to the immediate surroundings but also to the consideration of reflections from other volumes and surfaces.\nNOTE \t2\tFor contamination sensitive items more stringent requirements can be applied based on analysis and mission requirements.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2h","Requirement","ECSS-Q-ST-70-01_1650033",1,"Created","The outgassing criteria for materials in the view of cryogenic surfaces shall conform to Table 5‑3.","NOTE \tFor materials in the view of cryogenic surfaces, more stringent requirements can be applied based on analysis and mission requirements.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.1.2i","Requirement","ECSS-Q-ST-70-01_1650034",1,"Created","Volatile metals shall not be used.","NOTE \t1\tThis is especially the case when the temperatures are above room temperatures.\nNOTE \t2\tSome metals such as cadmium and zinc have high vapour pressures and deposit metallic films can occur on adjacent surfaces.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1a","Requirement","ECSS-Q-ST-70-01_1650038",1,"Created","Personnel involved in the manufacturing of sensitive items shall be trained with respect to the cleanliness control policy."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1b","Requirement","ECSS-Q-ST-70-01_1650039",1,"Created","All elements manufactured in non­controlled areas or under non­clean conditions shall be the object of a cleaning process until the cleanliness requirements are met, before they are packaged for delivery."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1c","Requirement","ECSS-Q-ST-70-01_1650040",1,"Created","Cleaning and packaging operations for all elements shall be processed according to procedures approved by the customer for the specific application/product."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1d","Requirement","ECSS-Q-ST-70-01_1650041",1,"Created","Elements that can be cleaned after manufacturing shall be cleaned till the cleanliness requirements are met."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1e","Requirement","ECSS-Q-ST-70-01_1650042",1,"Created","For elements that cannot be cleaned after manufacturing, then manufacturing and assembling areas shall meet the cleanliness level requirements specification."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1f","Requirement","ECSS-Q-ST-70-01_1650043",1,"Created","The cleanliness conformity of the facilities shall be verified:\n1.\tfor manufacturing at MRR;\n2.\tfor integration at IRR;\n3.\tfor testing at TRR."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.1g","Requirement","ECSS-Q-ST-70-01_1650044",1,"Created","An audit of the manufacturing facilities shall be performed according to ECSS-Q-ST-10 clause 5.2.3 criteria. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2a","Requirement","ECSS-Q-ST-70-01_1650045",1,"Created","Involved personnel shall be trained with respect to the cleanliness policy."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2b","Requirement","ECSS-Q-ST-70-01_1650046",1,"Created","Contamination critical and contamination sensitive elements shall only be exposed during a predefined MAIT activity.","NOTE \t1\tExposure of sensitive and critical elements cannot be avoided e.g., during optical calibration or alignment.\nNOTE \t2\tDepending on the type of contamination, critical elements can be exposed to specific environments.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2c","Requirement","ECSS-Q-ST-70-01_1650047",1,"Created","When an exposure of contamination critical and contaminaton sensitive elements to an environmentally controlled area cannot be avoided, the exposure time and conditions shall be recorded."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2d","Requirement","ECSS-Q-ST-70-01_1650048",1,"Created","A set of assembly tools and equipment for assembly and integration shall be used and maintained in clean conditions."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2e","Requirement","ECSS-Q-ST-70-01_1650049",1,"Created","Procedures for assembly and integration shall be established for contamination critical item assembly."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2f","Requirement","ECSS-Q-ST-70-01_1650050",1,"Created","For the selection of the cleanroom, the allocated contamination budget and the duration of the integration shall be known. ","NOTE \tThe correlation between the airborne contamination and the particle fallout for normal cleanrooms is basically known (see clause 5.3.1), and so a rough estimate can be made of the type of cleanroom required. A practical contamination level for the cleanroom can be measured with representative activities and a representative number of operators. The expected contamination levels depend on the type of protection applied to critical hardware (e.g. covers, shields and purging).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2g","Requirement","ECSS-Q-ST-70-01_1650051",1,"Created","The conformity of the facilities shall be verified during MRR or TRR. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.2h","Requirement","ECSS-Q-ST-70-01_1650052",1,"Created","An audit of the integration facilities shall be performed according to ECSS-Q-ST-10 clause 5.2.3 criteria."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.3a","Requirement","ECSS-Q-ST-70-01_1650053",1,"Created","Involved personnel shall be trained with respect to the cleanliness policy."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.3b","Requirement","ECSS-Q-ST-70-01_1650054",1,"Created","For test centres, ECSS-Q-ST-20-07 shall apply."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.2.3c","Requirement","ECSS-Q-ST-70-01_1650055",1,"Created","The conformity of the facilities shall be verified during TRR."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1a","Requirement","ECSS-Q-ST-70-01_1650056",1,"Created","End to end launch campaign shall be designed and planned in accordance with the CRS, controlled by the C&CCP and verified in the C&CCV.","NOTE \tLaunch campaign is intended to cover the activities from arrival to the launch site until the S/C separation including contributions from the separation.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1b","Requirement","ECSS-Q-ST-70-01_1650057",1,"Created","A dedicated C&CCP shall be provided for the launch campaign by the launch provider."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1c","Requirement","ECSS-Q-ST-70-01_1650058",1,"Created","Personnel involved in pre-launch activities shall be trained with respect to the cleanliness policy of\n1.\tthe launch provider;\n2.\tspacecraft. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1d","Requirement","ECSS-Q-ST-70-01_1650059",1,"Created","The space system shall be shipped to the launch base under clean conditions as defined in the CRS, controlled by the C&CCP and verified in the C&CCV."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1e","Requirement","ECSS-Q-ST-70-01_1650060",1,"Created","The potential contamination during launch preparation shall be controlled.","NOTE \tThis can be done through the C&CCP or through specific launch base procedures approved by the project.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1f","Requirement","ECSS-Q-ST-70-01_1650061",1,"Created","Contamination during launch shall be controlled through specific preventive actions and design provisions.","NOTE \tPreventive actions can consist of cleaning and purging of the fairing. Specific design provisions can consist of shields controlling the depressurization.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.1g","Requirement","ECSS-Q-ST-70-01_1650062",1,"Created","Contamination control activities for launch shall include:\n1.\tif available, providing heritage data from previous launches;\n2.\tcleanliness verification of fairing prior to encapsulation at the latest possible moment;\n3.\tverification of all specific design provisions including but not limited to purging, shields, depressurization."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.2a","Requirement","ECSS-Q-ST-70-01_1650063",1,"Created","Launcher parts shall be clean to comply with CRS, and in line with the C&CCV of the space system.","NOTE \tLauncher parts can be fairings and mechanical systems for double or multiple launches.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.2b","Requirement","ECSS-Q-ST-70-01_1650064",1,"Created","The materials of the launch hardware in the direct and indirect view of the space system shall comply with CRS, and in line with the C&CCV of the space system itself."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.3.2c","Requirement","ECSS-Q-ST-70-01_1650065",1,"Created","The environment in which the spacecraft is put inside the fairing shall be compatible with the spacecraft characteristics.","NOTE \t1\tSpecific spacecraft design provisions can be protection mechanisms used to limit the launch contaminants, especially the “unknown” figure of particle transfer during launch.\nNOTE \t2\tA second design aspect is the location of the contamination­sensitive items with respect to the position of thrusters and of pyrotechnics or other contamination sources.\nNOTE \t3\tThe reflection by atmospheric molecules (i.e. atmospheric scattering) or by outgassing molecules (i.e. self­scattering) can take place and some form of modelling is of interest.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.4a","Requirement","ECSS-Q-ST-70-01_1650066",1,"Created","Spacecraft contamination control during mission shall be done through preventive actions, specific design provisions and operations.","NOTE \t1\tPreventive actions include materials selection (see clause 5.5.3 in ECSS-Q-ST-70-02), bakeout (see clause 5.4.2.4) and purging (see clause 5.4.2.5).\nNOTE \t2\tSpecific design provisions include the implementation of heaters for decontamination of sensitive surfaces, of shutters and baffles.\nNOTE \t3\tOperations include shielding during dumping, thrusters firing or venting, decontamination of sensitive surfaces through exposure to the Sun.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.4b","Requirement","ECSS-Q-ST-70-01_1650067",1,"Created","Fluids that can emerge to the exterior by leakage or intentional use of valves shall be considered in the design and operational requirements of system and equipment hardware."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.2.4c","Requirement","ECSS-Q-ST-70-01_1650068",1,"Created","A specific analysis shall be performed to ensure an optimum level of detection, location and isolation techniques.","NOTE \tThese fluids are originating from thermal, environmental or life support systems or subsystems or released due to crew activities (nutrients, wastes), during maintenance and repair and from experiments or payloads as well as the propellant systems.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1a","Requirement","ECSS-Q-ST-70-01_1650069",1,"Created","Cleanroom shell, floors, walls and ceiling shall be low shedding and the finish readily cleanable."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1b","Requirement","ECSS-Q-ST-70-01_1650070",1,"Created","The covering floor shall consist of one piece or, if this is not feasible, have a minimum number of joints."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1c","Requirement","ECSS-Q-ST-70-01_1650071",1,"Created","The floor shall be resistant to withstand wear by personnel and operations within the room."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1d","Requirement","ECSS-Q-ST-70-01_1650072",1,"Created","The room shall be designed such that only one door or entrance can be opened at one time, except in case of emergency."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1e","Requirement","ECSS-Q-ST-70-01_1650073",1,"Created","Entrances shall provide an air lock to allow a maintained pressurisation of the area."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1f","Requirement","ECSS-Q-ST-70-01_1650074",1,"Created","Anterooms shall be equipped for the changing of clothes and the storage of clothing, personal belongings and cleaning equipment."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.1g","Requirement","ECSS-Q-ST-70-01_1650075",1,"Created","Cleanrooms shall comply with ISO 14644-4:2022 requirements."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.2a","Requirement","ECSS-Q-ST-70-01_1650076",1,"Created","Air supply and filtration equipment shall have the capacity to filter all new and recirculated air entering the room to guarantee the defined ISO class."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.2b","Requirement","ECSS-Q-ST-70-01_1650077",1,"Created","Air conditioning equipment for prefiltering (particular and molecular), cooling, heating, humidification and dehumidification of the cleanroom air supply shall be supplied to guarantee the environmental conditions.","NOTE \tSee clauses 5.3.1.8, 5.3.1.9, 5.3.1.10 and 5.3.1.11.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.2c","Requirement","ECSS-Q-ST-70-01_1650078",1,"Created","In laminar flow cleanrooms, the air flow velocity through the cross section of the room shall be maintained at 27 m/min with a uniformity within ± 20 % throughout the undisturbed room."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.2d","Requirement","ECSS-Q-ST-70-01_1650079",1,"Created","Airflow patterns shall be uniform with minimum turbulence."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.3a","Requirement","ECSS-Q-ST-70-01_1650080",1,"Created","In laminar flow cleanrooms, (HEPA) filters shall cover either one entire wall or the entire ceiling, except when diffusion ceiling or wall systems are used or when built­in benches are included in the incoming air end of the room."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.3b","Requirement","ECSS-Q-ST-70-01_1650081",1,"Created","Monitoring shall be done and any work with highly sensitive equipment not be performed before the defined ISO class for the hardware has been reached. as specified in the C&CCP for the following situations:\n1.\tafter the installation of new filters,\n2.\tafter “at rest“ period,\n3.\tafter stand by period.","NOTE \tDue to the transitory pressure gradients, contamination previously trapped by HEPA filters, together with a reduction in the operating life of the filters themselves can be released.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.3c","Requirement","ECSS-Q-ST-70-01_1650082",1,"Created","The air flow inside cleanrooms and independent HEPA filtering systems shall be maintained during “at rest” periods, except for the maintenance operations.","NOTE \t1\tFor example, during filters replacement.\nNOTE \t2\tIndependent HEPA filtering systems can be like those used for the laminar flow tents and benches.\nNOTE \t3\tThis is to avoid the risk of redistribution of particles at restart of the flow.\nNOTE \t4\tException can be made for independent HEPA filtering systems that can work with a reduced air flow rate during stand­by periods.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.3d","Requirement","ECSS-Q-ST-70-01_1650083",1,"Created","In cases where a uniform and controlled molecular environment is required, the filtering system shall be equipped with additional molecular absorption filters positioned before the HEPA filters.","NOTE \tFiltering systems can be equipped with, for example, charcoal and zeolites.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.3e","Requirement","ECSS-Q-ST-70-01_1650084",1,"Created","When molecular absorption filters are used, the initial charge shall be assessed on installation and analysed regularly.","NOTE \tIt can be useful to evaluate the charge in contaminants of the filtering system which can release its charge in contaminants trapped. in order to be able to monitor the evolution and when a failure occurs.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.4a","Requirement","ECSS-Q-ST-70-01_1650085",1,"Created","Any airborne controlled environment shall be classified according to the Table 5‑4 reproduced from ISO 14644-1:2015.","NOTE \t1\tSuitability of the cleanroom class can only be assessed once the specified obscuration factors for critical surfaces are determined.\nNOTE \t2\tParticles of 5 μm are more critical than smaller particles, as fallout is mainly influenced by particles of this size or larger. \nNOTE \t3\tThe 5 μm particle size is often used as a benchmark because particles larger than 5 μm are particularly detrimental to optical surfaces, while particles in the 10 μm to 40 μm range are generally more harmful to bearings and gears. However, more stringent criteria can be applied in certain situations to ensure even higher levels of cleanliness and protection for sensitive components.\nNOTE \t4\tThe cleanroom classification can be determined based on at least two particle sizes (e.g., between 0,1 µm and 5 µm) relevant to the activities and sensitive items present in the cleanroom.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5a","Requirement","ECSS-Q-ST-70-01_1650087",1,"Created","The cleanroom air shall be monitored with dust counters."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5b","Requirement","ECSS-Q-ST-70-01_1650088",1,"Created","Accuracy and repeatability of instrumentation shall be demonstrated."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5c","Requirement","ECSS-Q-ST-70-01_1650089",1,"Created","Particle counts shall be acquired continuously for the monitoring of the cleanroom itself."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5d","Requirement","ECSS-Q-ST-70-01_1650090",1,"Created","A minimum of two particles counters shall be installed, one close to the air inlet and one or more according to the surface extent of the cleanroom by using the following law:\nN = log10 (S)\nwhere N is the number of particle counters and S is the surface of the cleanroom in m².","NOTE \tThe purpose of the location close to the air inlet is to check the quality of the in-coming air.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5e","Requirement","ECSS-Q-ST-70-01_1650091",1,"Created","For any contamination sensitive hardware and contamination critical operation, sampling frequency and locations shall be defined in the C&CCP. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5f","Requirement","ECSS-Q-ST-70-01_1650092",1,"Created","Monitoring techniques and routines shall be established to meet the requirements of a specific category of cleanroom or clean workstation."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5g","Requirement","ECSS-Q-ST-70-01_1650093",1,"Created","Sampling air volume for the cleanroom classification shall be established on the basis of the ISO 14644-1:2015, Annex B."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5h","Requirement","ECSS-Q-ST-70-01_1650094",1,"Created","Compliance with particles concentration limits shall be done with a frequency as specified per ISO 14644-2:2015, Clause 4.2.1."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5i","Requirement","ECSS-Q-ST-70-01_1650095",1,"Created","Determining the extent to which particles are deposited on surfaces shall be achieved. ","NOTE \tThis can be done through the exposure of test surfaces or samples to an environmentally controlled area and counting the settled particles by appropriate methods.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5j","Requirement","ECSS-Q-ST-70-01_1650096",1,"Created","Air monitoring of class ISO 8 or better shall be achieved by means of light scattering equipment."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5k","Requirement","ECSS-Q-ST-70-01_1650097",1,"Created","Tests shall be performed to determine if leaks exceed the specified limits, according to the filter characteristics:\n1.\tin the filter media themselves,\n2.\tin the bond between filter media and the interior of the filter frame,\n3.\tbetween filter frame gasket and filter bank supporting frames,\n4.\tbetween supporting frames and walls or ceilings."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5l","Requirement","ECSS-Q-ST-70-01_1650098",1,"Created","The cleanrooms shall have a monitoring function of the contamination levels and the environmental parameters."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5m","Requirement","ECSS-Q-ST-70-01_1650099",1,"Created","The cleanroom shall have an alarm function activated when warning levels are exceeded.","NOTE \t1\tThose warning levels are usually defined well below the out of specification limits in order to prevent their exceedance.\nNOTE \t2\tEnvironmental parameters are temperature, relative humidity and differential pressure.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.5n","Requirement","ECSS-Q-ST-70-01_1650100",1,"Created","Planned corrective actions shall be initiated to re­establish the nominal conditions in the shortest possible time and to prevent recurrence."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6a","Requirement","ECSS-Q-ST-70-01_1650101",1,"Created","Predictions shall assume particulate contamination deposition in cleanroom environments based on the correlation between airborne particles and PFO as established at rest values in Table 5‑5, until actual PFO measurements are available.","NOTE \t1\tPFO calculation from Table 5‑5 is not a conservative calculation and for this reason confirmation by PFO measurements as per this requirement is needed.\nNOTE \t2\tThe PFO calculation in Table 5‑5 is based on the particle size distribution as defined for the cleanroom classes in the ISO 14644-1:2015 and does not consider bigger particles or fibres.\nNOTE \t3\tAt-rest values need to be adjusted with the predicted in-operation durations of the mission.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6b","Requirement","ECSS-Q-ST-70-01_1650102",1,"Created","The budget, during the different project phases, shall be consolidated with in-situ measurements."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6c","Requirement","ECSS-Q-ST-70-01_1650103",1,"Created","PFO shall be monitored by witness plate exposure in an environmentally controlled area and measured according to ECSS-Q-ST-70-50."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6d","Requirement","ECSS-Q-ST-70-01_1650104",1,"Created","PFO levels shall be measured during a cleanroom acceptance, or after rework."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6e","Requirement","ECSS-Q-ST-70-01_1650105",1,"Created","Exposition duration shall be sufficient to ensure that the measured values are exceeding the method uncertainties."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6f","Requirement","ECSS-Q-ST-70-01_1650106",1,"Created","Measured PFO rates of a cleanroom at-rest shall be compliant with Table 5‑5."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6g","Requirement","ECSS-Q-ST-70-01_1650107",1,"Created","Location and number of witness plates shall be selected in order to measure particles in significant points of the environment."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.6h","Requirement","ECSS-Q-ST-70-01_1650108",1,"Created","When MAIT activities are ongoing, local particulate contamination monitoring shall be implemented as per clause5.4.2.2 and adapted to hardware configuration and sensitivity.","NOTE \t1\tParticulate deposit are strongly correlated to the level and type of activities in close vicinity, and therefore localized effects are expected \nNOTE \t2\tThe ISO class of the cleanroom is guaranteed through airborne particle measurements (see clause 5.3.1.5).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7a","Requirement","ECSS-Q-ST-70-01_1650110",1,"Created","Predictions shall assume a molecular contamination deposition of 0,5 × 10‐7 g/cm² in cleanroom environments over a continuous one-week period, until actual MOC measurements are available.","NOTE \tPredictions can also be based on reliable historical molecular contamination deposition records and proven trends for a given environment.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7b","Requirement","ECSS-Q-ST-70-01_1650111",1,"Created","Molecular contamination in controlled environments shall not exceed 2 ´ 10‑7 g/cm2 during a continuous period of one month, independently of the cleanroom classes.","NOTE \t1\tIn case of contamination sensitive equipment, a lower level can be required, and more stringent requirements can be set in agreement with the customer based on the contamination budget including exposure time.\nNOTE \t2\tCleanliness verification frequency can be adjusted depending on the customer needs.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7c","Requirement","ECSS-Q-ST-70-01_1650112",1,"Created","Molecular contamination measurements shall be monitored, measured, and reported according to ECSS-Q-ST-70-05, using at least two sets of witness plates, each set comprising two plates, and minimum in two different locations.","NOTE \t1\tThe number of sets of witnesses can be increased depending on the size of the cleanroom.\nNOTE \t2\tA technical justification supported by actual measurements can be used to reduce the number of exposed witness samples within the specific cleanroom configuration in agreement with the customer.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7d","Requirement","ECSS-Q-ST-70-01_1650113",1,"Created","One of the two witness of each set, namely step witness plate, shall be analysed at least once per month.","NOTE \tMeasurement frequency can be adjusted depending on the customer needs.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7e","Requirement","ECSS-Q-ST-70-01_1650114",1,"Created","The second witness plate of each set, namely cumulative witness plate, shall be analyzed:\n1.\tnot longer than 6 months after the previous cumulative witness measurement, and\n2.\tprior to cleanroom maintenance, cleaning and rework or other major activities performed in the cleanroom.","NOTE \tto item 1: Measurement frequency can be adjusted depending on the customer needs.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.7f","Requirement","ECSS-Q-ST-70-01_1650115",1,"Created","MOC measurement locations shall be selected to measure molecular contamination in significant points of the environment with at least one representative of the cleanroom at rest."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.8a","Requirement","ECSS-Q-ST-70-01_1650116",1,"Created","Cleanroom temperature shall be maintained and continuously monitored at nominally 22 °C ± 3 °C .","NOTE \tMore stringent temperature variations conditions can be imposed in case of critical operations.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.8b","Requirement","ECSS-Q-ST-70-01_1650117",1,"Created","The temperature distribution inside a cleanroom shall be controlled at representative locations for the hardware items.","NOTE \t1\tIn order to ensure that a nominal temperature is achieved throughout the room. Automatic devices can be used for temperature monitoring.\nNOTE \t2\tIf items being worked on are extremely sensitive to temperature changes, automatic devices with a warning system that comes into operation when a temperature change occurs can be used.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.9a","Requirement","ECSS-Q-ST-70-01_1650118",1,"Created","Segregation of the controlled environment shall be specified according to ISO 14644-4:2022 Section B.2.2 Segregation."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.9b","Requirement","ECSS-Q-ST-70-01_1650119",1,"Created","In case a physical barrier segregation is specified the pressure differential between adjacent areas shall at least be 5 Pa, where\n1.\ta positive pressure differential is maintained between the cleanroom and the personnel lock, and\n2.\tthe pressure decreases successively between the cleanroom, personnel lock and the surroundings."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.9c","Requirement","ECSS-Q-ST-70-01_1650120",1,"Created","The effectiveness of the utilised segregation concept shall be demonstrated as per utilised methodology defined in the ISO 14644-3:2019.","NOTE \t1\tThe effectiveness of the physical barrier concept can be demonstrated by undertaking a containment leak test and experimental airflow visualization as described in ISO 14644-3:2019.\nNOTE \t2\tOperational limitations that affect segregation can occur during certain activities, such as logistics in and out of the airlock. All impacted cleanroom users need to be informed in advance to implement appropriate contamination protection measures.\nNOTE \t3\tThe effectiveness can be reassessed with an agreement to the customer.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.9d","Requirement","ECSS-Q-ST-70-01_1650121",1,"Created","Pressure in all areas shall be monitored continuously.","NOTE \tIn order to take timely corrective actions in case of a pressure drop.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.10a","Requirement","ECSS-Q-ST-70-01_1650122",1,"Created","The relative humidity shall be maintained at (55 ± 10) % for general applications and be monitored continuously.","NOTE \tRelative humidity environments can be adjusted due to specific hardware constraints (see Annex J).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11a","Requirement","ECSS-Q-ST-70-01_1650123",1,"Created","All maintenance and cleaning activities shall be reported in a logbook."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11b","Requirement","ECSS-Q-ST-70-01_1650124",1,"Created","A maintenance and cleaning procedure or document shall be available, along with a planning."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11c","Requirement","ECSS-Q-ST-70-01_1650125",1,"Created","Maintenance shall comprise regular inspections of the cleanroom, its control facilities and its operating equipment, including calibration of all inspection and monitoring devices as specified in ECSS-Q-ST-20."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11d","Requirement","ECSS-Q-ST-70-01_1650126",1,"Created","Inspections of the cleanroom shall be performed at specified frequency, depending on the ISO class.","NOTE \tThose inspections assess the quality of the clean facility and describe any contamination production or events that are detrimental to the cleanroom cleanliness (e.g. repairs, system modifications, replacements, filter resistance measurements, leak checks or air speed measurements).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11e","Requirement","ECSS-Q-ST-70-01_1650127",1,"Created","The frequency of inspections and cleaning processes for a cleanroom shall be optimized.","NOTE \tThe inspections and cleaning can themselves be the source of contamination.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11f","Requirement","ECSS-Q-ST-70-01_1650128",1,"Created","Data shall be recorded in a logbook."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11g","Requirement","ECSS-Q-ST-70-01_1650129",1,"Created","Regular cleaning shall be performed depending on the ISO class."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11h","Requirement","ECSS-Q-ST-70-01_1650130",1,"Created","Procedures shall cover the cleaning of the cleanroom including personnel air lock; equipment air lock, walls, floors, furniture, crane lifting devices and GSE."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11i","Requirement","ECSS-Q-ST-70-01_1650131",1,"Created","The cleanliness after the cleaning operations shall be verified by inspection by means of UV or high intensity white light."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11j","Requirement","ECSS-Q-ST-70-01_1650132",1,"Created","Any personnel involved in cleaning operations shall be trained and informed about the criticality of a cleaning operation within a cleanroom."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11k","Requirement","ECSS-Q-ST-70-01_1650133",1,"Created","Cleaning tools, solvents and gases that are used for cleaning purposes shall be chosen not to have a detrimental effect on the hardware within the cleanroom.","NOTE \tCleanroom air of better than class ISO 8 is transported in a close loop. Since only a limited percentage of fresh air is fed to the loop, excessive use of solvents offgassing into the air, even if not flammable or toxic, can cause health problems.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.11l","Requirement","ECSS-Q-ST-70-01_1650134",1,"Created","When the level of contamination exceeds the cleanliness requirements specification, corrective actions shall be taken.","NOTE \tThe decision as to whether or not to clean depends on the integration flow of the unit within the cleanroom.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12a","Requirement","ECSS-Q-ST-70-01_1650135",1,"Created","An access control system shall be available independently for cleanrooms, storage area and equipment airlock."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12b","Requirement","ECSS-Q-ST-70-01_1650136",1,"Created","The access to the areas shall be controlled by a permanently operating access control or door lock system."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12c","Requirement","ECSS-Q-ST-70-01_1650137",1,"Created","Only authorized personnel shall have access to the cleanroom.","NOTE \tAccess control areas have a security lock at the entrance.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12d","Requirement","ECSS-Q-ST-70-01_1650138",1,"Created","Visitors and personnel without a work order shall not be allowed to enter the cleanroom."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12e","Requirement","ECSS-Q-ST-70-01_1650139",1,"Created","Visitors working in the cleanroom, shall: \n1.\twear specified cleanroom clothing,\n2.\tbe identifiable,\n3.\tbe instructed about the behaviour in a cleanroom."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12f","Requirement","ECSS-Q-ST-70-01_1650140",1,"Created","Racks or cabinets for street clothing shall be separated from those used for cleanroom clothing."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12g","Requirement","ECSS-Q-ST-70-01_1650141",1,"Created","Barriers or similar means separating clean and not clean zones inside the airlock shall be placed.","NOTE \tSimilar means can be tacky mats.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12h","Requirement","ECSS-Q-ST-70-01_1650142",1,"Created","Lint­free clothing shall be available and worn by all personnel within cleanroom area."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12i","Requirement","ECSS-Q-ST-70-01_1650143",1,"Created","Head covers or other garments shall be used as required to trap loose particles of hair, including but not only beard, moustache or skin flakes."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12j","Requirement","ECSS-Q-ST-70-01_1650144",1,"Created","Gloves, approved finger cots, tweezers or clean handling methods and equipment shall be used while working with or handling sensitive parts.","NOTE \tThis is to avoid contamination of those parts by loose skin or natural skin oils.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12k","Requirement","ECSS-Q-ST-70-01_1650145",1,"Created","All equipment shall be cleaned by dusting, vacuum suction, washing, or other means suited to the equipment involved before being brought into the area."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12l","Requirement","ECSS-Q-ST-70-01_1650146",1,"Created","Exhaust systems for grinding, welding or soldering, machining or related operations shall be installed."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12m","Requirement","ECSS-Q-ST-70-01_1650147",1,"Created","Actions related to equipment items with cooling fans shall be identified and mitigated in order to avoid contamination of critical hardware.","NOTE \tEquipment items with cooling fans are potential contamination sources.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12n","Requirement","ECSS-Q-ST-70-01_1650148",1,"Created","Personnel shall be instructed about the behaviour in a cleanroom."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12o","Requirement","ECSS-Q-ST-70-01_1650149",1,"Created","Personnel movements to and from the cleanroom shall be kept to a minimum."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12p","Requirement","ECSS-Q-ST-70-01_1650150",1,"Created","Smoking, eating and drinking shall not be permitted in the cleanroom, including the entering areas and air locks."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12q","Requirement","ECSS-Q-ST-70-01_1650151",1,"Created","Local cleanroom instructions shall specify the amount of protective clothing to be worn to reduce the contaminant transfer."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12r","Requirement","ECSS-Q-ST-70-01_1650152",1,"Created","If air showers are used, only suitably clothed personnel shall be allowed to enter."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12s","Requirement","ECSS-Q-ST-70-01_1650153",1,"Created","Paper, pencils or erasers shall be kept outside the clean facilities and only special non­shedding papers and ball­points be used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12t","Requirement","ECSS-Q-ST-70-01_1650154",1,"Created","Cosmetics and medicaments that can produce contamination shall not be used by any personnel.","NOTE \tIn particular, eye make­up, rouge, face powder, hair spray and fingernail polish.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12u","Requirement","ECSS-Q-ST-70-01_1650155",1,"Created","Fingernail polish shall not be permitted in the area."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12v","Requirement","ECSS-Q-ST-70-01_1650156",1,"Created","Before entering a cleanroom, hand lotions, creams or soap containing lanolin to tighten skin particles shall be used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.1.12w","Requirement","ECSS-Q-ST-70-01_1650157",1,"Created","Contact of hands with solvents shall be avoided.","NOTE \tMany solvents remove natural oils and cause excessive skin peeling or flaking.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2a","Requirement","ECSS-Q-ST-70-01_1650158",1,"Created","Procedures shall be available for:\n1.\tThe cleaning of the test facilities.\n2.\tThe pump­down and recovery sequences with respect to contamination redistribution.\n3.\tThe regeneration of sorption pumps.\n4.\tThe cleaning of cold traps.\n5.\tVerifying the cleanliness of the cold traps.\n6.\tContamination monitoring strategy:\n(a)\tQCM locations in the facility and operating procedures,\n(b)\tMOC witness locations in the facility and operating procedures,\n(c)\tPFO witness locations in the facility and operating procedures.","NOTE \t1\tto item 1: Handling of solvents and running a bakeout.\nNOTE \t2\tto item 2: A good solution, for chamber repressurization, is to add an HEPA filter to the repressurization piping and to collect the air for repressurization in a clean area (preferably ISO class 5).\nNOTE \t3\tto item 3: Sorption pumps can be e.g. cryopumps, zeolites, or charcoal.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2b","Requirement","ECSS-Q-ST-70-01_1650159",1,"Created","During testing in a vacuum facility, the test item shall not exceed the contamination limits specified by the test facility including the following:\n1.\tThreshold PFO values defined by the test facility in agreement with the customer.\n2.\tThreshold MOC values and measurement techniques defined by the test facility in agreement with the customer. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2c","Requirement","ECSS-Q-ST-70-01_1650160",1,"Created","A minimum vacuum level of 1 ´ 10-5 hPa shall be reached for TVAC testing."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2d","Requirement","ECSS-Q-ST-70-01_1650161",1,"Created","An approved declared material list (DML) of the hardware under test, including the test adapter and all connections shall be provided.","NOTE \tIncluding, for example mechanical and electrical connexions.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2e","Requirement","ECSS-Q-ST-70-01_1650162",1,"Created","The cleanliness verification of the blank TVAC chamber shall be demonstrated by either:\n1.\ta pre-TV to prove the cleanliness of the facility with a representative temperature and a duration of a single cycle of the TVAC test not less than 24 hours, after reaching the required in vacuum temperature and pressure for the item under test, or\n2.\tas an alternative to performing a dedicated pre-TV, and subject to customer approval, using documented test results obtained immediately prior to the TVAC test, provided these tests meet or exceed the TVAC test in terms of temperature, duration, sequence, and contamination sensitivity."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2f","Requirement","ECSS-Q-ST-70-01_1650163",1,"Created","During the pre-TV test, pump down and repressurization sequences shall be the same to the actual test.  "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2g","Requirement","ECSS-Q-ST-70-01_1650164",1,"Created","During the pre-TV test, test equipment, support equipment and cabling shall be included in the facility."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2h","Requirement","ECSS-Q-ST-70-01_1650165",1,"Created","Thermal vacuum test facilities shall demonstrate meeting requirement for a total molecular contamination below 1,0 x 10-7 g/cm² per vacuum cycle during pre-TV test. ","NOTE \t1\tMore stringent requirements can be defined on the specific project needs.\nNOTE \t2\tLess stringent requirement can be defined for non-contamination sensitive missions e.g. some telecommunication missions in agreement with the customer.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2i","Requirement","ECSS-Q-ST-70-01_1650166",1,"Created","The temperature and location of the witness sample shall be representative for the most contamination sensitive hardware in the vacuum chamber during the pre-TV test and actual TVAC testing. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2j","Requirement","ECSS-Q-ST-70-01_1650167",1,"Created","Surface particle contamination deposition levels per TVAC cycles shall be\n1.\tcompatible with customer TVAC cycle budget allocations;\n2.\tverified and demonstrated to be compatible against the PFO values specified in Table 5-6.","NOTE \tMore stringent requirement can be specified due to mission/hardware constraints.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.2k","Requirement","ECSS-Q-ST-70-01_1650168",1,"Created","The locations and temperatures of QCMs during TVAC cycles shall be assessed if TVAC is used as the verification activity for the in-flight molecular contamination model."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.3.3a","Requirement","ECSS-Q-ST-70-01_1650170",1,"Created","The CRS and the C&CCP shall address the cleanliness and contamination control policy for any other facility such as acoustic chamber, vibration facilities, anechoic chamber, and EMC chamber."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.1a","Requirement","ECSS-Q-ST-70-01_1650171",1,"Created","Cleaning shall be performed in order to ensure that the required cleanliness levels, expected in the contamination budget, and the final product cleanliness level are achieved.","NOTE \tIn order to meet the BOL requirements, a final cleaning of external surfaces can take place just before the entry of the space system into the fairing, or even just before closing the fairing.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.1b","Requirement","ECSS-Q-ST-70-01_1650172",1,"Created","The choice of the cleaning method shall be determined by the following criteria: \n1.\tThe type of contaminants to be removed.\n2.\tThe physical or chemical nature of the item to be cleaned.\n3.\tThe actual on ground phase.","NOTE \t1\tSome examples are provided in Annex K for removal of both particulate and molecular contamination.\nNOTE \t2\tThe cleaning of some parts is particularly important during the course of manufacture or before processing (e.g. prior to bonding, painting, vacuum, coating, welding and soldering).\nNOTE \t3\tAny detrimental effect of cleaning is evaluated as well as the order of the defined cleaning methods.\nNOTE \t4\tFor those items that are too delicate to withstand cleaning, preventive contamination control is of the utmost importance.\nNOTE \t5\tSee also ECSS-Q-ST-70-54 “Ultracleaning of flight hardware”.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.1c","Requirement","ECSS-Q-ST-70-01_1650173",1,"Created","The cleaning procedures shall be mentioned in the process specification."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.1d","Requirement","ECSS-Q-ST-70-01_1650174",1,"Created","The cleaning procedures shall be validated by tests on representative samples, or by experience from previous and similar projects, in which they were validated."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1a","Requirement","ECSS-Q-ST-70-01_1650175",1,"Created","Cleaning aids shall not increase the contaminant levels of the items to be cleaned."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1b","Requirement","ECSS-Q-ST-70-01_1650176",1,"Created","Aids, such as wipe tissues, papers, cloths, brushes and foams shall be non­flaking, lint free and dust free."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1c","Requirement","ECSS-Q-ST-70-01_1650177",1,"Created","Damage to surfaces as scratches shall be minimal."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1d","Requirement","ECSS-Q-ST-70-01_1650178",1,"Created","NVR of cleaning wipe materials shall be less than 0,01g/m2 for wiping extremely clean surfaces when extracted with IPA.","NOTE \tDifferent examples of NVR for common tissues are given in Annex A.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1e","Requirement","ECSS-Q-ST-70-01_1650179",1,"Created","When wipe materials are selected for cleaning, measurements shall be taken to determine their contaminant content."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.1f","Recommendation","ECSS-Q-ST-70-01_1650180",1,"Created","All wipe materials should be precleaned to achieve the specified level of cleanliness.","NOTE \tExtraction by solvents is the way for precleaning the wipes materials.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2a","Requirement","ECSS-Q-ST-70-01_1650181",1,"Created","The cleaning solvent shall be selected based on its compatibility with the material or item to be cleaned and its efficiency in removing contaminants.","NOTE \tA compatibility table between materials and solvents is given in Annex H.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2b","Requirement","ECSS-Q-ST-70-01_1650182",1,"Created","Toxicity and flammability of solvents shall be evaluated to demonstrate fit for use for the intended environment (see MIL-HDBK-406)."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2c","Requirement","ECSS-Q-ST-70-01_1650183",1,"Created","For precision cleaning, solvents of high purity shall be used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2d","Requirement","ECSS-Q-ST-70-01_1650184",1,"Created","Verified cleaning processes shall be applied to clean sensitive surfaces."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2e","Requirement","ECSS-Q-ST-70-01_1650185",1,"Created","The cleaning gas shall be: \n1.\tverified clean or certified,\n2.\tfree of oil,\n3.\tfiltered to remove water contamination, molecular or particulate contamination in accordance with the mission needs."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.1.2.2f","Requirement","ECSS-Q-ST-70-01_1650186",1,"Created","The use of chemicals shall be in line with applicable local laws.","NOTE \t1\tEU REACH, UK REACH, Swiss Chemicals Ordinance (ChemO) regulation and others ban or restrict the use of certain substances.\nNOTE \t2\tBasics of chemical regulatory framework and associated obsolescence risk management is described in detail in ECSS-Q-HB-70-23A, Annex D.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.1a","Requirement","ECSS-Q-ST-70-01_1650187",1,"Created","Particulate and molecular contamination shall be monitored.\n1.\tduring all the on-ground phases;\n2.\tfor specific missions during launch and in space.","NOTE \tIf monitoring is not feasible, advanced modelling (e.g. outgassing via CVCMs, PAC redistribution under fairing, decontamination efficiency) can be used as an alternative.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.2.1a","Requirement","ECSS-Q-ST-70-01_1650188",1,"Created","Particulate contamination shall be monitored through visual inspection and be quantified through optical monitoring of surfaces as per ECSS-Q-ST-70-50."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.2.1b","Requirement","ECSS-Q-ST-70-01_1650189",1,"Created","Surfaces shall be examined using a suitable methodology and inspection sensitivity as outlined in ECSS-Q-ST-70-50:\n1.\tvisibly clean standard to be performed under oblique white light of more than 540 lx and from a distance of 150 cm to 300 cm using normal vision;\n2.\tvisibly clean sensitive to be performed under oblique white light of more than 540 lx and from a distance of 60 cm to 120 cm using normal vision;\n3.\tvisibly clean highly sensitive to be performed under oblique white light of more than 1080 lx and from a distance of 15 cm to 45 cm using normal or magnified vision.","NOTE \t1\tDifferent kinds of lights can be used: portable diving light or “white light” is often used for standard inspection. In addition, ultra­violet lamp or “black light” (365 nm) can be used for inspection of organic residues and dust particles as it increases their visibility.\nNOTE \t2\tTypical methods are the measurement of transmission or reflection loss and nephelometry (i.e. scattering of light). These methods can be used for all types of contaminants, both organic and inorganic. Photographic determination of dust particles on surfaces is also possible, as is automatic counting.\nNOTE \t3\tExtraction methods can be performed by:\n·\ttape lift, using sticky tapes (according to ECSS-Q-ST-70-50);\n·\tblowing and suction of air;\n·\twashing of the surface of interest and counting the particles in the washing fluid either directly using a commercial instrument, or on a filter after filtration of the liquid.\nNOTE \t4\tVisible inspection cannot be used to quantify surface cleanliness levels, it is only a qualitative method as per ECSS-Q-ST-70-50.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.2.1c","Requirement","ECSS-Q-ST-70-01_1650190",1,"Created","When using ultra­violet or “black light” (365 nm) lamps for inspection of organic residues, the induced thermal and health effects shall be assessed."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.2.2a","Requirement","ECSS-Q-ST-70-01_1650191",1,"Created","Molecular contamination shall be monitored as follows:\n1.\tvisual inspection methodology used only for qualitative assessment;\n2.\tquantitative methods using direct surface measurements, and witness materials, or indirect methods as described in ECSS-Q-ST-70-05.","NOTE \t1\tto item 1: Surfaces can be examined by the same visual inspection methods as for particulate contamination., A contamination can be revealed by contrast. \nNOTE \t2\tto item 2: Direct measurements can be made in situ using quartz crystal microbalances (QCM).\nNOTE \t3\tto item 2: Further analyses can be performed to characterize molecular contamination (e.g. gas chromatography, mass spectrometry, SEM).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.3a","Requirement","ECSS-Q-ST-70-01_1650192",1,"Created","Monitoring of molecular and particulate contaminants in vacuum facilities shall be achieved using: \n1.\tfor all contamination sensitive and contamination critical items the QCM together with the witness method, including auxiliary items, and\n2.\tfor all non-contamination sensitive and non-contamination critical items the QCM or the witness method or a combination of both."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.3b","Requirement","ECSS-Q-ST-70-01_1650193",1,"Created","When using the witness method the temperature and location of witnesses shall be representative of the item.","NOTE \t1\tWitnesses (for both molecular and particulate contamination) can be placed on or near suspect places for a specified time and then subjected to one of the standard analyses.\nNOTE \t2\tA QCM can be used to detect contamination levels down to 1 ´ 10‑9 g/cm2, and to measure condensation rates. Such QCMs can operate down to liquid nitrogen temperatures.\nNOTE \t3\tA mass spectrometer is not sufficient to monitor the condensable contaminants but in combination with a QCM, it can help describing the different condensed species during a controlled re­evaporation from the QCM.\nNOTE \t4\tA cryopanel can be used to collect all molecular contaminants for further analyses.\nNOTE \t5\tAdditional representative witness materials can be used to evaluate contaminant-surface interactions.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4a","Requirement","ECSS-Q-ST-70-01_1650194",1,"Created","The supplier shall perform vacuum bakeouts to reduce the non-water contaminants outgassed in vacuum and the surface contamination collected during ground life.","NOTE \t1\tBakeouts started at the lowest possible product level allow to reach highest bakeout temperatures (i.e. avoiding the temperature constraints at higher assembly level) and hence a more efficient bakeout programme.\nNOTE \t2\tTypical materials on which bakeout is applied are:\n·\tHarness,\n·\tMLI,\n·\tCarbon and glass fibre components,\n·\tGlued, coated or potted materials,\n·\tContamination critical items/ equipment / sub-system,\n·\tContamination sensitive items/ equipment / sub-system.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4b","Requirement","ECSS-Q-ST-70-01_1650195",1,"Created","The bakeout conditions (temperature, time, pressure) shall not have a detrimental effect on the functionality of the item / equipment / sub-system  under bakeout."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4c","Requirement","ECSS-Q-ST-70-01_1650196",1,"Created","The bakeout chamber shall incorporate (by design) at least one “cryo-panel” (Liquid Nitrogen cooled plate - “scavenger plate” or “cold trap”) to collect and trap outgassed components evolved during the bake-out."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4d","Requirement","ECSS-Q-ST-70-01_1650197",1,"Created","When determining the bakeout temperature, the following aspects shall be considered:\n1.\tThe maximum survivable temperature of the limiting material within the item, equipment, or subsystem is determined, ensuring no degradation occurs.\n2.\tThe maximum temperature experienced during the mission, whether in operational or non-operational mode, is identified.\n3.\tThe qualification temperature of the item, equipment, or subsystem does not exceed, accounting for the temperature measurement uncertainties of the facility.","NOTE \t1\tIt is more efficient to perform a bakeout at the lowest possible product level to allow reaching higher bakeout temperature to avoid temperature constraints at higher assembly level.\nNOTE \t2\tItems with cavities and venting holes require an effective bakeout strategy due to potential inefficiencies during the process. Outgassed products can take a long time to fully vent and can potentially cross-contaminate sensitive surfaces within the cavity.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4e","Requirement","ECSS-Q-ST-70-01_1650198",1,"Created","The effectiveness of the bakeout shall be monitored by using a QCM considering:\n1.\tthe QCM is properly installed and operated;\n2.\tthe observed frequency change during the hardware test is large enough to avoid artefacts in the measurement while avoiding saturation of the sensor;\n3.\tThe bakeout is performed when all parts have reached temperature within 0,5 °C of the steady state temperature;\n4.\ttemperature fluctuations and temperature r.m.s. variation cannot be more than ±1,0 °C in an hour and no more than ±2,0 °C in a day;\n5.\ttemperature drift cannot be more than a 1,0 °C change in the average temperature of consecutive 24-hour periods;\n6.\tQCM temperature is constant;\n7.\tsample temperature and facility pressure data is provided along with the QCM data.","NOTE \t1\tto item 2: Depending on which type of the QCM is used, the dynamic range of a QCM can be anywhere from a few kHz to a few 100 kHz.\nNOTE \t2 \tto item 2: The actual observed frequency rate depends on the view factor (VF) of the QCM with the hardware. Ideally, the VF is such that the full range of the QCM is used. If the VF is too small, the observed frequency change can contain artefacts from the temperature dependence of the sensor crystals and/or electronics. These artefacts are typically of the order of a few Hz, so a sensor signal of 10s of a few Hz is necessary to avoid that the artefacts become dominant in the analysis. On the other hand, if the VF is too large, the risk is that the sensor saturates within hours making analysis impossible.\nNOTE \t3\tto item 2: A saturated QCM in-situ can be cleaned by thermal evaporation of the contaminants on the sensor crystal, by temporarily setting the sensor temperature to the maximum temperature before returning to the original (or new) set point.\nNOTE \t4\tto item 6: In addition to the QCM, other complementary methods e.g. Residual Gas Analysis (RGA) can be used to monitor the chemical species in vacuum.\nNOTE \t5\tto item 6: QCM sensor temperatures are typically maintained at temperatures in the range from -50 °C to 0 °C. Since the deposition rate on the QCM depends on the QCM temperature, with low sensor temperatures showing a higher deposition rate than high sensor temperatures, QCM sensor temperature can be used to modify the QCM signal during the bake-out. \n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4f","Requirement","ECSS-Q-ST-70-01_1650199",1,"Created","If the steady state temperature as specified in 5.4.2.4e.3 changes during the bakeout the following shall be performed:\n1.\ta re-evaporation of the QCM, and\n2.\trestarting of the timer on the 48 hours of data requirement for the analysis."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4g","Requirement","ECSS-Q-ST-70-01_1650200",1,"Created","Independently of the chosen method, success criteria shall be established and approved before starting the bakeout."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4h","Requirement","ECSS-Q-ST-70-01_1650201",1,"Created","Independently of any stopping and verification criteria, the minimum bakeout duration shall be 72 hours."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4i","Requirement","ECSS-Q-ST-70-01_1650202",1,"Created","A bakeout \"stopping criterion\" of a 1 % per hour deviation from linearity shall be used based on QCM monitoring, with a minimum bakeout duration of 72 hours.","NOTE \t1\tThis \"stopping\" criterion is a method to assess whether continuing the bakeout is worthwhile. For example, this criterion can be based on the change in the mass rate, specifically the second derivative of the QCM frequency.\nNOTE \t2\tThe deviation from linearity of the parameter can be optimized based on the contamination sensitivity of the item.\nNOTE \t3\tIf a facility that has a demonstrated QCM view factor is used for the bakeout stopping criterion can be based on deposition rate e.g. grams/hour.\nNOTE \t4\tSee Annex L for detailed information about Bakeout Analysis Methodology.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4j","Requirement","ECSS-Q-ST-70-01_1650203",1,"Created","The background of the baking facility shall be determined before starting the bakeout."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.4k","Requirement","ECSS-Q-ST-70-01_1650204",1,"Created","Baking time shall start when the material/item under baking has reached the predefined bakeout temperature."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5a","Requirement","ECSS-Q-ST-70-01_1650205",1,"Created","The purging shall be performed inside a cavity to maintain a constant exchange of the gas present in the cavity. ","NOTE \t1\tThis exchange depends on the entry flow rate of the gas and the total surface leaks.\nNOTE \t2\tThe aim of the purging is not only to protect the critical hardware such as optics from contamination by injecting a non­ionized high­purity dry gas inside a cavity but also a way for decontamination (e.g. removal of water for dimensional stability of composite).\nNOTE \t3\tThe purging can be implemented at instrument or spacecraft level during functional and performance tests at ambient conditions, during repressurization after TB/TV and TV tests, during all the phases without activities and during storage, transport and pre-launch phases up to the final close of the fairing. (In case of an aborted launch, purging can be not re­installed).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5b","Requirement","ECSS-Q-ST-70-01_1650206",1,"Created","The analytical method used to verify the purge system cleanliness shall be agreed with the customer depending on one or more of the following items:\n1.\tchemical species of interest;\n2.\twater content;\n3.\tnumber of locations to be verified;\n4.\tnumber of gas outlets;\n5.\tlimit(s) of detection of the measurement(s)."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5c","Requirement","ECSS-Q-ST-70-01_1650207",1,"Created","The cleanliness of each pipe shall be verified when multiple purge system pipes are used throughout the system lifetime."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5d","Requirement","ECSS-Q-ST-70-01_1650208",1,"Created","The purity of the gas at each outlet of the purge system shall be verified using an analytical technique agreed with the customer.","NOTE \t1\tFor example, purging the gas through a sorption tube followed by thermal desorption GC-MS is an established technique for verifying VOC. \nNOTE \t2\tIn practice, multiple purge system pipes are used throughout the lifetime of the project. Thus, it is a good practice to verify the cleanliness of each pipe individually. \nNOTE \t3\tIn this context “each outlet” is not limited to the final interfaces between the purge system and the spacecraft. Rather, outlets preceding the final interface are also described by this term. For example, connection between the gas source and the purge cart is also considered an outlet.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5e","Requirement","ECSS-Q-ST-70-01_1650209",1,"Created","Filtering systems (both for MOC and PAC) compatible with the relevant cleanliness requirements shall be provided before the gas comes into contact with the hardware."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.2.5f","Requirement","ECSS-Q-ST-70-01_1650210",1,"Created","The purging strategy of the mission shall be described and delivered as a part of the CRS in conformance with the DRD in Annex A."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3a","Requirement","ECSS-Q-ST-70-01_1650211",1,"Created","Provisions shall be taken for packaging, containerization, transportation and storage.","NOTE \tIn order to maintain the cleanliness levels achieved at any point from initial precision cleaning to delivery to the launch site.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3b","Requirement","ECSS-Q-ST-70-01_1650212",1,"Created","Cleanliness protection shall be provided prior to leaving the controlled areas, or whenever a storage period is planned."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3c","Requirement","ECSS-Q-ST-70-01_1650213",1,"Created","Transport and storage containers shall be made of non-particle shedding materials."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3d","Requirement","ECSS-Q-ST-70-01_1650214",1,"Created","Containers carrying sensitive items shall be pressurized with gaseous nitrogen.","NOTE \tOptical units and payloads are examples of sensitive units \n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3e","Requirement","ECSS-Q-ST-70-01_1650215",1,"Created","Containers carrying sensitive items shall also have as rigorous cleaning schedule as the parts themselves."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3f","Requirement","ECSS-Q-ST-70-01_1650216",1,"Created","It shall be ensured that containers used for transportation of clean parts do not transfer contamination from surface to surface within the cleanroom itself.","NOTE \tWitness plates can be placed inside containers.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3g","Requirement","ECSS-Q-ST-70-01_1650217",1,"Created","When sensitive items are packaged, containers for long­term storage or transportation, shall include provision for internal flushing with dry high­purity nitrogen and over­pressurization of 100 hPa minimum, except if units are put in sealed bags."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3h","Requirement","ECSS-Q-ST-70-01_1650218",1,"Created","For long term storage of sensitive items, containers shall be equipped with an inlet valve and an outlet valve clearly identified."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3i","Requirement","ECSS-Q-ST-70-01_1650219",1,"Created","The design of the container shall facilitate easy cleaning and inspection of its surfaces, avoiding any kind of dirt traps."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3j","Requirement","ECSS-Q-ST-70-01_1650220",1,"Created","Small clean parts shall be double bagged in airtight envelopes during storage or transportation outside controlled clean areas."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3k","Requirement","ECSS-Q-ST-70-01_1650221",1,"Created","Bags for contamination sensitive items shall be flushed with dry nitrogen or dry clean air and then sealed."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3l","Requirement","ECSS-Q-ST-70-01_1650222",1,"Created","Only approved materials that were procured as cleaned films shall be used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3m","Requirement","ECSS-Q-ST-70-01_1650223",1,"Created","Static sensitive items shall use metallized films."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3n","Requirement","ECSS-Q-ST-70-01_1650224",1,"Created","Outer bags shall not enter controlled clean areas."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3o","Requirement","ECSS-Q-ST-70-01_1650225",1,"Created","When used, desiccants shall be in bags that are clean and do not produce particulate contamination."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3p","Requirement","ECSS-Q-ST-70-01_1650226",1,"Created","Desiccants and humidity indicators shall be placed in the external envelope."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","5.4.3q","Requirement","ECSS-Q-ST-70-01_1650227",1,"Created","Procedures shall be provided for packaging, containerization, transportation and storage."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<1>a","Requirement","ECSS-Q-ST-70-01_1650228",1,"Created","The CRS shall give a general overview of the item to which the CRS refers, describing sensitive items and contamination sources, in consideration of:\n1.\tpossible impacts of contaminants on their physical or functional characteristics; \n2.\tpossible effects of contamination on the performance; \n3.\ttheir impact as potential sources of contamination."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<1>b","Requirement","ECSS-Q-ST-70-01_1650229",1,"Created","The CRS shall specify the pressures (or other molecular fluxes) that can be reached in connection with voltage breakdown, arcing, corona discharges, multipaction, opening time of shutters and ejection time of covers."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<2>a","Requirement","ECSS-Q-ST-70-01_1650230",1,"Created","The CRS shall basically specify major on­ground activities to be analysed for their impact on contamination and the relevant on-ground contamination environment.","NOTE \tUsually, the preparation of a flowchart, that can be added as appendix to the CRS, helps in the description (see Annex D).\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<2>b","Requirement","ECSS-Q-ST-70-01_1650231",1,"Created","The CRS shall specify the flight environmental factors (natural and induced) that affect the contamination phenomena, such as solar radiation, electron, proton and AO fluxes, together with the planned mission profile/duration."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<2>c","Requirement","ECSS-Q-ST-70-01_1650232",1,"Created","The CRS shall specify sensitive item temperatures to be used for the analyses during ground and in-flight operations.","NOTE \tThe expected temperatures and temperature profiles of these items can be important for condensation and the residence times of the contaminants.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<3>a","Requirement","ECSS-Q-ST-70-01_1650233",1,"Created","The CRS shall describe all possible contamination sources to be analysed and the maximum acceptable emissions.","NOTE \tFor example: Materials outgassing, lubricants escaping from bearings, wear particles from moving parts, terrestrial contaminants such as dust, plume contaminants from thrusters and engines, leaks from fuel systems and from hermetically sealed components, dumps and EVA, co­passengers, fairing and equipment bay items of the launcher.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<3>b","Requirement","ECSS-Q-ST-70-01_1650234",1,"Created","The CRS shall specify the chemical nature of the contaminants listed under <3>a. with their vapour pressures or relevant condensation conditions."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<3>c","Requirement","ECSS-Q-ST-70-01_1650235",1,"Created","The CRS shall specify the transport mechanisms of the potential contaminants from the sources under <3>a. to the contamination sensitive items or areas to be considered in the contamination analysis.","NOTE \tFor example: direct flux, reflected flux, ambient scatter, self­scatter and creeping.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<3>d","Requirement","ECSS-Q-ST-70-01_1650236",1,"Created","The CRS shall specify the contamination environment to be applied for design.","NOTE \tFor example, molecular column density, maximum molecular deposition on the sensitive items.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<3>e","Requirement","ECSS-Q-ST-70-01_1650237",1,"Created","The CRS shall specify the maximum allowable contamination levels for all contamination-sensitive items, where the limits are determined through analysis, based on the acceptable performance losses expected by the mission's EOL.","NOTE \tLaboratory test data could be necessary for adequate analyses.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<4>a","Requirement","ECSS-Q-ST-70-01_1650238",1,"Created","The CRS shall specify all cleanliness requirements allocated to the major integration and testing phases. "]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","A.2.1<4>b","Requirement","ECSS-Q-ST-70-01_1650239",1,"Created","The CRS shall specify acceptable contamination levels of MOC and PAC for all on ground and in-flight phases."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<1>a","Requirement","ECSS-Q-ST-70-01_1650240",1,"Created","The C&CCP shall contain description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<2>a","Requirement","ECSS-Q-ST-70-01_1650241",1,"Created","The C&CCP shall list the applicable and reference documents to support the generation of the document."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<3>a","Requirement","ECSS-Q-ST-70-01_1650242",1,"Created","The C&CCP shall include any additional terms, definitions or abbreviated terms used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<4>a","Requirement","ECSS-Q-ST-70-01_1650243",1,"Created","The C&CCP shall give a general overview of the item it pertains to."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<4>b","Requirement","ECSS-Q-ST-70-01_1650244",1,"Created","The C&CCP shall describe sensitive items and contamination critical items and contamination sources, listing those surfaces/items to be strictly controlled or protected from the cleanliness point of view due to:\n1.\tThe possible impacts of contaminants on their physical or functional characteristics.\n2.\tTheir impact as potential sources of contamination."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<5.1>a","Requirement","ECSS-Q-ST-70-01_1650245",1,"Created","The C&CCP shall contain a summary of cleanliness requirements, relevant for the system or hardware and eventual sub-assemblies, as given in CRS or dedicated analysis.","NOTE \tExample of such requirements are MOC, PAC, and during the different phases on ground and in-flight.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<5.2>a","Requirement","ECSS-Q-ST-70-01_1650246",1,"Created","The C&CCP shall contain the allocation of contamination levels through the splitting of cleanliness requirements during the major integration and testing phases.","NOTE \tIn case the outgassing contribution to the performance loss is large with respect to other contributions (mainly for sensitive instruments with tight requirements), more detailed modelling are performed.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<5.3>a","Requirement","ECSS-Q-ST-70-01_1650247",1,"Created","The C&CCP shall define the requirements that have design impacts like PMP selection criteria (see ECSS-Q-ST-70), venting, purging and thrusters’ locations, in accordance with the mission cleanliness and outgassing requirements and the outcome of the clauses 5.1 and 5.2."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<5.4>a","Requirement","ECSS-Q-ST-70-01_1650248",1,"Created","The C&CCP shall describe the preventative and corrective measures for the coordination and resolution of cleanliness and contamination control issues among the parties involved in the project."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<5.4>b","Requirement","ECSS-Q-ST-70-01_1650249",1,"Created","The C&CCP shall describe the preventative and corrective actions in terms of design, shielding, purging, bakeout in case the predictions are outside acceptance limits and in cases where corrective actions are necessary because of deviation from the original cleanliness policy.","NOTE \tIn general, the organization of regular workshops dedicated to cleanliness and contamination control for a specific programme is a good practice.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<6>a","Requirement","ECSS-Q-ST-70-01_1650250",1,"Created","The C&CCP shall contain a brief description of MAIT areas, their classification, facility location and tools for contamination control."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<6>b","Requirement","ECSS-Q-ST-70-01_1650251",1,"Created","References for internal procedures dedicated to area or facilities verification, control and maintenance shall be included."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<6>c","Requirement","ECSS-Q-ST-70-01_1650252",1,"Created","The C&CCP shall contain a list (or brief description) of internal procedures for personnel training and rules to operate under contamination control conditions."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.1>a","Requirement","ECSS-Q-ST-70-01_1650253",1,"Created","The C&CCP shall detail the splitting of cleanliness prediction during MAIT phases, according to planned duration, environment class, type of operation, and dedicated provisions adopted."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.1>b","Requirement","ECSS-Q-ST-70-01_1650254",1,"Created","The C&CCP shall list all phases where contamination can be expected and where the levels can exceed the allocated levels."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.2>a","Requirement","ECSS-Q-ST-70-01_1650255",1,"Created","The C&CCP shall describe selected methods, procedures and instruments to control contamination levels during MAIT activities on systems or equipment and relevant documentation; in particular:\n1.\tContamination monitoring methods and tools.\n2.\tInspection procedures and tools.\n3.\tVerification of tools or hardware.\n4.\tDedicated cautions for critical AIV operations."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.3>a","Requirement","ECSS-Q-ST-70-01_1650256",1,"Created","The C&CCP shall define the cleaning and decontamination methods, procedures and tools, also making reference to their applicability and eventual process parameters.","NOTE \tList of items and process parameters (e.g. for a bakeout: temperature, pressure and minimum durations, stop criteria are part of the information of this clause.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.4>a","Requirement","ECSS-Q-ST-70-01_1650257",1,"Created","The C&CCP shall describe the provisions for the transportation of contamination sensitive, contamination critical items, including processes or functions defined in the critical item list (CIL). ","NOTE \tProcesses or functions that are identified in the Critical Item List susceptible to degradation, failure, or non-compliance and that can negatively affect mission performance result in non-fulfilment of requirements due to cleanliness and contamination control. These items typically require dedicated monitoring, handling, and control measures throughout all project phases, from procurement to launch.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.4>b","Requirement","ECSS-Q-ST-70-01_1650258",1,"Created","The C&CCP shall include:\n1.\tA description of containers and packaging tools to be used during hardware transportation.\n2.\tThe way they are stored.\n3.\tThe way they are handled.\n4.\tThe way they are monitored and cleaned.\n5.\tThe way their cleanliness is verified.\n6.\tThe way their cleanliness is maintained."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.5>a","Requirement","ECSS-Q-ST-70-01_1650259",1,"Created","The C&CCP shall define:\n1.\tthe sampling plan for PAC and MOC,\n2.\tcleaning operations (when planned), and\n3.\tinspection points."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.5>b","Requirement","ECSS-Q-ST-70-01_1650260",1,"Created","A cleanliness control flow chart shall be established, showing the stages at which specific cleanliness controls are undertaken as defined in the C&CCP, reported in an annex to the C&CCP."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.6>a","Requirement","ECSS-Q-ST-70-01_1650261",1,"Created","Responsibility and authority shall be assigned for the implementation of the cleanliness and contamination control tasks."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<7.6>b","Requirement","ECSS-Q-ST-70-01_1650262",1,"Created","The C&CCP shall describe responsibilities for:\n1.\tHardware inspections\n2.\tCleanrooms and facilities\n3.\tContamination monitoring (hardware)."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<8>a","Requirement","ECSS-Q-ST-70-01_1650263",1,"Created","The C&CCP shall define the forms that are used to document the cleanliness and contamination control activities defined by the C&CCP."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","B.2.1<8>b","Requirement","ECSS-Q-ST-70-01_1650264",1,"Created","As minimum, the following forms shall be defined:\n1.\tPAC and MOC measurement report.\n2.\tCleanliness declaration of conformity (see ECSS-Q-ST-20)."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<1>a","Requirement","ECSS-Q-ST-70-01_1650265",1,"Created","The C&CCV shall contain description of the purpose, objective, content and the reason prompting its preparation."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<2>a","Requirement","ECSS-Q-ST-70-01_1650266",1,"Created","The C&CCV shall list the applicable and reference documents to support the generation of the document."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<3>a","Requirement","ECSS-Q-ST-70-01_1650267",1,"Created","The C&CCV shall include any additional terms, definitions or abbreviated terms used."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<4>a","Requirement","ECSS-Q-ST-70-01_1650268",1,"Created","The C&CCV shall provide a table of:\n1.\tcontamination sensitive items and contamination critical items as defined in Annex B;\n2.\timpacted performance for the contamination sensitive items;\n3.\tthe implemented contamination verification techniques including but not only for the allocated budgets, but also for major MAIT activities, transportation, storage, launch campaign, launch, in-flight and in-orbit;\n4.\tcontamination mitigation measures;\n5.\tcontamination preventive measures;\n6.\tcontamination corrective measures."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<4>b","Requirement","ECSS-Q-ST-70-01_1650269",1,"Created","The C&CCV shall provide a list and status of all RFAs, RFDs and RFWs impacting the analysis of all the contamination critical and contamination sensitive items."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<5>a","Requirement","ECSS-Q-ST-70-01_1650270",1,"Created","The C&CCV shall provide:\n1.\ta verification and a validation matrix and reference to supporting documents for all items in the C.2.1<4>;\n2.\ta verification matrix for all requirements in Annex A and Annex B for all contamination sensitive items; \n3.\ta verification matrix for all cleanliness and contamination control impacted items defined in critical item list (CIL);\n4.\tthe values of the verified efficiency of contamination corrective, mitigation  and preventive actions to reduce contamination agreed with the customer;\n5.\tall mathematical models and simulations verified against experimental data to ensure its accuracy and validity.","NOTE \tto item 3: Processes or functions that are identified in the Critical Item List susceptible to degradation, failure, or non-compliance and that can negatively affect mission performance result in non-fulfilment of requirements due to cleanliness and contamination control. These items typically require dedicated monitoring, handling, and control measures throughout all project phases, from procurement to launch.\n"]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<6>a","Requirement","ECSS-Q-ST-70-01_1650271",1,"Created","The C&CCV shall provide a table comparing the maximum allowable contamination levels for each contamination sensitive item with the contamination levels verified by measurement for on-ground phases and by modelling for the in-orbit phases."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<7>a","Requirement","ECSS-Q-ST-70-01_1650272",1,"Created","The C&CCV shall certify the compliancy of the contamination levels regarding the contamination requirements for each sensitive items."]
["ECSS-Q-ST-70-01C Rev.1 DIR1  impl. DRRs","ECSS - Current v1.0","C.2.1<7>b","Requirement","ECSS-Q-ST-70-01_1650273",1,"Created","The C&CCV shall provide the acceptability status of the contamination levels documented in the Table requested by requirement <6>a. regarding the impacted system performances."]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.2a","Requirement","ECSS-S-ST-00_1000001",1,"Unchanged","The customer shall select which ECSS Standards to make applicable and to use to establish the project/product requirements, including use of ECSS-S-ST-00-01 for terms and definitions.\n"]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.2b","Requirement","ECSS-S-ST-00_1000002",1,"Unchanged","The customer shall define, as part of the project requirements documentation (PRD), the set of requirements tailored from ECSS documents to the project specificities which are made applicable.\n"]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.2c","Requirement","ECSS-S-ST-00_1000003",1,"Unchanged","The customer shall produce, as part of the PRD, a documentation identifying the ECSS requirements applicable to the project.\n","NOTE \tAn “ECSS applicable requirements matrix” (EARM) is a recommended method for this component of the PRD.\n"]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.2d","Requirement","ECSS-S-ST-00_1000004",1,"Unchanged","The documentation identifying the requirements applicable to the project shall include following data (e.g. EARM):\n1.\tThe complete list of ECSS standards either fully or partially applicable to the project/product, including any standard (ECSS or not) made applicable via the chain of normative references;\n2.\tFor each partially applicable standard, the status of each requirement:\napplicable without modification\napplicable with modification\nnot applicable\n3.\tThe complete list of additional requirements\n4.\tFor modified and additional requirements, their complete formulation \n"]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.3a","Requirement","ECSS-S-ST-00_1000005",1,"Unchanged","The supplier shall demonstrate compliance with the PRD requirements.\n","NOTE \tAn “ECSS compliance matrix” (ECM) is a recommended method to document the demonstration of this compliance. The ECM is part of the project compliance matrix, addressing compliance to the applicable ECSS requirements (e.g. EARM).\n"]
["ECSS-S-ST-00C Rev.1","ECSS - Current v1.0","9.3b","Requirement","ECSS-S-ST-00_1000006",1,"Unchanged","The documentation identifying the compliance to ECSS requirements applicable to the project (e.g. the ECM) shall include following data:\n1.\tThe complete list of ECSS requirements applicable to the project (e.g. in the EARM).\n2.\tFor each requirement, the actual indication of compliance. When deviation is identified the justification is provided.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1a","Requirement","ECSS-U-ST-20_1430001",1,"Created","The PPAA shall provide to the supplier planetary protection related obligations of relevant external authorities.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1b","Requirement","ECSS-U-ST-20_1430002",1,"Created","The supplier shall prepare a preliminary Planetary Protection Requirements document in conformance with the DRD in Annex A during the Phase A and no later than the PRR.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1c","Requirement","ECSS-U-ST-20_1430003",1,"Created","For missions that target or encounter multiple Solar system bodies, the preliminary Planetary Protection Requirements document shall include requirements for all the protected Solar system bodies.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1d","Requirement","ECSS-U-ST-20_1430004",1,"Created","The Planetary Protection Requirements document shall be subject to approval by the PPAA and released at the latest at SRR.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1e","Requirement","ECSS-U-ST-20_1430005",1,"Created","The delivery of hardware and services to a third-party mission with planetary protection constraints shall be subject to approval by the PPAA.\n","NOTE \tThe customer of the mission lead of the third-part mission bears the overall planetary protection responsibility at mission level, including assigning, monitoring, reviewing and approving planetary protection categories and associated requirements.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1f","Requirement","ECSS-U-ST-20_1430006",1,"Created","Impact of significant changes in the mission concept on the planetary protection requirements and implementation approach shall be assessed by the supplier and are subject to approval by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.1g","Requirement","ECSS-U-ST-20_1430007",1,"Created","The PPAA, or its designated entity, shall conduct independent verification assays on flight hardware and controlled environments, including launch site, during the course of the project at times and intervals planned and agreed with the supplier.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.2.1a","Requirement","ECSS-U-ST-20_1430008",1,"Created","Except as specified in 5.3.2.1d, all flight hardware subject to planetary protection constraints shall be assembled and maintained until and including launch in ISO class 8 cleanrooms “in operation”, or better, as specified in ECSS-Q-ST-70-01.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.2.2a","Requirement","ECSS-U-ST-20_1430009",1,"Created","A probability of impact analysis on protected Solar system bodies shall be performed and a report delivered for customer and PPAA review.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.2.2b","Requirement","ECSS-U-ST-20_1430010",1,"Created","The probability of impact analysis specified in 5.2.2a shall include:\n1.\tSingle and multiple pass analysis;\n2.\tHardware, software and operational reliability;\n3.\tMeteoroid impacts and effects on spacecraft reliability;\n(a)\tMeteoroid model (e.g., IMEM 1.1) and parameters (fluence, directionality, velocity, density and margins) as defined in the project applicable environmental specifications\n(b)\tDamage equations in IADC-WD-00-03 for the damage assessment\n4.\tSpacecraft state including location, and velocity vector;\n5.\tManoeuvre and planet and satellite ephemeris uncertainty;\n6.\tStochastic variability of the atmospheric density with the amplitude of the Solar cycle estimated for the mission and sun epoch.\n","NOTE \t1\tDifferent meteoroid models are used depending on the mission profile; dedicated models are currently developed for the Jovian system.\nNOTE \t2\tRequirements that need a probability of impact analysis to demonstrate compliance are described in 5.3.2.1d, 5.3.2.1e.1, and 5.3.3.1b.4.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.2.3a","Requirement","ECSS-U-ST-20_1430011",1,"Created","Except where numerical requirements are otherwise specified in this document, the probability of contaminating a Solar system body with viable terrestrial organisms shall be ≤ 1x10-3 over a period of 50 years after the arrival of the mission at the protected Solar system body.\n","NOTE \tDescription how compliance to this requirement will be demonstrated needs to be described in the Planetary Protection Plan DRD in B.2.1a.3.(e).\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.1a","Requirement","ECSS-U-ST-20_1430012",1,"Created","An organic materials inventory of bulk constituents present in quantities above the limit agreed with the PPAA shall be provided by the project in conformance with DRD in Annex H.\n","NOTE \tThis also applies to missions not going to the Moon but having a final disposition that would end up on the Moon.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.1a","Requirement","ECSS-U-ST-20_1430013",1,"Created","An organic materials inventory of bulk constituents present on the spacecraft in quantities ≥1 kg shall be provided by the supplier in conformance with DRD in Annex H.\n","NOTE \tThis requirement is not applicable in case requirement 5.3.2.1e.1 is met.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.1b","Requirement","ECSS-U-ST-20_1430014",1,"Created","A 50 gram sample for each organic material used on the spacecraft in quantities ≥25 kg shall be provided by the supplier and stored by the customer under controlled conditions for 50 years after launch.\n","NOTE \tThis requirement is not applicable in case requirement  5.3.2.1e.1 is met.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.1c","Requirement","ECSS-U-ST-20_1430015",1,"Created","Compliance to all bioburden requirements shall be verified pre-launch.\n","NOTE \tThis verification is usually done on last physical access of the flight hardware or hardware elements, i.e., at delivery of flight hardware to next level contractor, delivery to launch site, and at the launch site prior to fairing closure.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.1d","Requirement","ECSS-U-ST-20_1430016",1,"Created","The probability of impact on Mars by any element not assembled and maintained in at least ISO class 8 conditions shall be ≤ 1x10-4 for the first 50 years after launch for nominal and off-nominal flight conditions.\n","NOTE \tExamples are upper stages.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.1e","Requirement","ECSS-U-ST-20_1430017",1,"Created","One of the following conditions shall be met:\n1.\tThe probability of impact on Mars by any part of a spacecraft assembled and maintained in ISO class 8 conditions, or better, is ≤ 1x10-2 for the first 20 years after launch, and ≤ 5x10-2 for the time period from 20 to 50 years after launch for nominal and off-nominal flight conditions.\n2.\tThe total bioburden of the spacecraft on Mars, including surface, mated, and encapsulated bioburden, is ≤ 5x105 bacterial spores.\n","NOTE \tThis requirement is also applicable for fly-by and gravity assist manoeuvres.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2a","Requirement","ECSS-U-ST-20_1430018",1,"Created","The bioburden of the landed system on Mars shall be ≤ 3x105 bacterial spores on exposed internal and external surfaces.\n","NOTE \tAttention – for bioburden allocations to hardware and payload suppliers take into account re-contamination during different on-ground phases (e.g., testing at sub-system and system level, launch).\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2b","Requirement","ECSS-U-ST-20_1430019",1,"Created","The average bioburden of the landed system on Mars shall be ≤ 300 bacterial spores/m2 on exposed internal and external surfaces.\n","NOTE \t1\tAttention – for bioburden allocations to hardware and payload suppliers take into account re-contamination during different on ground phases (e.g., testing at sub-system and system level, launch).\nNOTE \t2\tAttention – for large spacecraft systems the average bioburden to meet requirement 5.3.2.2.2a needs to be much lower than 300 bacterial spore/m2.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2c","Requirement","ECSS-U-ST-20_1430020",1,"Created","The supplier shall provide an analysis or assessment whether the spacecraft during nominal and off-nominal conditions has the potential to modify the local martian environment in a way that can create a Mars special region.\n","NOTE \tSuch an analysis or assessment is in particular important for spacecraft using radioisotope heat sources targeting areas with surface or sub-surface water ice.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2d","Requirement","ECSS-U-ST-20_1430021",1,"Created","Planned 3-sigma pre-launch landing ellipses shall be evaluated and documented on a case-by-case basis as part of the landing site selection process to determine whether the mission can land or come within contamination range of areas or volumes meeting the parameter definition for Mars Special Regions or impinge on already described features that can be treated as Mars Special Regions. \n","NOTE \tThis means at least no areas or volumes meeting the parameter definition for Mars Special Regions or already described features that can be treated as Mars Special Regions can be within the 3-sigma landing ellipse.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2e","Requirement","ECSS-U-ST-20_1430022",1,"Created","The evaluations specified in 5.3.2.2.2c and 5.3.2.2.2d shall be based on the latest scientific evidence and include an assessment of the extent to which the temperature and water activity values specified for Mars Special Regions are separated in time. \n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.2f","Requirement","ECSS-U-ST-20_1430023",1,"Created","The evaluation specified in 5.3.2.2.2d shall be updated during the mission whenever new evidence indicates that the landing ellipse and the operational environment contain, or are in contamination range of areas or volumes meeting the parameter definition for Mars Special Regions.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.3a","Requirement","ECSS-U-ST-20_1430024",1,"Created","For surface mission with life detection one of the following conditions shall be met:\n1.\tThe bioburden of the surface system on Mars is ≤ 30 bacterial spores on exposed internal and external surfaces, or at a contamination level driven by the nature and sensitivity of the particular life-detection investigations.\n2.\tThe average bioburden of the subsystems that are involved in the acquisition, delivery, and analysis of samples used for life-detection investigations is either:\n(a)\t≤ 0,03 bacterial spores/m2, or\n(b)\tat a contamination level driven by the nature and sensitivity of the particular life-detection investigations.\n","NOTE \tThe contamination level driven by the particular life-detection investigation needs to be described in the Planetary Protection Plan DRR, Annex B.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.3b","Requirement","ECSS-U-ST-20_1430025",1,"Created","The specific contamination level driven by the nature and sensitivity of the particular life-detection investigation described in 5.3.2.2.3a.1 and 5.3.2.2.3a.2(b) shall be subject to review and approval by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.3c","Requirement","ECSS-U-ST-20_1430026",1,"Created","Recontamination prevention of the subsystems specified in 5.3.2.2.3a.2 and the samples to be analysed shall be in place until the end of the life-detection investigations.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.4a","Requirement","ECSS-U-ST-20_1430027",1,"Created","If a Mars special region is within the 3-sigma landing ellipse, the bioburden of the entire surface system on Mars shall be ≤ 30 bacterial spores on exposed internal and external surfaces.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.4b","Requirement","ECSS-U-ST-20_1430028",1,"Created","If a Mars special region is accessed through horizontal or vertical mobility, one of the following conditions shall be met:\n1.\tThe bioburden of the entire surface system on Mars is ≤ 30 bacterial spores on exposed internal and external surfaces.\n2.\tThe subsystems which directly contact the Mars special region are sterilized to levels specified in 5.3.2.2.4b.1, and a method of preventing their recontamination prior to accessing the Mars special region is in place.\n","NOTE \tExample of accessing Mars special regions are by roving (horizontal mobility) or by drilling (vertical mobility).\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.2.4c","Requirement","ECSS-U-ST-20_1430029",1,"Created","If an off-nominal condition can cause a high probability of inadvertent biological contamination of a Mars special region by the spacecraft the bioburden shall be the following:\n1.\tThe bioburden of the entire surface system on Mars is ≤ 30 bacterial spores on exposed internal and external surfaces, and \n2.\tThe total surface, mated, and encapsulated bioburden level on Mars is ≤ 30 + 1,5 x 104 bacterial spores.\n","NOTE \tExample for off-nominal condition is a hard landing.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3a","Requirement","ECSS-U-ST-20_1430030",1,"Created","Requirements in clause 5.3.2.2.3 shall be applied to the outbound leg of a Mars sample return mission.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3b","Requirement","ECSS-U-ST-20_1430031",1,"Created","The severity of potential consequences of releasing unsterilized material from Mars and flight hardware that has been exposed to unsterilized material from Mars into the terrestrial environment shall be categorised as catastrophic in accordance with ECSS-Q-ST-40.\n","NOTE \tThe categorization of this severity level is not because a catastrophic consequence is expected but only following the precautionary principle due to the large number of unknowns.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3c","Requirement","ECSS-U-ST-20_1430032",1,"Created","Safety critical functions as defined in 3.2.19 shall be treated as severity function criticality level 1 in accordance with ECSS-Q-ST-40.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3d","Requirement","ECSS-U-ST-20_1430033",1,"Created","The probability that a single unsterilized martian particle of ≥ 0,01 μm in diameter is released into the terrestrial environment shall be ≤ 1x10-6 for the first 100 years after launch from Mars.\n","NOTE \t1\tRational for this requirement is to “break the chain of contact” between Mars and Earth.\nNOTE \t2\tSource and context for numerical values in [5].\nNOTE \t3\tThe term ‘particle’ includes material from Mars and flight hardware exposed to material from Mars.\nNOTE \t4\tIf the size requirement of 0,01 μm cannot be met without decreasing the overall level of assurance for the non-release of such a particle, the release of a single unsterilised particle of up to 0,05 μm can be considered as a potentially tolerable systems-level adjustment, assuming that it has been demonstrated that this size is the lowest achievable at a reasonable cost (BAT approach) and it has been independently reviewed.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3e","Requirement","ECSS-U-ST-20_1430034",1,"Created","A quantitative PRA shall be conducted as part of evaluating the risk of releasing unsterilized material from Mars and flight hardware that has been exposed to unsterilized material from Mars into the terrestrial environment.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.2.3f","Requirement","ECSS-U-ST-20_1430035",1,"Created","No unsterilised portion of the materials returned from Mars shall be released from containment unless approved by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.1a","Requirement","ECSS-U-ST-20_1430036",1,"Created","The probability of inadvertent contamination of a subsurface ocean by viable terrestrial organisms shall be ≤ 1 x 10-4 per mission.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.1b","Requirement","ECSS-U-ST-20_1430037",1,"Created","The calculation of the probability specified in 5.3.3.1a of inadvertent contamination shall address the following factors, at a minimum:\n1.\tBioburden at launch;\n2.\tCruise survival for bioburden;\n3.\tBioburden survival in the respective radiation environment;\n4.\tProbability of landing on Solar system body;\n5.\tThe mechanisms and timescales of transport to the subsurface;\n6.\tBioburden survival and proliferation before, during, and after subsurface transfer.\n","NOTE \tMethods of bioburden reduction reflect the type of environments found on Europa or Enceladus, focusing on terrestrial organisms most likely to survive on Europa or Enceladus, such with cold, desiccation and radiation tolerance. \n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.1c","Requirement","ECSS-U-ST-20_1430038",1,"Created","When computing the calculation of requirement 5.3.3.1b the estimate for poorly known parameters shall be subject to approval by the customer and the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.2.2a","Requirement","ECSS-U-ST-20_1430039",1,"Created","Requirements in clause 5.3.2.2.3, shall be applied to the outbound leg of a sample return mission.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.2.2b","Requirement","ECSS-U-ST-20_1430040",1,"Created","The severity of potential consequences of releasing unsterilized material from Europa or Enceladus and flight hardware that were exposed to unsterilized material from Europa or Enceladus into the terrestrial environment shall be categorised as catastrophic in accordance with ECSS-Q-ST-40.\n","NOTE \tThe categorization of this severity level is not because a catastrophic consequence is expected but only following the precautionary principle due to the large number of unknowns.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.2.2c","Requirement","ECSS-U-ST-20_1430041",1,"Created","Safety critical functions as defined in 3.2.19 shall be treated as severity function criticality level 1 in accordance with ECSS-Q-ST-40.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.3.2.2d","Requirement","ECSS-U-ST-20_1430042",1,"Created","No unsterilised portion of the materials returned from Europa or Enceladus shall be released from containment unless approved by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.1a","Requirement","ECSS-U-ST-20_1430043",1,"Created","Categorization of missions to small Solar system bodies shall be made on a case-by-case basis.\n","NOTE \tThe small Solar system bodies (SB) not elsewhere discussed in this document represent a large class of objects. Most missions to SB are classified as Category I or Category II missions for forward contamination, and Category V, unrestricted Earth return, for backward contamination.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.1b","Requirement","ECSS-U-ST-20_1430044",1,"Created","The mission shall be categorized as “restricted Earth return” if the answer to all the following six questions is \"no\" or “uncertain”, otherwise the mission is categorized as “unrestricted”:\n1.\tDoes scientific evidence indicate that there was never liquid water in or on the target body?\n2.\tDoes scientific evidence indicate that metabolically useful energy sources were never present?\n3.\tDoes scientific evidence indicate that there was never sufficient organic matter or CO2 or carbonates and an appropriate source of reducing equivalents in or on the target body to support life?\n4.\tDoes scientific evidence indicate that subsequent to the disappearance of liquid water, the target body has been subjected to extreme temperatures >160 °C?\n5.\tDoes scientific evidence indicate that there is or was sufficient radiation for sterilization of terrestrial life forms?\n6.\tDoes scientific evidence indicate that there has been a natural influx to Earth, via meteorites, of material equivalent to a sample returned from the target body?\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.1c","Requirement","ECSS-U-ST-20_1430045",1,"Created","If a mission is categorized as “restricted Earth return” in accordance with 5.3.4.1b, procedures shall be applied to the mission as specified in requirements from clause 5.3.4.2\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.2.2a","Requirement","ECSS-U-ST-20_1430046",1,"Created","Category IVb requirements in clause 5.3.2.2.3, shall be applied to the outbound leg of a sample return mission.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.2.2b","Requirement","ECSS-U-ST-20_1430047",1,"Created","The severity of potential consequences of releasing unsterilized material from specific small solar system bodies and flight hardware that has been exposed to unsterilized material from specific small solar system bodies into the terrestrial environment shall be categorised as catastrophic in accordance with ECSS-Q-ST-40.\n","NOTE \tThe categorization of this severity level is not because a catastrophic consequence is expected but only following the precautionary principle due to the large number of unknowns..\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.2.2c","Requirement","ECSS-U-ST-20_1430048",1,"Created","Safety critical functions as defined in 3.2.19 shall be treated as severity function criticality level 1 in accordance with ECSS-Q-ST-40.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.3.4.2.2d","Requirement","ECSS-U-ST-20_1430049",1,"Created","No unsterilised portion of the materials returned from Mars shall be released from containment unless approved by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.1a","Requirement","ECSS-U-ST-20_1430050",1,"Created","Requirements from clause 5 of ECSS-Q-ST-70-58 shall be applied for bioburden controlled environments.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2a","Requirement","ECSS-U-ST-20_1430051",1,"Created","Bioburden assessment on flight hardware shall be performed, using procedures \"Swab assay 1 (standard swab assay)\" or \"Wipe assay 1 (standard wipe assay) \"as per procedures D.1 and E.1 from Annex D and Annex E of ECSS-Q-ST-70-55.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2b","Requirement","ECSS-U-ST-20_1430052",1,"Created","If direct assays are not possible, estimation of the flight hardware bioburden using the highest number in the respective category of Table 5‑1 shall be used.\n","NOTE \tThe encapsulated bioburden values in Table 5‑1 cannot be used for ALM produced hardware.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2c","Requirement","ECSS-U-ST-20_1430054",1,"Created","Use of assay procedures not described in Annex D, Annex E, Annex F and Annex G of ECSS-Q-ST-70-55 shall be approved by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2d","Requirement","ECSS-U-ST-20_1430055",1,"Created","The number of samples to evaluate the bioburden for the flight hardware shall be agreed with the PPAA and meet the following conditions:\n1.\tFive swabs for each surface area on flight hardware of 0,1 m2;\n2.\tA proportionate number, but at least one swab, for each surface area on flight hardware smaller than 0,1 m2;\n3.\tOne wipe for each surface area on flight hardware in the size range of 1 m2;\n4.\tTwo wipes for each individual surface area on flight hardware per 10 m2.\n","NOTE \tAlthough the sampling plan is specific to the size and geometry of the sampled hardware, sampling at least 20 % of the surface area is a reasonable guideline. To reduce the conservatism in the overall bioburden calculations it is better to sample larger surface areas.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2e","Requirement","ECSS-U-ST-20_1430056",1,"Created","The methods for calculation surface bioburden and bioburden densities shall be agreed with PPAA. \n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.2f","Requirement","ECSS-U-ST-20_1430057",1,"Created","Bioburden prior to the application of a bioburden reduction procedure shall be established by using procedures specified in requirements 5.4.2a or 5.4.2b.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.3a","Requirement","ECSS-U-ST-20_1430058",1,"Created","Biodiversity assessment on flight hardware and bioburden controlled environment(s) shall be performed using procedures D.3-D.6 for Swab assays and procedures E.3-E.6 for Wipe assays as per Annex D and Annex E of ECSS-Q-ST-70-55.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.4a","Requirement","ECSS-U-ST-20_1430059",1,"Created","Dry heat microbial reduction shall be performed in compliance with requirements from clause 5 of ECSS-Q-ST-70-57.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.4b","Requirement","ECSS-U-ST-20_1430060",1,"Created","Hydrogen peroxide microbial reduction shall be performed in compliance with requirements from clause 5 of ECSS-Q-ST-70-56.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.4c","Requirement","ECSS-U-ST-20_1430061",1,"Created","Use of other bioburden reduction procedures shall be approved by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.4.4d","Requirement","ECSS-U-ST-20_1430062",1,"Created","Evaluation of material and hardware compatibility with bioburden reduction procedures shall be performed in compliance with requirements from clause 5 of ECSS-Q-ST-70-53.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.5a","Requirement","ECSS-U-ST-20_1430063",1,"Created","Planetary protection documentation shall be provided according to the matrix in Table 5‑2.\n","NOTE \t1\tTable 5‑2 can be tailored to the respective project.\nNOTE \t2\tDocumenting the implementation of planetary protection requirements is not limited to the dedicated planetary protection documents but needs to be reflected in the affected project documentation, e.g., management plan, quality plan, AIV and AIT plan, VCD.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.5b","Requirement","ECSS-U-ST-20_1430064",1,"Created","The supplier shall support the PPAA, for the preparation of the customer level planetary protection report of a mission.\n","NOTE \t1\tThe report is delivered no later than nine months after launch to the President of COSPAR and the chair of the COSPAR panel on planetary protection.\nNOTE \t2\tContent of the customer level planetary protection report to COSPAR is described in the COSPAR Planetary Protection Policy [2].\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.6a","Requirement","ECSS-U-ST-20_1430066",1,"Created","Planetary protection implementation activities and applicable planetary protection documentation specified in Table 5‑2, including any documentation to support conclusions of analysis, shall be reviewed during regular reviews to which PPAA participates.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.6b","Requirement","ECSS-U-ST-20_1430067",1,"Created","Planetary protection reviews shall be held for Earth return missions to authorize the different segments of the return phase:\n1.\tSubsequent to sample collection and prior to a manoeuvre to enter a Earth return trajectory;\n2.\tPrior to commitment for Earth entry.\n","NOTE \t1\tThe objective of these reviews is to demonstrate that the mission continues to meet the planetary protection requirements in general, and Earth safety in particular.\nNOTE \t2\tThe planetary protection reviews can be part of regular project reviews.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.7a","Requirement","ECSS-U-ST-20_1430068",1,"Created","ECSS-Q-ST-10-09 shall be applied for nonconformances and waivers.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.7b","Requirement","ECSS-U-ST-20_1430069",1,"Created","All nonconformance related to planetary protection shall be specified as major nonconformance.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.7c","Requirement","ECSS-U-ST-20_1430070",1,"Created","The disposition of nonconformances related to planetary protection requirements shall be subject to approval by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","5.7d","Requirement","ECSS-U-ST-20_1430071",1,"Created","The approval of waivers related to planetary protection requirements shall be subject to approval by the PPAA.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","A.2.1a","Requirement","ECSS-U-ST-20_1430072",1,"Created","The planetary protection requirements document shall include at least the following items:\n1.\tMission description\n(a)\tScientific objectives and payload description\n(b)\tMission type fly-by, orbiter, lander, Earth return\n(c)\tDescription of mission phases\n(d)\tDescription of launch vehicle and launch site\n(e)\tIdentification of targeted and encountered Solar system bodies\n(f)\tIdentification and use of nuclear heat and power sources\n(g)\tIdentification and use of aerobraking and aerocapture manoeuvres\n(h)\tDescription of entry, descent and landing phases\n(i)\tDescription of intended landing site and expected landing accuracy\n(j)\tIntended final disposition of all launched hardware\n(k)\tDescription of international cooperation\n2.\tPlanetary protection category\n3.\tPlanetary protection management requirements, tailored ECSS-U-ST-20\n4.\tTechnical planetary protection requirements, tailored ECSS-U-ST-20\n5.\tPlanetary protection methods and procedures, tailored ECSS-U-ST-20\n6.\tPlanetary protection documentation and reviews, tailored ECSS-U-ST-20\n","NOTE \tPlanetary protection requirements for the payload are usually described in the payload interface requirements.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","A.2.2a","Permission","ECSS-U-ST-20_1430073",1,"Created","The Mission description, specified in A.2.1a.1, may be covered by a reference to another project document.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","B.2.1a","Requirement","ECSS-U-ST-20_1430074",1,"Created","The planetary protection plan shall include the following items:\n1.\tMission description.\n2.\tAssessment of the consequences to implement the planetary protection requirements with respect to design, development, schedule and operations.\n3.\tGeneral implementation approach:\n(a)\tPlanetary protection management and organisation.\n(b)\tDescription of bioburden control approach for all major flight hardware elements, including payload and launch recontamination.\n(c)\tDescription of bioburden allocations with identified margins and uncertainties for all major flight hardware elements.\n(d)\tDescription of bioburden control approach and/or contamination control approach for life-detection investigation, in accordance with ECSS-U-ST-20 requirement 5.3.2.2.3a.\n(e)\tDescription of probability of impact analysis, in accordance with ECSS-U-ST-20 requirements 5.2.2a, 5.2.2b, 5.3.2.1d, 5.3.2.1e including: \n(1)\tImpact analysis for launcher and spacecraft elements against target bodies identified in the “planetary protection requirements” document, with analysis supporting the conclusions providing evidence that the selected approach is feasible for the specific mission; \n(1)\tIf probability of impact approach is not possible or selected, break-up, burn-up and general atmospheric entry heating analysis providing evidence that the selected approach is feasible for the specific mission.\n(f)\tDescription of probability of contamination analysis, in accordance with ECSS-U-ST-20 requirements 5.2.3a, 5.3.2.2.2c, d, e, f, 5.3.2.2.3c and 5.3.3.2.2a.\n(g)\tDescription for methods and procedures to be used, in accordance with ECSS-U-ST-20 requirements in clause 5.4.\n(h)\tDescription of planned requests for using methods, procedures or values not described in this standard, in accordance with ECSS-U-ST-20 requirements in clause 5.7.\n4.\tPlanetary protection documentation and reviews, in accordance with ECSS-U-ST-20 requirements in clauses 5.5 and 5.6.\n5.\tIdentify planetary protection activities and events in the project schedule.\n6.\tCompliance matrix against the planetary protection requirements.\n7.\tAnalysis and conclusions of consequences for planned non-conformances or waivers.\n8.\tVerification matrix against the planetary protection requirements.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","B.2.2a","Permission","ECSS-U-ST-20_1430075",1,"Created","The Mission description, as per B.2.1a.1. may be covered by a reference to another project document.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","B.2.2b","Permission","ECSS-U-ST-20_1430076",1,"Created","The Assessment of the consequences, as per B.2.1a.2. may summarize the consequences with references to other project documentation for detailed descriptions.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","B.2.2c","Permission","ECSS-U-ST-20_1430077",1,"Created","The compliance matrix, as per B.2.1a.6. may be included in a project level compliance and verification matrix.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","B.2.2d","Permission","ECSS-U-ST-20_1430078",1,"Created","The Verification matrix as per B.2.1a.8. may be included in a project level compliance and verification matrix.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","C.2.1a","Requirement","ECSS-U-ST-20_1430079",1,"Created","The planetary protection implementation plan shall include the following items:\n1.\tFlight system description\n(a)\tHardware description\n(1)\tSystem and sub-system description, including payload\n(2)\tPlanetary protection description vs. subsystem names\n(b)\tCriteria for exposed surfaces and planetary protection accountable volumes\n(c)\tMission planetary protection issues as they are intended to be implemented, accounting for the following data: \n(1)\tProbability of impact analysis, in accordance with ECSS-U-ST-20 requirements 5.2.2a, 5.2.2b, 5.3.2.1d, 5.3.2.1e; \n(2)\tProbability of contamination analysis in accordance with ECSS-U-ST-20 requirements 5.2.3a, 5.3.3.2.2a;\n(3)\tSpacecraft induced special regions, in accordance with ECSS-U-ST-20 requirement 5.3.2.2.2c; \n(4)\tLanding site selection; \n(5)\tDraft organic material inventory in accordance with ECSS-U-ST-20 requirements 5.3.1a, 5.3.2.1a.\n2.\tDescription of Facilities\n(a)\tFormal system including \n(1)\tRisk assessment;\n(2)\tAlerts and action levels;\n(3)\tControl approach.\n(b)\tCommissioning\n(c)\tOperation\n3.\tBioburden control plan for the flight system\n(a)\tBioburden allocation including:\n(1)\tExposed surface bioburden allocation; \n(2)\tTotal bioburden allocation;\n(3)\tHardware exceptions.\n(b)\tSampling and Assay plan including:\n(1)\tFraction of exposed surfaces sampled;\n(2)\tNumber of samples; \n(3)\tSampling site selection;\n(4)\tSampling schedule.\n(c)\tStatistical treatment of the assay results including:\n(1)\tCase for total spore count greater than one;\n(2)\tCase for total spore count of zero or one;\n(3)\tCase for treatment of bulk assay;\n(4)\tBasis for bioburden density standard deviation;\n(5)\tAssay results acceptance guidelines.\n(d)\tBioburden assessment, in accordance with ECSS-U-ST-20 requirements 5.4.1a, and requirements from clause 5.4.2 including: \n(1)\tCalculation of surface bioburden density and number of spores from assay data;\n(2)\tSurface bioburden density and number of spores without assay data;\n(3)\tSurface bioburden density and number of spores for hardware treated by a bioburden reduction procedures;\n(4)\tEncapsulated bioburden density and number of spores with assay data;\n(5)\tEncapsulated bioburden density and number of spores without assay data.\n(e)\tBiodiversity assessment, in accordance with ECSS-U-ST-20 requirement 5.4.3a.\n4.\tBioburden reduction plan for the flight system, in accordance with ECSS-U-ST-20 requirements in clause 5.4.4\n(a)\tSpacecraft hardware subject to bioburden reduction processes;\n(b)\tProcess analysis;\n(c)\tProcess verification and control;\n(d)\tRecontamination prevention approach.\n5.\tGeneral implementation approach for the flight system\n(a)\tPre-AIV, AIT and launch operations including: \n(1)\tGeneral approach at hardware manufacturing sites;\n(2)\tGeneral approach at Customer, supplier and instrument provider site.\n(b)\tAIV, AIT and launch operations including: \n(1)\tAcceptance criteria; \n(2)\tGeneral approach at Customer and supplier and payload provider site; \n(3)\tGeneral approach at test site; \n(4)\tGeneral approach at launch site.\n(c)\tInside surface of the launch vehicle fairing, launch vehicle air conditioning, and white room air conditioning.\n(d)\tUpper stage and propulsion module.\n6.\tUpdated list of the foreseen waivers and NCRs and the associated impact analysis.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","D.2.1a","Requirement","ECSS-U-ST-20_1430080",1,"Created","The pre-launch planetary protection report shall include the following items:\n1.\tDeviation from planetary protection requirements and plan;\n2.\tDeviation from the planetary protection implementation plan;\n3.\tResults of contamination control measures, including raw and processed data of bioburden assays for the entire product tree;\n4.\tUpdate of probability of impact analysis, in accordance with ECSS-U-ST-20 requirements 5.2.2a, 5.2.2b, 5.3.2.1d, 5.3.2.1e;\n5.\tUpdate for probability of contamination analysis in accordance with ECSS-U-ST-20 requirements 5.2.3a, 5.3.3.2.2a;\n6.\tOrganic materials inventory, in accordance with ECSS-U-ST-20 requirements 5.3.1a, 5.3.2.1a;\n7.\tConclusions of the report.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","E.2.1a","Requirement","ECSS-U-ST-20_1430081",1,"Created","The post-launch planetary protection report shall include the following items:\n1.\tGround processing affecting bioburden control;\n2.\tLast verification assay results;\n3.\tLaunch events affecting bioburden control;\n4.\tPost Launch effects within the deployment and in orbit commissioning timeframe;\n5.\tConclusions of the report.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","F.2.1a","Requirement","ECSS-U-ST-20_1430082",1,"Created","The extended mission planetary protection report shall include the following items:\n1.\tDeviation from planetary protection requirements and plan;\n2.\tDeviation from the planetary protection implementation plan;\n3.\tUpdate of probability of impact analysis, in accordance with ECSS-U-ST-20 requirements 5.2.2a, 5.2.2b, 5.3.2.1d, 5.3.2.1e;\n4.\tUpdate for probability of contamination analysis, in accordance with ECSS-U-ST-20 requirements 5.2.3a, 5.3.3.2.2a;\n5.\tConclusions of the report.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","G.2.1a","Requirement","ECSS-U-ST-20_1430083",1,"Created","The end-of-mission planetary protection report shall include the following items:\n1.\tDisposition and condition of all launched flight hardware including the launcher upper stage, either in space describing the orbital parameters or for landed or impacting elements by position on the target body;\n2.\tDeviation from planetary protection requirements and plan;\n3.\tDeviation from the planetary protection implementation plan;\n4.\tUpdate of probability of impact analysis in accordance with ECSS-U-ST-20 requirements 5.2.2a, 5.2.2b, 5.3.2.1d, 5.3.2.1e;\n5.\tUpdate for probability of contamination analysis, in accordance with ECSS-U-ST-20 requirements 5.2.3a, 5.3.3.2.2a;\n6.\tConclusions of the report.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","H.2.1a","Requirement","ECSS-U-ST-20_1430084",1,"Created","The organic material inventory shall include the following for each organic material present above a specified limit agreed with PPAA:\n1.\tIdentity;\n2.\tChemical composition;\n3.\tUsage, with respect to product tree;\n4.\tMass estimate using the mass codes specified in ECSS-Q-ST-70-01;\n5.\tRating and reference for outgassing for each item using ECSS-Q-ST-70-01;\n6.\tSupplier for each item.\n"]
["ECSS-U-ST-20C","ECSS - Current v1.0","H.2.1b","Requirement","ECSS-U-ST-20_1430085",1,"Created","For missions to the Moon, including fly-by-gravity assist, a description of the products released by the propulsion and life-support system, as applicable, into the lunar environment shall be provided, including:\n1.\tA quantitative and qualitative description of the major chemical species, and\n2.\tAn indication of the minor chemical species and quantity.\n"]
["ECSS-U-AS-10C Rev.2","ECSS - Current v1.0","3a","Requirement","ECSS-U-AS-10_1300001",3,"Normative Change","ISO 24113:2023, Space systems - Space debris mitigation requirements, fourth edition 2023-05 shall apply with the modifications and clarifications listed in Table 3‑1."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.2.2a","Requirement","ECSS-I-ST-30-10_1610001",1,"Created","The IPS function shall analyse requirements for the system issued by the customer in conformance with the Mission Description Document (MDD) and provide the IPS requirements."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.2.2b","Requirement","ECSS-I-ST-30-10_1610002",1,"Created","The IPS function shall ensure the IPS requirements traceability."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.2.2c","Requirement","ECSS-I-ST-30-10_1610003",1,"Created","The IPS function shall ensure that each requirement for the lower-level elements has been validated and verified."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.2.3a","Requirement","ECSS-I-ST-30-10_1610004",1,"Created","The supplier shall establish an IPS function in the project."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.2.3b","Requirement","ECSS-I-ST-30-10_1610005",1,"Created","The supplier shall issue an IPS plan in conformance with Annex A.","NOTE\tThe IPS plan is called by the System Engineering Plan (SEP).\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.2.3a","Requirement","ECSS-I-ST-30-10_1610006",1,"Created","The PSA function shall issue a PSA Plan, in conformance with the DRD in Annex B."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.2.3b","Requirement","ECSS-I-ST-30-10_1610007",1,"Created","The PSA function shall validate and verify the PSA requirements."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.2.3c","Requirement","ECSS-I-ST-30-10_1610008",1,"Created","The supplier shall use the PSA Record Database to monitor all the logistic data."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.2.3d","Requirement","ECSS-I-ST-30-10_1610009",1,"Created","The PSA function shall manage the central repository PSA Record Database."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.3.3a","Requirement","ECSS-I-ST-30-10_1610010",1,"Created","The PSA function shall provide maintenance plan.","NOTE\tThe maintenance plan contains preventive and corrective operations.\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.3.3b","Requirement","ECSS-I-ST-30-10_1610011",1,"Created","The PSA function shall monitor and record IPS performance targets in the PSAR.","NOTE\tThe IPS plan is called by the System Engineering Plan (SEP). \n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.4.3a","Requirement","ECSS-I-ST-30-10_1610012",1,"Created","The IPS function shall identify at early stage of system development the resources and skill needed."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.5.3a","Requirement","ECSS-I-ST-30-10_1610013",1,"Created","The PSA function shall specify a list of needed Support Equipment and include this into the product tree.","NOTE\tExamples of support equipment are: GSE, GHS, test benches and electronic tools.\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.6.3a","Requirement","ECSS-I-ST-30-10_1610014",1,"Created","The PSA function shall specify the Software Support Analysis (SSA)."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.6.3b","Requirement","ECSS-I-ST-30-10_1610015",1,"Created","The supplier shall establish and maintain a Software Support Analysis (SSA) during the complete project life cycle."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.7.3a","Requirement","ECSS-I-ST-30-10_1610016",1,"Created","The PSA function shall ensure the assessment of the maintenance procedures is completed before entry into service."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.8.3a","Requirement","ECSS-I-ST-30-10_1610017",1,"Created","The IPS shall deliver the training needs analysis and the material resource availability before entry into service."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.9.3a","Requirement","ECSS-I-ST-30-10_1610018",1,"Created","The IPS function shall specify and verify the Information System (IS) requirements before entry into service."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.10.3a","Requirement","ECSS-I-ST-30-10_1610019",1,"Created","The IPS function shall specify and verify the Facilities and Infrastructures requirements before entry into service."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.11.3a","Requirement","ECSS-I-ST-30-10_1610020",1,"Created","The PHST requirements shall be consolidated with PSA requirements at early stage of system development.","NOTE\tIt is good practice to perform the consolidation before the Preliminary Design Review (PDR).\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.12.3a","Requirement","ECSS-I-ST-30-10_1610021",1,"Created","The IPS function shall specify and agree obsolescence strategy with Customer at early stage of system development ","NOTE\tIt is good practice to agree on the obsolescence strategy before the Preliminary design review (PDR).\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","5.3.13.3a","Requirement","ECSS-I-ST-30-10_1610022",1,"Created","The PSA function shall agree and issue a list of spares before validating the Design Solution and agreed with Customer. ","NOTE\tThe list of spares is an output of the PSA Plan that is described in Annex B.\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<1>a","Requirement","ECSS-I-ST-30-10_1610023",1,"Created","The IPSP shall specify the purpose, objective and the reason for its preparation."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<2>a","Requirement","ECSS-I-ST-30-10_1610024",1,"Created","The IPSP shall list the applicable and reference documents used in support of the generation of the document."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<3>a","Requirement","ECSS-I-ST-30-10_1610025",1,"Created","The IPSP shall contain a high-level description of the space system mission requirements to IPS system and its elements."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<4>a","Requirement","ECSS-I-ST-30-10_1610026",1,"Created","The IPSP shall specify the objectives and constraints of the logistic support management process in conformance with the project management documents."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<4>b","Requirement","ECSS-I-ST-30-10_1610027",1,"Created","The IPSP shall contain the following information:\n1.\tA description of IPS management in terms of industrial organization,\n2.\tAn introduction to the IPS team,\n3.\tAn approach adopted to develop the IPS plan,\n4.\tA summary of the IPS concepts, or a reference to the document defining it, resulting from the analysis of the applicable documents, including:\n(a)\tdefinition of all the logistics needs, to cover the mission definition,\n(b)\toperation concept,\n(c)\tdefinition of the overall Maintenance concept.","NOTE\tThe Maintenance concept includes for example maintenance environment (hardware and software) and levels of maintenance (hardware and software) strategy.\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<4>c","Requirement","ECSS-I-ST-30-10_1610028",1,"Created","The IPSP shall include a description of the working relationship and interfaces among IPS elements with other disciplines, other project functions and organizations.","NOTE\tExamples of other disciplines include product assurance, RAMS, configuration management, system engineering.\n"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<4>d","Requirement","ECSS-I-ST-30-10_1610029",1,"Created","The IPSP shall include the schedule and the inter-dependency for all tasks in the IPS programme, integrating information from the IPSP of the elements of the support segment."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<4>e","Requirement","ECSS-I-ST-30-10_1610030",1,"Created","The IPSP shall describe the risk mitigation strategy."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<5>a","Requirement","ECSS-I-ST-30-10_1610031",1,"Created","The IPSP shall specify the development process of the support segment, its reviews and the milestones."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<5>b","Requirement","ECSS-I-ST-30-10_1610032",1,"Created","The IPSP shall specify the maintenance concept of the support segment throughout the entire project lifecycle."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<5>c","Requirement","ECSS-I-ST-30-10_1610033",1,"Created","The IPSP shall specify the monitoring concept of the support segment by mean of the KPI’s. "]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<5>d","Requirement","ECSS-I-ST-30-10_1610034",1,"Created","The IPSP shall specify how to analyse the data obtained through monitoring in order to improve the support segment throughout its lifecycle."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<6>a","Requirement","ECSS-I-ST-30-10_1610035",1,"Created","The IPSP shall specify the covered logistic activities to be performed and their implementation."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<6>b","Requirement","ECSS-I-ST-30-10_1610036",1,"Created","The IPSP shall identify the resources necessary to perform the logistic activities and their mapping into the project’s WBS."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<7>a","Requirement","ECSS-I-ST-30-10_1610037",1,"Created","The IPSP shall include or refer to the PSAP in conformance with Annex B. "]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<8>a","Requirement","ECSS-I-ST-30-10_1610038",1,"Created","The IPSP shall specify how information is managed within the IPS programme."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<8>b","Requirement","ECSS-I-ST-30-10_1610039",1,"Created","The IPSP shall describe how information needs are mapped into the information recording."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<8>c","Requirement","ECSS-I-ST-30-10_1610040",1,"Created","The IPSP shall specify the information security measures"]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<8>d","Requirement","ECSS-I-ST-30-10_1610041",1,"Created","The IPSP shall describe the measures to ensure the data quality, their integrity and consistency."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","A.2.1<9>a","Requirement","ECSS-I-ST-30-10_1610042",1,"Created","The IPSP shall describe the method to control and specify IPS‐related activities and requirements at suppliers’ and lower tier suppliers’ premises."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<1>a","Requirement","ECSS-I-ST-30-10_1610043",1,"Created","The PSAP shall contain a description of the purpose, objective and the reason for its preparation."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<2>a","Requirement","ECSS-I-ST-30-10_1610044",1,"Created","The PSAP shall list the applicable and reference documents used in support of the generation of the PSAP."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<3>a","Requirement","ECSS-I-ST-30-10_1610045",1,"Created","The PSAP shall describe the Product Support Analysis programme and its implementation."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<3>b","Requirement","ECSS-I-ST-30-10_1610046",1,"Created","The PSAP shall describe the management structure and authorities applicable to PSA, including the description of the interfaces with other IPS and non-IPS disciplines."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<4>a","Requirement","ECSS-I-ST-30-10_1610047",1,"Created","The PSAP shall specify the main PSA tasks and how these tasks are performed to cover the following:\n1.\tProgramme planning and control\n2.\tMission and support segment definition\n3.\tPreparation and evaluation of alternatives for the support segment\n4.\tDetermination of the logistic support requirements\n5.\tLogistic support assessment."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<5>a","Requirement","ECSS-I-ST-30-10_1610048",1,"Created","The PSAP shall describe the logistic data development, data documentation and data exchange."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<5>b","Requirement","ECSS-I-ST-30-10_1610049",1,"Created","The PSAP shall provide the following:\n1.\tScheme for uniquely identification of Logistic Data Records\n2.\tProcedures for updating and validating PSA data, including configuration control procedures\n3.\tDescription of the data collection system to be used to document, disseminate and control PSA and related design data."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<6>a","Requirement","ECSS-I-ST-30-10_1610050",1,"Created","The PSAP shall describe or make reference to the IPSP about the information management within the IPS programme."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<6>b","Requirement","ECSS-I-ST-30-10_1610051",1,"Created","The PSAP shall describe or make reference to the IPSP about the mapping of information needs into the envisaged information recording."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<6>c","Requirement","ECSS-I-ST-30-10_1610052",1,"Created","The PSAP shall describe or make reference to the IPSP about the information security measures."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<6>d","Requirement","ECSS-I-ST-30-10_1610053",1,"Created","The PSAP shall describe or make reference to the IPSP about the measures to ensure the data quality, their integrity and consistency."]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<7>a","Requirement","ECSS-I-ST-30-10_1610054",1,"Created","The PSAP shall contain the planning and the scheduling for each PSA iteration during the project phases after phase A. "]
["ECSS-I-ST-30-10C","ECSS - Current v1.0","B.2.1<7>b","Requirement","ECSS-I-ST-30-10_1610055",1,"Created","The PSAP shall identify all PSA tasks, schedule relationship with other IPS programme requirements and associated system engineering activities."]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}